NOTICE:  fast_boot:0

S
F
L
O
NOTICE:  efuse cpu_cfg = 0
W
NOTICE:  Booting Trusted Firmware
NOTICE:  BL1: v1.4(release):HR-ROM-Rel-v1.1-141-ga91d4dd-dirty
NOTICE:  BL1: Built : 11:24:44, Oct 23 2019
NOTICE:  Waiting connect ...
NOTICE:  boot src: 2
NOTICE:  GigaDev SPI NAND was found.
NOTICE:  Block size: 128 KiB, page size: 2048
NOTICE:  BL1: Booting BL2
Auth pass
NOTICE:  bl1_main exit
SPL cold boot flow
check_reset_state (0): wakeup address = 0x0, hw wakeup status = 0x0, wakeup src=0x100
patch for sys_pll 1200 with 100M eth
SFLOW_INIT
CHIP ID:PCB941/WAFER: W04/ X: X20/ Y: Y36
secondary_jump_to_spl: secure chip flow
X3 SPL : secondary core wake up and jump to spl done (cpu_core_cfg=0)
SFLOW_FIN_HW_A

U-Boot SPL 2018.09-g4ca851534c-dirty (May 11 2022 - 20:09:50 +0800)
SPACC Init - ID: (00000061)
SPL nand boot mode (from strap)
GigaDev SPI NAND was found.
Block size: 128 KiB, page size: 2048
ddr_type = 1 (LPDDR4)
hb_chip_package_type:3
load ddr header src_addr: 100000, load_addr: 802ca020, src_len: a00
find valid ddr image
ddr_hdr.ecc_gran: 0x0
ddr_hdr.ecc_map: 0x0
ddr_hdr.sbr_pattern0: 0x8bc9098c
ddr_hdr.sbr_pattern1: 0xcb9fabdf
ddr_freq = 05
board id = 31540334
ddr datarate: 3200
### SAMSUNG DDR ###
no ddr pin set
detect part number: 108
detect ddr freq: c80
board id alternative:0x3
index is 12
index is 15
index is 19
hb_ddr_index: 19
ddr_type = 1, ddr_vendor=3, ddr_freq=3200
dram_pll_init
sscg disabled
control load ddrc src_addr: 15ae00, load_addr: 802caa20, src_len: 920
[DDR INFO]      ==ddr_release_info==
[DDR INFO]      VERSION:        develop
[DDR INFO]      BUILD:          2022-05-11-20:09
[DDR INFO]      GIT COMMIT:     4ca851534c1616ace920fdaa000c6fb717c1fb74
[DDR INFO]      GIT TIME:       Wed, 20 Apr 2022 18:28:49 +0800
[DDR INFO]      ==ddr_features==
[DDR INFO]      RDBI:           0
[DDR INFO]      WDBI:           1
[DDR INFO]      InlineECC:      0
[DDR INFO]      DM:             1
[DDR INFO]      DDC:            1
[DDR INFO]      SSCG:           0
[DDR INFO]      BOARD:          XS_ENABLE
[DDR INFO] ddr_controller_cfg done
load ddr phy src_addr: 15b800, load_addr: 802caa20, src_len: 420
ATxSlewRate     : 15f
ATxImpedance    : 7f
TxSlewRate      : 19f
TxOdtDrvStren   : 600
TxImpedanceCtrl : e3f
CalDrvStr0      : 11
VrefInGlobal    : 104
board_type = 4 (CUSTOMER_BOARD)
load dqmap src addr: 15d600, load_addr: 802caa20, src_len: 20
[DDR INFO] dwc_ddrphy_train start
magic = 544f4248
load imem1 src_addr: 11ce00, load_addr: 802caa20, src_len: 8000
load dmem1 src_addr: 15a000, load_addr: 802caa20, src_len: 684
executing 1D fw
load imem2 src_addr: 124e00, load_addr: 802caa20, src_len: 8000
load dmem2 src_addr: 15a800, load_addr: 802caa20, src_len: 564

*******************************************************
p_dmem_lpddr4_2d_16b->MR11_A0:54
p_dmem_lpddr4_2d_16b->MR14_A0:54
p_dmem_lpddr4_2d_16b->MR12_A0:51
p_dmem_lpddr4_2d_16b->MR22_A0:14

p_dmem_lpddr4_2d_16b->MR3_A0:b3
p_dmem_lpddr4_2d_16b->Reserved00:40
p_dmem_lpddr4_2d_16b->Reserved0E:4
p_dmem_lpddr4_2d_16b->Delay_Weight2D:20
p_dmem_lpddr4_2d_16b->Voltage_Weight2D:80
*******************************************************

executing 2D fw
load pie src_addr: 15be00, load_addr: 802caa20, src_len: 11f0
Set QoS.
get_ddr_mr_info:cs_num=1, mr5=0x1, mr8=0x10
no magic in efuse file,bypass efuse
total_sz = 4096
SPL_VERSION:7
uboot partition is uboot_A
load u-boot: src_addr=0x380000, dest_addr=0x4000000, len=2097152
load warm boot spl: addr=0x800, dest_addr=0x80000000, len=31232
load bl31: addr=0x300000, dest_addr=0x0, len=524288
SFLOW_AUTH_BL31
verify signature of header:  verify ok!
verify signature of image:  verify ok!
bypass bpu image
clear keybank!!!!
SFLOW_DBG_EN
Trying to boot from RAM
SPL: bl31 will jump to u-boot or other entry (0x4000000)
SFLOW_CLR_KEY
SFLOW_REG_LD
install_portal copy portal
install_portal call smc and jump to bl31 cold entry(0x0)
hb som type: 5
X3 PI reset VDD_SD done

U-Boot 2018.09-g40785bca (May 27 2022 - 16:30:48 +0800)

Model: Hobot XJ3 Soc Board
DRAM:  system DDR size: 0xffe00000
4 GiB
MMC:   dwmmc@A5010000: 0, dwmmc@A5011000: 1, dwmmc@A5012000: 2 (SD)
Loading Environment from UBI... GigaDevice SPI NAND was found.
128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
*** Warning - bad CRC, using default environment

In:    serial@a5000000
Out:   serial@a5000000
Err:   serial@a5000000
Net:   x3 sdb reset eth phy done

Warning: ethernet@A5014000 (eth0) using random MAC address - 32:08:46:0d:08:d1
eth0: ethernet@A5014000
Disable cnn cores ..
dtb_name:hobot-x3-pi.dtb
base board type: X3 SDB
bootmode: NAND
board_id = 31540334
damaged volume, update marker is setdamaged volume, update marker is setdamaged volume, update marker is sethb_boot_args_cmd_set custom_bootargs 0 ubuntu_boot 0
Hit any key to stop autoboot:  0
enable watchdog success !
switch to partitions #0, OK
mmc2 is current device
Scanning mmc 2:2...
Found U-Boot script /boot/boot.scr
664 bytes read in 1 ms (648.4 KiB/s)
## Executing script at 03c10000
Boot script loaded from devtype:mmc devnum:2 devplist:2
bootargs = console=ttyS0,921600 raid=noautodetect hobotboot.reson=POWER_RESET rootfstype=ext4 root=/dev/mmcblk2p2
Loading fdt file: /boot/hobot/hobot-x3-pi.dtb
69633 bytes read in 8 ms (8.3 MiB/s)
Loading kernel: /boot/Image
19163144 bytes read in 845 ms (21.6 MiB/s)
## Flattened Device Tree blob at 03c00000
   Booting using the fdt blob at 0x3c00000
   Loading Device Tree to 0000000003c00000, end 0000000003c1ffff ... OK
chip_id: ab36300
The address of the fdt is 0x3c00000
Changed status Done
Can't get fdt_addr !!!Orign(MAX) bpu model Reserve Mem Size to 64M!!

Starting kernel ...

[    0.000000] OF: reserved mem: OVERLAP DETECTED!
[    0.000000] image_r5_mem (0x0000000080000000--0x0000000080010000) overlaps with msg_r5_mem (0x000000008000f000--0x0000000080010000)
[    0.000000] Reserved memory: created CMA memory pool at 0x0000000004000000, size 672 MiB
[    0.000000] OF: reserved mem: initialized node ion_cma, compatible id shared-dma-pool
[    0.000000] cma: Reserved 16 MiB at 0x000000007f000000
[    0.000000] On node 0 totalpages: 1047808
[    0.000000]   DMA zone: 8180 pages used for memmap
[    0.000000]   DMA zone: 0 pages reserved
[    0.000000]   DMA zone: 523520 pages, LIFO batch:31
[    0.000000]   Normal zone: 8192 pages used for memmap
[    0.000000]   Normal zone: 524288 pages, LIFO batch:31
[    0.000000] psci: probing for conduit method from DT.
[    0.000000] psci: PSCIv1.1 detected in firmware.
[    0.000000] psci: Using standard PSCI v0.2 function IDs
[    0.000000] psci: MIGRATE_INFO_TYPE not supported.
[    0.000000] psci: SMC Calling Convention v1.1
[    0.000000] percpu: Embedded 25 pages/cpu @ffffffc17ff2a000 s65176 r8192 d29032 u102400
[    0.000000] pcpu-alloc: s65176 r8192 d29032 u102400 alloc=25*4096
[    0.000000] pcpu-alloc: [0] 0 [0] 1 [0] 2 [0] 3
[    0.000000] Detected VIPT I-cache on CPU0
[    0.000000] CPU features: enabling workaround for ARM erratum 845719
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 1031436
[    0.000000] Kernel command line: earlycon loglevel=8 kgdboc=ttyS0 video=hobot:x3sdb-hdmi  console=ttyS0,921600 raid=noautodetect hobotboot.reson=POWER_RESET rootfstype=ext4 root=/dev/mmcblk2p2
[    0.000000] PID hash table entries: 4096 (order: 3, 32768 bytes)
[    0.000000] Dentry cache hash table entries: 524288 (order: 10, 4194304 bytes)
[    0.000000] Inode-cache hash table entries: 262144 (order: 9, 2097152 bytes)
[    0.000000] software IO TLB [mem 0x7afff000-0x7efff000] (64MB) mapped at [ffffffc07afff000-ffffffc07effefff]
[    0.000000] Memory: 3319580K/4191232K available (10494K kernel code, 1306K rwdata, 5756K rodata, 1088K init, 9553K bss, 167140K reserved, 704512K cma-reserved)
[    0.000000] Virtual kernel memory layout:
[    0.000000]     modules : 0xffffff8000000000 - 0xffffff8008000000   (   128 MB)
[    0.000000]     vmalloc : 0xffffff8008000000 - 0xffffffbebfff0000   (   250 GB)
[    0.000000]       .text : 0xffffff8008000000 - 0xffffff8008a40000   ( 10496 KB)
[    0.000000]     .rodata : 0xffffff8008a40000 - 0xffffff8008ff0000   (  5824 KB)
[    0.000000]       .init : 0xffffff8008ff0000 - 0xffffff8009100000   (  1088 KB)
[    0.000000]       .data : 0xffffff8009100000 - 0xffffff8009246808   (  1307 KB)
[    0.000000]        .bss : 0xffffff8009246808 - 0xffffff8009b9aed8   (  9554 KB)
[    0.000000]     fixed   : 0xffffffbefe7fd000 - 0xffffffbefec00000   (  4108 KB)
[    0.000000]     PCI I/O : 0xffffffbefee00000 - 0xffffffbeffe00000   (    16 MB)
[    0.000000]     vmemmap : 0xffffffbf00000000 - 0xffffffc000000000   (     4 GB maximum)
[    0.000000]               0xffffffbf00008000 - 0xffffffbf06000000   (    95 MB actual)
[    0.000000]     memory  : 0xffffffc000200000 - 0xffffffc180000000   (  6142 MB)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=4, Nodes=1
[    0.000000] ftrace: allocating 36277 entries in 142 pages
[    0.000000] Preemptible hierarchical RCU implementation.
[    0.000000]  Tasks RCU enabled.
[    0.000000] NR_IRQS: 64, nr_irqs: 64, preallocated irqs: 0
[    0.000000] parent_rate: 0,  dclk->rate:2666000000, pre_ddr_rate:0, res.a0:139716712
[    0.000000] arch_timer: cp15 timer(s) running at 24.00MHz (virt).
[    0.000000] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0x588fe9dc0, max_idle_ns: 440795202592 ns
[    0.000003] sched_clock: 56 bits at 24MHz, resolution 41ns, wraps every 4398046511097ns
[    0.001192] clocksource: hobot_clocksource: mask: 0xffffffffffffffff max_cycles: 0x1d854df40, max_idle_ns: 3526361616960 ns
[    0.002961] Console: colour dummy device 80x25
[    0.003532] Calibrating delay loop (skipped), value calculated using timer frequency.. 48.00 BogoMIPS (lpj=96000)
[    0.004838] pid_max: default: 32768 minimum: 301
[    0.005492] Security Framework initialized
[    0.006010] AppArmor: AppArmor disabled by boot time parameter
[    0.006854] Mount-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.007722] Mountpoint-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.023764] ASID allocator initialised with 65536 entries
[    0.031762] Hierarchical SRCU implementation.
[    0.063821] smp: Bringing up secondary CPUs ...
[    0.100028] Detected VIPT I-cache on CPU1
[    0.100063] CPU1: Booted secondary processor [410fd034]
[    0.136078] Detected VIPT I-cache on CPU2
[    0.136099] CPU2: Booted secondary processor [410fd034]
[    0.172137] Detected VIPT I-cache on CPU3
[    0.172157] CPU3: Booted secondary processor [410fd034]
[    0.172211] smp: Brought up 1 node, 4 CPUs
[    0.176274] SMP: Total of 4 processors activated.
[    0.176868] CPU features: detected feature: 32-bit EL0 Support
[    0.177687] CPU: All CPU(s) started at EL1
[    0.178215] alternatives: patching kernel code
[    0.179779] devtmpfs: initialized
[    0.188832] random: get_random_u32 called from bucket_table_alloc+0x108/0x270 with crng_init=0
[    0.190393] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 7645041785100000 ns
[    0.191639] futex hash table entries: 1024 (order: 5, 131072 bytes)
[    0.207895] xor: automatically using best checksumming function   32regs
[    0.208832] pinctrl core: initialized pinctrl subsystem
[    0.210054] NET: Registered protocol family 16
[    0.211366] vdso: 2 pages (1 code @ ffffff8008a46000, 1 data @ ffffff8009104000)
[    0.212311] hw-breakpoint: found 6 breakpoint and 4 watchpoint registers.
[    0.213896] DMA: preallocated 256 KiB pool for atomic allocations
[    0.214950] pstore: using zlib compression
[    0.215741] console [pstore-1] enabled
[    0.216354] pstore: Registered ramoops as persistent store backend
[    0.217139] ramoops: attached 0x40000@0x3fc0000, ecc: 0/0
[    0.222097] hobot_dma a1005000.dma: Hobot DMA Engine Driver Probed!!
[    0.235676] SCSI subsystem initialized
[    0.236296] media: Linux media interface: v0.10
[    0.236941] Linux video capture interface: v2.00
[    0.237575] pps_core: LinuxPPS API ver. 1 registered
[    0.238203] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.239378] PTP clock support registered
[    0.240494] ion_dummy: not reserve carveout memory, try to alloc from cma
[    0.376937] Advanced Linux Sound Architecture Driver Initialized.
[    0.378126] usbcore: registered new interface driver usbfs
[    0.378853] usbcore: registered new interface driver hub
[    0.379579] usbcore: registered new device driver usb
[    0.380520] clocksource: Switched to clocksource arch_sys_counter
[    0.427916] VFS: Disk quotas dquot_6.6.0
[    0.428458] VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
[    0.429427] FS-Cache: Loaded
[    0.429911] CacheFiles: Loaded
[    0.435202] NET: Registered protocol family 2
[    0.436119] TCP established hash table entries: 32768 (order: 6, 262144 bytes)
[    0.437251] TCP bind hash table entries: 32768 (order: 7, 524288 bytes)
[    0.438476] TCP: Hash tables configured (established 32768 bind 32768)
[    0.439384] UDP hash table entries: 2048 (order: 4, 65536 bytes)
[    0.440213] UDP-Lite hash table entries: 2048 (order: 4, 65536 bytes)
[    0.441236] NET: Registered protocol family 1
[    0.442067] RPC: Registered named UNIX socket transport module.
[    0.442819] RPC: Registered udp transport module.
[    0.443415] RPC: Registered tcp transport module.
[    0.444014] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.445525] hw perfevents: enabled with armv8_cortex_a53 PMU driver, 7 counters available
[    0.447723] audit: initializing netlink subsys (disabled)
[    0.448496] audit: type=2000 audit(0.440:1): state=initialized audit_enabled=0 res=1
[    0.448782] Initialise system trusted keyrings
[    0.448856] workingset: timestamp_bits=46 max_order=20 bucket_order=0
[    0.452391] zbud: loaded
[    0.454101] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.454959] exFAT: Version 1.2.9
[    0.455437] FS-Cache: Netfs 'nfs' registered for caching
[    0.456733] NFS: Registering the id_resolver key type
[    0.457387] Key type id_resolver registered
[    0.457913] Key type id_legacy registered
[    0.458429] nfs4filelayout_init: NFSv4 File Layout Driver Registering...
[    0.459283] Installing knfsd (copyright (C) 1996 okir@monad.swb.de).
[    0.463421] NET: Registered protocol family 38
[    0.463992] async_tx: api initialized (async)
[    0.464589] Key type asymmetric registered
[    0.465107] Asymmetric key parser 'x509' registered
[    0.465787] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 245)
[    0.466799] io scheduler noop registered
[    0.467456] io scheduler cfq registered (default)
[    0.468051] io scheduler mq-deadline registered
[    0.468648] io scheduler kyber registered
[    0.469824] pinctrl-single a6003170.pinctrl_voltag: 64 pins at pa ffffff8009c4d170 size 8
[    0.471156] pinctrl-single a6004000.pinctrl: 128 pins at pa ffffff8009c61000 size 512
[    0.472364] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: start probe
[    0.473279] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: probe ok
[    0.474156] gpio-x3 a6003000.gpio: x3 gpio probe start!!!
[    0.474846] gpio-x3 a6003000.gpio: x3 gpio add gpiochip start!!!
[    0.475771] gpio-x3 a6003000.gpio: diable all gpio irq
[    0.478029] gpio-x3 a6003000.gpio: irqbase:57
[    0.478580] gpio-x3 a6003000.gpio: x3 irq add start!!!
[    0.479237] irq: Cannot allocate irq_descs @ IRQ57, assuming pre-allocated
[    0.480267] gpio-x3 a6003000.gpio: x3 irq add ok!!!
[    0.481059] gpio-x3 a6003000.gpio: x3 irqchip ops add ok!!!
[    0.481766] gpio-x3 a6003000.gpio: x3 gpio probe ok!!!
[    0.482864] hobot-pwm: hobot-pwmchip0 registered
[    0.483617] hobot-pwm: hobot-pwmchip1 registered
[    0.484976] diag dev [ver:1.1] init done
[    0.485861] hobot_ddr_monitor: LPDDR4 detected
[    0.486614] hobot_ddr_monitor: ddr monitor init finished.
[    0.486997] [vcam] init start
[    0.488058] vcam probe start
[    0.488507] vcam probe end successful
[    0.488996] [vcam] init end
[    0.489917] a5000000.serial: ttyS0 at MMIO 0xa5000000 (irq = 10, base_baud = 12000000) is a hobot-uart
[    0.491129] console [ttyS0] enabled
[    0.491129] console [ttyS0] enabled
[    0.492013] bootconsole [hobot0] disabled
[    0.492013] bootconsole [hobot0] disabled
[    0.493525] hobot-uart a5001000.serial: Failed to create debugfs root directory
[    0.494531] a5001000.serial: ttyS1 at MMIO 0xa5001000 (irq = 11, base_baud = 12000000) is a hobot-uart
[    0.495974] hobot-uart a5003000.serial: Failed to create debugfs root directory
[    0.496985] a5003000.serial: ttyS3 at MMIO 0xa5003000 (irq = 12, base_baud = 12000000) is a hobot-uart
[    0.498520] KGDB: Registered I/O driver kgdboc
[    0.499356] cacheinfo: Unable to detect cache hierarchy for CPU 0
[    0.504849] brd: module loaded
[    0.509386] loop: module loaded
[    0.510905] spi-nand hr_nand.0: GigaDevice SPI NAND was found.
[    0.511664] spi-nand hr_nand.0: 128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
[    0.514293] hobot_spi a5006000.spi: ver: HOBOT-spi_V20.200330 master
[    0.515337] libphy: Fixed MDIO Bus: probed
[    0.516613] st_gmac a5014000.ethernet: found phy-handle subnode
[    0.517457] st_gmac a5014000.ethernet: xj3_mtl_setup, plat->rx-queues-to-use:4, and tx:4
[    0.518646] st_gmac a5014000.ethernet: xj3_probe_config_dt, clk_ptp_rate:250000000
[    0.519648] set mac address 00:11:22:7c:46:57:
[    0.519651] (using random mac adress)
[    0.520780] (NULL device *): xj3_get_hw_features, tx_fifo_size:16384
[    0.521598] (NULL device *): xj3_get_hw_features, rx_fifo_size:16384
[    0.522415] st_gmac a5014000.ethernet: TSO supported
[    0.523055] st_gmac a5014000.ethernet: TSO feature enabled
[    0.523761] st_gmac a5014000.ethernet: Enable Rx Mitigation via HW Watchdog Timer
[    0.644850] libphy: hobot-mac-mdio: probed
[    0.646364] st_gmac a5014000.ethernet: hobot_eth_probe: probe sucessfully
[    0.647563] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_0v8 not found, using dummy regulator
[    0.648806] dwc3-of-simple b2000000.usb: usb regulator 0v8 enable succeed
[    0.649684] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_3v3 not found, using dummy regulator
[    0.650886] dwc3-of-simple b2000000.usb: usb regulator 3v3 enable succeed
[    0.652413] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    0.654091] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    0.655524] usbcore: registered new interface driver cdc_acm
[    0.656253] cdc_acm: USB Abstract Control Model driver for USB modems and ISDN adapters
[    0.657326] usbcore: registered new interface driver uas
[    0.658043] usbcore: registered new interface driver usb-storage
[    0.658878] usbcore: registered new interface driver usbserial
[    0.659650] usbcore: registered new interface driver usbserial_generic
[    0.660507] usbserial: USB Serial support registered for generic
[    0.661320] usbcore: registered new interface driver usb_serial_simple
[    0.662178] usbserial: USB Serial support registered for carelink
[    0.662981] usbserial: USB Serial support registered for zio
[    0.663726] usbserial: USB Serial support registered for funsoft
[    0.664525] usbserial: USB Serial support registered for flashloader
[    0.665360] usbserial: USB Serial support registered for google
[    0.666138] usbserial: USB Serial support registered for libtransistor
[    0.666994] usbserial: USB Serial support registered for vivopay
[    0.667786] usbserial: USB Serial support registered for moto_modem
[    0.668628] usbserial: USB Serial support registered for motorola_tetra
[    0.669496] usbserial: USB Serial support registered for novatel_gps
[    0.670330] usbserial: USB Serial support registered for hp4x
[    0.671086] usbserial: USB Serial support registered for suunto
[    0.671865] usbserial: USB Serial support registered for siemens_mpi
[    0.672727] usbcore: registered new interface driver rio500
[    0.673557] mousedev: PS/2 mouse device common for all mice
[    0.684626] hobot-rtc a6002000.rtc: rtc core: registered hobot-rtc as rtc0
[    0.685616] i2c /dev entries driver
[    0.686224] hobot-i2c a5009000.i2c: hobot i2c probe start
[    0.686986] hobot-i2c a5009000.i2c: round_rate:96000000
[    0.687663] hobot-i2c a5009000.i2c: I2C bus speed is 400000
[    0.688381] hobot-i2c a5009000.i2c: clkdiv = 0x1d
[    0.689008] hobot-i2c a5009000.i2c: i2c0 diag register....
[    0.690105] hobot-i2c a5009000.i2c: hobot_i2c_0 probe done
[    0.690908] hobot-i2c a500a000.i2c: hobot i2c probe start
[    0.691667] hobot-i2c a500a000.i2c: round_rate:96000000
[    0.692344] hobot-i2c a500a000.i2c: I2C bus speed is 400000
[    0.693083] hobot-i2c a500a000.i2c: clkdiv = 0x1d
[    0.693690] hobot-i2c a500a000.i2c: i2c1 diag register....
[    0.694701] hobot-i2c a500a000.i2c: hobot_i2c_1 probe done
[    0.695659] lirc_dev: IR Remote Control driver registered, major 239
[    0.696477] IR LIRC bridge handler initialized
[    0.697254] sif_mclk clock frequence is 544000000
[    0.697892] mipi_rx0_ipi clock frequence is 544000000
[    0.698580] mipi_rx1_ipi clock frequence is 544000000
[    0.699279] mipi_rx2_ipi clock frequence is 544000000
[    0.699988] mipi_rx3_ipi clock frequence is 544000000
[    0.700728] mipi_tx_ipi clock frequence is 544000000
[    0.701448] mipi_cfg_host clock frequence is 102000000
[    0.702202] pym_mclk clock frequence is 1188000000
[    0.702921] mipi_dev_ref clock frequence is 24000000
[    0.703675] mipi_host_ref clock frequence is 24000000
[    0.704451] sensor0_mclk clock frequence is 37125000
[    0.705238] sensor1_mclk clock frequence is 37125000
[    0.706025] sensor2_mclk clock frequence is 37125000
[    0.706826] sensor3_mclk clock frequence is 37125000
[    0.707466] [FRT:D] x3_ips_probe(0)
[    0.708470] hobot swinfo sel reg ro=0x1 boot dump
[    0.709411] pvt a1009000.pvt: SCRATCH test: 1234abcd, pvt is alive.
[    0.710337] pvt a1009000.pvt: VM Calibrated data detected
[    0.711529] hobot_wdt a1002000.watchdog: watchdog setting [pet:6s bark:11s bite:15s]
[    0.712880] hobot_wdt a1002000.watchdog: Hobot Watchdog Timer at ffffff8009db3000 with timeout 15s
[    0.714232] device-mapper: uevent: version 1.0.3
[    0.714990] device-mapper: ioctl: 4.37.0-ioctl (2017-09-20) initialised: dm-devel@redhat.com
[    0.716146] device-mapper: verity-avb: AVB error handler initialized with vbmeta device:
[    0.718579] Synopsys Designware Multimedia Card Interface Driver
[    0.719577] dwmmc_hobot a5010000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.720403] dwmmc_hobot a5010000.dwmmc: card-detect-delay not found.
[    0.721278] dwmmc_hobot a5010000.dwmmc: data-addr not found.
[    0.722323] mmc_host mmc0: card is non-removable.
[    0.761731] dwmmc_hobot a5011000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.764583] dwmmc_hobot a5011000.dwmmc: card-detect-delay not found.
[    0.765410] dwmmc_hobot a5011000.dwmmc: data-addr not found.
[    0.770183] dwmmc_hobot a5011000.dwmmc: mmc set to fixed voltage 1800
[    0.771250] mmc_host mmc1: card is non-removable.
[    0.868750] dwmmc_hobot a5012000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.869572] dwmmc_hobot a5012000.dwmmc: card-detect-delay not found.
[    0.870406] dwmmc_hobot a5012000.dwmmc: data-addr not found.
[    0.871372] dwmmc_hobot a5012000.dwmmc: Got CD GPIO
[    0.979890] mmc1: queuing unknown CIS tuple 0x80 (2 bytes)
[    0.982086] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.984268] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.987643] mmc1: queuing unknown CIS tuple 0x80 (7 bytes)
[    0.991600] mmc1: queuing unknown CIS tuple 0x81 (9 bytes)
[    1.052824] ledtrig-cpu: registered to indicate activity on CPUs
[    1.053651] hidraw: raw HID events driver (C) Jiri Kosina
[    1.054489] usbcore: registered new interface driver usbhid
[    1.055206] usbhid: USB HID core driver
[    1.055786] logger: created 256K log 'log_main'
[    1.056445] logger: created 256K log 'log_events'
[    1.057136] logger: created 256K log 'log_radio'
[    1.057794] logger: created 256K log 'log_system'
[    1.058845] set dmc devfreq governor to performance
[    1.059488] hobot_dmcfreq_target: dmcfreq->rate:2666000000, target_rate:2666000000
[    1.060470] buf:, powersave_rate:2666000000, dmcfreq->pre_state:0
[    1.067345] usbcore: registered new interface driver snd-usb-audio
[    1.068536] Netfilter messages via NETLINK v0.30.
[    1.069174] ip_set: protocol 6
[    1.069665] ipip: IPv4 and MPLS over IPv4 tunneling driver
[    1.070667] ip_tables: (C) 2000-2006 Netfilter Core Team
[    1.071602] arp_tables: arp_tables: (C) 2002 David S. Miller
[    1.072398] Initializing XFRM netlink socket
[    1.073309] NET: Registered protocol family 10
[    1.074559] Segment Routing with IPv6
[    1.075077] sit: IPv6, IPv4 and MPLS over IPv4 tunneling driver
[    1.076199] NET: Registered protocol family 17
[    1.076854] Key type dns_resolver registered
[    1.078573] Loading compiled-in X.509 certificates
[    1.082147] Loaded X.509 cert 'Build time autogenerated kernel key: 81cb0ef77db2fac76e9588c2120c82422367d268'
[    1.083490] zswap: loaded using pool lzo/zbud
[    1.094801] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    1.096463] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    1.097566] console [netcon0] enabled
[    1.098042] netconsole: network logging started
[    1.098825] hobot-rtc a6002000.rtc: setting system clock to 1970-01-01 00:00:00 UTC (0)
[    1.100009] vps mipi_dphy: probe with x3vio done
[    1.100756] hobot_wdt_test: wdt_test_init: wdt test init
[    1.103460] VCC_CNN0: disabling
[    1.103869] VCC_CNN1: disabling
[    1.104857] vps mipi_host0: ver 140* port0(0:0)
[    1.105766] vps mipi_host1: ver 140* port1(1:0)
[    1.106655] vps mipi_host2: ver 140* port2(0:1)
[    1.107443] vps mipi_host3: ver 140* port3(1:1)
[    1.108274] ALSA device list:
[    1.108737]   No soundcards found.
[    1.109374] md: Skipping autodetection of RAID arrays. (raid=autodetect will force)
[    1.110508] VFS: Cannot open root device "mmcblk2p2" or unknown-block(0,0): error -6
[    1.111502] Please append a correct "root=" boot option; here are the available partitions:
[    1.112595] 0100          102400 ram0
[    1.112598]  (driver?)
[    1.113387] 0101          102400 ram1
[    1.113389]  (driver?)
[    1.114176] 0102          102400 ram2
[    1.114178]  (driver?)
[    1.114966] 0103          102400 ram3
[    1.114968]  (driver?)
[    1.115756] 0104          102400 ram4
[    1.115757]  (driver?)
[    1.116584] 0105          102400 ram5
[    1.116586]  (driver?)
[    1.117375] 0106          102400 ram6
[    1.117377]  (driver?)
[    1.118165] 0107          102400 ram7
[    1.118167]  (driver?)
[    1.118955] 0108          102400 ram8
[    1.118957]  (driver?)
[    1.119745] 0109          102400 ram9
[    1.119747]  (driver?)
[    1.120550] 010a          102400 ram10
[    1.120552]  (driver?)
[    1.121352] 010b          102400 ram11
[    1.121354]  (driver?)
[    1.122153] 010c          102400 ram12
[    1.122155]  (driver?)
[    1.122954] 010d          102400 ram13
[    1.122955]  (driver?)
[    1.123755] 010e          102400 ram14
[    1.123756]  (driver?)
[    1.124563] 010f          102400 ram15
[    1.124565]  (driver?)
[    1.125367] 1f00          131072 mtdblock0
[    1.125369]  (driver?)
[    1.126212] hobot_fusa: set_fusa_error_pin:75 set error pin to 1
[    1.126983] hobot_fusa: fusa errpin not ready
[    1.126987] Kernel panic - not syncing: VFS: Unable to mount root fs on unknown-block(0,0)
[    1.128605] Kernel Offset: disabled
[    1.129056] CPU features: 0x0002004
[    1.129506] Memory Limit: none
[    1.134067] Rebooting in 1 seconds..
[    1.204760] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.205482] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 1
[    1.206939] xhci-hcd xhci-hcd.0.auto: hcc params 0x0220fe6d hci version 0x110 quirks 0x0000000000010010
[    1.208174] xhci-hcd xhci-hcd.0.auto: irq 178, io mem 0xb2000000
[    1.209151] usb usb1: New USB device found, idVendor=1d6b, idProduct=0002, bcdDevice= 4.14
[    1.210215] usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.211143] usb usb1: Product: xHCI Host Controller
[    1.211772] usb usb1: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.212478] usb usb1: SerialNumber: xhci-hcd.0.auto
[    1.213446] hub 1-0:1.0: USB hub found
[    1.213948] hub 1-0:1.0: 1 port detected
[    1.214634] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.215347] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 2
[    1.216336] xhci-hcd xhci-hcd.0.auto: Host supports USB 3.0 SuperSpeed
[    1.217230] usb usb2: We don't know the algorithms for LPM for this host, disabling LPM.
[    1.218344] usb usb2: New USB device found, idVendor=1d6b, idProduct=0003, bcdDevice= 4.14
[    1.219407] usb usb2: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.220335] usb usb2: Product: xHCI Host Controller
[    1.220973] usb usb2: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.221680] usb usb2: SerialNumber: xhci-hcd.0.auto
[    1.222578] hub 2-0:1.0: USB hub found
[    1.223078] hub 2-0:1.0: 1 port detected
[    1.468529] usb 1-1: new high-speed USB device number 2 using xhci-hcd
[    1.616715] usb 1-1: New USB device found, idVendor=1a40, idProduct=0101, bcdDevice= 1.11
[    1.617768] usb 1-1: New USB device strings: Mfr=0, Product=1, SerialNumber=0
[    1.618685] usb 1-1: Product: USB 2.0 Hub
[    1.665386] hub 1-1:1.0: USB hub found
[    1.665906] hub 1-1:1.0: 4 ports detected
[    1.956533] mmc2: new UHS SDR104 SDHC card at address 0001
[    1.957551] mmcblk2: mmc2:0001 SD16G 29.8 GiB
[    1.959172]  mmcblk2: p1 p2
[    2.134579] SMP: stopping secondary CPUs
[    2.135087] psci: psci_sys_reset(reboot_mode=0)
NOTICE:  fast_boot:0

S
F
L
O
NOTICE:  efuse cpu_cfg = 0
W
NOTICE:  Booting Trusted Firmware
NOTICE:  BL1: v1.4(release):HR-ROM-Rel-v1.1-141-ga91d4dd-dirty
NOTICE:  BL1: Built : 11:24:44, Oct 23 2019
NOTICE:  boot src: 2
NOTICE:  GigaDev SPI NAND was found.
NOTICE:  Block size: 128 KiB, page size: 2048
NOTICE:  BL1: Booting BL2
Auth pass
NOTICE:  bl1_main exit
SPL normal reset flow
check_reset_state (2): wakeup address = 0x0, hw wakeup status = 0x3, wakeup src=0x100
patch for sys_pll 1200 with 100M eth
SFLOW_INIT
CHIP ID:PCB941/WAFER: W04/ X: X20/ Y: Y36
secondary_jump_to_spl: secure chip flow
X3 SPL : secondary core wake up and jump to spl done (cpu_core_cfg=0)
SFLOW_FIN_HW_A

U-Boot SPL 2018.09-g4ca851534c-dirty (May 11 2022 - 20:09:50 +0800)
SPACC Init - ID: (00000061)
SPL nand boot mode (from strap)
GigaDev SPI NAND was found.
Block size: 128 KiB, page size: 2048
ddr_type = 1 (LPDDR4)
hb_chip_package_type:3
load ddr header src_addr: 100000, load_addr: 802ca020, src_len: a00
find valid ddr image
ddr_hdr.ecc_gran: 0x0
ddr_hdr.ecc_map: 0x0
ddr_hdr.sbr_pattern0: 0x0
ddr_hdr.sbr_pattern1: 0x0
ddr_freq = 05
board id = 31540334
ddr datarate: 3200
### SAMSUNG DDR ###
no ddr pin set
detect part number: 108
detect ddr freq: c80
board id alternative:0x3
index is 12
index is 15
index is 19
hb_ddr_index: 19
ddr_type = 1, ddr_vendor=3, ddr_freq=3200
dram_pll_init
sscg disabled
control load ddrc src_addr: 15ae00, load_addr: 802caa20, src_len: 920
[DDR INFO]      ==ddr_release_info==
[DDR INFO]      VERSION:        develop
[DDR INFO]      BUILD:          2022-05-11-20:09
[DDR INFO]      GIT COMMIT:     4ca851534c1616ace920fdaa000c6fb717c1fb74
[DDR INFO]      GIT TIME:       Wed, 20 Apr 2022 18:28:49 +0800
[DDR INFO]      ==ddr_features==
[DDR INFO]      RDBI:           0
[DDR INFO]      WDBI:           1
[DDR INFO]      InlineECC:      0
[DDR INFO]      DM:             1
[DDR INFO]      DDC:            1
[DDR INFO]      SSCG:           0
[DDR INFO]      BOARD:          XS_ENABLE
[DDR INFO] ddr_controller_cfg done
load ddr phy src_addr: 15b800, load_addr: 802caa20, src_len: 420
ATxSlewRate     : 15f
ATxImpedance    : 7f
TxSlewRate      : 19f
TxOdtDrvStren   : 600
TxImpedanceCtrl : e3f
CalDrvStr0      : 11
VrefInGlobal    : 104
board_type = 4 (CUSTOMER_BOARD)
load dqmap src addr: 15d600, load_addr: 802caa20, src_len: 20
[DDR INFO] dwc_ddrphy_train start
magic = 544f4248
load imem1 src_addr: 11ce00, load_addr: 802caa20, src_len: 8000
load dmem1 src_addr: 15a000, load_addr: 802caa20, src_len: 684
executing 1D fw
load imem2 src_addr: 124e00, load_addr: 802caa20, src_len: 8000
load dmem2 src_addr: 15a800, load_addr: 802caa20, src_len: 564

*******************************************************
p_dmem_lpddr4_2d_16b->MR11_A0:54
p_dmem_lpddr4_2d_16b->MR14_A0:54
p_dmem_lpddr4_2d_16b->MR12_A0:51
p_dmem_lpddr4_2d_16b->MR22_A0:14

p_dmem_lpddr4_2d_16b->MR3_A0:b3
p_dmem_lpddr4_2d_16b->Reserved00:40
p_dmem_lpddr4_2d_16b->Reserved0E:4
p_dmem_lpddr4_2d_16b->Delay_Weight2D:20
p_dmem_lpddr4_2d_16b->Voltage_Weight2D:80
*******************************************************

executing 2D fw
load pie src_addr: 15be00, load_addr: 802caa20, src_len: 11f0
Set QoS.
get_ddr_mr_info:cs_num=1, mr5=0x1, mr8=0x10
no magic in efuse file,bypass efuse
total_sz = 4096
SPL_VERSION:7
uboot partition is uboot_A
load u-boot: src_addr=0x380000, dest_addr=0x4000000, len=2097152
load warm boot spl: addr=0x800, dest_addr=0x80000000, len=31232
load bl31: addr=0x300000, dest_addr=0x0, len=524288
SFLOW_AUTH_BL31
verify signature of header:  verify ok!
verify signature of image:  verify ok!
bypass bpu image
clear keybank!!!!
SFLOW_DBG_EN
Trying to boot from RAM
SPL: bl31 will jump to u-boot or other entry (0x4000000)
SFLOW_CLR_KEY
SFLOW_REG_LD
install_portal copy portal
install_portal call smc and jump to bl31 cold entry(0x0)
hb som type: 5
X3 PI reset VDD_SD done

U-Boot 2018.09-g40785bca (May 27 2022 - 16:30:48 +0800)

Model: Hobot XJ3 Soc Board
DRAM:  system DDR size: 0xffe00000
4 GiB
MMC:   dwmmc@A5010000: 0, dwmmc@A5011000: 1, dwmmc@A5012000: 2
Loading Environment from UBI... GigaDevice SPI NAND was found.
128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
*** Warning - bad CRC, using default environment

In:    serial@a5000000
Out:   serial@a5000000
Err:   serial@a5000000
Net:   x3 sdb reset eth phy done

Warning: ethernet@A5014000 (eth0) using random MAC address - 32:51:45:a3:6f:4b
eth0: ethernet@A5014000
Disable cnn cores ..
dtb_name:hobot-x3-pi.dtb
base board type: X3 SDB
bootmode: NAND
board_id = 31540334
damaged volume, update marker is setdamaged volume, update marker is setdamaged volume, update marker is sethb_boot_args_cmd_set custom_bootargs 0 ubuntu_boot 0
Hit any key to stop autoboot:  0
enable watchdog success !
switch to partitions #0, OK
mmc2 is current device
Scanning mmc 2:2...
Found U-Boot script /boot/boot.scr
664 bytes read in 2 ms (324.2 KiB/s)
## Executing script at 03c10000
Boot script loaded from devtype:mmc devnum:2 devplist:2
bootargs = console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
Loading fdt file: /boot/hobot/hobot-x3-pi.dtb
69633 bytes read in 8 ms (8.3 MiB/s)
Loading kernel: /boot/Image
19163144 bytes read in 845 ms (21.6 MiB/s)
## Flattened Device Tree blob at 03c00000
   Booting using the fdt blob at 0x3c00000
   Loading Device Tree to 0000000003c00000, end 0000000003c1ffff ... OK
chip_id: ab36300
The address of the fdt is 0x3c00000
Changed status Done
Can't get fdt_addr !!!Orign(MAX) bpu model Reserve Mem Size to 64M!!

Starting kernel ...

[    0.000000] OF: reserved mem: OVERLAP DETECTED!
[    0.000000] image_r5_mem (0x0000000080000000--0x0000000080010000) overlaps with msg_r5_mem (0x000000008000f000--0x0000000080010000)
[    0.000000] Reserved memory: created CMA memory pool at 0x0000000004000000, size 672 MiB
[    0.000000] OF: reserved mem: initialized node ion_cma, compatible id shared-dma-pool
[    0.000000] cma: Reserved 16 MiB at 0x000000007f000000
[    0.000000] On node 0 totalpages: 1047808
[    0.000000]   DMA zone: 8180 pages used for memmap
[    0.000000]   DMA zone: 0 pages reserved
[    0.000000]   DMA zone: 523520 pages, LIFO batch:31
[    0.000000]   Normal zone: 8192 pages used for memmap
[    0.000000]   Normal zone: 524288 pages, LIFO batch:31
[    0.000000] psci: probing for conduit method from DT.
[    0.000000] psci: PSCIv1.1 detected in firmware.
[    0.000000] psci: Using standard PSCI v0.2 function IDs
[    0.000000] psci: MIGRATE_INFO_TYPE not supported.
[    0.000000] psci: SMC Calling Convention v1.1
[    0.000000] percpu: Embedded 25 pages/cpu @ffffffc17ff2a000 s65176 r8192 d29032 u102400
[    0.000000] pcpu-alloc: s65176 r8192 d29032 u102400 alloc=25*4096
[    0.000000] pcpu-alloc: [0] 0 [0] 1 [0] 2 [0] 3
[    0.000000] Detected VIPT I-cache on CPU0
[    0.000000] CPU features: enabling workaround for ARM erratum 845719
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 1031436
[    0.000000] Kernel command line: earlycon loglevel=8 kgdboc=ttyS0 video=hobot:x3sdb-hdmi  console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
[    0.000000] PID hash table entries: 4096 (order: 3, 32768 bytes)
[    0.000000] Dentry cache hash table entries: 524288 (order: 10, 4194304 bytes)
[    0.000000] Inode-cache hash table entries: 262144 (order: 9, 2097152 bytes)
[    0.000000] software IO TLB [mem 0x7afff000-0x7efff000] (64MB) mapped at [ffffffc07afff000-ffffffc07effefff]
[    0.000000] Memory: 3319580K/4191232K available (10494K kernel code, 1306K rwdata, 5756K rodata, 1088K init, 9553K bss, 167140K reserved, 704512K cma-reserved)
[    0.000000] Virtual kernel memory layout:
[    0.000000]     modules : 0xffffff8000000000 - 0xffffff8008000000   (   128 MB)
[    0.000000]     vmalloc : 0xffffff8008000000 - 0xffffffbebfff0000   (   250 GB)
[    0.000000]       .text : 0xffffff8008000000 - 0xffffff8008a40000   ( 10496 KB)
[    0.000000]     .rodata : 0xffffff8008a40000 - 0xffffff8008ff0000   (  5824 KB)
[    0.000000]       .init : 0xffffff8008ff0000 - 0xffffff8009100000   (  1088 KB)
[    0.000000]       .data : 0xffffff8009100000 - 0xffffff8009246808   (  1307 KB)
[    0.000000]        .bss : 0xffffff8009246808 - 0xffffff8009b9aed8   (  9554 KB)
[    0.000000]     fixed   : 0xffffffbefe7fd000 - 0xffffffbefec00000   (  4108 KB)
[    0.000000]     PCI I/O : 0xffffffbefee00000 - 0xffffffbeffe00000   (    16 MB)
[    0.000000]     vmemmap : 0xffffffbf00000000 - 0xffffffc000000000   (     4 GB maximum)
[    0.000000]               0xffffffbf00008000 - 0xffffffbf06000000   (    95 MB actual)
[    0.000000]     memory  : 0xffffffc000200000 - 0xffffffc180000000   (  6142 MB)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=4, Nodes=1
[    0.000000] ftrace: allocating 36277 entries in 142 pages
[    0.000000] Preemptible hierarchical RCU implementation.
[    0.000000]  Tasks RCU enabled.
[    0.000000] NR_IRQS: 64, nr_irqs: 64, preallocated irqs: 0
[    0.000000] parent_rate: 0,  dclk->rate:2666000000, pre_ddr_rate:0, res.a0:139716712
[    0.000000] arch_timer: cp15 timer(s) running at 24.00MHz (virt).
[    0.000000] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0x588fe9dc0, max_idle_ns: 440795202592 ns
[    0.000003] sched_clock: 56 bits at 24MHz, resolution 41ns, wraps every 4398046511097ns
[    0.001194] clocksource: hobot_clocksource: mask: 0xffffffffffffffff max_cycles: 0x1d854df40, max_idle_ns: 3526361616960 ns
[    0.002966] Console: colour dummy device 80x25
[    0.003537] Calibrating delay loop (skipped), value calculated using timer frequency.. 48.00 BogoMIPS (lpj=96000)
[    0.004843] pid_max: default: 32768 minimum: 301
[    0.005497] Security Framework initialized
[    0.006015] AppArmor: AppArmor disabled by boot time parameter
[    0.006859] Mount-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.007727] Mountpoint-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.023768] ASID allocator initialised with 65536 entries
[    0.031766] Hierarchical SRCU implementation.
[    0.063826] smp: Bringing up secondary CPUs ...
[    0.100033] Detected VIPT I-cache on CPU1
[    0.100067] CPU1: Booted secondary processor [410fd034]
[    0.136084] Detected VIPT I-cache on CPU2
[    0.136105] CPU2: Booted secondary processor [410fd034]
[    0.172142] Detected VIPT I-cache on CPU3
[    0.172162] CPU3: Booted secondary processor [410fd034]
[    0.172216] smp: Brought up 1 node, 4 CPUs
[    0.176279] SMP: Total of 4 processors activated.
[    0.176873] CPU features: detected feature: 32-bit EL0 Support
[    0.177691] CPU: All CPU(s) started at EL1
[    0.178219] alternatives: patching kernel code
[    0.179808] devtmpfs: initialized
[    0.188874] random: get_random_u32 called from bucket_table_alloc+0x108/0x270 with crng_init=0
[    0.190459] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 7645041785100000 ns
[    0.191705] futex hash table entries: 1024 (order: 5, 131072 bytes)
[    0.208212] xor: automatically using best checksumming function   32regs
[    0.209150] pinctrl core: initialized pinctrl subsystem
[    0.210384] NET: Registered protocol family 16
[    0.211706] vdso: 2 pages (1 code @ ffffff8008a46000, 1 data @ ffffff8009104000)
[    0.212651] hw-breakpoint: found 6 breakpoint and 4 watchpoint registers.
[    0.214240] DMA: preallocated 256 KiB pool for atomic allocations
[    0.218369] pstore: using zlib compression
[    0.219163] console [pstore-1] enabled
[    0.219760] pstore: Registered ramoops as persistent store backend
[    0.220545] ramoops: attached 0x40000@0x3fc0000, ecc: 0/0
[    0.225512] hobot_dma a1005000.dma: Hobot DMA Engine Driver Probed!!
[    0.239532] SCSI subsystem initialized
[    0.240155] media: Linux media interface: v0.10
[    0.240766] Linux video capture interface: v2.00
[    0.241394] pps_core: LinuxPPS API ver. 1 registered
[    0.242021] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.243196] PTP clock support registered
[    0.244328] ion_dummy: not reserve carveout memory, try to alloc from cma
[    0.380609] Advanced Linux Sound Architecture Driver Initialized.
[    0.381789] usbcore: registered new interface driver usbfs
[    0.382516] usbcore: registered new interface driver hub
[    0.383242] usbcore: registered new device driver usb
[    0.384184] clocksource: Switched to clocksource arch_sys_counter
[    0.431643] VFS: Disk quotas dquot_6.6.0
[    0.432234] VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
[    0.433173] FS-Cache: Loaded
[    0.433655] CacheFiles: Loaded
[    0.438998] NET: Registered protocol family 2
[    0.439879] TCP established hash table entries: 32768 (order: 6, 262144 bytes)
[    0.441020] TCP bind hash table entries: 32768 (order: 7, 524288 bytes)
[    0.442246] TCP: Hash tables configured (established 32768 bind 32768)
[    0.443154] UDP hash table entries: 2048 (order: 4, 65536 bytes)
[    0.443984] UDP-Lite hash table entries: 2048 (order: 4, 65536 bytes)
[    0.445005] NET: Registered protocol family 1
[    0.445795] RPC: Registered named UNIX socket transport module.
[    0.446545] RPC: Registered udp transport module.
[    0.447143] RPC: Registered tcp transport module.
[    0.447741] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.449249] hw perfevents: enabled with armv8_cortex_a53 PMU driver, 7 counters available
[    0.451467] audit: initializing netlink subsys (disabled)
[    0.452280] audit: type=2000 audit(0.448:1): state=initialized audit_enabled=0 res=1
[    0.452550] Initialise system trusted keyrings
[    0.452627] workingset: timestamp_bits=46 max_order=20 bucket_order=0
[    0.456155] zbud: loaded
[    0.457867] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.458724] exFAT: Version 1.2.9
[    0.459204] FS-Cache: Netfs 'nfs' registered for caching
[    0.460321] NFS: Registering the id_resolver key type
[    0.460973] Key type id_resolver registered
[    0.461499] Key type id_legacy registered
[    0.462014] nfs4filelayout_init: NFSv4 File Layout Driver Registering...
[    0.462867] Installing knfsd (copyright (C) 1996 okir@monad.swb.de).
[    0.466929] NET: Registered protocol family 38
[    0.467500] async_tx: api initialized (async)
[    0.468052] Key type asymmetric registered
[    0.468588] Asymmetric key parser 'x509' registered
[    0.469264] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 245)
[    0.470280] io scheduler noop registered
[    0.470937] io scheduler cfq registered (default)
[    0.471532] io scheduler mq-deadline registered
[    0.472108] io scheduler kyber registered
[    0.473298] pinctrl-single a6003170.pinctrl_voltag: 64 pins at pa ffffff8009c4d170 size 8
[    0.474629] pinctrl-single a6004000.pinctrl: 128 pins at pa ffffff8009c61000 size 512
[    0.475830] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: start probe
[    0.476885] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: probe ok
[    0.477767] gpio-x3 a6003000.gpio: x3 gpio probe start!!!
[    0.478457] gpio-x3 a6003000.gpio: x3 gpio add gpiochip start!!!
[    0.479378] gpio-x3 a6003000.gpio: diable all gpio irq
[    0.481644] gpio-x3 a6003000.gpio: irqbase:57
[    0.482196] gpio-x3 a6003000.gpio: x3 irq add start!!!
[    0.482853] irq: Cannot allocate irq_descs @ IRQ57, assuming pre-allocated
[    0.483883] gpio-x3 a6003000.gpio: x3 irq add ok!!!
[    0.484547] gpio-x3 a6003000.gpio: x3 irqchip ops add ok!!!
[    0.485253] gpio-x3 a6003000.gpio: x3 gpio probe ok!!!
[    0.486332] hobot-pwm: hobot-pwmchip0 registered
[    0.487085] hobot-pwm: hobot-pwmchip1 registered
[    0.488583] diag dev [ver:1.1] init done
[    0.489480] hobot_ddr_monitor: LPDDR4 detected
[    0.490248] hobot_ddr_monitor: ddr monitor init finished.
[    0.490632] [vcam] init start
[    0.491692] vcam probe start
[    0.492142] vcam probe end successful
[    0.492614] [vcam] init end
[    0.493534] a5000000.serial: ttyS0 at MMIO 0xa5000000 (irq = 10, base_baud = 12000000) is a hobot-uart
[    0.494756] console [ttyS0] enabled
[    0.494756] console [ttyS0] enabled
[    0.495661] bootconsole [hobot0] disabled
[    0.495661] bootconsole [hobot0] disabled
[    0.497131] hobot-uart a5001000.serial: Failed to create debugfs root directory
[    0.498138] a5001000.serial: ttyS1 at MMIO 0xa5001000 (irq = 11, base_baud = 12000000) is a hobot-uart
[    0.499586] hobot-uart a5003000.serial: Failed to create debugfs root directory
[    0.500596] a5003000.serial: ttyS3 at MMIO 0xa5003000 (irq = 12, base_baud = 12000000) is a hobot-uart
[    0.502133] KGDB: Registered I/O driver kgdboc
[    0.502968] cacheinfo: Unable to detect cache hierarchy for CPU 0
[    0.508451] brd: module loaded
[    0.513126] loop: module loaded
[    0.514672] spi-nand hr_nand.0: GigaDevice SPI NAND was found.
[    0.515433] spi-nand hr_nand.0: 128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
[    0.518060] hobot_spi a5006000.spi: ver: HOBOT-spi_V20.200330 master
[    0.519106] libphy: Fixed MDIO Bus: probed
[    0.520364] st_gmac a5014000.ethernet: found phy-handle subnode
[    0.521199] st_gmac a5014000.ethernet: xj3_mtl_setup, plat->rx-queues-to-use:4, and tx:4
[    0.522383] st_gmac a5014000.ethernet: xj3_probe_config_dt, clk_ptp_rate:250000000
[    0.523385] set mac address 00:11:22:e9:d4:8e:
[    0.523388] (using random mac adress)
[    0.524472] (NULL device *): xj3_get_hw_features, tx_fifo_size:16384
[    0.525289] (NULL device *): xj3_get_hw_features, rx_fifo_size:16384
[    0.526107] st_gmac a5014000.ethernet: TSO supported
[    0.526747] st_gmac a5014000.ethernet: TSO feature enabled
[    0.527454] st_gmac a5014000.ethernet: Enable Rx Mitigation via HW Watchdog Timer
[    0.648546] libphy: hobot-mac-mdio: probed
[    0.650109] st_gmac a5014000.ethernet: hobot_eth_probe: probe sucessfully
[    0.651308] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_0v8 not found, using dummy regulator
[    0.652563] dwc3-of-simple b2000000.usb: usb regulator 0v8 enable succeed
[    0.653442] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_3v3 not found, using dummy regulator
[    0.654643] dwc3-of-simple b2000000.usb: usb regulator 3v3 enable succeed
[    0.656171] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    0.657849] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    0.659357] usbcore: registered new interface driver cdc_acm
[    0.660087] cdc_acm: USB Abstract Control Model driver for USB modems and ISDN adapters
[    0.661165] usbcore: registered new interface driver uas
[    0.661886] usbcore: registered new interface driver usb-storage
[    0.662713] usbcore: registered new interface driver usbserial
[    0.663485] usbcore: registered new interface driver usbserial_generic
[    0.664418] usbserial: USB Serial support registered for generic
[    0.665215] usbcore: registered new interface driver usb_serial_simple
[    0.666075] usbserial: USB Serial support registered for carelink
[    0.666876] usbserial: USB Serial support registered for zio
[    0.667621] usbserial: USB Serial support registered for funsoft
[    0.668431] usbserial: USB Serial support registered for flashloader
[    0.669265] usbserial: USB Serial support registered for google
[    0.670044] usbserial: USB Serial support registered for libtransistor
[    0.670903] usbserial: USB Serial support registered for vivopay
[    0.671693] usbserial: USB Serial support registered for moto_modem
[    0.672533] usbserial: USB Serial support registered for motorola_tetra
[    0.673401] usbserial: USB Serial support registered for novatel_gps
[    0.674235] usbserial: USB Serial support registered for hp4x
[    0.674992] usbserial: USB Serial support registered for suunto
[    0.675773] usbserial: USB Serial support registered for siemens_mpi
[    0.676636] usbcore: registered new interface driver rio500
[    0.677465] mousedev: PS/2 mouse device common for all mice
[    0.688514] hobot-rtc a6002000.rtc: rtc core: registered hobot-rtc as rtc0
[    0.689505] i2c /dev entries driver
[    0.690112] hobot-i2c a5009000.i2c: hobot i2c probe start
[    0.690876] hobot-i2c a5009000.i2c: round_rate:96000000
[    0.691553] hobot-i2c a5009000.i2c: I2C bus speed is 400000
[    0.692291] hobot-i2c a5009000.i2c: clkdiv = 0x1d
[    0.692898] hobot-i2c a5009000.i2c: i2c0 diag register....
[    0.693987] hobot-i2c a5009000.i2c: hobot_i2c_0 probe done
[    0.694790] hobot-i2c a500a000.i2c: hobot i2c probe start
[    0.695545] hobot-i2c a500a000.i2c: round_rate:96000000
[    0.696243] hobot-i2c a500a000.i2c: I2C bus speed is 400000
[    0.696961] hobot-i2c a500a000.i2c: clkdiv = 0x1d
[    0.697568] hobot-i2c a500a000.i2c: i2c1 diag register....
[    0.698577] hobot-i2c a500a000.i2c: hobot_i2c_1 probe done
[    0.699538] lirc_dev: IR Remote Control driver registered, major 239
[    0.700377] IR LIRC bridge handler initialized
[    0.701133] sif_mclk clock frequence is 544000000
[    0.701769] mipi_rx0_ipi clock frequence is 544000000
[    0.702457] mipi_rx1_ipi clock frequence is 544000000
[    0.703155] mipi_rx2_ipi clock frequence is 544000000
[    0.703864] mipi_rx3_ipi clock frequence is 544000000
[    0.704603] mipi_tx_ipi clock frequence is 544000000
[    0.705324] mipi_cfg_host clock frequence is 102000000
[    0.706078] pym_mclk clock frequence is 1188000000
[    0.706798] mipi_dev_ref clock frequence is 24000000
[    0.707553] mipi_host_ref clock frequence is 24000000
[    0.708345] sensor0_mclk clock frequence is 37125000
[    0.709121] sensor1_mclk clock frequence is 37125000
[    0.709910] sensor2_mclk clock frequence is 37125000
[    0.710711] sensor3_mclk clock frequence is 37125000
[    0.711350] [FRT:D] x3_ips_probe(0)
[    0.712395] hobot swinfo sel reg ro=0x1 boot dump
[    0.713327] pvt a1009000.pvt: SCRATCH test: 1234abcd, pvt is alive.
[    0.714254] pvt a1009000.pvt: VM Calibrated data detected
[    0.715443] hobot_wdt a1002000.watchdog: watchdog setting [pet:6s bark:11s bite:15s]
[    0.716784] hobot_wdt a1002000.watchdog: Hobot Watchdog Timer at ffffff8009db3000 with timeout 15s
[    0.718138] device-mapper: uevent: version 1.0.3
[    0.718900] device-mapper: ioctl: 4.37.0-ioctl (2017-09-20) initialised: dm-devel@redhat.com
[    0.720055] device-mapper: verity-avb: AVB error handler initialized with vbmeta device:
[    0.722552] Synopsys Designware Multimedia Card Interface Driver
[    0.723553] dwmmc_hobot a5010000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.724409] dwmmc_hobot a5010000.dwmmc: card-detect-delay not found.
[    0.725228] dwmmc_hobot a5010000.dwmmc: data-addr not found.
[    0.726265] mmc_host mmc0: card is non-removable.
[    0.769397] dwmmc_hobot a5011000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.772237] dwmmc_hobot a5011000.dwmmc: card-detect-delay not found.
[    0.773056] dwmmc_hobot a5011000.dwmmc: data-addr not found.
[    0.777829] dwmmc_hobot a5011000.dwmmc: mmc set to fixed voltage 1800
[    0.778892] mmc_host mmc1: card is non-removable.
[    0.876383] dwmmc_hobot a5012000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.877202] dwmmc_hobot a5012000.dwmmc: card-detect-delay not found.
[    0.878033] dwmmc_hobot a5012000.dwmmc: data-addr not found.
[    0.879002] dwmmc_hobot a5012000.dwmmc: Got CD GPIO
[    0.989905] mmc1: queuing unknown CIS tuple 0x80 (2 bytes)
[    0.992089] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.994286] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.997660] mmc1: queuing unknown CIS tuple 0x80 (7 bytes)
[    1.001616] mmc1: queuing unknown CIS tuple 0x81 (9 bytes)
[    1.068502] ledtrig-cpu: registered to indicate activity on CPUs
[    1.069332] hidraw: raw HID events driver (C) Jiri Kosina
[    1.070156] usbcore: registered new interface driver usbhid
[    1.070873] usbhid: USB HID core driver
[    1.071464] logger: created 256K log 'log_main'
[    1.072107] logger: created 256K log 'log_events'
[    1.072789] logger: created 256K log 'log_radio'
[    1.073438] logger: created 256K log 'log_system'
[    1.074459] set dmc devfreq governor to performance
[    1.075092] hobot_dmcfreq_target: dmcfreq->rate:2666000000, target_rate:2666000000
[    1.076064] buf:, powersave_rate:2666000000, dmcfreq->pre_state:0
[    1.082893] usbcore: registered new interface driver snd-usb-audio
[    1.084058] Netfilter messages via NETLINK v0.30.
[    1.084714] ip_set: protocol 6
[    1.085198] ipip: IPv4 and MPLS over IPv4 tunneling driver
[    1.086193] ip_tables: (C) 2000-2006 Netfilter Core Team
[    1.087113] arp_tables: arp_tables: (C) 2002 David S. Miller
[    1.087901] Initializing XFRM netlink socket
[    1.088783] NET: Registered protocol family 10
[    1.090015] Segment Routing with IPv6
[    1.090525] sit: IPv6, IPv4 and MPLS over IPv4 tunneling driver
[    1.091615] NET: Registered protocol family 17
[    1.092260] Key type dns_resolver registered
[    1.093902] Loading compiled-in X.509 certificates
[    1.097399] Loaded X.509 cert 'Build time autogenerated kernel key: 81cb0ef77db2fac76e9588c2120c82422367d268'
[    1.098730] zswap: loaded using pool lzo/zbud
[    1.110004] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    1.111666] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    1.112751] console [netcon0] enabled
[    1.113226] netconsole: network logging started
[    1.114006] hobot-rtc a6002000.rtc: setting system clock to 1970-01-01 00:00:00 UTC (0)
[    1.115189] vps mipi_dphy: probe with x3vio done
[    1.115895] hobot_wdt_test: wdt_test_init: wdt test init
[    1.118624] VCC_CNN0: disabling
[    1.119033] VCC_CNN1: disabling
[    1.119978] vps mipi_host0: ver 140* port0(0:0)
[    1.120966] vps mipi_host1: ver 140* port1(1:0)
[    1.121856] vps mipi_host2: ver 140* port2(0:1)
[    1.122645] vps mipi_host3: ver 140* port3(1:1)
[    1.123485] ALSA device list:
[    1.123870]   No soundcards found.
[    1.124535] md: Skipping autodetection of RAID arrays. (raid=autodetect will force)
[    1.125670] VFS: Cannot open root device "mmcblk2p2" or unknown-block(0,0): error -6
[    1.126663] Please append a correct "root=" boot option; here are the available partitions:
[    1.127737] 0100          102400 ram0
[    1.127739]  (driver?)
[    1.128581] 0101          102400 ram1
[    1.128583]  (driver?)
[    1.129372] 0102          102400 ram2
[    1.129374]  (driver?)
[    1.130162] 0103          102400 ram3
[    1.130164]  (driver?)
[    1.130951] 0104          102400 ram4
[    1.130953]  (driver?)
[    1.131741] 0105          102400 ram5
[    1.131743]  (driver?)
[    1.132573] 0106          102400 ram6
[    1.132575]  (driver?)
[    1.133363] 0107          102400 ram7
[    1.133365]  (driver?)
[    1.134153] 0108          102400 ram8
[    1.134155]  (driver?)
[    1.134943] 0109          102400 ram9
[    1.134945]  (driver?)
[    1.135732] 010a          102400 ram10
[    1.135734]  (driver?)
[    1.136543] 010b          102400 ram11
[    1.136545]  (driver?)
[    1.137344] 010c          102400 ram12
[    1.137346]  (driver?)
[    1.138145] 010d          102400 ram13
[    1.138146]  (driver?)
[    1.138946] 010e          102400 ram14
[    1.138947]  (driver?)
[    1.139747] 010f          102400 ram15
[    1.139748]  (driver?)
[    1.140570] 1f00          131072 mtdblock0
[    1.140572]  (driver?)
[    1.141416] hobot_fusa: set_fusa_error_pin:75 set error pin to 1
[    1.142186] hobot_fusa: fusa errpin not ready
[    1.142190] Kernel panic - not syncing: VFS: Unable to mount root fs on unknown-block(0,0)
[    1.143808] Kernel Offset: disabled
[    1.144260] CPU features: 0x0002004
[    1.144709] Memory Limit: none
[    1.149270] Rebooting in 1 seconds..
[    1.225397] mmc1: new HSSDIO card at address 0001
[    2.149781] SMP: stopping secondary CPUs
[    2.150289] psci: psci_sys_reset(reboot_mode=0)
NOTICE:  fast_boot:0

S
F
L
O
NOTICE:  efuse cpu_cfg = 0
W
NOTICE:  Booting Trusted Firmware
NOTICE:  BL1: v1.4(release):HR-ROM-Rel-v1.1-141-ga91d4dd-dirty
NOTICE:  BL1: Built : 11:24:44, Oct 23 2019
NOTICE:  boot src: 2
NOTICE:  GigaDev SPI NAND was found.
NOTICE:  Block size: 128 KiB, page size: 2048
NOTICE:  BL1: Booting BL2
Auth pass
NOTICE:  bl1_main exit
SPL normal reset flow
check_reset_state (2): wakeup address = 0x0, hw wakeup status = 0x3, wakeup src=0x100
patch for sys_pll 1200 with 100M eth
SFLOW_INIT
CHIP ID:PCB941/WAFER: W04/ X: X20/ Y: Y36
secondary_jump_to_spl: secure chip flow
X3 SPL : secondary core wake up and jump to spl done (cpu_core_cfg=0)
SFLOW_FIN_HW_A

U-Boot SPL 2018.09-g4ca851534c-dirty (May 11 2022 - 20:09:50 +0800)
SPACC Init - ID: (00000061)
SPL nand boot mode (from strap)
GigaDev SPI NAND was found.
Block size: 128 KiB, page size: 2048
ddr_type = 1 (LPDDR4)
hb_chip_package_type:3
load ddr header src_addr: 100000, load_addr: 802ca020, src_len: a00
find valid ddr image
ddr_hdr.ecc_gran: 0x0
ddr_hdr.ecc_map: 0x0
ddr_hdr.sbr_pattern0: 0x0
ddr_hdr.sbr_pattern1: 0x0
ddr_freq = 05
board id = 31540334
ddr datarate: 3200
### SAMSUNG DDR ###
no ddr pin set
detect part number: 108
detect ddr freq: c80
board id alternative:0x3
index is 12
index is 15
index is 19
hb_ddr_index: 19
ddr_type = 1, ddr_vendor=3, ddr_freq=3200
dram_pll_init
sscg disabled
control load ddrc src_addr: 15ae00, load_addr: 802caa20, src_len: 920
[DDR INFO]      ==ddr_release_info==
[DDR INFO]      VERSION:        develop
[DDR INFO]      BUILD:          2022-05-11-20:09
[DDR INFO]      GIT COMMIT:     4ca851534c1616ace920fdaa000c6fb717c1fb74
[DDR INFO]      GIT TIME:       Wed, 20 Apr 2022 18:28:49 +0800
[DDR INFO]      ==ddr_features==
[DDR INFO]      RDBI:           0
[DDR INFO]      WDBI:           1
[DDR INFO]      InlineECC:      0
[DDR INFO]      DM:             1
[DDR INFO]      DDC:            1
[DDR INFO]      SSCG:           0
[DDR INFO]      BOARD:          XS_ENABLE
[DDR INFO] ddr_controller_cfg done
load ddr phy src_addr: 15b800, load_addr: 802caa20, src_len: 420
ATxSlewRate     : 15f
ATxImpedance    : 7f
TxSlewRate      : 19f
TxOdtDrvStren   : 600
TxImpedanceCtrl : e3f
CalDrvStr0      : 11
VrefInGlobal    : 104
board_type = 4 (CUSTOMER_BOARD)
load dqmap src addr: 15d600, load_addr: 802caa20, src_len: 20
[DDR INFO] dwc_ddrphy_train start
magic = 544f4248
load imem1 src_addr: 11ce00, load_addr: 802caa20, src_len: 8000
load dmem1 src_addr: 15a000, load_addr: 802caa20, src_len: 684
executing 1D fw
load imem2 src_addr: 124e00, load_addr: 802caa20, src_len: 8000
load dmem2 src_addr: 15a800, load_addr: 802caa20, src_len: 564

*******************************************************
p_dmem_lpddr4_2d_16b->MR11_A0:54
p_dmem_lpddr4_2d_16b->MR14_A0:54
p_dmem_lpddr4_2d_16b->MR12_A0:51
p_dmem_lpddr4_2d_16b->MR22_A0:14

p_dmem_lpddr4_2d_16b->MR3_A0:b3
p_dmem_lpddr4_2d_16b->Reserved00:40
p_dmem_lpddr4_2d_16b->Reserved0E:4
p_dmem_lpddr4_2d_16b->Delay_Weight2D:20
p_dmem_lpddr4_2d_16b->Voltage_Weight2D:80
*******************************************************

executing 2D fw
load pie src_addr: 15be00, load_addr: 802caa20, src_len: 11f0
Set QoS.
get_ddr_mr_info:cs_num=1, mr5=0x1, mr8=0x10
no magic in efuse file,bypass efuse
total_sz = 4096
SPL_VERSION:7
uboot partition is uboot_A
load u-boot: src_addr=0x380000, dest_addr=0x4000000, len=2097152
load warm boot spl: addr=0x800, dest_addr=0x80000000, len=31232
load bl31: addr=0x300000, dest_addr=0x0, len=524288
SFLOW_AUTH_BL31
verify signature of header:  verify ok!
verify signature of image:  verify ok!
bypass bpu image
clear keybank!!!!
SFLOW_DBG_EN
Trying to boot from RAM
SPL: bl31 will jump to u-boot or other entry (0x4000000)
SFLOW_CLR_KEY
SFLOW_REG_LD
install_portal copy portal
install_portal call smc and jump to bl31 cold entry(0x0)
hb som type: 5
X3 PI reset VDD_SD done

U-Boot 2018.09-g40785bca (May 27 2022 - 16:30:48 +0800)

Model: Hobot XJ3 Soc Board
DRAM:  system DDR size: 0xffe00000
4 GiB
MMC:   dwmmc@A5010000: 0, dwmmc@A5011000: 1, dwmmc@A5012000: 2 (SD)
Loading Environment from UBI... GigaDevice SPI NAND was found.
128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
*** Warning - bad CRC, using default environment

In:    serial@a5000000
Out:   serial@a5000000
Err:   serial@a5000000
Net:   x3 sdb reset eth phy done

Warning: ethernet@A5014000 (eth0) using random MAC address - 62:24:b6:96:3a:7a
eth0: ethernet@A5014000
Disable cnn cores ..
dtb_name:hobot-x3-pi.dtb
base board type: X3 SDB
bootmode: NAND
board_id = 31540334
damaged volume, update marker is setdamaged volume, update marker is setdamaged volume, update marker is sethb_boot_args_cmd_set custom_bootargs 0 ubuntu_boot 0
Hit any key to stop autoboot:  0
enable watchdog success !
switch to partitions #0, OK
mmc2 is current device
Scanning mmc 2:2...
Found U-Boot script /boot/boot.scr
664 bytes read in 1 ms (648.4 KiB/s)
## Executing script at 03c10000
Boot script loaded from devtype:mmc devnum:2 devplist:2
bootargs = console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
Loading fdt file: /boot/hobot/hobot-x3-pi.dtb
69633 bytes read in 8 ms (8.3 MiB/s)
Loading kernel: /boot/Image
19163144 bytes read in 845 ms (21.6 MiB/s)
## Flattened Device Tree blob at 03c00000
   Booting using the fdt blob at 0x3c00000
   Loading Device Tree to 0000000003c00000, end 0000000003c1ffff ... OK
chip_id: ab36300
The address of the fdt is 0x3c00000
Changed status Done
Can't get fdt_addr !!!Orign(MAX) bpu model Reserve Mem Size to 64M!!

Starting kernel ...

[    0.000000] OF: reserved mem: OVERLAP DETECTED!
[    0.000000] image_r5_mem (0x0000000080000000--0x0000000080010000) overlaps with msg_r5_mem (0x000000008000f000--0x0000000080010000)
[    0.000000] Reserved memory: created CMA memory pool at 0x0000000004000000, size 672 MiB
[    0.000000] OF: reserved mem: initialized node ion_cma, compatible id shared-dma-pool
[    0.000000] cma: Reserved 16 MiB at 0x000000007f000000
[    0.000000] On node 0 totalpages: 1047808
[    0.000000]   DMA zone: 8180 pages used for memmap
[    0.000000]   DMA zone: 0 pages reserved
[    0.000000]   DMA zone: 523520 pages, LIFO batch:31
[    0.000000]   Normal zone: 8192 pages used for memmap
[    0.000000]   Normal zone: 524288 pages, LIFO batch:31
[    0.000000] psci: probing for conduit method from DT.
[    0.000000] psci: PSCIv1.1 detected in firmware.
[    0.000000] psci: Using standard PSCI v0.2 function IDs
[    0.000000] psci: MIGRATE_INFO_TYPE not supported.
[    0.000000] psci: SMC Calling Convention v1.1
[    0.000000] percpu: Embedded 25 pages/cpu @ffffffc17ff2a000 s65176 r8192 d29032 u102400
[    0.000000] pcpu-alloc: s65176 r8192 d29032 u102400 alloc=25*4096
[    0.000000] pcpu-alloc: [0] 0 [0] 1 [0] 2 [0] 3
[    0.000000] Detected VIPT I-cache on CPU0
[    0.000000] CPU features: enabling workaround for ARM erratum 845719
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 1031436
[    0.000000] Kernel command line: earlycon loglevel=8 kgdboc=ttyS0 video=hobot:x3sdb-hdmi  console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
[    0.000000] PID hash table entries: 4096 (order: 3, 32768 bytes)
[    0.000000] Dentry cache hash table entries: 524288 (order: 10, 4194304 bytes)
[    0.000000] Inode-cache hash table entries: 262144 (order: 9, 2097152 bytes)
[    0.000000] software IO TLB [mem 0x7afff000-0x7efff000] (64MB) mapped at [ffffffc07afff000-ffffffc07effefff]
[    0.000000] Memory: 3319580K/4191232K available (10494K kernel code, 1306K rwdata, 5756K rodata, 1088K init, 9553K bss, 167140K reserved, 704512K cma-reserved)
[    0.000000] Virtual kernel memory layout:
[    0.000000]     modules : 0xffffff8000000000 - 0xffffff8008000000   (   128 MB)
[    0.000000]     vmalloc : 0xffffff8008000000 - 0xffffffbebfff0000   (   250 GB)
[    0.000000]       .text : 0xffffff8008000000 - 0xffffff8008a40000   ( 10496 KB)
[    0.000000]     .rodata : 0xffffff8008a40000 - 0xffffff8008ff0000   (  5824 KB)
[    0.000000]       .init : 0xffffff8008ff0000 - 0xffffff8009100000   (  1088 KB)
[    0.000000]       .data : 0xffffff8009100000 - 0xffffff8009246808   (  1307 KB)
[    0.000000]        .bss : 0xffffff8009246808 - 0xffffff8009b9aed8   (  9554 KB)
[    0.000000]     fixed   : 0xffffffbefe7fd000 - 0xffffffbefec00000   (  4108 KB)
[    0.000000]     PCI I/O : 0xffffffbefee00000 - 0xffffffbeffe00000   (    16 MB)
[    0.000000]     vmemmap : 0xffffffbf00000000 - 0xffffffc000000000   (     4 GB maximum)
[    0.000000]               0xffffffbf00008000 - 0xffffffbf06000000   (    95 MB actual)
[    0.000000]     memory  : 0xffffffc000200000 - 0xffffffc180000000   (  6142 MB)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=4, Nodes=1
[    0.000000] ftrace: allocating 36277 entries in 142 pages
[    0.000000] Preemptible hierarchical RCU implementation.
[    0.000000]  Tasks RCU enabled.
[    0.000000] NR_IRQS: 64, nr_irqs: 64, preallocated irqs: 0
[    0.000000] parent_rate: 0,  dclk->rate:2666000000, pre_ddr_rate:0, res.a0:139716712
[    0.000000] arch_timer: cp15 timer(s) running at 24.00MHz (virt).
[    0.000000] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0x588fe9dc0, max_idle_ns: 440795202592 ns
[    0.000004] sched_clock: 56 bits at 24MHz, resolution 41ns, wraps every 4398046511097ns
[    0.001194] clocksource: hobot_clocksource: mask: 0xffffffffffffffff max_cycles: 0x1d854df40, max_idle_ns: 3526361616960 ns
[    0.002967] Console: colour dummy device 80x25
[    0.003538] Calibrating delay loop (skipped), value calculated using timer frequency.. 48.00 BogoMIPS (lpj=96000)
[    0.004843] pid_max: default: 32768 minimum: 301
[    0.005497] Security Framework initialized
[    0.006015] AppArmor: AppArmor disabled by boot time parameter
[    0.006857] Mount-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.007726] Mountpoint-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.023769] ASID allocator initialised with 65536 entries
[    0.031766] Hierarchical SRCU implementation.
[    0.063824] smp: Bringing up secondary CPUs ...
[    0.100030] Detected VIPT I-cache on CPU1
[    0.100065] CPU1: Booted secondary processor [410fd034]
[    0.136080] Detected VIPT I-cache on CPU2
[    0.136101] CPU2: Booted secondary processor [410fd034]
[    0.172140] Detected VIPT I-cache on CPU3
[    0.172160] CPU3: Booted secondary processor [410fd034]
[    0.172214] smp: Brought up 1 node, 4 CPUs
[    0.176278] SMP: Total of 4 processors activated.
[    0.176872] CPU features: detected feature: 32-bit EL0 Support
[    0.177691] CPU: All CPU(s) started at EL1
[    0.178219] alternatives: patching kernel code
[    0.179811] devtmpfs: initialized
[    0.188905] random: get_random_u32 called from bucket_table_alloc+0x108/0x270 with crng_init=0
[    0.190478] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 7645041785100000 ns
[    0.191723] futex hash table entries: 1024 (order: 5, 131072 bytes)
[    0.208232] xor: automatically using best checksumming function   32regs
[    0.209169] pinctrl core: initialized pinctrl subsystem
[    0.210407] NET: Registered protocol family 16
[    0.211725] vdso: 2 pages (1 code @ ffffff8008a46000, 1 data @ ffffff8009104000)
[    0.212670] hw-breakpoint: found 6 breakpoint and 4 watchpoint registers.
[    0.214260] DMA: preallocated 256 KiB pool for atomic allocations
[    0.218857] pstore: using zlib compression
[    0.219649] console [pstore-1] enabled
[    0.220245] pstore: Registered ramoops as persistent store backend
[    0.221030] ramoops: attached 0x40000@0x3fc0000, ecc: 0/0
[    0.226012] hobot_dma a1005000.dma: Hobot DMA Engine Driver Probed!!
[    0.239646] SCSI subsystem initialized
[    0.240273] media: Linux media interface: v0.10
[    0.240886] Linux video capture interface: v2.00
[    0.241518] pps_core: LinuxPPS API ver. 1 registered
[    0.242146] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.243321] PTP clock support registered
[    0.244447] ion_dummy: not reserve carveout memory, try to alloc from cma
[    0.380978] Advanced Linux Sound Architecture Driver Initialized.
[    0.382170] usbcore: registered new interface driver usbfs
[    0.382898] usbcore: registered new interface driver hub
[    0.383624] usbcore: registered new device driver usb
[    0.384570] clocksource: Switched to clocksource arch_sys_counter
[    0.431978] VFS: Disk quotas dquot_6.6.0
[    0.432523] VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
[    0.433489] FS-Cache: Loaded
[    0.433969] CacheFiles: Loaded
[    0.439228] NET: Registered protocol family 2
[    0.440141] TCP established hash table entries: 32768 (order: 6, 262144 bytes)
[    0.441287] TCP bind hash table entries: 32768 (order: 7, 524288 bytes)
[    0.442513] TCP: Hash tables configured (established 32768 bind 32768)
[    0.443422] UDP hash table entries: 2048 (order: 4, 65536 bytes)
[    0.444251] UDP-Lite hash table entries: 2048 (order: 4, 65536 bytes)
[    0.445271] NET: Registered protocol family 1
[    0.446088] RPC: Registered named UNIX socket transport module.
[    0.446839] RPC: Registered udp transport module.
[    0.447436] RPC: Registered tcp transport module.
[    0.448034] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.449665] hw perfevents: enabled with armv8_cortex_a53 PMU driver, 7 counters available
[    0.451860] audit: initializing netlink subsys (disabled)
[    0.452684] audit: type=2000 audit(0.448:1): state=initialized audit_enabled=0 res=1
[    0.452988] Initialise system trusted keyrings
[    0.453065] workingset: timestamp_bits=46 max_order=20 bucket_order=0
[    0.456893] zbud: loaded
[    0.458449] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.459307] exFAT: Version 1.2.9
[    0.459786] FS-Cache: Netfs 'nfs' registered for caching
[    0.460938] NFS: Registering the id_resolver key type
[    0.461591] Key type id_resolver registered
[    0.462118] Key type id_legacy registered
[    0.462634] nfs4filelayout_init: NFSv4 File Layout Driver Registering...
[    0.463487] Installing knfsd (copyright (C) 1996 okir@monad.swb.de).
[    0.467643] NET: Registered protocol family 38
[    0.468213] async_tx: api initialized (async)
[    0.468792] Key type asymmetric registered
[    0.469309] Asymmetric key parser 'x509' registered
[    0.469986] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 245)
[    0.470999] io scheduler noop registered
[    0.471659] io scheduler cfq registered (default)
[    0.472254] io scheduler mq-deadline registered
[    0.472967] io scheduler kyber registered
[    0.474153] pinctrl-single a6003170.pinctrl_voltag: 64 pins at pa ffffff8009c4d170 size 8
[    0.475489] pinctrl-single a6004000.pinctrl: 128 pins at pa ffffff8009c61000 size 512
[    0.476761] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: start probe
[    0.477652] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: probe ok
[    0.478525] gpio-x3 a6003000.gpio: x3 gpio probe start!!!
[    0.479215] gpio-x3 a6003000.gpio: x3 gpio add gpiochip start!!!
[    0.480138] gpio-x3 a6003000.gpio: diable all gpio irq
[    0.482391] gpio-x3 a6003000.gpio: irqbase:57
[    0.482943] gpio-x3 a6003000.gpio: x3 irq add start!!!
[    0.483603] irq: Cannot allocate irq_descs @ IRQ57, assuming pre-allocated
[    0.484741] gpio-x3 a6003000.gpio: x3 irq add ok!!!
[    0.485396] gpio-x3 a6003000.gpio: x3 irqchip ops add ok!!!
[    0.486102] gpio-x3 a6003000.gpio: x3 gpio probe ok!!!
[    0.487190] hobot-pwm: hobot-pwmchip0 registered
[    0.487944] hobot-pwm: hobot-pwmchip1 registered
[    0.489298] diag dev [ver:1.1] init done
[    0.490188] hobot_ddr_monitor: LPDDR4 detected
[    0.490939] hobot_ddr_monitor: ddr monitor init finished.
[    0.491316] [vcam] init start
[    0.492377] vcam probe start
[    0.492950] vcam probe end successful
[    0.493412] [vcam] init end
[    0.494324] a5000000.serial: ttyS0 at MMIO 0xa5000000 (irq = 10, base_baud = 12000000) is a hobot-uart
[    0.495535] console [ttyS0] enabled
[    0.495535] console [ttyS0] enabled
[    0.496419] bootconsole [hobot0] disabled
[    0.496419] bootconsole [hobot0] disabled
[    0.497771] hobot-uart a5001000.serial: Failed to create debugfs root directory
[    0.498771] a5001000.serial: ttyS1 at MMIO 0xa5001000 (irq = 11, base_baud = 12000000) is a hobot-uart
[    0.500227] hobot-uart a5003000.serial: Failed to create debugfs root directory
[    0.501265] a5003000.serial: ttyS3 at MMIO 0xa5003000 (irq = 12, base_baud = 12000000) is a hobot-uart
[    0.502798] KGDB: Registered I/O driver kgdboc
[    0.503633] cacheinfo: Unable to detect cache hierarchy for CPU 0
[    0.509102] brd: module loaded
[    0.513641] loop: module loaded
[    0.515223] spi-nand hr_nand.0: GigaDevice SPI NAND was found.
[    0.515983] spi-nand hr_nand.0: 128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
[    0.518658] hobot_spi a5006000.spi: ver: HOBOT-spi_V20.200330 master
[    0.519703] libphy: Fixed MDIO Bus: probed
[    0.521073] st_gmac a5014000.ethernet: found phy-handle subnode
[    0.521912] st_gmac a5014000.ethernet: xj3_mtl_setup, plat->rx-queues-to-use:4, and tx:4
[    0.523094] st_gmac a5014000.ethernet: xj3_probe_config_dt, clk_ptp_rate:250000000
[    0.524097] set mac address 00:11:22:27:7a:ac:
[    0.524099] (using random mac adress)
[    0.525289] (NULL device *): xj3_get_hw_features, tx_fifo_size:16384
[    0.526107] (NULL device *): xj3_get_hw_features, rx_fifo_size:16384
[    0.526924] st_gmac a5014000.ethernet: TSO supported
[    0.527564] st_gmac a5014000.ethernet: TSO feature enabled
[    0.528271] st_gmac a5014000.ethernet: Enable Rx Mitigation via HW Watchdog Timer
[    0.649348] libphy: hobot-mac-mdio: probed
[    0.650893] st_gmac a5014000.ethernet: hobot_eth_probe: probe sucessfully
[    0.652093] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_0v8 not found, using dummy regulator
[    0.653337] dwc3-of-simple b2000000.usb: usb regulator 0v8 enable succeed
[    0.654215] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_3v3 not found, using dummy regulator
[    0.655416] dwc3-of-simple b2000000.usb: usb regulator 3v3 enable succeed
[    0.656955] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    0.658611] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    0.660055] usbcore: registered new interface driver cdc_acm
[    0.660804] cdc_acm: USB Abstract Control Model driver for USB modems and ISDN adapters
[    0.661859] usbcore: registered new interface driver uas
[    0.662576] usbcore: registered new interface driver usb-storage
[    0.663408] usbcore: registered new interface driver usbserial
[    0.664183] usbcore: registered new interface driver usbserial_generic
[    0.665061] usbserial: USB Serial support registered for generic
[    0.665857] usbcore: registered new interface driver usb_serial_simple
[    0.666714] usbserial: USB Serial support registered for carelink
[    0.667515] usbserial: USB Serial support registered for zio
[    0.668260] usbserial: USB Serial support registered for funsoft
[    0.669063] usbserial: USB Serial support registered for flashloader
[    0.669898] usbserial: USB Serial support registered for google
[    0.670676] usbserial: USB Serial support registered for libtransistor
[    0.671532] usbserial: USB Serial support registered for vivopay
[    0.672322] usbserial: USB Serial support registered for moto_modem
[    0.673164] usbserial: USB Serial support registered for motorola_tetra
[    0.674035] usbserial: USB Serial support registered for novatel_gps
[    0.674869] usbserial: USB Serial support registered for hp4x
[    0.675625] usbserial: USB Serial support registered for suunto
[    0.676404] usbserial: USB Serial support registered for siemens_mpi
[    0.677264] usbcore: registered new interface driver rio500
[    0.678095] mousedev: PS/2 mouse device common for all mice
[    0.689146] hobot-rtc a6002000.rtc: rtc core: registered hobot-rtc as rtc0
[    0.690138] i2c /dev entries driver
[    0.690743] hobot-i2c a5009000.i2c: hobot i2c probe start
[    0.691507] hobot-i2c a5009000.i2c: round_rate:96000000
[    0.692185] hobot-i2c a5009000.i2c: I2C bus speed is 400000
[    0.692928] hobot-i2c a5009000.i2c: clkdiv = 0x1d
[    0.693535] hobot-i2c a5009000.i2c: i2c0 diag register....
[    0.694625] hobot-i2c a5009000.i2c: hobot_i2c_0 probe done
[    0.695425] hobot-i2c a500a000.i2c: hobot i2c probe start
[    0.696180] hobot-i2c a500a000.i2c: round_rate:96000000
[    0.696883] hobot-i2c a500a000.i2c: I2C bus speed is 400000
[    0.697601] hobot-i2c a500a000.i2c: clkdiv = 0x1d
[    0.698207] hobot-i2c a500a000.i2c: i2c1 diag register....
[    0.699216] hobot-i2c a500a000.i2c: hobot_i2c_1 probe done
[    0.700172] lirc_dev: IR Remote Control driver registered, major 239
[    0.701012] IR LIRC bridge handler initialized
[    0.701768] sif_mclk clock frequence is 544000000
[    0.702405] mipi_rx0_ipi clock frequence is 544000000
[    0.703093] mipi_rx1_ipi clock frequence is 544000000
[    0.703792] mipi_rx2_ipi clock frequence is 544000000
[    0.704500] mipi_rx3_ipi clock frequence is 544000000
[    0.705240] mipi_tx_ipi clock frequence is 544000000
[    0.705960] mipi_cfg_host clock frequence is 102000000
[    0.706713] pym_mclk clock frequence is 1188000000
[    0.707433] mipi_dev_ref clock frequence is 24000000
[    0.708186] mipi_host_ref clock frequence is 24000000
[    0.708978] sensor0_mclk clock frequence is 37125000
[    0.709756] sensor1_mclk clock frequence is 37125000
[    0.710545] sensor2_mclk clock frequence is 37125000
[    0.711345] sensor3_mclk clock frequence is 37125000
[    0.711985] [FRT:D] x3_ips_probe(0)
[    0.713021] hobot swinfo sel reg ro=0x1 boot dump
[    0.713941] pvt a1009000.pvt: SCRATCH test: 1234abcd, pvt is alive.
[    0.714863] pvt a1009000.pvt: VM Calibrated data detected
[    0.716043] hobot_wdt a1002000.watchdog: watchdog setting [pet:6s bark:11s bite:15s]
[    0.717381] hobot_wdt a1002000.watchdog: Hobot Watchdog Timer at ffffff8009db3000 with timeout 15s
[    0.718740] device-mapper: uevent: version 1.0.3
[    0.719509] device-mapper: ioctl: 4.37.0-ioctl (2017-09-20) initialised: dm-devel@redhat.com
[    0.720733] device-mapper: verity-avb: AVB error handler initialized with vbmeta device:
[    0.723143] Synopsys Designware Multimedia Card Interface Driver
[    0.724140] dwmmc_hobot a5010000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.724997] dwmmc_hobot a5010000.dwmmc: card-detect-delay not found.
[    0.725816] dwmmc_hobot a5010000.dwmmc: data-addr not found.
[    0.726862] mmc_host mmc0: card is non-removable.
[    0.765793] dwmmc_hobot a5011000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.768624] dwmmc_hobot a5011000.dwmmc: card-detect-delay not found.
[    0.769443] dwmmc_hobot a5011000.dwmmc: data-addr not found.
[    0.774213] dwmmc_hobot a5011000.dwmmc: mmc set to fixed voltage 1800
[    0.775278] mmc_host mmc1: card is non-removable.
[    0.872779] dwmmc_hobot a5012000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.873611] dwmmc_hobot a5012000.dwmmc: card-detect-delay not found.
[    0.874447] dwmmc_hobot a5012000.dwmmc: data-addr not found.
[    0.875419] dwmmc_hobot a5012000.dwmmc: Got CD GPIO
[    0.986317] mmc1: queuing unknown CIS tuple 0x80 (2 bytes)
[    0.988502] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.990697] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.994066] mmc1: queuing unknown CIS tuple 0x80 (7 bytes)
[    0.998022] mmc1: queuing unknown CIS tuple 0x81 (9 bytes)
[    1.064888] ledtrig-cpu: registered to indicate activity on CPUs
[    1.065713] hidraw: raw HID events driver (C) Jiri Kosina
[    1.066549] usbcore: registered new interface driver usbhid
[    1.067267] usbhid: USB HID core driver
[    1.067843] logger: created 256K log 'log_main'
[    1.068490] logger: created 256K log 'log_events'
[    1.069175] logger: created 256K log 'log_radio'
[    1.069822] logger: created 256K log 'log_system'
[    1.070849] set dmc devfreq governor to performance
[    1.071483] hobot_dmcfreq_target: dmcfreq->rate:2666000000, target_rate:2666000000
[    1.072455] buf:, powersave_rate:2666000000, dmcfreq->pre_state:0
[    1.079277] usbcore: registered new interface driver snd-usb-audio
[    1.080425] Netfilter messages via NETLINK v0.30.
[    1.081078] ip_set: protocol 6
[    1.081561] ipip: IPv4 and MPLS over IPv4 tunneling driver
[    1.082551] ip_tables: (C) 2000-2006 Netfilter Core Team
[    1.083476] arp_tables: arp_tables: (C) 2002 David S. Miller
[    1.084264] Initializing XFRM netlink socket
[    1.085146] NET: Registered protocol family 10
[    1.086406] Segment Routing with IPv6
[    1.086916] sit: IPv6, IPv4 and MPLS over IPv4 tunneling driver
[    1.088016] NET: Registered protocol family 17
[    1.088682] Key type dns_resolver registered
[    1.090347] Loading compiled-in X.509 certificates
[    1.093885] Loaded X.509 cert 'Build time autogenerated kernel key: 81cb0ef77db2fac76e9588c2120c82422367d268'
[    1.095219] zswap: loaded using pool lzo/zbud
[    1.106506] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    1.108168] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    1.109171] console [netcon0] enabled
[    1.109646] netconsole: network logging started
[    1.110426] hobot-rtc a6002000.rtc: setting system clock to 1970-01-01 00:00:00 UTC (0)
[    1.111605] vps mipi_dphy: probe with x3vio done
[    1.112308] hobot_wdt_test: wdt_test_init: wdt test init
[    1.115058] VCC_CNN0: disabling
[    1.115467] VCC_CNN1: disabling
[    1.116423] vps mipi_host0: ver 140* port0(0:0)
[    1.117373] vps mipi_host1: ver 140* port1(1:0)
[    1.118264] vps mipi_host2: ver 140* port2(0:1)
[    1.119051] vps mipi_host3: ver 140* port3(1:1)
[    1.119888] ALSA device list:
[    1.120273]   No soundcards found.
[    1.120945] md: Skipping autodetection of RAID arrays. (raid=autodetect will force)
[    1.122089] VFS: Cannot open root device "mmcblk2p2" or unknown-block(0,0): error -6
[    1.123083] Please append a correct "root=" boot option; here are the available partitions:
[    1.124157] 0100          102400 ram0
[    1.124159]  (driver?)
[    1.124973] 0101          102400 ram1
[    1.124976]  (driver?)
[    1.125764] 0102          102400 ram2
[    1.125766]  (driver?)
[    1.126554] 0103          102400 ram3
[    1.126556]  (driver?)
[    1.127344] 0104          102400 ram4
[    1.127345]  (driver?)
[    1.128133] 0105          102400 ram5
[    1.128135]  (driver?)
[    1.128964] 0106          102400 ram6
[    1.128966]  (driver?)
[    1.129755] 0107          102400 ram7
[    1.129757]  (driver?)
[    1.130545] 0108          102400 ram8
[    1.130547]  (driver?)
[    1.131335] 0109          102400 ram9
[    1.131337]  (driver?)
[    1.132125] 010a          102400 ram10
[    1.132127]  (driver?)
[    1.132945] 010b          102400 ram11
[    1.132947]  (driver?)
[    1.133746] 010c          102400 ram12
[    1.133748]  (driver?)
[    1.134547] 010d          102400 ram13
[    1.134549]  (driver?)
[    1.135347] 010e          102400 ram14
[    1.135349]  (driver?)
[    1.136148] 010f          102400 ram15
[    1.136150]  (driver?)
[    1.136974] 1f00          131072 mtdblock0
[    1.136976]  (driver?)
[    1.137820] hobot_fusa: set_fusa_error_pin:75 set error pin to 1
[    1.138590] hobot_fusa: fusa errpin not ready
[    1.138594] Kernel panic - not syncing: VFS: Unable to mount root fs on unknown-block(0,0)
[    1.140213] Kernel Offset: disabled
[    1.140664] CPU features: 0x0002004
[    1.141113] Memory Limit: none
[    1.145663] Rebooting in 1 seconds..
[    1.216815] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.217537] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 1
[    1.218992] xhci-hcd xhci-hcd.0.auto: hcc params 0x0220fe6d hci version 0x110 quirks 0x0000000000010010
[    1.220228] xhci-hcd xhci-hcd.0.auto: irq 178, io mem 0xb2000000
[    1.221197] usb usb1: New USB device found, idVendor=1d6b, idProduct=0002, bcdDevice= 4.14
[    1.221788] mmc1: new HSSDIO card at address 0001
[    1.222864] usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.223792] usb usb1: Product: xHCI Host Controller
[    1.224421] usb usb1: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.225137] usb usb1: SerialNumber: xhci-hcd.0.auto
[    1.226068] hub 1-0:1.0: USB hub found
[    1.226574] hub 1-0:1.0: 1 port detected
[    1.227258] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.227972] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 2
[    1.228974] xhci-hcd xhci-hcd.0.auto: Host supports USB 3.0 SuperSpeed
[    1.229851] usb usb2: We don't know the algorithms for LPM for this host, disabling LPM.
[    1.230958] usb usb2: New USB device found, idVendor=1d6b, idProduct=0003, bcdDevice= 4.14
[    1.232021] usb usb2: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.232958] usb usb2: Product: xHCI Host Controller
[    1.233587] usb usb2: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.234293] usb usb2: SerialNumber: xhci-hcd.0.auto
[    1.235184] hub 2-0:1.0: USB hub found
[    1.235683] hub 2-0:1.0: 1 port detected
[    1.488575] usb 1-1: new high-speed USB device number 2 using xhci-hcd
[    1.648761] usb 1-1: New USB device found, idVendor=1a40, idProduct=0101, bcdDevice= 1.11
[    1.649814] usb 1-1: New USB device strings: Mfr=0, Product=1, SerialNumber=0
[    1.650731] usb 1-1: Product: USB 2.0 Hub
[    1.710020] hub 1-1:1.0: USB hub found
[    1.710541] hub 1-1:1.0: 4 ports detected
[    1.960578] mmc2: new UHS SDR104 SDHC card at address 0001
[    1.961595] mmcblk2: mmc2:0001 SD16G 29.8 GiB
[    1.963212]  mmcblk2: p1 p2
[    2.146174] SMP: stopping secondary CPUs
[    2.146682] psci: psci_sys_reset(reboot_mode=0)
NOTICE:  fast_boot:0

S
F
L
O
NOTICE:  efuse cpu_cfg = 0
W
NOTICE:  Booting Trusted Firmware
NOTICE:  BL1: v1.4(release):HR-ROM-Rel-v1.1-141-ga91d4dd-dirty
NOTICE:  BL1: Built : 11:24:44, Oct 23 2019
NOTICE:  boot src: 2
NOTICE:  GigaDev SPI NAND was found.
NOTICE:  Block size: 128 KiB, page size: 2048
NOTICE:  BL1: Booting BL2
Auth pass
NOTICE:  bl1_main exit
SPL normal reset flow
check_reset_state (2): wakeup address = 0x0, hw wakeup status = 0x3, wakeup src=0x100
patch for sys_pll 1200 with 100M eth
SFLOW_INIT
CHIP ID:PCB941/WAFER: W04/ X: X20/ Y: Y36
secondary_jump_to_spl: secure chip flow
X3 SPL : secondary core wake up and jump to spl done (cpu_core_cfg=0)
SFLOW_FIN_HW_A

U-Boot SPL 2018.09-g4ca851534c-dirty (May 11 2022 - 20:09:50 +0800)
SPACC Init - ID: (00000061)
SPL nand boot mode (from strap)
GigaDev SPI NAND was found.
Block size: 128 KiB, page size: 2048
ddr_type = 1 (LPDDR4)
hb_chip_package_type:3
load ddr header src_addr: 100000, load_addr: 802ca020, src_len: a00
find valid ddr image
ddr_hdr.ecc_gran: 0x0
ddr_hdr.ecc_map: 0x0
ddr_hdr.sbr_pattern0: 0x0
ddr_hdr.sbr_pattern1: 0x0
ddr_freq = 05
board id = 31540334
ddr datarate: 3200
### SAMSUNG DDR ###
no ddr pin set
detect part number: 108
detect ddr freq: c80
board id alternative:0x3
index is 12
index is 15
index is 19
hb_ddr_index: 19
ddr_type = 1, ddr_vendor=3, ddr_freq=3200
dram_pll_init
sscg disabled
control load ddrc src_addr: 15ae00, load_addr: 802caa20, src_len: 920
[DDR INFO]      ==ddr_release_info==
[DDR INFO]      VERSION:        develop
[DDR INFO]      BUILD:          2022-05-11-20:09
[DDR INFO]      GIT COMMIT:     4ca851534c1616ace920fdaa000c6fb717c1fb74
[DDR INFO]      GIT TIME:       Wed, 20 Apr 2022 18:28:49 +0800
[DDR INFO]      ==ddr_features==
[DDR INFO]      RDBI:           0
[DDR INFO]      WDBI:           1
[DDR INFO]      InlineECC:      0
[DDR INFO]      DM:             1
[DDR INFO]      DDC:            1
[DDR INFO]      SSCG:           0
[DDR INFO]      BOARD:          XS_ENABLE
[DDR INFO] ddr_controller_cfg done
load ddr phy src_addr: 15b800, load_addr: 802caa20, src_len: 420
ATxSlewRate     : 15f
ATxImpedance    : 7f
TxSlewRate      : 19f
TxOdtDrvStren   : 600
TxImpedanceCtrl : e3f
CalDrvStr0      : 11
VrefInGlobal    : 104
board_type = 4 (CUSTOMER_BOARD)
load dqmap src addr: 15d600, load_addr: 802caa20, src_len: 20
[DDR INFO] dwc_ddrphy_train start
magic = 544f4248
load imem1 src_addr: 11ce00, load_addr: 802caa20, src_len: 8000
load dmem1 src_addr: 15a000, load_addr: 802caa20, src_len: 684
executing 1D fw
load imem2 src_addr: 124e00, load_addr: 802caa20, src_len: 8000
load dmem2 src_addr: 15a800, load_addr: 802caa20, src_len: 564

*******************************************************
p_dmem_lpddr4_2d_16b->MR11_A0:54
p_dmem_lpddr4_2d_16b->MR14_A0:54
p_dmem_lpddr4_2d_16b->MR12_A0:51
p_dmem_lpddr4_2d_16b->MR22_A0:14

p_dmem_lpddr4_2d_16b->MR3_A0:b3
p_dmem_lpddr4_2d_16b->Reserved00:40
p_dmem_lpddr4_2d_16b->Reserved0E:4
p_dmem_lpddr4_2d_16b->Delay_Weight2D:20
p_dmem_lpddr4_2d_16b->Voltage_Weight2D:80
*******************************************************

executing 2D fw
load pie src_addr: 15be00, load_addr: 802caa20, src_len: 11f0
Set QoS.
get_ddr_mr_info:cs_num=1, mr5=0x1, mr8=0x10
no magic in efuse file,bypass efuse
total_sz = 4096
SPL_VERSION:7
uboot partition is uboot_A
load u-boot: src_addr=0x380000, dest_addr=0x4000000, len=2097152
load warm boot spl: addr=0x800, dest_addr=0x80000000, len=31232
load bl31: addr=0x300000, dest_addr=0x0, len=524288
SFLOW_AUTH_BL31
verify signature of header:  verify ok!
verify signature of image:  verify ok!
bypass bpu image
clear keybank!!!!
SFLOW_DBG_EN
Trying to boot from RAM
SPL: bl31 will jump to u-boot or other entry (0x4000000)
SFLOW_CLR_KEY
SFLOW_REG_LD
install_portal copy portal
install_portal call smc and jump to bl31 cold entry(0x0)
hb som type: 5
X3 PI reset VDD_SD done

U-Boot 2018.09-g40785bca (May 27 2022 - 16:30:48 +0800)

Model: Hobot XJ3 Soc Board
DRAM:  system DDR size: 0xffe00000
4 GiB
MMC:   dwmmc@A5010000: 0, dwmmc@A5011000: 1, dwmmc@A5012000: 2
Loading Environment from UBI... GigaDevice SPI NAND was found.
128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
*** Warning - bad CRC, using default environment

In:    serial@a5000000
Out:   serial@a5000000
Err:   serial@a5000000
Net:   x3 sdb reset eth phy done

Warning: ethernet@A5014000 (eth0) using random MAC address - 16:87:7f:7a:55:81
eth0: ethernet@A5014000
Disable cnn cores ..
dtb_name:hobot-x3-pi.dtb
base board type: X3 SDB
bootmode: NAND
board_id = 31540334
damaged volume, update marker is setdamaged volume, update marker is setdamaged volume, update marker is sethb_boot_args_cmd_set custom_bootargs 0 ubuntu_boot 0
Hit any key to stop autoboot:  0
enable watchdog success !
switch to partitions #0, OK
mmc2 is current device
Scanning mmc 2:2...
Found U-Boot script /boot/boot.scr
664 bytes read in 2 ms (324.2 KiB/s)
## Executing script at 03c10000
Boot script loaded from devtype:mmc devnum:2 devplist:2
bootargs = console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
Loading fdt file: /boot/hobot/hobot-x3-pi.dtb
69633 bytes read in 8 ms (8.3 MiB/s)
Loading kernel: /boot/Image
19163144 bytes read in 845 ms (21.6 MiB/s)
## Flattened Device Tree blob at 03c00000
   Booting using the fdt blob at 0x3c00000
   Loading Device Tree to 0000000003c00000, end 0000000003c1ffff ... OK
chip_id: ab36300
The address of the fdt is 0x3c00000
Changed status Done
Can't get fdt_addr !!!Orign(MAX) bpu model Reserve Mem Size to 64M!!

Starting kernel ...

[    0.000000] OF: reserved mem: OVERLAP DETECTED!
[    0.000000] image_r5_mem (0x0000000080000000--0x0000000080010000) overlaps with msg_r5_mem (0x000000008000f000--0x0000000080010000)
[    0.000000] Reserved memory: created CMA memory pool at 0x0000000004000000, size 672 MiB
[    0.000000] OF: reserved mem: initialized node ion_cma, compatible id shared-dma-pool
[    0.000000] cma: Reserved 16 MiB at 0x000000007f000000
[    0.000000] On node 0 totalpages: 1047808
[    0.000000]   DMA zone: 8180 pages used for memmap
[    0.000000]   DMA zone: 0 pages reserved
[    0.000000]   DMA zone: 523520 pages, LIFO batch:31
[    0.000000]   Normal zone: 8192 pages used for memmap
[    0.000000]   Normal zone: 524288 pages, LIFO batch:31
[    0.000000] psci: probing for conduit method from DT.
[    0.000000] psci: PSCIv1.1 detected in firmware.
[    0.000000] psci: Using standard PSCI v0.2 function IDs
[    0.000000] psci: MIGRATE_INFO_TYPE not supported.
[    0.000000] psci: SMC Calling Convention v1.1
[    0.000000] percpu: Embedded 25 pages/cpu @ffffffc17ff2a000 s65176 r8192 d29032 u102400
[    0.000000] pcpu-alloc: s65176 r8192 d29032 u102400 alloc=25*4096
[    0.000000] pcpu-alloc: [0] 0 [0] 1 [0] 2 [0] 3
[    0.000000] Detected VIPT I-cache on CPU0
[    0.000000] CPU features: enabling workaround for ARM erratum 845719
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 1031436
[    0.000000] Kernel command line: earlycon loglevel=8 kgdboc=ttyS0 video=hobot:x3sdb-hdmi  console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
[    0.000000] PID hash table entries: 4096 (order: 3, 32768 bytes)
[    0.000000] Dentry cache hash table entries: 524288 (order: 10, 4194304 bytes)
[    0.000000] Inode-cache hash table entries: 262144 (order: 9, 2097152 bytes)
[    0.000000] software IO TLB [mem 0x7afff000-0x7efff000] (64MB) mapped at [ffffffc07afff000-ffffffc07effefff]
[    0.000000] Memory: 3319580K/4191232K available (10494K kernel code, 1306K rwdata, 5756K rodata, 1088K init, 9553K bss, 167140K reserved, 704512K cma-reserved)
[    0.000000] Virtual kernel memory layout:
[    0.000000]     modules : 0xffffff8000000000 - 0xffffff8008000000   (   128 MB)
[    0.000000]     vmalloc : 0xffffff8008000000 - 0xffffffbebfff0000   (   250 GB)
[    0.000000]       .text : 0xffffff8008000000 - 0xffffff8008a40000   ( 10496 KB)
[    0.000000]     .rodata : 0xffffff8008a40000 - 0xffffff8008ff0000   (  5824 KB)
[    0.000000]       .init : 0xffffff8008ff0000 - 0xffffff8009100000   (  1088 KB)
[    0.000000]       .data : 0xffffff8009100000 - 0xffffff8009246808   (  1307 KB)
[    0.000000]        .bss : 0xffffff8009246808 - 0xffffff8009b9aed8   (  9554 KB)
[    0.000000]     fixed   : 0xffffffbefe7fd000 - 0xffffffbefec00000   (  4108 KB)
[    0.000000]     PCI I/O : 0xffffffbefee00000 - 0xffffffbeffe00000   (    16 MB)
[    0.000000]     vmemmap : 0xffffffbf00000000 - 0xffffffc000000000   (     4 GB maximum)
[    0.000000]               0xffffffbf00008000 - 0xffffffbf06000000   (    95 MB actual)
[    0.000000]     memory  : 0xffffffc000200000 - 0xffffffc180000000   (  6142 MB)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=4, Nodes=1
[    0.000000] ftrace: allocating 36277 entries in 142 pages
[    0.000000] Preemptible hierarchical RCU implementation.
[    0.000000]  Tasks RCU enabled.
[    0.000000] NR_IRQS: 64, nr_irqs: 64, preallocated irqs: 0
[    0.000000] parent_rate: 0,  dclk->rate:2666000000, pre_ddr_rate:0, res.a0:139716712
[    0.000000] arch_timer: cp15 timer(s) running at 24.00MHz (virt).
[    0.000000] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0x588fe9dc0, max_idle_ns: 440795202592 ns
[    0.000004] sched_clock: 56 bits at 24MHz, resolution 41ns, wraps every 4398046511097ns
[    0.001195] clocksource: hobot_clocksource: mask: 0xffffffffffffffff max_cycles: 0x1d854df40, max_idle_ns: 3526361616960 ns
[    0.002969] Console: colour dummy device 80x25
[    0.003540] Calibrating delay loop (skipped), value calculated using timer frequency.. 48.00 BogoMIPS (lpj=96000)
[    0.004845] pid_max: default: 32768 minimum: 301
[    0.005500] Security Framework initialized
[    0.006018] AppArmor: AppArmor disabled by boot time parameter
[    0.006860] Mount-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.007728] Mountpoint-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.023771] ASID allocator initialised with 65536 entries
[    0.031768] Hierarchical SRCU implementation.
[    0.063826] smp: Bringing up secondary CPUs ...
[    0.100032] Detected VIPT I-cache on CPU1
[    0.100067] CPU1: Booted secondary processor [410fd034]
[    0.136083] Detected VIPT I-cache on CPU2
[    0.136104] CPU2: Booted secondary processor [410fd034]
[    0.172142] Detected VIPT I-cache on CPU3
[    0.172162] CPU3: Booted secondary processor [410fd034]
[    0.172216] smp: Brought up 1 node, 4 CPUs
[    0.176279] SMP: Total of 4 processors activated.
[    0.176873] CPU features: detected feature: 32-bit EL0 Support
[    0.177693] CPU: All CPU(s) started at EL1
[    0.178221] alternatives: patching kernel code
[    0.179809] devtmpfs: initialized
[    0.188885] random: get_random_u32 called from bucket_table_alloc+0x108/0x270 with crng_init=0
[    0.190455] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 7645041785100000 ns
[    0.191700] futex hash table entries: 1024 (order: 5, 131072 bytes)
[    0.208217] xor: automatically using best checksumming function   32regs
[    0.209154] pinctrl core: initialized pinctrl subsystem
[    0.210375] NET: Registered protocol family 16
[    0.211686] vdso: 2 pages (1 code @ ffffff8008a46000, 1 data @ ffffff8009104000)
[    0.212631] hw-breakpoint: found 6 breakpoint and 4 watchpoint registers.
[    0.214216] DMA: preallocated 256 KiB pool for atomic allocations
[    0.218835] pstore: using zlib compression
[    0.219627] console [pstore-1] enabled
[    0.220222] pstore: Registered ramoops as persistent store backend
[    0.221007] ramoops: attached 0x40000@0x3fc0000, ecc: 0/0
[    0.225992] hobot_dma a1005000.dma: Hobot DMA Engine Driver Probed!!
[    0.240105] SCSI subsystem initialized
[    0.240763] media: Linux media interface: v0.10
[    0.241357] Linux video capture interface: v2.00
[    0.242137] pps_core: LinuxPPS API ver. 1 registered
[    0.242765] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.243941] PTP clock support registered
[    0.245080] ion_dummy: not reserve carveout memory, try to alloc from cma
[    0.381543] Advanced Linux Sound Architecture Driver Initialized.
[    0.382700] usbcore: registered new interface driver usbfs
[    0.383426] usbcore: registered new interface driver hub
[    0.384153] usbcore: registered new device driver usb
[    0.385119] clocksource: Switched to clocksource arch_sys_counter
[    0.432532] VFS: Disk quotas dquot_6.6.0
[    0.433074] VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
[    0.434037] FS-Cache: Loaded
[    0.434515] CacheFiles: Loaded
[    0.439748] NET: Registered protocol family 2
[    0.440677] TCP established hash table entries: 32768 (order: 6, 262144 bytes)
[    0.441824] TCP bind hash table entries: 32768 (order: 7, 524288 bytes)
[    0.443050] TCP: Hash tables configured (established 32768 bind 32768)
[    0.443957] UDP hash table entries: 2048 (order: 4, 65536 bytes)
[    0.444786] UDP-Lite hash table entries: 2048 (order: 4, 65536 bytes)
[    0.445809] NET: Registered protocol family 1
[    0.446616] RPC: Registered named UNIX socket transport module.
[    0.447366] RPC: Registered udp transport module.
[    0.447963] RPC: Registered tcp transport module.
[    0.448562] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.450177] hw perfevents: enabled with armv8_cortex_a53 PMU driver, 7 counters available
[    0.452383] audit: initializing netlink subsys (disabled)
[    0.453190] audit: type=2000 audit(0.452:1): state=initialized audit_enabled=0 res=1
[    0.453449] Initialise system trusted keyrings
[    0.453524] workingset: timestamp_bits=46 max_order=20 bucket_order=0
[    0.457090] zbud: loaded
[    0.458775] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.459635] exFAT: Version 1.2.9
[    0.460113] FS-Cache: Netfs 'nfs' registered for caching
[    0.461403] NFS: Registering the id_resolver key type
[    0.462056] Key type id_resolver registered
[    0.462583] Key type id_legacy registered
[    0.463098] nfs4filelayout_init: NFSv4 File Layout Driver Registering...
[    0.463951] Installing knfsd (copyright (C) 1996 okir@monad.swb.de).
[    0.467959] NET: Registered protocol family 38
[    0.468529] async_tx: api initialized (async)
[    0.469081] Key type asymmetric registered
[    0.469612] Asymmetric key parser 'x509' registered
[    0.470289] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 245)
[    0.471306] io scheduler noop registered
[    0.471957] io scheduler cfq registered (default)
[    0.472551] io scheduler mq-deadline registered
[    0.473279] io scheduler kyber registered
[    0.474459] pinctrl-single a6003170.pinctrl_voltag: 64 pins at pa ffffff8009c4d170 size 8
[    0.475793] pinctrl-single a6004000.pinctrl: 128 pins at pa ffffff8009c61000 size 512
[    0.476989] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: start probe
[    0.477891] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: probe ok
[    0.478767] gpio-x3 a6003000.gpio: x3 gpio probe start!!!
[    0.479457] gpio-x3 a6003000.gpio: x3 gpio add gpiochip start!!!
[    0.480379] gpio-x3 a6003000.gpio: diable all gpio irq
[    0.482641] gpio-x3 a6003000.gpio: irqbase:57
[    0.483193] gpio-x3 a6003000.gpio: x3 irq add start!!!
[    0.483850] irq: Cannot allocate irq_descs @ IRQ57, assuming pre-allocated
[    0.484878] gpio-x3 a6003000.gpio: x3 irq add ok!!!
[    0.485646] gpio-x3 a6003000.gpio: x3 irqchip ops add ok!!!
[    0.486352] gpio-x3 a6003000.gpio: x3 gpio probe ok!!!
[    0.487447] hobot-pwm: hobot-pwmchip0 registered
[    0.488198] hobot-pwm: hobot-pwmchip1 registered
[    0.489546] diag dev [ver:1.1] init done
[    0.490436] hobot_ddr_monitor: LPDDR4 detected
[    0.491195] hobot_ddr_monitor: ddr monitor init finished.
[    0.491596] [vcam] init start
[    0.492655] vcam probe start
[    0.493102] vcam probe end successful
[    0.493641] [vcam] init end
[    0.494580] a5000000.serial: ttyS0 at MMIO 0xa5000000 (irq = 10, base_baud = 12000000) is a hobot-uart
[    0.495792] console [ttyS0] enabled
[    0.495792] console [ttyS0] enabled
[    0.496675] bootconsole [hobot0] disabled
[    0.496675] bootconsole [hobot0] disabled
[    0.498030] hobot-uart a5001000.serial: Failed to create debugfs root directory
[    0.499033] a5001000.serial: ttyS1 at MMIO 0xa5001000 (irq = 11, base_baud = 12000000) is a hobot-uart
[    0.500482] hobot-uart a5003000.serial: Failed to create debugfs root directory
[    0.501543] a5003000.serial: ttyS3 at MMIO 0xa5003000 (irq = 12, base_baud = 12000000) is a hobot-uart
[    0.503081] KGDB: Registered I/O driver kgdboc
[    0.503928] cacheinfo: Unable to detect cache hierarchy for CPU 0
[    0.509388] brd: module loaded
[    0.513942] loop: module loaded
[    0.515480] spi-nand hr_nand.0: GigaDevice SPI NAND was found.
[    0.516240] spi-nand hr_nand.0: 128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
[    0.518957] hobot_spi a5006000.spi: ver: HOBOT-spi_V20.200330 master
[    0.520001] libphy: Fixed MDIO Bus: probed
[    0.521299] st_gmac a5014000.ethernet: found phy-handle subnode
[    0.522135] st_gmac a5014000.ethernet: xj3_mtl_setup, plat->rx-queues-to-use:4, and tx:4
[    0.523321] st_gmac a5014000.ethernet: xj3_probe_config_dt, clk_ptp_rate:250000000
[    0.524324] set mac address 00:11:22:6d:f2:d9:
[    0.524326] (using random mac adress)
[    0.525504] (NULL device *): xj3_get_hw_features, tx_fifo_size:16384
[    0.526321] (NULL device *): xj3_get_hw_features, rx_fifo_size:16384
[    0.527139] st_gmac a5014000.ethernet: TSO supported
[    0.527779] st_gmac a5014000.ethernet: TSO feature enabled
[    0.528485] st_gmac a5014000.ethernet: Enable Rx Mitigation via HW Watchdog Timer
[    0.649558] libphy: hobot-mac-mdio: probed
[    0.651113] st_gmac a5014000.ethernet: hobot_eth_probe: probe sucessfully
[    0.652313] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_0v8 not found, using dummy regulator
[    0.653557] dwc3-of-simple b2000000.usb: usb regulator 0v8 enable succeed
[    0.654434] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_3v3 not found, using dummy regulator
[    0.655636] dwc3-of-simple b2000000.usb: usb regulator 3v3 enable succeed
[    0.657184] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    0.658841] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    0.660277] usbcore: registered new interface driver cdc_acm
[    0.661006] cdc_acm: USB Abstract Control Model driver for USB modems and ISDN adapters
[    0.662084] usbcore: registered new interface driver uas
[    0.662801] usbcore: registered new interface driver usb-storage
[    0.663628] usbcore: registered new interface driver usbserial
[    0.664402] usbcore: registered new interface driver usbserial_generic
[    0.665281] usbserial: USB Serial support registered for generic
[    0.666078] usbcore: registered new interface driver usb_serial_simple
[    0.666935] usbserial: USB Serial support registered for carelink
[    0.667735] usbserial: USB Serial support registered for zio
[    0.668480] usbserial: USB Serial support registered for funsoft
[    0.669287] usbserial: USB Serial support registered for flashloader
[    0.670124] usbserial: USB Serial support registered for google
[    0.670903] usbserial: USB Serial support registered for libtransistor
[    0.671759] usbserial: USB Serial support registered for vivopay
[    0.672549] usbserial: USB Serial support registered for moto_modem
[    0.673388] usbserial: USB Serial support registered for motorola_tetra
[    0.674256] usbserial: USB Serial support registered for novatel_gps
[    0.675093] usbserial: USB Serial support registered for hp4x
[    0.675849] usbserial: USB Serial support registered for suunto
[    0.676635] usbserial: USB Serial support registered for siemens_mpi
[    0.677499] usbcore: registered new interface driver rio500
[    0.678333] mousedev: PS/2 mouse device common for all mice
[    0.689381] hobot-rtc a6002000.rtc: rtc core: registered hobot-rtc as rtc0
[    0.690372] i2c /dev entries driver
[    0.690981] hobot-i2c a5009000.i2c: hobot i2c probe start
[    0.691743] hobot-i2c a5009000.i2c: round_rate:96000000
[    0.692420] hobot-i2c a5009000.i2c: I2C bus speed is 400000
[    0.693159] hobot-i2c a5009000.i2c: clkdiv = 0x1d
[    0.693766] hobot-i2c a5009000.i2c: i2c0 diag register....
[    0.694864] hobot-i2c a5009000.i2c: hobot_i2c_0 probe done
[    0.695666] hobot-i2c a500a000.i2c: hobot i2c probe start
[    0.696417] hobot-i2c a500a000.i2c: round_rate:96000000
[    0.697093] hobot-i2c a500a000.i2c: I2C bus speed is 400000
[    0.697832] hobot-i2c a500a000.i2c: clkdiv = 0x1d
[    0.698439] hobot-i2c a500a000.i2c: i2c1 diag register....
[    0.699450] hobot-i2c a500a000.i2c: hobot_i2c_1 probe done
[    0.700409] lirc_dev: IR Remote Control driver registered, major 239
[    0.701248] IR LIRC bridge handler initialized
[    0.701998] sif_mclk clock frequence is 544000000
[    0.702635] mipi_rx0_ipi clock frequence is 544000000
[    0.703324] mipi_rx1_ipi clock frequence is 544000000
[    0.704022] mipi_rx2_ipi clock frequence is 544000000
[    0.704731] mipi_rx3_ipi clock frequence is 544000000
[    0.705464] mipi_tx_ipi clock frequence is 544000000
[    0.706185] mipi_cfg_host clock frequence is 102000000
[    0.706939] pym_mclk clock frequence is 1188000000
[    0.707658] mipi_dev_ref clock frequence is 24000000
[    0.708412] mipi_host_ref clock frequence is 24000000
[    0.709197] sensor0_mclk clock frequence is 37125000
[    0.709973] sensor1_mclk clock frequence is 37125000
[    0.710763] sensor2_mclk clock frequence is 37125000
[    0.711561] sensor3_mclk clock frequence is 37125000
[    0.712201] [FRT:D] x3_ips_probe(0)
[    0.713232] hobot swinfo sel reg ro=0x1 boot dump
[    0.714162] pvt a1009000.pvt: SCRATCH test: 1234abcd, pvt is alive.
[    0.715085] pvt a1009000.pvt: VM Calibrated data detected
[    0.716270] hobot_wdt a1002000.watchdog: watchdog setting [pet:6s bark:11s bite:15s]
[    0.717611] hobot_wdt a1002000.watchdog: Hobot Watchdog Timer at ffffff8009db3000 with timeout 15s
[    0.718951] device-mapper: uevent: version 1.0.3
[    0.719708] device-mapper: ioctl: 4.37.0-ioctl (2017-09-20) initialised: dm-devel@redhat.com
[    0.720868] device-mapper: verity-avb: AVB error handler initialized with vbmeta device:
[    0.723338] Synopsys Designware Multimedia Card Interface Driver
[    0.724336] dwmmc_hobot a5010000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.725190] dwmmc_hobot a5010000.dwmmc: card-detect-delay not found.
[    0.726009] dwmmc_hobot a5010000.dwmmc: data-addr not found.
[    0.727046] mmc_host mmc0: card is non-removable.
[    0.766342] dwmmc_hobot a5011000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.769255] dwmmc_hobot a5011000.dwmmc: card-detect-delay not found.
[    0.770075] dwmmc_hobot a5011000.dwmmc: data-addr not found.
[    0.774848] dwmmc_hobot a5011000.dwmmc: mmc set to fixed voltage 1800
[    0.775918] mmc_host mmc1: card is non-removable.
[    0.873315] dwmmc_hobot a5012000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.874132] dwmmc_hobot a5012000.dwmmc: card-detect-delay not found.
[    0.874963] dwmmc_hobot a5012000.dwmmc: data-addr not found.
[    0.875927] dwmmc_hobot a5012000.dwmmc: Got CD GPIO
[    0.986829] mmc1: queuing unknown CIS tuple 0x80 (2 bytes)
[    0.989014] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.991208] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.994574] mmc1: queuing unknown CIS tuple 0x80 (7 bytes)
[    0.998529] mmc1: queuing unknown CIS tuple 0x81 (9 bytes)
[    1.065441] ledtrig-cpu: registered to indicate activity on CPUs
[    1.066266] hidraw: raw HID events driver (C) Jiri Kosina
[    1.067113] usbcore: registered new interface driver usbhid
[    1.067859] usbhid: USB HID core driver
[    1.068443] logger: created 256K log 'log_main'
[    1.069096] logger: created 256K log 'log_events'
[    1.069792] logger: created 256K log 'log_radio'
[    1.070454] logger: created 256K log 'log_system'
[    1.071507] set dmc devfreq governor to performance
[    1.072150] hobot_dmcfreq_target: dmcfreq->rate:2666000000, target_rate:2666000000
[    1.073148] buf:, powersave_rate:2666000000, dmcfreq->pre_state:0
[    1.080005] usbcore: registered new interface driver snd-usb-audio
[    1.081197] Netfilter messages via NETLINK v0.30.
[    1.081834] ip_set: protocol 6
[    1.082328] ipip: IPv4 and MPLS over IPv4 tunneling driver
[    1.083350] ip_tables: (C) 2000-2006 Netfilter Core Team
[    1.084355] arp_tables: arp_tables: (C) 2002 David S. Miller
[    1.085169] Initializing XFRM netlink socket
[    1.086035] NET: Registered protocol family 10
[    1.087253] Segment Routing with IPv6
[    1.087762] sit: IPv6, IPv4 and MPLS over IPv4 tunneling driver
[    1.088856] NET: Registered protocol family 17
[    1.089550] Key type dns_resolver registered
[    1.091186] Loading compiled-in X.509 certificates
[    1.094698] Loaded X.509 cert 'Build time autogenerated kernel key: 81cb0ef77db2fac76e9588c2120c82422367d268'
[    1.096029] zswap: loaded using pool lzo/zbud
[    1.107301] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    1.108963] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    1.109971] console [netcon0] enabled
[    1.110446] netconsole: network logging started
[    1.111228] hobot-rtc a6002000.rtc: setting system clock to 1970-01-01 00:00:00 UTC (0)
[    1.112410] vps mipi_dphy: probe with x3vio done
[    1.113140] hobot_wdt_test: wdt_test_init: wdt test init
[    1.115846] VCC_CNN0: disabling
[    1.116256] VCC_CNN1: disabling
[    1.117249] vps mipi_host0: ver 140* port0(0:0)
[    1.118164] vps mipi_host1: ver 140* port1(1:0)
[    1.119056] vps mipi_host2: ver 140* port2(0:1)
[    1.119856] vps mipi_host3: ver 140* port3(1:1)
[    1.120690] ALSA device list:
[    1.121075]   No soundcards found.
[    1.121813] md: Skipping autodetection of RAID arrays. (raid=autodetect will force)
[    1.122957] VFS: Cannot open root device "mmcblk2p2" or unknown-block(0,0): error -6
[    1.123951] Please append a correct "root=" boot option; here are the available partitions:
[    1.125026] 0100          102400 ram0
[    1.125028]  (driver?)
[    1.125844] 0101          102400 ram1
[    1.125846]  (driver?)
[    1.126635] 0102          102400 ram2
[    1.126636]  (driver?)
[    1.127424] 0103          102400 ram3
[    1.127426]  (driver?)
[    1.128214] 0104          102400 ram4
[    1.128216]  (driver?)
[    1.129003] 0105          102400 ram5
[    1.129005]  (driver?)
[    1.129846] 0106          102400 ram6
[    1.129848]  (driver?)
[    1.130637] 0107          102400 ram7
[    1.130639]  (driver?)
[    1.131426] 0108          102400 ram8
[    1.131428]  (driver?)
[    1.132216] 0109          102400 ram9
[    1.132218]  (driver?)
[    1.133006] 010a          102400 ram10
[    1.133008]  (driver?)
[    1.133826] 010b          102400 ram11
[    1.133828]  (driver?)
[    1.134627] 010c          102400 ram12
[    1.134629]  (driver?)
[    1.135428] 010d          102400 ram13
[    1.135430]  (driver?)
[    1.136229] 010e          102400 ram14
[    1.136230]  (driver?)
[    1.137029] 010f          102400 ram15
[    1.137031]  (driver?)
[    1.137858] 1f00          131072 mtdblock0
[    1.137860]  (driver?)
[    1.138704] hobot_fusa: set_fusa_error_pin:75 set error pin to 1
[    1.139474] hobot_fusa: fusa errpin not ready
[    1.139478] Kernel panic - not syncing: VFS: Unable to mount root fs on unknown-block(0,0)
[    1.141096] Kernel Offset: disabled
[    1.141548] CPU features: 0x0002004
[    1.141997] Memory Limit: none
[    1.146519] Rebooting in 1 seconds..
[    1.217371] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.218093] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 1
[    1.219549] xhci-hcd xhci-hcd.0.auto: hcc params 0x0220fe6d hci version 0x110 quirks 0x0000000000010010
[    1.220784] xhci-hcd xhci-hcd.0.auto: irq 178, io mem 0xb2000000
[    1.221752] usb usb1: New USB device found, idVendor=1d6b, idProduct=0002, bcdDevice= 4.14
[    1.222815] usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.223744] usb usb1: Product: xHCI Host Controller
[    1.224373] usb usb1: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.225079] usb usb1: SerialNumber: xhci-hcd.0.auto
[    1.226032] hub 1-0:1.0: USB hub found
[    1.226534] hub 1-0:1.0: 1 port detected
[    1.227221] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.227934] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 2
[    1.228923] xhci-hcd xhci-hcd.0.auto: Host supports USB 3.0 SuperSpeed
[    1.229859] usb usb2: We don't know the algorithms for LPM for this host, disabling LPM.
[    1.231028] usb usb2: New USB device found, idVendor=1d6b, idProduct=0003, bcdDevice= 4.14
[    1.232102] usb usb2: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.233041] usb usb2: Product: xHCI Host Controller
[    1.233685] usb usb2: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.234398] usb usb2: SerialNumber: xhci-hcd.0.auto
[    1.235529] hub 2-0:1.0: USB hub found
[    1.236051] hub 2-0:1.0: 1 port detected
[    1.237046] mmc1: new HSSDIO card at address 0001
[    1.481127] usb 1-1: new high-speed USB device number 2 using xhci-hcd
[    1.629316] usb 1-1: New USB device found, idVendor=1a40, idProduct=0101, bcdDevice= 1.11
[    1.630369] usb 1-1: New USB device strings: Mfr=0, Product=1, SerialNumber=0
[    1.631286] usb 1-1: Product: USB 2.0 Hub
[    1.677984] hub 1-1:1.0: USB hub found
[    1.678503] hub 1-1:1.0: 4 ports detected
[    1.961131] mmc2: new UHS SDR104 SDHC card at address 0001
[    1.962151] mmcblk2: mmc2:0001 SD16G 29.8 GiB
[    1.963766]  mmcblk2: p1 p2
[    2.147030] SMP: stopping secondary CPUs
[    2.147538] psci: psci_sys_reset(reboot_mode=0)
NOTICE:  fast_boot:0

S
F
L
O
NOTICE:  efuse cpu_cfg = 0
W
NOTICE:  Booting Trusted Firmware
NOTICE:  BL1: v1.4(release):HR-ROM-Rel-v1.1-141-ga91d4dd-dirty
NOTICE:  BL1: Built : 11:24:44, Oct 23 2019
NOTICE:  boot src: 2
NOTICE:  GigaDev SPI NAND was found.
NOTICE:  Block size: 128 KiB, page size: 2048
NOTICE:  BL1: Booting BL2
Auth pass
NOTICE:  bl1_main exit
SPL normal reset flow
check_reset_state (2): wakeup address = 0x0, hw wakeup status = 0x3, wakeup src=0x100
patch for sys_pll 1200 with 100M eth
SFLOW_INIT
CHIP ID:PCB941/WAFER: W04/ X: X20/ Y: Y36
secondary_jump_to_spl: secure chip flow
X3 SPL : secondary core wake up and jump to spl done (cpu_core_cfg=0)
SFLOW_FIN_HW_A

U-Boot SPL 2018.09-g4ca851534c-dirty (May 11 2022 - 20:09:50 +0800)
SPACC Init - ID: (00000061)
SPL nand boot mode (from strap)
GigaDev SPI NAND was found.
Block size: 128 KiB, page size: 2048
ddr_type = 1 (LPDDR4)
hb_chip_package_type:3
load ddr header src_addr: 100000, load_addr: 802ca020, src_len: a00
find valid ddr image
ddr_hdr.ecc_gran: 0x0
ddr_hdr.ecc_map: 0x0
ddr_hdr.sbr_pattern0: 0x0
ddr_hdr.sbr_pattern1: 0x0
ddr_freq = 05
board id = 31540334
ddr datarate: 3200
### SAMSUNG DDR ###
no ddr pin set
detect part number: 108
detect ddr freq: c80
board id alternative:0x3
index is 12
index is 15
index is 19
hb_ddr_index: 19
ddr_type = 1, ddr_vendor=3, ddr_freq=3200
dram_pll_init
sscg disabled
control load ddrc src_addr: 15ae00, load_addr: 802caa20, src_len: 920
[DDR INFO]      ==ddr_release_info==
[DDR INFO]      VERSION:        develop
[DDR INFO]      BUILD:          2022-05-11-20:09
[DDR INFO]      GIT COMMIT:     4ca851534c1616ace920fdaa000c6fb717c1fb74
[DDR INFO]      GIT TIME:       Wed, 20 Apr 2022 18:28:49 +0800
[DDR INFO]      ==ddr_features==
[DDR INFO]      RDBI:           0
[DDR INFO]      WDBI:           1
[DDR INFO]      InlineECC:      0
[DDR INFO]      DM:             1
[DDR INFO]      DDC:            1
[DDR INFO]      SSCG:           0
[DDR INFO]      BOARD:          XS_ENABLE
[DDR INFO] ddr_controller_cfg done
load ddr phy src_addr: 15b800, load_addr: 802caa20, src_len: 420
ATxSlewRate     : 15f
ATxImpedance    : 7f
TxSlewRate      : 19f
TxOdtDrvStren   : 600
TxImpedanceCtrl : e3f
CalDrvStr0      : 11
VrefInGlobal    : 104
board_type = 4 (CUSTOMER_BOARD)
load dqmap src addr: 15d600, load_addr: 802caa20, src_len: 20
[DDR INFO] dwc_ddrphy_train start
magic = 544f4248
load imem1 src_addr: 11ce00, load_addr: 802caa20, src_len: 8000
load dmem1 src_addr: 15a000, load_addr: 802caa20, src_len: 684
executing 1D fw
load imem2 src_addr: 124e00, load_addr: 802caa20, src_len: 8000
load dmem2 src_addr: 15a800, load_addr: 802caa20, src_len: 564

*******************************************************
p_dmem_lpddr4_2d_16b->MR11_A0:54
p_dmem_lpddr4_2d_16b->MR14_A0:54
p_dmem_lpddr4_2d_16b->MR12_A0:51
p_dmem_lpddr4_2d_16b->MR22_A0:14

p_dmem_lpddr4_2d_16b->MR3_A0:b3
p_dmem_lpddr4_2d_16b->Reserved00:40
p_dmem_lpddr4_2d_16b->Reserved0E:4
p_dmem_lpddr4_2d_16b->Delay_Weight2D:20
p_dmem_lpddr4_2d_16b->Voltage_Weight2D:80
*******************************************************

executing 2D fw
load pie src_addr: 15be00, load_addr: 802caa20, src_len: 11f0
Set QoS.
get_ddr_mr_info:cs_num=1, mr5=0x1, mr8=0x10
no magic in efuse file,bypass efuse
total_sz = 4096
SPL_VERSION:7
uboot partition is uboot_A
load u-boot: src_addr=0x380000, dest_addr=0x4000000, len=2097152
load warm boot spl: addr=0x800, dest_addr=0x80000000, len=31232
load bl31: addr=0x300000, dest_addr=0x0, len=524288
SFLOW_AUTH_BL31
verify signature of header:  verify ok!
verify signature of image:  verify ok!
bypass bpu image
clear keybank!!!!
SFLOW_DBG_EN
Trying to boot from RAM
SPL: bl31 will jump to u-boot or other entry (0x4000000)
SFLOW_CLR_KEY
SFLOW_REG_LD
install_portal copy portal
install_portal call smc and jump to bl31 cold entry(0x0)
hb som type: 5
X3 PI reset VDD_SD done

U-Boot 2018.09-g40785bca (May 27 2022 - 16:30:48 +0800)

Model: Hobot XJ3 Soc Board
DRAM:  system DDR size: 0xffe00000
4 GiB
MMC:   dwmmc@A5010000: 0, dwmmc@A5011000: 1, dwmmc@A5012000: 2
Loading Environment from UBI... GigaDevice SPI NAND was found.
128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
*** Warning - bad CRC, using default environment

In:    serial@a5000000
Out:   serial@a5000000
Err:   serial@a5000000
Net:   x3 sdb reset eth phy done

Warning: ethernet@A5014000 (eth0) using random MAC address - ea:ef:66:d9:91:45
eth0: ethernet@A5014000
Disable cnn cores ..
dtb_name:hobot-x3-pi.dtb
base board type: X3 SDB
bootmode: NAND
board_id = 31540334
damaged volume, update marker is setdamaged volume, update marker is setdamaged volume, update marker is sethb_boot_args_cmd_set custom_bootargs 0 ubuntu_boot 0
Hit any key to stop autoboot:  0
enable watchdog success !
switch to partitions #0, OK
mmc2 is current device
Scanning mmc 2:2...
Found U-Boot script /boot/boot.scr
664 bytes read in 2 ms (324.2 KiB/s)
## Executing script at 03c10000
Boot script loaded from devtype:mmc devnum:2 devplist:2
bootargs = console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
Loading fdt file: /boot/hobot/hobot-x3-pi.dtb
69633 bytes read in 8 ms (8.3 MiB/s)
Loading kernel: /boot/Image
19163144 bytes read in 845 ms (21.6 MiB/s)
## Flattened Device Tree blob at 03c00000
   Booting using the fdt blob at 0x3c00000
   Loading Device Tree to 0000000003c00000, end 0000000003c1ffff ... OK
chip_id: ab36300
The address of the fdt is 0x3c00000
Changed status Done
Can't get fdt_addr !!!Orign(MAX) bpu model Reserve Mem Size to 64M!!

Starting kernel ...

[    0.000000] OF: reserved mem: OVERLAP DETECTED!
[    0.000000] image_r5_mem (0x0000000080000000--0x0000000080010000) overlaps with msg_r5_mem (0x000000008000f000--0x0000000080010000)
[    0.000000] Reserved memory: created CMA memory pool at 0x0000000004000000, size 672 MiB
[    0.000000] OF: reserved mem: initialized node ion_cma, compatible id shared-dma-pool
[    0.000000] cma: Reserved 16 MiB at 0x000000007f000000
[    0.000000] On node 0 totalpages: 1047808
[    0.000000]   DMA zone: 8180 pages used for memmap
[    0.000000]   DMA zone: 0 pages reserved
[    0.000000]   DMA zone: 523520 pages, LIFO batch:31
[    0.000000]   Normal zone: 8192 pages used for memmap
[    0.000000]   Normal zone: 524288 pages, LIFO batch:31
[    0.000000] psci: probing for conduit method from DT.
[    0.000000] psci: PSCIv1.1 detected in firmware.
[    0.000000] psci: Using standard PSCI v0.2 function IDs
[    0.000000] psci: MIGRATE_INFO_TYPE not supported.
[    0.000000] psci: SMC Calling Convention v1.1
[    0.000000] percpu: Embedded 25 pages/cpu @ffffffc17ff2a000 s65176 r8192 d29032 u102400
[    0.000000] pcpu-alloc: s65176 r8192 d29032 u102400 alloc=25*4096
[    0.000000] pcpu-alloc: [0] 0 [0] 1 [0] 2 [0] 3
[    0.000000] Detected VIPT I-cache on CPU0
[    0.000000] CPU features: enabling workaround for ARM erratum 845719
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 1031436
[    0.000000] Kernel command line: earlycon loglevel=8 kgdboc=ttyS0 video=hobot:x3sdb-hdmi  console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
[    0.000000] PID hash table entries: 4096 (order: 3, 32768 bytes)
[    0.000000] Dentry cache hash table entries: 524288 (order: 10, 4194304 bytes)
[    0.000000] Inode-cache hash table entries: 262144 (order: 9, 2097152 bytes)
[    0.000000] software IO TLB [mem 0x7afff000-0x7efff000] (64MB) mapped at [ffffffc07afff000-ffffffc07effefff]
[    0.000000] Memory: 3319580K/4191232K available (10494K kernel code, 1306K rwdata, 5756K rodata, 1088K init, 9553K bss, 167140K reserved, 704512K cma-reserved)
[    0.000000] Virtual kernel memory layout:
[    0.000000]     modules : 0xffffff8000000000 - 0xffffff8008000000   (   128 MB)
[    0.000000]     vmalloc : 0xffffff8008000000 - 0xffffffbebfff0000   (   250 GB)
[    0.000000]       .text : 0xffffff8008000000 - 0xffffff8008a40000   ( 10496 KB)
[    0.000000]     .rodata : 0xffffff8008a40000 - 0xffffff8008ff0000   (  5824 KB)
[    0.000000]       .init : 0xffffff8008ff0000 - 0xffffff8009100000   (  1088 KB)
[    0.000000]       .data : 0xffffff8009100000 - 0xffffff8009246808   (  1307 KB)
[    0.000000]        .bss : 0xffffff8009246808 - 0xffffff8009b9aed8   (  9554 KB)
[    0.000000]     fixed   : 0xffffffbefe7fd000 - 0xffffffbefec00000   (  4108 KB)
[    0.000000]     PCI I/O : 0xffffffbefee00000 - 0xffffffbeffe00000   (    16 MB)
[    0.000000]     vmemmap : 0xffffffbf00000000 - 0xffffffc000000000   (     4 GB maximum)
[    0.000000]               0xffffffbf00008000 - 0xffffffbf06000000   (    95 MB actual)
[    0.000000]     memory  : 0xffffffc000200000 - 0xffffffc180000000   (  6142 MB)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=4, Nodes=1
[    0.000000] ftrace: allocating 36277 entries in 142 pages
[    0.000000] Preemptible hierarchical RCU implementation.
[    0.000000]  Tasks RCU enabled.
[    0.000000] NR_IRQS: 64, nr_irqs: 64, preallocated irqs: 0
[    0.000000] parent_rate: 0,  dclk->rate:2666000000, pre_ddr_rate:0, res.a0:139716712
[    0.000000] arch_timer: cp15 timer(s) running at 24.00MHz (virt).
[    0.000000] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0x588fe9dc0, max_idle_ns: 440795202592 ns
[    0.000004] sched_clock: 56 bits at 24MHz, resolution 41ns, wraps every 4398046511097ns
[    0.001194] clocksource: hobot_clocksource: mask: 0xffffffffffffffff max_cycles: 0x1d854df40, max_idle_ns: 3526361616960 ns
[    0.002964] Console: colour dummy device 80x25
[    0.003535] Calibrating delay loop (skipped), value calculated using timer frequency.. 48.00 BogoMIPS (lpj=96000)
[    0.004840] pid_max: default: 32768 minimum: 301
[    0.005494] Security Framework initialized
[    0.006013] AppArmor: AppArmor disabled by boot time parameter
[    0.006855] Mount-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.007723] Mountpoint-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.023765] ASID allocator initialised with 65536 entries
[    0.031763] Hierarchical SRCU implementation.
[    0.063821] smp: Bringing up secondary CPUs ...
[    0.100027] Detected VIPT I-cache on CPU1
[    0.100061] CPU1: Booted secondary processor [410fd034]
[    0.136078] Detected VIPT I-cache on CPU2
[    0.136099] CPU2: Booted secondary processor [410fd034]
[    0.172137] Detected VIPT I-cache on CPU3
[    0.172157] CPU3: Booted secondary processor [410fd034]
[    0.172210] smp: Brought up 1 node, 4 CPUs
[    0.176273] SMP: Total of 4 processors activated.
[    0.176867] CPU features: detected feature: 32-bit EL0 Support
[    0.177686] CPU: All CPU(s) started at EL1
[    0.178215] alternatives: patching kernel code
[    0.179802] devtmpfs: initialized
[    0.188883] random: get_random_u32 called from bucket_table_alloc+0x108/0x270 with crng_init=0
[    0.190465] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 7645041785100000 ns
[    0.191711] futex hash table entries: 1024 (order: 5, 131072 bytes)
[    0.208264] xor: automatically using best checksumming function   32regs
[    0.209205] pinctrl core: initialized pinctrl subsystem
[    0.210441] NET: Registered protocol family 16
[    0.211760] vdso: 2 pages (1 code @ ffffff8008a46000, 1 data @ ffffff8009104000)
[    0.212705] hw-breakpoint: found 6 breakpoint and 4 watchpoint registers.
[    0.214297] DMA: preallocated 256 KiB pool for atomic allocations
[    0.219131] pstore: using zlib compression
[    0.219925] console [pstore-1] enabled
[    0.220526] pstore: Registered ramoops as persistent store backend
[    0.221310] ramoops: attached 0x40000@0x3fc0000, ecc: 0/0
[    0.226320] hobot_dma a1005000.dma: Hobot DMA Engine Driver Probed!!
[    0.240229] SCSI subsystem initialized
[    0.241016] media: Linux media interface: v0.10
[    0.241612] Linux video capture interface: v2.00
[    0.242245] pps_core: LinuxPPS API ver. 1 registered
[    0.242873] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.244048] PTP clock support registered
[    0.245194] ion_dummy: not reserve carveout memory, try to alloc from cma
[    0.381824] Advanced Linux Sound Architecture Driver Initialized.
[    0.382985] usbcore: registered new interface driver usbfs
[    0.383711] usbcore: registered new interface driver hub
[    0.384438] usbcore: registered new device driver usb
[    0.385404] clocksource: Switched to clocksource arch_sys_counter
[    0.432802] VFS: Disk quotas dquot_6.6.0
[    0.433346] VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
[    0.434309] FS-Cache: Loaded
[    0.434790] CacheFiles: Loaded
[    0.440081] NET: Registered protocol family 2
[    0.440996] TCP established hash table entries: 32768 (order: 6, 262144 bytes)
[    0.442141] TCP bind hash table entries: 32768 (order: 7, 524288 bytes)
[    0.443365] TCP: Hash tables configured (established 32768 bind 32768)
[    0.444276] UDP hash table entries: 2048 (order: 4, 65536 bytes)
[    0.445106] UDP-Lite hash table entries: 2048 (order: 4, 65536 bytes)
[    0.446127] NET: Registered protocol family 1
[    0.446954] RPC: Registered named UNIX socket transport module.
[    0.447705] RPC: Registered udp transport module.
[    0.448302] RPC: Registered tcp transport module.
[    0.448900] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.450412] hw perfevents: enabled with armv8_cortex_a53 PMU driver, 7 counters available
[    0.452613] audit: initializing netlink subsys (disabled)
[    0.453386] audit: type=2000 audit(0.448:1): state=initialized audit_enabled=0 res=1
[    0.453674] Initialise system trusted keyrings
[    0.453748] workingset: timestamp_bits=46 max_order=20 bucket_order=0
[    0.457292] zbud: loaded
[    0.459009] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.459869] exFAT: Version 1.2.9
[    0.460348] FS-Cache: Netfs 'nfs' registered for caching
[    0.461503] NFS: Registering the id_resolver key type
[    0.462156] Key type id_resolver registered
[    0.462684] Key type id_legacy registered
[    0.463200] nfs4filelayout_init: NFSv4 File Layout Driver Registering...
[    0.464052] Installing knfsd (copyright (C) 1996 okir@monad.swb.de).
[    0.468114] NET: Registered protocol family 38
[    0.468689] async_tx: api initialized (async)
[    0.469240] Key type asymmetric registered
[    0.469772] Asymmetric key parser 'x509' registered
[    0.470448] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 245)
[    0.471462] io scheduler noop registered
[    0.472112] io scheduler cfq registered (default)
[    0.472707] io scheduler mq-deadline registered
[    0.473282] io scheduler kyber registered
[    0.474476] pinctrl-single a6003170.pinctrl_voltag: 64 pins at pa ffffff8009c4d170 size 8
[    0.475812] pinctrl-single a6004000.pinctrl: 128 pins at pa ffffff8009c61000 size 512
[    0.477008] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: start probe
[    0.478053] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: probe ok
[    0.478933] gpio-x3 a6003000.gpio: x3 gpio probe start!!!
[    0.479623] gpio-x3 a6003000.gpio: x3 gpio add gpiochip start!!!
[    0.480546] gpio-x3 a6003000.gpio: diable all gpio irq
[    0.482816] gpio-x3 a6003000.gpio: irqbase:57
[    0.483370] gpio-x3 a6003000.gpio: x3 irq add start!!!
[    0.484026] irq: Cannot allocate irq_descs @ IRQ57, assuming pre-allocated
[    0.485055] gpio-x3 a6003000.gpio: x3 irq add ok!!!
[    0.485717] gpio-x3 a6003000.gpio: x3 irqchip ops add ok!!!
[    0.486423] gpio-x3 a6003000.gpio: x3 gpio probe ok!!!
[    0.487538] hobot-pwm: hobot-pwmchip0 registered
[    0.488288] hobot-pwm: hobot-pwmchip1 registered
[    0.489790] diag dev [ver:1.1] init done
[    0.490681] hobot_ddr_monitor: LPDDR4 detected
[    0.491431] hobot_ddr_monitor: ddr monitor init finished.
[    0.491814] [vcam] init start
[    0.492874] vcam probe start
[    0.493322] vcam probe end successful
[    0.493806] [vcam] init end
[    0.494733] a5000000.serial: ttyS0 at MMIO 0xa5000000 (irq = 10, base_baud = 12000000) is a hobot-uart
[    0.495945] console [ttyS0] enabled
[    0.495945] console [ttyS0] enabled
[    0.496829] bootconsole [hobot0] disabled
[    0.496829] bootconsole [hobot0] disabled
[    0.498187] hobot-uart a5001000.serial: Failed to create debugfs root directory
[    0.499187] a5001000.serial: ttyS1 at MMIO 0xa5001000 (irq = 11, base_baud = 12000000) is a hobot-uart
[    0.500631] hobot-uart a5003000.serial: Failed to create debugfs root directory
[    0.501650] a5003000.serial: ttyS3 at MMIO 0xa5003000 (irq = 12, base_baud = 12000000) is a hobot-uart
[    0.503186] KGDB: Registered I/O driver kgdboc
[    0.504023] cacheinfo: Unable to detect cache hierarchy for CPU 0
[    0.509430] brd: module loaded
[    0.514011] loop: module loaded
[    0.515567] spi-nand hr_nand.0: GigaDevice SPI NAND was found.
[    0.516328] spi-nand hr_nand.0: 128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
[    0.518964] hobot_spi a5006000.spi: ver: HOBOT-spi_V20.200330 master
[    0.520008] libphy: Fixed MDIO Bus: probed
[    0.521253] st_gmac a5014000.ethernet: found phy-handle subnode
[    0.522253] st_gmac a5014000.ethernet: xj3_mtl_setup, plat->rx-queues-to-use:4, and tx:4
[    0.523440] st_gmac a5014000.ethernet: xj3_probe_config_dt, clk_ptp_rate:250000000
[    0.524442] set mac address 00:11:22:8b:f6:81:
[    0.524445] (using random mac adress)
[    0.525512] (NULL device *): xj3_get_hw_features, tx_fifo_size:16384
[    0.526329] (NULL device *): xj3_get_hw_features, rx_fifo_size:16384
[    0.527147] st_gmac a5014000.ethernet: TSO supported
[    0.527786] st_gmac a5014000.ethernet: TSO feature enabled
[    0.528493] st_gmac a5014000.ethernet: Enable Rx Mitigation via HW Watchdog Timer
[    0.649697] libphy: hobot-mac-mdio: probed
[    0.651254] st_gmac a5014000.ethernet: hobot_eth_probe: probe sucessfully
[    0.652455] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_0v8 not found, using dummy regulator
[    0.653700] dwc3-of-simple b2000000.usb: usb regulator 0v8 enable succeed
[    0.654578] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_3v3 not found, using dummy regulator
[    0.655791] dwc3-of-simple b2000000.usb: usb regulator 3v3 enable succeed
[    0.657317] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    0.658996] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    0.660430] usbcore: registered new interface driver cdc_acm
[    0.661159] cdc_acm: USB Abstract Control Model driver for USB modems and ISDN adapters
[    0.662233] usbcore: registered new interface driver uas
[    0.662954] usbcore: registered new interface driver usb-storage
[    0.663784] usbcore: registered new interface driver usbserial
[    0.664555] usbcore: registered new interface driver usbserial_generic
[    0.665434] usbserial: USB Serial support registered for generic
[    0.666231] usbcore: registered new interface driver usb_serial_simple
[    0.667092] usbserial: USB Serial support registered for carelink
[    0.667893] usbserial: USB Serial support registered for zio
[    0.668638] usbserial: USB Serial support registered for funsoft
[    0.669447] usbserial: USB Serial support registered for flashloader
[    0.670281] usbserial: USB Serial support registered for google
[    0.671059] usbserial: USB Serial support registered for libtransistor
[    0.671918] usbserial: USB Serial support registered for vivopay
[    0.672708] usbserial: USB Serial support registered for moto_modem
[    0.673548] usbserial: USB Serial support registered for motorola_tetra
[    0.674415] usbserial: USB Serial support registered for novatel_gps
[    0.675250] usbserial: USB Serial support registered for hp4x
[    0.676006] usbserial: USB Serial support registered for suunto
[    0.676788] usbserial: USB Serial support registered for siemens_mpi
[    0.677642] usbcore: registered new interface driver rio500
[    0.678471] mousedev: PS/2 mouse device common for all mice
[    0.689538] hobot-rtc a6002000.rtc: rtc core: registered hobot-rtc as rtc0
[    0.690531] i2c /dev entries driver
[    0.691142] hobot-i2c a5009000.i2c: hobot i2c probe start
[    0.691905] hobot-i2c a5009000.i2c: round_rate:96000000
[    0.692582] hobot-i2c a5009000.i2c: I2C bus speed is 400000
[    0.693300] hobot-i2c a5009000.i2c: clkdiv = 0x1d
[    0.693918] hobot-i2c a5009000.i2c: i2c0 diag register....
[    0.695014] hobot-i2c a5009000.i2c: hobot_i2c_0 probe done
[    0.695816] hobot-i2c a500a000.i2c: hobot i2c probe start
[    0.696572] hobot-i2c a500a000.i2c: round_rate:96000000
[    0.697248] hobot-i2c a500a000.i2c: I2C bus speed is 400000
[    0.697989] hobot-i2c a500a000.i2c: clkdiv = 0x1d
[    0.698597] hobot-i2c a500a000.i2c: i2c1 diag register....
[    0.699606] hobot-i2c a500a000.i2c: hobot_i2c_1 probe done
[    0.700566] lirc_dev: IR Remote Control driver registered, major 239
[    0.701384] IR LIRC bridge handler initialized
[    0.702164] sif_mclk clock frequence is 544000000
[    0.702800] mipi_rx0_ipi clock frequence is 544000000
[    0.703488] mipi_rx1_ipi clock frequence is 544000000
[    0.704187] mipi_rx2_ipi clock frequence is 544000000
[    0.704896] mipi_rx3_ipi clock frequence is 544000000
[    0.705627] mipi_tx_ipi clock frequence is 544000000
[    0.706347] mipi_cfg_host clock frequence is 102000000
[    0.707101] pym_mclk clock frequence is 1188000000
[    0.707820] mipi_dev_ref clock frequence is 24000000
[    0.708574] mipi_host_ref clock frequence is 24000000
[    0.709350] sensor0_mclk clock frequence is 37125000
[    0.710146] sensor1_mclk clock frequence is 37125000
[    0.710934] sensor2_mclk clock frequence is 37125000
[    0.711734] sensor3_mclk clock frequence is 37125000
[    0.712373] [FRT:D] x3_ips_probe(0)
[    0.713382] hobot swinfo sel reg ro=0x1 boot dump
[    0.714339] pvt a1009000.pvt: SCRATCH test: 1234abcd, pvt is alive.
[    0.715264] pvt a1009000.pvt: VM Calibrated data detected
[    0.716448] hobot_wdt a1002000.watchdog: watchdog setting [pet:6s bark:11s bite:15s]
[    0.717784] hobot_wdt a1002000.watchdog: Hobot Watchdog Timer at ffffff8009db3000 with timeout 15s
[    0.719139] device-mapper: uevent: version 1.0.3
[    0.719899] device-mapper: ioctl: 4.37.0-ioctl (2017-09-20) initialised: dm-devel@redhat.com
[    0.721057] device-mapper: verity-avb: AVB error handler initialized with vbmeta device:
[    0.723492] Synopsys Designware Multimedia Card Interface Driver
[    0.724499] dwmmc_hobot a5010000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.725325] dwmmc_hobot a5010000.dwmmc: card-detect-delay not found.
[    0.726186] dwmmc_hobot a5010000.dwmmc: data-addr not found.
[    0.727227] mmc_host mmc0: card is non-removable.
[    0.766615] dwmmc_hobot a5011000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.769464] dwmmc_hobot a5011000.dwmmc: card-detect-delay not found.
[    0.770292] dwmmc_hobot a5011000.dwmmc: data-addr not found.
[    0.775062] dwmmc_hobot a5011000.dwmmc: mmc set to fixed voltage 1800
[    0.776122] mmc_host mmc1: card is non-removable.
[    0.873603] dwmmc_hobot a5012000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.874420] dwmmc_hobot a5012000.dwmmc: card-detect-delay not found.
[    0.875251] dwmmc_hobot a5012000.dwmmc: data-addr not found.
[    0.876217] dwmmc_hobot a5012000.dwmmc: Got CD GPIO
[    0.984585] mmc1: queuing unknown CIS tuple 0x80 (2 bytes)
[    0.986772] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.988954] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.992340] mmc1: queuing unknown CIS tuple 0x80 (7 bytes)
[    0.996295] mmc1: queuing unknown CIS tuple 0x81 (9 bytes)
[    1.057694] ledtrig-cpu: registered to indicate activity on CPUs
[    1.058537] hidraw: raw HID events driver (C) Jiri Kosina
[    1.059386] usbcore: registered new interface driver usbhid
[    1.060110] usbhid: USB HID core driver
[    1.060693] logger: created 256K log 'log_main'
[    1.061342] logger: created 256K log 'log_events'
[    1.062036] logger: created 256K log 'log_radio'
[    1.062693] logger: created 256K log 'log_system'
[    1.063731] set dmc devfreq governor to performance
[    1.064372] hobot_dmcfreq_target: dmcfreq->rate:2666000000, target_rate:2666000000
[    1.065351] buf:, powersave_rate:2666000000, dmcfreq->pre_state:0
[    1.072205] usbcore: registered new interface driver snd-usb-audio
[    1.073383] Netfilter messages via NETLINK v0.30.
[    1.074046] ip_set: protocol 6
[    1.074536] ipip: IPv4 and MPLS over IPv4 tunneling driver
[    1.075551] ip_tables: (C) 2000-2006 Netfilter Core Team
[    1.076484] arp_tables: arp_tables: (C) 2002 David S. Miller
[    1.077281] Initializing XFRM netlink socket
[    1.078182] NET: Registered protocol family 10
[    1.079425] Segment Routing with IPv6
[    1.079936] sit: IPv6, IPv4 and MPLS over IPv4 tunneling driver
[    1.081036] NET: Registered protocol family 17
[    1.081688] Key type dns_resolver registered
[    1.083343] Loading compiled-in X.509 certificates
[    1.086880] Loaded X.509 cert 'Build time autogenerated kernel key: 81cb0ef77db2fac76e9588c2120c82422367d268'
[    1.088213] zswap: loaded using pool lzo/zbud
[    1.099517] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    1.101178] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    1.102188] console [netcon0] enabled
[    1.102663] netconsole: network logging started
[    1.103445] hobot-rtc a6002000.rtc: setting system clock to 1970-01-01 00:00:00 UTC (0)
[    1.104627] vps mipi_dphy: probe with x3vio done
[    1.105332] hobot_wdt_test: wdt_test_init: wdt test init
[    1.108103] VCC_CNN0: disabling
[    1.108512] VCC_CNN1: disabling
[    1.109501] vps mipi_host0: ver 140* port0(0:0)
[    1.110426] vps mipi_host1: ver 140* port1(1:0)
[    1.111327] vps mipi_host2: ver 140* port2(0:1)
[    1.112114] vps mipi_host3: ver 140* port3(1:1)
[    1.112952] ALSA device list:
[    1.113337]   No soundcards found.
[    1.114026] md: Skipping autodetection of RAID arrays. (raid=autodetect will force)
[    1.115150] VFS: Cannot open root device "mmcblk2p2" or unknown-block(0,0): error -6
[    1.116144] Please append a correct "root=" boot option; here are the available partitions:
[    1.117218] 0100          102400 ram0
[    1.117220]  (driver?)
[    1.118028] 0101          102400 ram1
[    1.118030]  (driver?)
[    1.118819] 0102          102400 ram2
[    1.118820]  (driver?)
[    1.119608] 0103          102400 ram3
[    1.119610]  (driver?)
[    1.120398] 0104          102400 ram4
[    1.120400]  (driver?)
[    1.121187] 0105          102400 ram5
[    1.121189]  (driver?)
[    1.122014] 0106          102400 ram6
[    1.122016]  (driver?)
[    1.122805] 0107          102400 ram7
[    1.122807]  (driver?)
[    1.123595] 0108          102400 ram8
[    1.123596]  (driver?)
[    1.124384] 0109          102400 ram9
[    1.124386]  (driver?)
[    1.125174] 010a          102400 ram10
[    1.125175]  (driver?)
[    1.125994] 010b          102400 ram11
[    1.125996]  (driver?)
[    1.126795] 010c          102400 ram12
[    1.126797]  (driver?)
[    1.127596] 010d          102400 ram13
[    1.127598]  (driver?)
[    1.128397] 010e          102400 ram14
[    1.128398]  (driver?)
[    1.129197] 010f          102400 ram15
[    1.129199]  (driver?)
[    1.130016] 1f00          131072 mtdblock0
[    1.130018]  (driver?)
[    1.130862] hobot_fusa: set_fusa_error_pin:75 set error pin to 1
[    1.131632] hobot_fusa: fusa errpin not ready
[    1.131636] Kernel panic - not syncing: VFS: Unable to mount root fs on unknown-block(0,0)
[    1.133255] Kernel Offset: disabled
[    1.133706] CPU features: 0x0002004
[    1.134155] Memory Limit: none
[    1.138714] Rebooting in 1 seconds..
[    1.173411] dwmmc_hobot a5012000.dwmmc: Unexpected interrupt latency
[    1.209402] dwmmc_hobot a5011000.dwmmc: Unexpected interrupt latency
[    1.209655] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.209669] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 1
[    1.210145] xhci-hcd xhci-hcd.0.auto: hcc params 0x0220fe6d hci version 0x110 quirks 0x0000000000010010
[    1.210177] xhci-hcd xhci-hcd.0.auto: irq 178, io mem 0xb2000000
[    1.210361] usb usb1: New USB device found, idVendor=1d6b, idProduct=0002, bcdDevice= 4.14
[    1.210365] usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.210369] usb usb1: Product: xHCI Host Controller
[    1.210372] usb usb1: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.210375] usb usb1: SerialNumber: xhci-hcd.0.auto
[    1.210712] hub 1-0:1.0: USB hub found
[    1.210732] hub 1-0:1.0: 1 port detected
[    1.210916] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.210925] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 2
[    1.210933] xhci-hcd xhci-hcd.0.auto: Host supports USB 3.0 SuperSpeed
[    1.210971] usb usb2: We don't know the algorithms for LPM for this host, disabling LPM.
[    1.211037] usb usb2: New USB device found, idVendor=1d6b, idProduct=0003, bcdDevice= 4.14
[    1.211041] usb usb2: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.211045] usb usb2: Product: xHCI Host Controller
[    1.211048] usb usb2: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.211051] usb usb2: SerialNumber: xhci-hcd.0.auto
[    1.211315] hub 2-0:1.0: USB hub found
[    1.211332] hub 2-0:1.0: 1 port detected
[    2.139227] SMP: stopping secondary CPUs
[    2.139734] psci: psci_sys_reset(reboot_mode=0)
NOTICE:  fast_boot:0

S
F
L
O
NOTICE:  efuse cpu_cfg = 0
W
NOTICE:  Booting Trusted Firmware
NOTICE:  BL1: v1.4(release):HR-ROM-Rel-v1.1-141-ga91d4dd-dirty
NOTICE:  BL1: Built : 11:24:44, Oct 23 2019
NOTICE:  boot src: 2
NOTICE:  GigaDev SPI NAND was found.
NOTICE:  Block size: 128 KiB, page size: 2048
NOTICE:  BL1: Booting BL2
Auth pass
NOTICE:  bl1_main exit
SPL normal reset flow
check_reset_state (2): wakeup address = 0x0, hw wakeup status = 0x3, wakeup src=0x100
patch for sys_pll 1200 with 100M eth
SFLOW_INIT
CHIP ID:PCB941/WAFER: W04/ X: X20/ Y: Y36
secondary_jump_to_spl: secure chip flow
X3 SPL : secondary core wake up and jump to spl done (cpu_core_cfg=0)
SFLOW_FIN_HW_A

U-Boot SPL 2018.09-g4ca851534c-dirty (May 11 2022 - 20:09:50 +0800)
SPACC Init - ID: (00000061)
SPL nand boot mode (from strap)
GigaDev SPI NAND was found.
Block size: 128 KiB, page size: 2048
ddr_type = 1 (LPDDR4)
hb_chip_package_type:3
load ddr header src_addr: 100000, load_addr: 802ca020, src_len: a00
find valid ddr image
ddr_hdr.ecc_gran: 0x0
ddr_hdr.ecc_map: 0x0
ddr_hdr.sbr_pattern0: 0x0
ddr_hdr.sbr_pattern1: 0x0
ddr_freq = 05
board id = 31540334
ddr datarate: 3200
### SAMSUNG DDR ###
no ddr pin set
detect part number: 108
detect ddr freq: c80
board id alternative:0x3
index is 12
index is 15
index is 19
hb_ddr_index: 19
ddr_type = 1, ddr_vendor=3, ddr_freq=3200
dram_pll_init
sscg disabled
control load ddrc src_addr: 15ae00, load_addr: 802caa20, src_len: 920
[DDR INFO]      ==ddr_release_info==
[DDR INFO]      VERSION:        develop
[DDR INFO]      BUILD:          2022-05-11-20:09
[DDR INFO]      GIT COMMIT:     4ca851534c1616ace920fdaa000c6fb717c1fb74
[DDR INFO]      GIT TIME:       Wed, 20 Apr 2022 18:28:49 +0800
[DDR INFO]      ==ddr_features==
[DDR INFO]      RDBI:           0
[DDR INFO]      WDBI:           1
[DDR INFO]      InlineECC:      0
[DDR INFO]      DM:             1
[DDR INFO]      DDC:            1
[DDR INFO]      SSCG:           0
[DDR INFO]      BOARD:          XS_ENABLE
[DDR INFO] ddr_controller_cfg done
load ddr phy src_addr: 15b800, load_addr: 802caa20, src_len: 420
ATxSlewRate     : 15f
ATxImpedance    : 7f
TxSlewRate      : 19f
TxOdtDrvStren   : 600
TxImpedanceCtrl : e3f
CalDrvStr0      : 11
VrefInGlobal    : 104
board_type = 4 (CUSTOMER_BOARD)
load dqmap src addr: 15d600, load_addr: 802caa20, src_len: 20
[DDR INFO] dwc_ddrphy_train start
magic = 544f4248
load imem1 src_addr: 11ce00, load_addr: 802caa20, src_len: 8000
load dmem1 src_addr: 15a000, load_addr: 802caa20, src_len: 684
executing 1D fw
load imem2 src_addr: 124e00, load_addr: 802caa20, src_len: 8000
load dmem2 src_addr: 15a800, load_addr: 802caa20, src_len: 564

*******************************************************
p_dmem_lpddr4_2d_16b->MR11_A0:54
p_dmem_lpddr4_2d_16b->MR14_A0:54
p_dmem_lpddr4_2d_16b->MR12_A0:51
p_dmem_lpddr4_2d_16b->MR22_A0:14

p_dmem_lpddr4_2d_16b->MR3_A0:b3
p_dmem_lpddr4_2d_16b->Reserved00:40
p_dmem_lpddr4_2d_16b->Reserved0E:4
p_dmem_lpddr4_2d_16b->Delay_Weight2D:20
p_dmem_lpddr4_2d_16b->Voltage_Weight2D:80
*******************************************************

executing 2D fw
load pie src_addr: 15be00, load_addr: 802caa20, src_len: 11f0
Set QoS.
get_ddr_mr_info:cs_num=1, mr5=0x1, mr8=0x10
no magic in efuse file,bypass efuse
total_sz = 4096
SPL_VERSION:7
uboot partition is uboot_A
load u-boot: src_addr=0x380000, dest_addr=0x4000000, len=2097152
load warm boot spl: addr=0x800, dest_addr=0x80000000, len=31232
load bl31: addr=0x300000, dest_addr=0x0, len=524288
SFLOW_AUTH_BL31
verify signature of header:  verify ok!
verify signature of image:  verify ok!
bypass bpu image
clear keybank!!!!
SFLOW_DBG_EN
Trying to boot from RAM
SPL: bl31 will jump to u-boot or other entry (0x4000000)
SFLOW_CLR_KEY
SFLOW_REG_LD
install_portal copy portal
install_portal call smc and jump to bl31 cold entry(0x0)
hb som type: 5
X3 PI reset VDD_SD done

U-Boot 2018.09-g40785bca (May 27 2022 - 16:30:48 +0800)

Model: Hobot XJ3 Soc Board
DRAM:  system DDR size: 0xffe00000
4 GiB
MMC:   dwmmc@A5010000: 0, dwmmc@A5011000: 1, dwmmc@A5012000: 2 (SD)
Loading Environment from UBI... GigaDevice SPI NAND was found.
128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
*** Warning - bad CRC, using default environment

In:    serial@a5000000
Out:   serial@a5000000
Err:   serial@a5000000
Net:   x3 sdb reset eth phy done

Warning: ethernet@A5014000 (eth0) using random MAC address - 5a:e1:0b:e6:04:89
eth0: ethernet@A5014000
Disable cnn cores ..
dtb_name:hobot-x3-pi.dtb
base board type: X3 SDB
bootmode: NAND
board_id = 31540334
damaged volume, update marker is setdamaged volume, update marker is setdamaged volume, update marker is sethb_boot_args_cmd_set custom_bootargs 0 ubuntu_boot 0
Hit any key to stop autoboot:  0
enable watchdog success !
switch to partitions #0, OK
mmc2 is current device
Scanning mmc 2:2...
Found U-Boot script /boot/boot.scr
664 bytes read in 2 ms (324.2 KiB/s)
## Executing script at 03c10000
Boot script loaded from devtype:mmc devnum:2 devplist:2
bootargs = console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
Loading fdt file: /boot/hobot/hobot-x3-pi.dtb
69633 bytes read in 8 ms (8.3 MiB/s)
Loading kernel: /boot/Image
19163144 bytes read in 845 ms (21.6 MiB/s)
## Flattened Device Tree blob at 03c00000
   Booting using the fdt blob at 0x3c00000
   Loading Device Tree to 0000000003c00000, end 0000000003c1ffff ... OK
chip_id: ab36300
The address of the fdt is 0x3c00000
Changed status Done
Can't get fdt_addr !!!Orign(MAX) bpu model Reserve Mem Size to 64M!!

Starting kernel ...

[    0.000000] OF: reserved mem: OVERLAP DETECTED!
[    0.000000] image_r5_mem (0x0000000080000000--0x0000000080010000) overlaps with msg_r5_mem (0x000000008000f000--0x0000000080010000)
[    0.000000] Reserved memory: created CMA memory pool at 0x0000000004000000, size 672 MiB
[    0.000000] OF: reserved mem: initialized node ion_cma, compatible id shared-dma-pool
[    0.000000] cma: Reserved 16 MiB at 0x000000007f000000
[    0.000000] On node 0 totalpages: 1047808
[    0.000000]   DMA zone: 8180 pages used for memmap
[    0.000000]   DMA zone: 0 pages reserved
[    0.000000]   DMA zone: 523520 pages, LIFO batch:31
[    0.000000]   Normal zone: 8192 pages used for memmap
[    0.000000]   Normal zone: 524288 pages, LIFO batch:31
[    0.000000] psci: probing for conduit method from DT.
[    0.000000] psci: PSCIv1.1 detected in firmware.
[    0.000000] psci: Using standard PSCI v0.2 function IDs
[    0.000000] psci: MIGRATE_INFO_TYPE not supported.
[    0.000000] psci: SMC Calling Convention v1.1
[    0.000000] percpu: Embedded 25 pages/cpu @ffffffc17ff2a000 s65176 r8192 d29032 u102400
[    0.000000] pcpu-alloc: s65176 r8192 d29032 u102400 alloc=25*4096
[    0.000000] pcpu-alloc: [0] 0 [0] 1 [0] 2 [0] 3
[    0.000000] Detected VIPT I-cache on CPU0
[    0.000000] CPU features: enabling workaround for ARM erratum 845719
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 1031436
[    0.000000] Kernel command line: earlycon loglevel=8 kgdboc=ttyS0 video=hobot:x3sdb-hdmi  console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
[    0.000000] PID hash table entries: 4096 (order: 3, 32768 bytes)
[    0.000000] Dentry cache hash table entries: 524288 (order: 10, 4194304 bytes)
[    0.000000] Inode-cache hash table entries: 262144 (order: 9, 2097152 bytes)
[    0.000000] software IO TLB [mem 0x7afff000-0x7efff000] (64MB) mapped at [ffffffc07afff000-ffffffc07effefff]
[    0.000000] Memory: 3319580K/4191232K available (10494K kernel code, 1306K rwdata, 5756K rodata, 1088K init, 9553K bss, 167140K reserved, 704512K cma-reserved)
[    0.000000] Virtual kernel memory layout:
[    0.000000]     modules : 0xffffff8000000000 - 0xffffff8008000000   (   128 MB)
[    0.000000]     vmalloc : 0xffffff8008000000 - 0xffffffbebfff0000   (   250 GB)
[    0.000000]       .text : 0xffffff8008000000 - 0xffffff8008a40000   ( 10496 KB)
[    0.000000]     .rodata : 0xffffff8008a40000 - 0xffffff8008ff0000   (  5824 KB)
[    0.000000]       .init : 0xffffff8008ff0000 - 0xffffff8009100000   (  1088 KB)
[    0.000000]       .data : 0xffffff8009100000 - 0xffffff8009246808   (  1307 KB)
[    0.000000]        .bss : 0xffffff8009246808 - 0xffffff8009b9aed8   (  9554 KB)
[    0.000000]     fixed   : 0xffffffbefe7fd000 - 0xffffffbefec00000   (  4108 KB)
[    0.000000]     PCI I/O : 0xffffffbefee00000 - 0xffffffbeffe00000   (    16 MB)
[    0.000000]     vmemmap : 0xffffffbf00000000 - 0xffffffc000000000   (     4 GB maximum)
[    0.000000]               0xffffffbf00008000 - 0xffffffbf06000000   (    95 MB actual)
[    0.000000]     memory  : 0xffffffc000200000 - 0xffffffc180000000   (  6142 MB)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=4, Nodes=1
[    0.000000] ftrace: allocating 36277 entries in 142 pages
[    0.000000] Preemptible hierarchical RCU implementation.
[    0.000000]  Tasks RCU enabled.
[    0.000000] NR_IRQS: 64, nr_irqs: 64, preallocated irqs: 0
[    0.000000] parent_rate: 0,  dclk->rate:2666000000, pre_ddr_rate:0, res.a0:139716712
[    0.000000] arch_timer: cp15 timer(s) running at 24.00MHz (virt).
[    0.000000] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0x588fe9dc0, max_idle_ns: 440795202592 ns
[    0.000004] sched_clock: 56 bits at 24MHz, resolution 41ns, wraps every 4398046511097ns
[    0.001193] clocksource: hobot_clocksource: mask: 0xffffffffffffffff max_cycles: 0x1d854df40, max_idle_ns: 3526361616960 ns
[    0.002967] Console: colour dummy device 80x25
[    0.003538] Calibrating delay loop (skipped), value calculated using timer frequency.. 48.00 BogoMIPS (lpj=96000)
[    0.004844] pid_max: default: 32768 minimum: 301
[    0.005498] Security Framework initialized
[    0.006016] AppArmor: AppArmor disabled by boot time parameter
[    0.006859] Mount-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.007727] Mountpoint-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.023768] ASID allocator initialised with 65536 entries
[    0.031766] Hierarchical SRCU implementation.
[    0.063825] smp: Bringing up secondary CPUs ...
[    0.100031] Detected VIPT I-cache on CPU1
[    0.100065] CPU1: Booted secondary processor [410fd034]
[    0.136081] Detected VIPT I-cache on CPU2
[    0.136102] CPU2: Booted secondary processor [410fd034]
[    0.172139] Detected VIPT I-cache on CPU3
[    0.172159] CPU3: Booted secondary processor [410fd034]
[    0.172213] smp: Brought up 1 node, 4 CPUs
[    0.176275] SMP: Total of 4 processors activated.
[    0.176870] CPU features: detected feature: 32-bit EL0 Support
[    0.177689] CPU: All CPU(s) started at EL1
[    0.178217] alternatives: patching kernel code
[    0.179809] devtmpfs: initialized
[    0.188870] random: get_random_u32 called from bucket_table_alloc+0x108/0x270 with crng_init=0
[    0.190452] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 7645041785100000 ns
[    0.191697] futex hash table entries: 1024 (order: 5, 131072 bytes)
[    0.208199] xor: automatically using best checksumming function   32regs
[    0.209135] pinctrl core: initialized pinctrl subsystem
[    0.210371] NET: Registered protocol family 16
[    0.211694] vdso: 2 pages (1 code @ ffffff8008a46000, 1 data @ ffffff8009104000)
[    0.212639] hw-breakpoint: found 6 breakpoint and 4 watchpoint registers.
[    0.214229] DMA: preallocated 256 KiB pool for atomic allocations
[    0.219020] pstore: using zlib compression
[    0.219819] console [pstore-1] enabled
[    0.220418] pstore: Registered ramoops as persistent store backend
[    0.221202] ramoops: attached 0x40000@0x3fc0000, ecc: 0/0
[    0.226196] hobot_dma a1005000.dma: Hobot DMA Engine Driver Probed!!
[    0.240151] SCSI subsystem initialized
[    0.240935] media: Linux media interface: v0.10
[    0.241533] Linux video capture interface: v2.00
[    0.242165] pps_core: LinuxPPS API ver. 1 registered
[    0.242793] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.243968] PTP clock support registered
[    0.245131] ion_dummy: not reserve carveout memory, try to alloc from cma
[    0.381955] Advanced Linux Sound Architecture Driver Initialized.
[    0.383155] usbcore: registered new interface driver usbfs
[    0.383882] usbcore: registered new interface driver hub
[    0.384608] usbcore: registered new device driver usb
[    0.385618] clocksource: Switched to clocksource arch_sys_counter
[    0.433344] VFS: Disk quotas dquot_6.6.0
[    0.433940] VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
[    0.434877] FS-Cache: Loaded
[    0.435362] CacheFiles: Loaded
[    0.440741] NET: Registered protocol family 2
[    0.441673] TCP established hash table entries: 32768 (order: 6, 262144 bytes)
[    0.442791] TCP bind hash table entries: 32768 (order: 7, 524288 bytes)
[    0.444039] TCP: Hash tables configured (established 32768 bind 32768)
[    0.444943] UDP hash table entries: 2048 (order: 4, 65536 bytes)
[    0.445799] UDP-Lite hash table entries: 2048 (order: 4, 65536 bytes)
[    0.446800] NET: Registered protocol family 1
[    0.447638] RPC: Registered named UNIX socket transport module.
[    0.448389] RPC: Registered udp transport module.
[    0.448986] RPC: Registered tcp transport module.
[    0.449585] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.451109] hw perfevents: enabled with armv8_cortex_a53 PMU driver, 7 counters available
[    0.453308] audit: initializing netlink subsys (disabled)
[    0.454217] audit: type=2000 audit(0.452:1): state=initialized audit_enabled=0 res=1
[    0.454466] Initialise system trusted keyrings
[    0.454551] workingset: timestamp_bits=46 max_order=20 bucket_order=0
[    0.458143] zbud: loaded
[    0.459703] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.460562] exFAT: Version 1.2.9
[    0.461042] FS-Cache: Netfs 'nfs' registered for caching
[    0.462208] NFS: Registering the id_resolver key type
[    0.462861] Key type id_resolver registered
[    0.463388] Key type id_legacy registered
[    0.463904] nfs4filelayout_init: NFSv4 File Layout Driver Registering...
[    0.464758] Installing knfsd (copyright (C) 1996 okir@monad.swb.de).
[    0.469046] NET: Registered protocol family 38
[    0.469659] async_tx: api initialized (async)
[    0.470212] Key type asymmetric registered
[    0.470731] Asymmetric key parser 'x509' registered
[    0.471414] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 245)
[    0.472430] io scheduler noop registered
[    0.473083] io scheduler cfq registered (default)
[    0.473705] io scheduler mq-deadline registered
[    0.474277] io scheduler kyber registered
[    0.475479] pinctrl-single a6003170.pinctrl_voltag: 64 pins at pa ffffff8009c4d170 size 8
[    0.476826] pinctrl-single a6004000.pinctrl: 128 pins at pa ffffff8009c61000 size 512
[    0.478077] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: start probe
[    0.478973] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: probe ok
[    0.479848] gpio-x3 a6003000.gpio: x3 gpio probe start!!!
[    0.480538] gpio-x3 a6003000.gpio: x3 gpio add gpiochip start!!!
[    0.481461] gpio-x3 a6003000.gpio: diable all gpio irq
[    0.483850] gpio-x3 a6003000.gpio: irqbase:57
[    0.484402] gpio-x3 a6003000.gpio: x3 irq add start!!!
[    0.485059] irq: Cannot allocate irq_descs @ IRQ57, assuming pre-allocated
[    0.486103] gpio-x3 a6003000.gpio: x3 irq add ok!!!
[    0.486756] gpio-x3 a6003000.gpio: x3 irqchip ops add ok!!!
[    0.487462] gpio-x3 a6003000.gpio: x3 gpio probe ok!!!
[    0.488558] hobot-pwm: hobot-pwmchip0 registered
[    0.489313] hobot-pwm: hobot-pwmchip1 registered
[    0.490662] diag dev [ver:1.1] init done
[    0.491562] hobot_ddr_monitor: LPDDR4 detected
[    0.492323] hobot_ddr_monitor: ddr monitor init finished.
[    0.492724] [vcam] init start
[    0.493957] vcam probe start
[    0.494422] vcam probe end successful
[    0.494883] [vcam] init end
[    0.495811] a5000000.serial: ttyS0 at MMIO 0xa5000000 (irq = 10, base_baud = 12000000) is a hobot-uart
[    0.497023] console [ttyS0] enabled
[    0.497023] console [ttyS0] enabled
[    0.497928] bootconsole [hobot0] disabled
[    0.497928] bootconsole [hobot0] disabled
[    0.499248] hobot-uart a5001000.serial: Failed to create debugfs root directory
[    0.500247] a5001000.serial: ttyS1 at MMIO 0xa5001000 (irq = 11, base_baud = 12000000) is a hobot-uart
[    0.501715] hobot-uart a5003000.serial: Failed to create debugfs root directory
[    0.502713] a5003000.serial: ttyS3 at MMIO 0xa5003000 (irq = 12, base_baud = 12000000) is a hobot-uart
[    0.504246] KGDB: Registered I/O driver kgdboc
[    0.505090] cacheinfo: Unable to detect cache hierarchy for CPU 0
[    0.510558] brd: module loaded
[    0.515091] loop: module loaded
[    0.516670] spi-nand hr_nand.0: GigaDevice SPI NAND was found.
[    0.517430] spi-nand hr_nand.0: 128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
[    0.520179] hobot_spi a5006000.spi: ver: HOBOT-spi_V20.200330 master
[    0.521221] libphy: Fixed MDIO Bus: probed
[    0.522483] st_gmac a5014000.ethernet: found phy-handle subnode
[    0.523318] st_gmac a5014000.ethernet: xj3_mtl_setup, plat->rx-queues-to-use:4, and tx:4
[    0.524506] st_gmac a5014000.ethernet: xj3_probe_config_dt, clk_ptp_rate:250000000
[    0.525507] set mac address 00:11:22:46:ca:3f:
[    0.525510] (using random mac adress)
[    0.526566] (NULL device *): xj3_get_hw_features, tx_fifo_size:16384
[    0.527383] (NULL device *): xj3_get_hw_features, rx_fifo_size:16384
[    0.528200] st_gmac a5014000.ethernet: TSO supported
[    0.528840] st_gmac a5014000.ethernet: TSO feature enabled
[    0.529547] st_gmac a5014000.ethernet: Enable Rx Mitigation via HW Watchdog Timer
[    0.650745] libphy: hobot-mac-mdio: probed
[    0.652320] st_gmac a5014000.ethernet: hobot_eth_probe: probe sucessfully
[    0.653521] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_0v8 not found, using dummy regulator
[    0.654775] dwc3-of-simple b2000000.usb: usb regulator 0v8 enable succeed
[    0.655653] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_3v3 not found, using dummy regulator
[    0.656853] dwc3-of-simple b2000000.usb: usb regulator 3v3 enable succeed
[    0.658393] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    0.660051] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    0.661550] usbcore: registered new interface driver cdc_acm
[    0.662306] cdc_acm: USB Abstract Control Model driver for USB modems and ISDN adapters
[    0.663362] usbcore: registered new interface driver uas
[    0.664082] usbcore: registered new interface driver usb-storage
[    0.664910] usbcore: registered new interface driver usbserial
[    0.665755] usbcore: registered new interface driver usbserial_generic
[    0.666614] usbserial: USB Serial support registered for generic
[    0.667410] usbcore: registered new interface driver usb_serial_simple
[    0.668269] usbserial: USB Serial support registered for carelink
[    0.669070] usbserial: USB Serial support registered for zio
[    0.669835] usbserial: USB Serial support registered for funsoft
[    0.670626] usbserial: USB Serial support registered for flashloader
[    0.671460] usbserial: USB Serial support registered for google
[    0.672239] usbserial: USB Serial support registered for libtransistor
[    0.673097] usbserial: USB Serial support registered for vivopay
[    0.673905] usbserial: USB Serial support registered for moto_modem
[    0.674728] usbserial: USB Serial support registered for motorola_tetra
[    0.675596] usbserial: USB Serial support registered for novatel_gps
[    0.676429] usbserial: USB Serial support registered for hp4x
[    0.677185] usbserial: USB Serial support registered for suunto
[    0.677985] usbserial: USB Serial support registered for siemens_mpi
[    0.678831] usbcore: registered new interface driver rio500
[    0.679658] mousedev: PS/2 mouse device common for all mice
[    0.690712] hobot-rtc a6002000.rtc: rtc core: registered hobot-rtc as rtc0
[    0.691705] i2c /dev entries driver
[    0.692316] hobot-i2c a5009000.i2c: hobot i2c probe start
[    0.693080] hobot-i2c a5009000.i2c: round_rate:96000000
[    0.693777] hobot-i2c a5009000.i2c: I2C bus speed is 400000
[    0.694495] hobot-i2c a5009000.i2c: clkdiv = 0x1d
[    0.695102] hobot-i2c a5009000.i2c: i2c0 diag register....
[    0.696194] hobot-i2c a5009000.i2c: hobot_i2c_0 probe done
[    0.696995] hobot-i2c a500a000.i2c: hobot i2c probe start
[    0.697771] hobot-i2c a500a000.i2c: round_rate:96000000
[    0.698448] hobot-i2c a500a000.i2c: I2C bus speed is 400000
[    0.699166] hobot-i2c a500a000.i2c: clkdiv = 0x1d
[    0.699772] hobot-i2c a500a000.i2c: i2c1 diag register....
[    0.700784] hobot-i2c a500a000.i2c: hobot_i2c_1 probe done
[    0.701769] lirc_dev: IR Remote Control driver registered, major 239
[    0.702588] IR LIRC bridge handler initialized
[    0.703338] sif_mclk clock frequence is 544000000
[    0.703975] mipi_rx0_ipi clock frequence is 544000000
[    0.704664] mipi_rx1_ipi clock frequence is 544000000
[    0.705363] mipi_rx2_ipi clock frequence is 544000000
[    0.706082] mipi_rx3_ipi clock frequence is 544000000
[    0.706803] mipi_tx_ipi clock frequence is 544000000
[    0.707531] mipi_cfg_host clock frequence is 102000000
[    0.708284] pym_mclk clock frequence is 1188000000
[    0.709005] mipi_dev_ref clock frequence is 24000000
[    0.709776] mipi_host_ref clock frequence is 24000000
[    0.710553] sensor0_mclk clock frequence is 37125000
[    0.711330] sensor1_mclk clock frequence is 37125000
[    0.712117] sensor2_mclk clock frequence is 37125000
[    0.712917] sensor3_mclk clock frequence is 37125000
[    0.713557] [FRT:D] x3_ips_probe(0)
[    0.714588] hobot swinfo sel reg ro=0x1 boot dump
[    0.715502] pvt a1009000.pvt: SCRATCH test: 1234abcd, pvt is alive.
[    0.716428] pvt a1009000.pvt: VM Calibrated data detected
[    0.717605] hobot_wdt a1002000.watchdog: watchdog setting [pet:6s bark:11s bite:15s]
[    0.718960] hobot_wdt a1002000.watchdog: Hobot Watchdog Timer at ffffff8009db3000 with timeout 15s
[    0.720310] device-mapper: uevent: version 1.0.3
[    0.721069] device-mapper: ioctl: 4.37.0-ioctl (2017-09-20) initialised: dm-devel@redhat.com
[    0.722248] device-mapper: verity-avb: AVB error handler initialized with vbmeta device:
[    0.724668] Synopsys Designware Multimedia Card Interface Driver
[    0.725700] dwmmc_hobot a5010000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.726528] dwmmc_hobot a5010000.dwmmc: card-detect-delay not found.
[    0.727347] dwmmc_hobot a5010000.dwmmc: data-addr not found.
[    0.728388] mmc_host mmc0: card is non-removable.
[    0.770827] dwmmc_hobot a5011000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.773669] dwmmc_hobot a5011000.dwmmc: card-detect-delay not found.
[    0.774489] dwmmc_hobot a5011000.dwmmc: data-addr not found.
[    0.779257] dwmmc_hobot a5011000.dwmmc: mmc set to fixed voltage 1800
[    0.780320] mmc_host mmc1: card is non-removable.
[    0.877845] dwmmc_hobot a5012000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.878667] dwmmc_hobot a5012000.dwmmc: card-detect-delay not found.
[    0.879507] dwmmc_hobot a5012000.dwmmc: data-addr not found.
[    0.880515] dwmmc_hobot a5012000.dwmmc: Got CD GPIO
[    0.988980] mmc1: queuing unknown CIS tuple 0x80 (2 bytes)
[    0.991185] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.993370] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.996750] mmc1: queuing unknown CIS tuple 0x80 (7 bytes)
[    1.000704] mmc1: queuing unknown CIS tuple 0x81 (9 bytes)
[    1.065910] ledtrig-cpu: registered to indicate activity on CPUs
[    1.066739] hidraw: raw HID events driver (C) Jiri Kosina
[    1.067617] usbcore: registered new interface driver usbhid
[    1.068335] usbhid: USB HID core driver
[    1.068915] logger: created 256K log 'log_main'
[    1.069561] logger: created 256K log 'log_events'
[    1.070250] logger: created 256K log 'log_radio'
[    1.070911] logger: created 256K log 'log_system'
[    1.071947] set dmc devfreq governor to performance
[    1.072590] hobot_dmcfreq_target: dmcfreq->rate:2666000000, target_rate:2666000000
[    1.073571] buf:, powersave_rate:2666000000, dmcfreq->pre_state:0
[    1.080448] usbcore: registered new interface driver snd-usb-audio
[    1.081659] Netfilter messages via NETLINK v0.30.
[    1.082295] ip_set: protocol 6
[    1.082790] ipip: IPv4 and MPLS over IPv4 tunneling driver
[    1.083807] ip_tables: (C) 2000-2006 Netfilter Core Team
[    1.084740] arp_tables: arp_tables: (C) 2002 David S. Miller
[    1.085536] Initializing XFRM netlink socket
[    1.086450] NET: Registered protocol family 10
[    1.087705] Segment Routing with IPv6
[    1.088213] sit: IPv6, IPv4 and MPLS over IPv4 tunneling driver
[    1.089313] NET: Registered protocol family 17
[    1.089966] Key type dns_resolver registered
[    1.091622] Loading compiled-in X.509 certificates
[    1.095124] Loaded X.509 cert 'Build time autogenerated kernel key: 81cb0ef77db2fac76e9588c2120c82422367d268'
[    1.096454] zswap: loaded using pool lzo/zbud
[    1.107736] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    1.109406] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    1.110388] console [netcon0] enabled
[    1.110863] netconsole: network logging started
[    1.111643] hobot-rtc a6002000.rtc: setting system clock to 1970-01-01 00:00:00 UTC (0)
[    1.112827] vps mipi_dphy: probe with x3vio done
[    1.113532] hobot_wdt_test: wdt_test_init: wdt test init
[    1.116276] VCC_CNN0: disabling
[    1.116687] VCC_CNN1: disabling
[    1.117686] vps mipi_host0: ver 140* port0(0:0)
[    1.118603] vps mipi_host1: ver 140* port1(1:0)
[    1.119494] vps mipi_host2: ver 140* port2(0:1)
[    1.120285] vps mipi_host3: ver 140* port3(1:1)
[    1.121114] ALSA device list:
[    1.121499]   No soundcards found.
[    1.122177] md: Skipping autodetection of RAID arrays. (raid=autodetect will force)
[    1.123314] VFS: Cannot open root device "mmcblk2p2" or unknown-block(0,0): error -6
[    1.124307] Please append a correct "root=" boot option; here are the available partitions:
[    1.125382] 0100          102400 ram0
[    1.125384]  (driver?)
[    1.126198] 0101          102400 ram1
[    1.126200]  (driver?)
[    1.126989] 0102          102400 ram2
[    1.126991]  (driver?)
[    1.127779] 0103          102400 ram3
[    1.127781]  (driver?)
[    1.128568] 0104          102400 ram4
[    1.128570]  (driver?)
[    1.129358] 0105          102400 ram5
[    1.129360]  (driver?)
[    1.130190] 0106          102400 ram6
[    1.130192]  (driver?)
[    1.130981] 0107          102400 ram7
[    1.130983]  (driver?)
[    1.131771] 0108          102400 ram8
[    1.131772]  (driver?)
[    1.132560] 0109          102400 ram9
[    1.132562]  (driver?)
[    1.133350] 010a          102400 ram10
[    1.133352]  (driver?)
[    1.134168] 010b          102400 ram11
[    1.134170]  (driver?)
[    1.134969] 010c          102400 ram12
[    1.134971]  (driver?)
[    1.135770] 010d          102400 ram13
[    1.135771]  (driver?)
[    1.136570] 010e          102400 ram14
[    1.136572]  (driver?)
[    1.137371] 010f          102400 ram15
[    1.137372]  (driver?)
[    1.138207] 1f00          131072 mtdblock0
[    1.138209]  (driver?)
[    1.139053] hobot_fusa: set_fusa_error_pin:75 set error pin to 1
[    1.139823] hobot_fusa: fusa errpin not ready
[    1.139827] Kernel panic - not syncing: VFS: Unable to mount root fs on unknown-block(0,0)
[    1.141446] Kernel Offset: disabled
[    1.141897] CPU features: 0x0002004
[    1.142346] Memory Limit: none
[    1.146905] Rebooting in 1 seconds..
[    1.217870] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.218591] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 1
[    1.220047] xhci-hcd xhci-hcd.0.auto: hcc params 0x0220fe6d hci version 0x110 quirks 0x0000000000010010
[    1.221281] xhci-hcd xhci-hcd.0.auto: irq 178, io mem 0xb2000000
[    1.222251] usb usb1: New USB device found, idVendor=1d6b, idProduct=0002, bcdDevice= 4.14
[    1.223314] usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.224243] usb usb1: Product: xHCI Host Controller
[    1.224872] usb usb1: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.225578] usb usb1: SerialNumber: xhci-hcd.0.auto
[    1.226531] hub 1-0:1.0: USB hub found
[    1.227033] hub 1-0:1.0: 1 port detected
[    1.227725] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.228438] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 2
[    1.229427] xhci-hcd xhci-hcd.0.auto: Host supports USB 3.0 SuperSpeed
[    1.230322] usb usb2: We don't know the algorithms for LPM for this host, disabling LPM.
[    1.231425] usb usb2: New USB device found, idVendor=1d6b, idProduct=0003, bcdDevice= 4.14
[    1.232488] usb usb2: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.233416] usb usb2: Product: xHCI Host Controller
[    1.234062] usb usb2: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.234775] usb usb2: SerialNumber: xhci-hcd.0.auto
[    1.235934] hub 2-0:1.0: USB hub found
[    1.236450] hub 2-0:1.0: 1 port detected
[    1.237651] mmc1: new HSSDIO card at address 0001
[    1.481636] usb 1-1: new high-speed USB device number 2 using xhci-hcd
[    1.629815] usb 1-1: New USB device found, idVendor=1a40, idProduct=0101, bcdDevice= 1.11
[    1.630868] usb 1-1: New USB device strings: Mfr=0, Product=1, SerialNumber=0
[    1.631785] usb 1-1: Product: USB 2.0 Hub
[    1.678481] hub 1-1:1.0: USB hub found
[    1.678996] hub 1-1:1.0: 4 ports detected
[    1.961627] mmc2: new UHS SDR104 SDHC card at address 0001
[    1.962645] mmcblk2: mmc2:0001 SD16G 29.8 GiB
[    1.964259]  mmcblk2: p1 p2
[    2.147417] SMP: stopping secondary CPUs
[    2.147925] psci: psci_sys_reset(reboot_mode=0)
NOTICE:  fast_boot:0

S
F
L
O
NOTICE:  efuse cpu_cfg = 0
W
NOTICE:  Booting Trusted Firmware
NOTICE:  BL1: v1.4(release):HR-ROM-Rel-v1.1-141-ga91d4dd-dirty
NOTICE:  BL1: Built : 11:24:44, Oct 23 2019
NOTICE:  boot src: 2
NOTICE:  GigaDev SPI NAND was found.
NOTICE:  Block size: 128 KiB, page size: 2048
NOTICE:  BL1: Booting BL2
Auth pass
NOTICE:  bl1_main exit
SPL normal reset flow
check_reset_state (2): wakeup address = 0x0, hw wakeup status = 0x3, wakeup src=0x100
patch for sys_pll 1200 with 100M eth
SFLOW_INIT
CHIP ID:PCB941/WAFER: W04/ X: X20/ Y: Y36
secondary_jump_to_spl: secure chip flow
X3 SPL : secondary core wake up and jump to spl done (cpu_core_cfg=0)
SFLOW_FIN_HW_A

U-Boot SPL 2018.09-g4ca851534c-dirty (May 11 2022 - 20:09:50 +0800)
SPACC Init - ID: (00000061)
SPL nand boot mode (from strap)
GigaDev SPI NAND was found.
Block size: 128 KiB, page size: 2048
ddr_type = 1 (LPDDR4)
hb_chip_package_type:3
load ddr header src_addr: 100000, load_addr: 802ca020, src_len: a00
find valid ddr image
ddr_hdr.ecc_gran: 0x0
ddr_hdr.ecc_map: 0x0
ddr_hdr.sbr_pattern0: 0x0
ddr_hdr.sbr_pattern1: 0x0
ddr_freq = 05
board id = 31540334
ddr datarate: 3200
### SAMSUNG DDR ###
no ddr pin set
detect part number: 108
detect ddr freq: c80
board id alternative:0x3
index is 12
index is 15
index is 19
hb_ddr_index: 19
ddr_type = 1, ddr_vendor=3, ddr_freq=3200
dram_pll_init
sscg disabled
control load ddrc src_addr: 15ae00, load_addr: 802caa20, src_len: 920
[DDR INFO]      ==ddr_release_info==
[DDR INFO]      VERSION:        develop
[DDR INFO]      BUILD:          2022-05-11-20:09
[DDR INFO]      GIT COMMIT:     4ca851534c1616ace920fdaa000c6fb717c1fb74
[DDR INFO]      GIT TIME:       Wed, 20 Apr 2022 18:28:49 +0800
[DDR INFO]      ==ddr_features==
[DDR INFO]      RDBI:           0
[DDR INFO]      WDBI:           1
[DDR INFO]      InlineECC:      0
[DDR INFO]      DM:             1
[DDR INFO]      DDC:            1
[DDR INFO]      SSCG:           0
[DDR INFO]      BOARD:          XS_ENABLE
[DDR INFO] ddr_controller_cfg done
load ddr phy src_addr: 15b800, load_addr: 802caa20, src_len: 420
ATxSlewRate     : 15f
ATxImpedance    : 7f
TxSlewRate      : 19f
TxOdtDrvStren   : 600
TxImpedanceCtrl : e3f
CalDrvStr0      : 11
VrefInGlobal    : 104
board_type = 4 (CUSTOMER_BOARD)
load dqmap src addr: 15d600, load_addr: 802caa20, src_len: 20
[DDR INFO] dwc_ddrphy_train start
magic = 544f4248
load imem1 src_addr: 11ce00, load_addr: 802caa20, src_len: 8000
load dmem1 src_addr: 15a000, load_addr: 802caa20, src_len: 684
executing 1D fw
load imem2 src_addr: 124e00, load_addr: 802caa20, src_len: 8000
load dmem2 src_addr: 15a800, load_addr: 802caa20, src_len: 564

*******************************************************
p_dmem_lpddr4_2d_16b->MR11_A0:54
p_dmem_lpddr4_2d_16b->MR14_A0:54
p_dmem_lpddr4_2d_16b->MR12_A0:51
p_dmem_lpddr4_2d_16b->MR22_A0:14

p_dmem_lpddr4_2d_16b->MR3_A0:b3
p_dmem_lpddr4_2d_16b->Reserved00:40
p_dmem_lpddr4_2d_16b->Reserved0E:4
p_dmem_lpddr4_2d_16b->Delay_Weight2D:20
p_dmem_lpddr4_2d_16b->Voltage_Weight2D:80
*******************************************************

executing 2D fw
load pie src_addr: 15be00, load_addr: 802caa20, src_len: 11f0
Set QoS.
get_ddr_mr_info:cs_num=1, mr5=0x1, mr8=0x10
no magic in efuse file,bypass efuse
total_sz = 4096
SPL_VERSION:7
uboot partition is uboot_A
load u-boot: src_addr=0x380000, dest_addr=0x4000000, len=2097152
load warm boot spl: addr=0x800, dest_addr=0x80000000, len=31232
load bl31: addr=0x300000, dest_addr=0x0, len=524288
SFLOW_AUTH_BL31
verify signature of header:  verify ok!
verify signature of image:  verify ok!
bypass bpu image
clear keybank!!!!
SFLOW_DBG_EN
Trying to boot from RAM
SPL: bl31 will jump to u-boot or other entry (0x4000000)
SFLOW_CLR_KEY
SFLOW_REG_LD
install_portal copy portal
install_portal call smc and jump to bl31 cold entry(0x0)
hb som type: 5
X3 PI reset VDD_SD done

U-Boot 2018.09-g40785bca (May 27 2022 - 16:30:48 +0800)

Model: Hobot XJ3 Soc Board
DRAM:  system DDR size: 0xffe00000
4 GiB
MMC:   dwmmc@A5010000: 0, dwmmc@A5011000: 1, dwmmc@A5012000: 2
Loading Environment from UBI... GigaDevice SPI NAND was found.
128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
*** Warning - bad CRC, using default environment

In:    serial@a5000000
Out:   serial@a5000000
Err:   serial@a5000000
Net:   x3 sdb reset eth phy done

Warning: ethernet@A5014000 (eth0) using random MAC address - c6:b7:95:6b:dc:c0
eth0: ethernet@A5014000
Disable cnn cores ..
dtb_name:hobot-x3-pi.dtb
base board type: X3 SDB
bootmode: NAND
board_id = 31540334
damaged volume, update marker is setdamaged volume, update marker is setdamaged volume, update marker is sethb_boot_args_cmd_set custom_bootargs 0 ubuntu_boot 0
Hit any key to stop autoboot:  0
enable watchdog success !
switch to partitions #0, OK
mmc2 is current device
Scanning mmc 2:2...
Found U-Boot script /boot/boot.scr
664 bytes read in 2 ms (324.2 KiB/s)
## Executing script at 03c10000
Boot script loaded from devtype:mmc devnum:2 devplist:2
bootargs = console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
Loading fdt file: /boot/hobot/hobot-x3-pi.dtb
69633 bytes read in 8 ms (8.3 MiB/s)
Loading kernel: /boot/Image
19163144 bytes read in 845 ms (21.6 MiB/s)
## Flattened Device Tree blob at 03c00000
   Booting using the fdt blob at 0x3c00000
   Loading Device Tree to 0000000003c00000, end 0000000003c1ffff ... OK
chip_id: ab36300
The address of the fdt is 0x3c00000
Changed status Done
Can't get fdt_addr !!!Orign(MAX) bpu model Reserve Mem Size to 64M!!

Starting kernel ...

[    0.000000] OF: reserved mem: OVERLAP DETECTED!
[    0.000000] image_r5_mem (0x0000000080000000--0x0000000080010000) overlaps with msg_r5_mem (0x000000008000f000--0x0000000080010000)
[    0.000000] Reserved memory: created CMA memory pool at 0x0000000004000000, size 672 MiB
[    0.000000] OF: reserved mem: initialized node ion_cma, compatible id shared-dma-pool
[    0.000000] cma: Reserved 16 MiB at 0x000000007f000000
[    0.000000] On node 0 totalpages: 1047808
[    0.000000]   DMA zone: 8180 pages used for memmap
[    0.000000]   DMA zone: 0 pages reserved
[    0.000000]   DMA zone: 523520 pages, LIFO batch:31
[    0.000000]   Normal zone: 8192 pages used for memmap
[    0.000000]   Normal zone: 524288 pages, LIFO batch:31
[    0.000000] psci: probing for conduit method from DT.
[    0.000000] psci: PSCIv1.1 detected in firmware.
[    0.000000] psci: Using standard PSCI v0.2 function IDs
[    0.000000] psci: MIGRATE_INFO_TYPE not supported.
[    0.000000] psci: SMC Calling Convention v1.1
[    0.000000] percpu: Embedded 25 pages/cpu @ffffffc17ff2a000 s65176 r8192 d29032 u102400
[    0.000000] pcpu-alloc: s65176 r8192 d29032 u102400 alloc=25*4096
[    0.000000] pcpu-alloc: [0] 0 [0] 1 [0] 2 [0] 3
[    0.000000] Detected VIPT I-cache on CPU0
[    0.000000] CPU features: enabling workaround for ARM erratum 845719
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 1031436
[    0.000000] Kernel command line: earlycon loglevel=8 kgdboc=ttyS0 video=hobot:x3sdb-hdmi  console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
[    0.000000] PID hash table entries: 4096 (order: 3, 32768 bytes)
[    0.000000] Dentry cache hash table entries: 524288 (order: 10, 4194304 bytes)
[    0.000000] Inode-cache hash table entries: 262144 (order: 9, 2097152 bytes)
[    0.000000] software IO TLB [mem 0x7afff000-0x7efff000] (64MB) mapped at [ffffffc07afff000-ffffffc07effefff]
[    0.000000] Memory: 3319580K/4191232K available (10494K kernel code, 1306K rwdata, 5756K rodata, 1088K init, 9553K bss, 167140K reserved, 704512K cma-reserved)
[    0.000000] Virtual kernel memory layout:
[    0.000000]     modules : 0xffffff8000000000 - 0xffffff8008000000   (   128 MB)
[    0.000000]     vmalloc : 0xffffff8008000000 - 0xffffffbebfff0000   (   250 GB)
[    0.000000]       .text : 0xffffff8008000000 - 0xffffff8008a40000   ( 10496 KB)
[    0.000000]     .rodata : 0xffffff8008a40000 - 0xffffff8008ff0000   (  5824 KB)
[    0.000000]       .init : 0xffffff8008ff0000 - 0xffffff8009100000   (  1088 KB)
[    0.000000]       .data : 0xffffff8009100000 - 0xffffff8009246808   (  1307 KB)
[    0.000000]        .bss : 0xffffff8009246808 - 0xffffff8009b9aed8   (  9554 KB)
[    0.000000]     fixed   : 0xffffffbefe7fd000 - 0xffffffbefec00000   (  4108 KB)
[    0.000000]     PCI I/O : 0xffffffbefee00000 - 0xffffffbeffe00000   (    16 MB)
[    0.000000]     vmemmap : 0xffffffbf00000000 - 0xffffffc000000000   (     4 GB maximum)
[    0.000000]               0xffffffbf00008000 - 0xffffffbf06000000   (    95 MB actual)
[    0.000000]     memory  : 0xffffffc000200000 - 0xffffffc180000000   (  6142 MB)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=4, Nodes=1
[    0.000000] ftrace: allocating 36277 entries in 142 pages
[    0.000000] Preemptible hierarchical RCU implementation.
[    0.000000]  Tasks RCU enabled.
[    0.000000] NR_IRQS: 64, nr_irqs: 64, preallocated irqs: 0
[    0.000000] parent_rate: 0,  dclk->rate:2666000000, pre_ddr_rate:0, res.a0:139716712
[    0.000000] arch_timer: cp15 timer(s) running at 24.00MHz (virt).
[    0.000000] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0x588fe9dc0, max_idle_ns: 440795202592 ns
[    0.000004] sched_clock: 56 bits at 24MHz, resolution 41ns, wraps every 4398046511097ns
[    0.001193] clocksource: hobot_clocksource: mask: 0xffffffffffffffff max_cycles: 0x1d854df40, max_idle_ns: 3526361616960 ns
[    0.002967] Console: colour dummy device 80x25
[    0.003538] Calibrating delay loop (skipped), value calculated using timer frequency.. 48.00 BogoMIPS (lpj=96000)
[    0.004844] pid_max: default: 32768 minimum: 301
[    0.005497] Security Framework initialized
[    0.006016] AppArmor: AppArmor disabled by boot time parameter
[    0.006858] Mount-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.007726] Mountpoint-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.023769] ASID allocator initialised with 65536 entries
[    0.031766] Hierarchical SRCU implementation.
[    0.063825] smp: Bringing up secondary CPUs ...
[    0.100032] Detected VIPT I-cache on CPU1
[    0.100066] CPU1: Booted secondary processor [410fd034]
[    0.136082] Detected VIPT I-cache on CPU2
[    0.136103] CPU2: Booted secondary processor [410fd034]
[    0.172141] Detected VIPT I-cache on CPU3
[    0.172161] CPU3: Booted secondary processor [410fd034]
[    0.172214] smp: Brought up 1 node, 4 CPUs
[    0.176277] SMP: Total of 4 processors activated.
[    0.176872] CPU features: detected feature: 32-bit EL0 Support
[    0.177691] CPU: All CPU(s) started at EL1
[    0.178219] alternatives: patching kernel code
[    0.179808] devtmpfs: initialized
[    0.188882] random: get_random_u32 called from bucket_table_alloc+0x108/0x270 with crng_init=0
[    0.190466] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 7645041785100000 ns
[    0.191711] futex hash table entries: 1024 (order: 5, 131072 bytes)
[    0.208249] xor: automatically using best checksumming function   32regs
[    0.209187] pinctrl core: initialized pinctrl subsystem
[    0.210428] NET: Registered protocol family 16
[    0.211750] vdso: 2 pages (1 code @ ffffff8008a46000, 1 data @ ffffff8009104000)
[    0.212695] hw-breakpoint: found 6 breakpoint and 4 watchpoint registers.
[    0.214288] DMA: preallocated 256 KiB pool for atomic allocations
[    0.218041] pstore: using zlib compression
[    0.218835] console [pstore-1] enabled
[    0.219432] pstore: Registered ramoops as persistent store backend
[    0.220216] ramoops: attached 0x40000@0x3fc0000, ecc: 0/0
[    0.225195] hobot_dma a1005000.dma: Hobot DMA Engine Driver Probed!!
[    0.243899] SCSI subsystem initialized
[    0.244533] media: Linux media interface: v0.10
[    0.245124] Linux video capture interface: v2.00
[    0.245745] pps_core: LinuxPPS API ver. 1 registered
[    0.246374] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.247557] PTP clock support registered
[    0.248754] ion_dummy: not reserve carveout memory, try to alloc from cma
[    0.385505] Advanced Linux Sound Architecture Driver Initialized.
[    0.386672] usbcore: registered new interface driver usbfs
[    0.387399] usbcore: registered new interface driver hub
[    0.388126] usbcore: registered new device driver usb
[    0.389160] clocksource: Switched to clocksource arch_sys_counter
[    0.436754] VFS: Disk quotas dquot_6.6.0
[    0.437327] VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
[    0.438271] FS-Cache: Loaded
[    0.438754] CacheFiles: Loaded
[    0.444064] NET: Registered protocol family 2
[    0.444997] TCP established hash table entries: 32768 (order: 6, 262144 bytes)
[    0.446140] TCP bind hash table entries: 32768 (order: 7, 524288 bytes)
[    0.447388] TCP: Hash tables configured (established 32768 bind 32768)
[    0.448297] UDP hash table entries: 2048 (order: 4, 65536 bytes)
[    0.449127] UDP-Lite hash table entries: 2048 (order: 4, 65536 bytes)
[    0.450149] NET: Registered protocol family 1
[    0.450978] RPC: Registered named UNIX socket transport module.
[    0.451729] RPC: Registered udp transport module.
[    0.452326] RPC: Registered tcp transport module.
[    0.452924] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.454449] hw perfevents: enabled with armv8_cortex_a53 PMU driver, 7 counters available
[    0.456666] audit: initializing netlink subsys (disabled)
[    0.457607] audit: type=2000 audit(0.456:1): state=initialized audit_enabled=0 res=1
[    0.457864] Initialise system trusted keyrings
[    0.457939] workingset: timestamp_bits=46 max_order=20 bucket_order=0
[    0.461666] zbud: loaded
[    0.463232] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.464093] exFAT: Version 1.2.9
[    0.464572] FS-Cache: Netfs 'nfs' registered for caching
[    0.465742] NFS: Registering the id_resolver key type
[    0.466394] Key type id_resolver registered
[    0.466921] Key type id_legacy registered
[    0.467437] nfs4filelayout_init: NFSv4 File Layout Driver Registering...
[    0.468290] Installing knfsd (copyright (C) 1996 okir@monad.swb.de).
[    0.472431] NET: Registered protocol family 38
[    0.473004] async_tx: api initialized (async)
[    0.473594] Key type asymmetric registered
[    0.474111] Asymmetric key parser 'x509' registered
[    0.474794] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 245)
[    0.475807] io scheduler noop registered
[    0.476467] io scheduler cfq registered (default)
[    0.477062] io scheduler mq-deadline registered
[    0.477654] io scheduler kyber registered
[    0.478843] pinctrl-single a6003170.pinctrl_voltag: 64 pins at pa ffffff8009c4d170 size 8
[    0.480187] pinctrl-single a6004000.pinctrl: 128 pins at pa ffffff8009c61000 size 512
[    0.481616] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: start probe
[    0.482511] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: probe ok
[    0.483379] gpio-x3 a6003000.gpio: x3 gpio probe start!!!
[    0.484070] gpio-x3 a6003000.gpio: x3 gpio add gpiochip start!!!
[    0.484996] gpio-x3 a6003000.gpio: diable all gpio irq
[    0.487256] gpio-x3 a6003000.gpio: irqbase:57
[    0.487808] gpio-x3 a6003000.gpio: x3 irq add start!!!
[    0.488468] irq: Cannot allocate irq_descs @ IRQ57, assuming pre-allocated
[    0.489507] gpio-x3 a6003000.gpio: x3 irq add ok!!!
[    0.490160] gpio-x3 a6003000.gpio: x3 irqchip ops add ok!!!
[    0.490866] gpio-x3 a6003000.gpio: x3 gpio probe ok!!!
[    0.491964] hobot-pwm: hobot-pwmchip0 registered
[    0.492717] hobot-pwm: hobot-pwmchip1 registered
[    0.494216] diag dev [ver:1.1] init done
[    0.495117] hobot_ddr_monitor: LPDDR4 detected
[    0.495877] hobot_ddr_monitor: ddr monitor init finished.
[    0.496259] [vcam] init start
[    0.497347] vcam probe start
[    0.497814] vcam probe end successful
[    0.498275] [vcam] init end
[    0.499211] a5000000.serial: ttyS0 at MMIO 0xa5000000 (irq = 10, base_baud = 12000000) is a hobot-uart
[    0.500423] console [ttyS0] enabled
[    0.500423] console [ttyS0] enabled
[    0.501343] bootconsole [hobot0] disabled
[    0.501343] bootconsole [hobot0] disabled
[    0.502658] hobot-uart a5001000.serial: Failed to create debugfs root directory
[    0.503660] a5001000.serial: ttyS1 at MMIO 0xa5001000 (irq = 11, base_baud = 12000000) is a hobot-uart
[    0.505108] hobot-uart a5003000.serial: Failed to create debugfs root directory
[    0.506129] a5003000.serial: ttyS3 at MMIO 0xa5003000 (irq = 12, base_baud = 12000000) is a hobot-uart
[    0.507663] KGDB: Registered I/O driver kgdboc
[    0.508492] cacheinfo: Unable to detect cache hierarchy for CPU 0
[    0.513909] brd: module loaded
[    0.518462] loop: module loaded
[    0.520006] spi-nand hr_nand.0: GigaDevice SPI NAND was found.
[    0.520767] spi-nand hr_nand.0: 128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
[    0.523393] hobot_spi a5006000.spi: ver: HOBOT-spi_V20.200330 master
[    0.524434] libphy: Fixed MDIO Bus: probed
[    0.525641] st_gmac a5014000.ethernet: found phy-handle subnode
[    0.526476] st_gmac a5014000.ethernet: xj3_mtl_setup, plat->rx-queues-to-use:4, and tx:4
[    0.527659] st_gmac a5014000.ethernet: xj3_probe_config_dt, clk_ptp_rate:250000000
[    0.528661] set mac address 00:11:22:0e:d7:96:
[    0.528664] (using random mac adress)
[    0.529823] (NULL device *): xj3_get_hw_features, tx_fifo_size:16384
[    0.530640] (NULL device *): xj3_get_hw_features, rx_fifo_size:16384
[    0.531458] st_gmac a5014000.ethernet: TSO supported
[    0.532098] st_gmac a5014000.ethernet: TSO feature enabled
[    0.532804] st_gmac a5014000.ethernet: Enable Rx Mitigation via HW Watchdog Timer
[    0.653890] libphy: hobot-mac-mdio: probed
[    0.655444] st_gmac a5014000.ethernet: hobot_eth_probe: probe sucessfully
[    0.656651] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_0v8 not found, using dummy regulator
[    0.657894] dwc3-of-simple b2000000.usb: usb regulator 0v8 enable succeed
[    0.658772] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_3v3 not found, using dummy regulator
[    0.659975] dwc3-of-simple b2000000.usb: usb regulator 3v3 enable succeed
[    0.661516] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    0.663172] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    0.664608] usbcore: registered new interface driver cdc_acm
[    0.665357] cdc_acm: USB Abstract Control Model driver for USB modems and ISDN adapters
[    0.666415] usbcore: registered new interface driver uas
[    0.667132] usbcore: registered new interface driver usb-storage
[    0.667961] usbcore: registered new interface driver usbserial
[    0.668733] usbcore: registered new interface driver usbserial_generic
[    0.669612] usbserial: USB Serial support registered for generic
[    0.670408] usbcore: registered new interface driver usb_serial_simple
[    0.671265] usbserial: USB Serial support registered for carelink
[    0.672066] usbserial: USB Serial support registered for zio
[    0.672811] usbserial: USB Serial support registered for funsoft
[    0.673612] usbserial: USB Serial support registered for flashloader
[    0.674449] usbserial: USB Serial support registered for google
[    0.675228] usbserial: USB Serial support registered for libtransistor
[    0.676084] usbserial: USB Serial support registered for vivopay
[    0.676874] usbserial: USB Serial support registered for moto_modem
[    0.677715] usbserial: USB Serial support registered for motorola_tetra
[    0.678586] usbserial: USB Serial support registered for novatel_gps
[    0.679422] usbserial: USB Serial support registered for hp4x
[    0.680179] usbserial: USB Serial support registered for suunto
[    0.680957] usbserial: USB Serial support registered for siemens_mpi
[    0.681818] usbcore: registered new interface driver rio500
[    0.682650] mousedev: PS/2 mouse device common for all mice
[    0.693698] hobot-rtc a6002000.rtc: rtc core: registered hobot-rtc as rtc0
[    0.694691] i2c /dev entries driver
[    0.695300] hobot-i2c a5009000.i2c: hobot i2c probe start
[    0.696070] hobot-i2c a5009000.i2c: round_rate:96000000
[    0.696747] hobot-i2c a5009000.i2c: I2C bus speed is 400000
[    0.697490] hobot-i2c a5009000.i2c: clkdiv = 0x1d
[    0.698098] hobot-i2c a5009000.i2c: i2c0 diag register....
[    0.699192] hobot-i2c a5009000.i2c: hobot_i2c_0 probe done
[    0.699991] hobot-i2c a500a000.i2c: hobot i2c probe start
[    0.700744] hobot-i2c a500a000.i2c: round_rate:96000000
[    0.701448] hobot-i2c a500a000.i2c: I2C bus speed is 400000
[    0.702166] hobot-i2c a500a000.i2c: clkdiv = 0x1d
[    0.702773] hobot-i2c a500a000.i2c: i2c1 diag register....
[    0.703785] hobot-i2c a500a000.i2c: hobot_i2c_1 probe done
[    0.704742] lirc_dev: IR Remote Control driver registered, major 239
[    0.705581] IR LIRC bridge handler initialized
[    0.706334] sif_mclk clock frequence is 544000000
[    0.706970] mipi_rx0_ipi clock frequence is 544000000
[    0.707659] mipi_rx1_ipi clock frequence is 544000000
[    0.708357] mipi_rx2_ipi clock frequence is 544000000
[    0.709067] mipi_rx3_ipi clock frequence is 544000000
[    0.709810] mipi_tx_ipi clock frequence is 544000000
[    0.710533] mipi_cfg_host clock frequence is 102000000
[    0.711288] pym_mclk clock frequence is 1188000000
[    0.712008] mipi_dev_ref clock frequence is 24000000
[    0.712762] mipi_host_ref clock frequence is 24000000
[    0.713555] sensor0_mclk clock frequence is 37125000
[    0.714331] sensor1_mclk clock frequence is 37125000
[    0.715120] sensor2_mclk clock frequence is 37125000
[    0.715920] sensor3_mclk clock frequence is 37125000
[    0.716559] [FRT:D] x3_ips_probe(0)
[    0.717591] hobot swinfo sel reg ro=0x1 boot dump
[    0.718498] pvt a1009000.pvt: SCRATCH test: 1234abcd, pvt is alive.
[    0.719421] pvt a1009000.pvt: VM Calibrated data detected
[    0.720614] hobot_wdt a1002000.watchdog: watchdog setting [pet:6s bark:11s bite:15s]
[    0.721964] hobot_wdt a1002000.watchdog: Hobot Watchdog Timer at ffffff8009db3000 with timeout 15s
[    0.723317] device-mapper: uevent: version 1.0.3
[    0.724077] device-mapper: ioctl: 4.37.0-ioctl (2017-09-20) initialised: dm-devel@redhat.com
[    0.725257] device-mapper: verity-avb: AVB error handler initialized with vbmeta device:
[    0.727667] Synopsys Designware Multimedia Card Interface Driver
[    0.728665] dwmmc_hobot a5010000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.729521] dwmmc_hobot a5010000.dwmmc: card-detect-delay not found.
[    0.730340] dwmmc_hobot a5010000.dwmmc: data-addr not found.
[    0.731389] mmc_host mmc0: card is non-removable.
[    0.774371] dwmmc_hobot a5011000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.777242] dwmmc_hobot a5011000.dwmmc: card-detect-delay not found.
[    0.779074] dwmmc_hobot a5011000.dwmmc: data-addr not found.
[    0.783847] dwmmc_hobot a5011000.dwmmc: mmc set to fixed voltage 1800
[    0.784908] mmc_host mmc1: card is non-removable.
[    0.881362] dwmmc_hobot a5012000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.882202] dwmmc_hobot a5012000.dwmmc: card-detect-delay not found.
[    0.883045] dwmmc_hobot a5012000.dwmmc: data-addr not found.
[    0.884011] dwmmc_hobot a5012000.dwmmc: Got CD GPIO
[    0.994965] mmc1: queuing unknown CIS tuple 0x80 (2 bytes)
[    0.997161] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.999354] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    1.002730] mmc1: queuing unknown CIS tuple 0x80 (7 bytes)
[    1.006697] mmc1: queuing unknown CIS tuple 0x81 (9 bytes)
[    1.073440] ledtrig-cpu: registered to indicate activity on CPUs
[    1.074271] hidraw: raw HID events driver (C) Jiri Kosina
[    1.075102] usbcore: registered new interface driver usbhid
[    1.075819] usbhid: USB HID core driver
[    1.076400] logger: created 256K log 'log_main'
[    1.077041] logger: created 256K log 'log_events'
[    1.077722] logger: created 256K log 'log_radio'
[    1.078377] logger: created 256K log 'log_system'
[    1.079393] set dmc devfreq governor to performance
[    1.080026] hobot_dmcfreq_target: dmcfreq->rate:2666000000, target_rate:2666000000
[    1.080999] buf:, powersave_rate:2666000000, dmcfreq->pre_state:0
[    1.087821] usbcore: registered new interface driver snd-usb-audio
[    1.088990] Netfilter messages via NETLINK v0.30.
[    1.089643] ip_set: protocol 6
[    1.090127] ipip: IPv4 and MPLS over IPv4 tunneling driver
[    1.091118] ip_tables: (C) 2000-2006 Netfilter Core Team
[    1.092039] arp_tables: arp_tables: (C) 2002 David S. Miller
[    1.092826] Initializing XFRM netlink socket
[    1.093704] NET: Registered protocol family 10
[    1.094934] Segment Routing with IPv6
[    1.095443] sit: IPv6, IPv4 and MPLS over IPv4 tunneling driver
[    1.096536] NET: Registered protocol family 17
[    1.097185] Key type dns_resolver registered
[    1.098829] Loading compiled-in X.509 certificates
[    1.102385] Loaded X.509 cert 'Build time autogenerated kernel key: 81cb0ef77db2fac76e9588c2120c82422367d268'
[    1.103722] zswap: loaded using pool lzo/zbud
[    1.114966] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    1.116627] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    1.117741] console [netcon0] enabled
[    1.118216] netconsole: network logging started
[    1.118997] hobot-rtc a6002000.rtc: setting system clock to 1970-01-01 00:00:00 UTC (0)
[    1.120181] vps mipi_dphy: probe with x3vio done
[    1.120888] hobot_wdt_test: wdt_test_init: wdt test init
[    1.125699] VCC_CNN0: disabling
[    1.126109] VCC_CNN1: disabling
[    1.127061] vps mipi_host0: ver 140* port0(0:0)
[    1.127965] vps mipi_host1: ver 140* port1(1:0)
[    1.128848] vps mipi_host2: ver 140* port2(0:1)
[    1.129710] vps mipi_host3: ver 140* port3(1:1)
[    1.130545] ALSA device list:
[    1.130929]   No soundcards found.
[    1.131565] md: Skipping autodetection of RAID arrays. (raid=autodetect will force)
[    1.132699] VFS: Cannot open root device "mmcblk2p2" or unknown-block(0,0): error -6
[    1.133724] Please append a correct "root=" boot option; here are the available partitions:
[    1.134800] 0100          102400 ram0
[    1.134802]  (driver?)
[    1.135591] 0101          102400 ram1
[    1.135593]  (driver?)
[    1.136381] 0102          102400 ram2
[    1.136383]  (driver?)
[    1.137231] 0103          102400 ram3
[    1.137233]  (driver?)
[    1.138022] 0104          102400 ram4
[    1.138024]  (driver?)
[    1.138812] 0105          102400 ram5
[    1.138813]  (driver?)
[    1.139601] 0106          102400 ram6
[    1.139603]  (driver?)
[    1.140391] 0107          102400 ram7
[    1.140393]  (driver?)
[    1.141197] 0108          102400 ram8
[    1.141199]  (driver?)
[    1.141988] 0109          102400 ram9
[    1.141989]  (driver?)
[    1.142777] 010a          102400 ram10
[    1.142779]  (driver?)
[    1.143578] 010b          102400 ram11
[    1.143580]  (driver?)
[    1.144379] 010c          102400 ram12
[    1.144381]  (driver?)
[    1.145212] 010d          102400 ram13
[    1.145215]  (driver?)
[    1.146014] 010e          102400 ram14
[    1.146016]  (driver?)
[    1.146816] 010f          102400 ram15
[    1.146818]  (driver?)
[    1.147619] 1f00          131072 mtdblock0
[    1.147621]  (driver?)
[    1.148465] hobot_fusa: set_fusa_error_pin:75 set error pin to 1
[    1.149250] hobot_fusa: fusa errpin not ready
[    1.149254] Kernel panic - not syncing: VFS: Unable to mount root fs on unknown-block(0,0)
[    1.150874] Kernel Offset: disabled
[    1.151325] CPU features: 0x0002004
[    1.151774] Memory Limit: none
[    1.156330] Rebooting in 1 seconds..
[    1.225414] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.226136] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 1
[    1.227591] xhci-hcd xhci-hcd.0.auto: hcc params 0x0220fe6d hci version 0x110 quirks 0x0000000000010010
[    1.228825] xhci-hcd xhci-hcd.0.auto: irq 178, io mem 0xb2000000
[    1.229794] usb usb1: New USB device found, idVendor=1d6b, idProduct=0002, bcdDevice= 4.14
[    1.230857] usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.231785] usb usb1: Product: xHCI Host Controller
[    1.232414] usb usb1: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.233120] usb usb1: SerialNumber: xhci-hcd.0.auto
[    1.234081] hub 1-0:1.0: USB hub found
[    1.234459] mmc1: new HSSDIO card at address 0001
[    1.235189] hub 1-0:1.0: 1 port detected
[    1.235881] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.236594] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 2
[    1.237599] xhci-hcd xhci-hcd.0.auto: Host supports USB 3.0 SuperSpeed
[    1.238476] usb usb2: We don't know the algorithms for LPM for this host, disabling LPM.
[    1.239583] usb usb2: New USB device found, idVendor=1d6b, idProduct=0003, bcdDevice= 4.14
[    1.240646] usb usb2: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.241582] usb usb2: Product: xHCI Host Controller
[    1.242211] usb usb2: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.242917] usb usb2: SerialNumber: xhci-hcd.0.auto
[    1.243839] hub 2-0:1.0: USB hub found
[    1.244339] hub 2-0:1.0: 1 port detected
[    2.156842] SMP: stopping secondary CPUs
[    2.157349] psci: psci_sys_reset(reboot_mode=0)
NOTICE:  fast_boot:0

S
F
L
O
NOTICE:  efuse cpu_cfg = 0
W
NOTICE:  Booting Trusted Firmware
NOTICE:  BL1: v1.4(release):HR-ROM-Rel-v1.1-141-ga91d4dd-dirty
NOTICE:  BL1: Built : 11:24:44, Oct 23 2019
NOTICE:  boot src: 2
NOTICE:  GigaDev SPI NAND was found.
NOTICE:  Block size: 128 KiB, page size: 2048
NOTICE:  BL1: Booting BL2
Auth pass
NOTICE:  bl1_main exit
SPL normal reset flow
check_reset_state (2): wakeup address = 0x0, hw wakeup status = 0x3, wakeup src=0x100
patch for sys_pll 1200 with 100M eth
SFLOW_INIT
CHIP ID:PCB941/WAFER: W04/ X: X20/ Y: Y36
secondary_jump_to_spl: secure chip flow
X3 SPL : secondary core wake up and jump to spl done (cpu_core_cfg=0)
SFLOW_FIN_HW_A

U-Boot SPL 2018.09-g4ca851534c-dirty (May 11 2022 - 20:09:50 +0800)
SPACC Init - ID: (00000061)
SPL nand boot mode (from strap)
GigaDev SPI NAND was found.
Block size: 128 KiB, page size: 2048
ddr_type = 1 (LPDDR4)
hb_chip_package_type:3
load ddr header src_addr: 100000, load_addr: 802ca020, src_len: a00
find valid ddr image
ddr_hdr.ecc_gran: 0x0
ddr_hdr.ecc_map: 0x0
ddr_hdr.sbr_pattern0: 0x0
ddr_hdr.sbr_pattern1: 0x0
ddr_freq = 05
board id = 31540334
ddr datarate: 3200
### SAMSUNG DDR ###
no ddr pin set
detect part number: 108
detect ddr freq: c80
board id alternative:0x3
index is 12
index is 15
index is 19
hb_ddr_index: 19
ddr_type = 1, ddr_vendor=3, ddr_freq=3200
dram_pll_init
sscg disabled
control load ddrc src_addr: 15ae00, load_addr: 802caa20, src_len: 920
[DDR INFO]      ==ddr_release_info==
[DDR INFO]      VERSION:        develop
[DDR INFO]      BUILD:          2022-05-11-20:09
[DDR INFO]      GIT COMMIT:     4ca851534c1616ace920fdaa000c6fb717c1fb74
[DDR INFO]      GIT TIME:       Wed, 20 Apr 2022 18:28:49 +0800
[DDR INFO]      ==ddr_features==
[DDR INFO]      RDBI:           0
[DDR INFO]      WDBI:           1
[DDR INFO]      InlineECC:      0
[DDR INFO]      DM:             1
[DDR INFO]      DDC:            1
[DDR INFO]      SSCG:           0
[DDR INFO]      BOARD:          XS_ENABLE
[DDR INFO] ddr_controller_cfg done
load ddr phy src_addr: 15b800, load_addr: 802caa20, src_len: 420
ATxSlewRate     : 15f
ATxImpedance    : 7f
TxSlewRate      : 19f
TxOdtDrvStren   : 600
TxImpedanceCtrl : e3f
CalDrvStr0      : 11
VrefInGlobal    : 104
board_type = 4 (CUSTOMER_BOARD)
load dqmap src addr: 15d600, load_addr: 802caa20, src_len: 20
[DDR INFO] dwc_ddrphy_train start
magic = 544f4248
load imem1 src_addr: 11ce00, load_addr: 802caa20, src_len: 8000
load dmem1 src_addr: 15a000, load_addr: 802caa20, src_len: 684
executing 1D fw
load imem2 src_addr: 124e00, load_addr: 802caa20, src_len: 8000
load dmem2 src_addr: 15a800, load_addr: 802caa20, src_len: 564

*******************************************************
p_dmem_lpddr4_2d_16b->MR11_A0:54
p_dmem_lpddr4_2d_16b->MR14_A0:54
p_dmem_lpddr4_2d_16b->MR12_A0:51
p_dmem_lpddr4_2d_16b->MR22_A0:14

p_dmem_lpddr4_2d_16b->MR3_A0:b3
p_dmem_lpddr4_2d_16b->Reserved00:40
p_dmem_lpddr4_2d_16b->Reserved0E:4
p_dmem_lpddr4_2d_16b->Delay_Weight2D:20
p_dmem_lpddr4_2d_16b->Voltage_Weight2D:80
*******************************************************

executing 2D fw
load pie src_addr: 15be00, load_addr: 802caa20, src_len: 11f0
Set QoS.
get_ddr_mr_info:cs_num=1, mr5=0x1, mr8=0x10
no magic in efuse file,bypass efuse
total_sz = 4096
SPL_VERSION:7
uboot partition is uboot_A
load u-boot: src_addr=0x380000, dest_addr=0x4000000, len=2097152
load warm boot spl: addr=0x800, dest_addr=0x80000000, len=31232
load bl31: addr=0x300000, dest_addr=0x0, len=524288
SFLOW_AUTH_BL31
verify signature of header:  verify ok!
verify signature of image:  verify ok!
bypass bpu image
clear keybank!!!!
SFLOW_DBG_EN
Trying to boot from RAM
SPL: bl31 will jump to u-boot or other entry (0x4000000)
SFLOW_CLR_KEY
SFLOW_REG_LD
install_portal copy portal
install_portal call smc and jump to bl31 cold entry(0x0)
hb som type: 5
X3 PI reset VDD_SD done

U-Boot 2018.09-g40785bca (May 27 2022 - 16:30:48 +0800)

Model: Hobot XJ3 Soc Board
DRAM:  system DDR size: 0xffe00000
4 GiB
MMC:   dwmmc@A5010000: 0, dwmmc@A5011000: 1, dwmmc@A5012000: 2 (SD)
Loading Environment from UBI... GigaDevice SPI NAND was found.
128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
*** Warning - bad CRC, using default environment

In:    serial@a5000000
Out:   serial@a5000000
Err:   serial@a5000000
Net:   x3 sdb reset eth phy done

Warning: ethernet@A5014000 (eth0) using random MAC address - 9e:1e:0d:f6:24:43
eth0: ethernet@A5014000
Disable cnn cores ..
dtb_name:hobot-x3-pi.dtb
base board type: X3 SDB
bootmode: NAND
board_id = 31540334
damaged volume, update marker is setdamaged volume, update marker is setdamaged volume, update marker is sethb_boot_args_cmd_set custom_bootargs 0 ubuntu_boot 0
Hit any key to stop autoboot:  0
enable watchdog success !
switch to partitions #0, OK
mmc2 is current device
Scanning mmc 2:2...
Found U-Boot script /boot/boot.scr
664 bytes read in 2 ms (324.2 KiB/s)
## Executing script at 03c10000
Boot script loaded from devtype:mmc devnum:2 devplist:2
bootargs = console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
Loading fdt file: /boot/hobot/hobot-x3-pi.dtb
69633 bytes read in 8 ms (8.3 MiB/s)
Loading kernel: /boot/Image
19163144 bytes read in 845 ms (21.6 MiB/s)
## Flattened Device Tree blob at 03c00000
   Booting using the fdt blob at 0x3c00000
   Loading Device Tree to 0000000003c00000, end 0000000003c1ffff ... OK
chip_id: ab36300
The address of the fdt is 0x3c00000
Changed status Done
Can't get fdt_addr !!!Orign(MAX) bpu model Reserve Mem Size to 64M!!

Starting kernel ...

[    0.000000] OF: reserved mem: OVERLAP DETECTED!
[    0.000000] image_r5_mem (0x0000000080000000--0x0000000080010000) overlaps with msg_r5_mem (0x000000008000f000--0x0000000080010000)
[    0.000000] Reserved memory: created CMA memory pool at 0x0000000004000000, size 672 MiB
[    0.000000] OF: reserved mem: initialized node ion_cma, compatible id shared-dma-pool
[    0.000000] cma: Reserved 16 MiB at 0x000000007f000000
[    0.000000] On node 0 totalpages: 1047808
[    0.000000]   DMA zone: 8180 pages used for memmap
[    0.000000]   DMA zone: 0 pages reserved
[    0.000000]   DMA zone: 523520 pages, LIFO batch:31
[    0.000000]   Normal zone: 8192 pages used for memmap
[    0.000000]   Normal zone: 524288 pages, LIFO batch:31
[    0.000000] psci: probing for conduit method from DT.
[    0.000000] psci: PSCIv1.1 detected in firmware.
[    0.000000] psci: Using standard PSCI v0.2 function IDs
[    0.000000] psci: MIGRATE_INFO_TYPE not supported.
[    0.000000] psci: SMC Calling Convention v1.1
[    0.000000] percpu: Embedded 25 pages/cpu @ffffffc17ff2a000 s65176 r8192 d29032 u102400
[    0.000000] pcpu-alloc: s65176 r8192 d29032 u102400 alloc=25*4096
[    0.000000] pcpu-alloc: [0] 0 [0] 1 [0] 2 [0] 3
[    0.000000] Detected VIPT I-cache on CPU0
[    0.000000] CPU features: enabling workaround for ARM erratum 845719
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 1031436
[    0.000000] Kernel command line: earlycon loglevel=8 kgdboc=ttyS0 video=hobot:x3sdb-hdmi  console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
[    0.000000] PID hash table entries: 4096 (order: 3, 32768 bytes)
[    0.000000] Dentry cache hash table entries: 524288 (order: 10, 4194304 bytes)
[    0.000000] Inode-cache hash table entries: 262144 (order: 9, 2097152 bytes)
[    0.000000] software IO TLB [mem 0x7afff000-0x7efff000] (64MB) mapped at [ffffffc07afff000-ffffffc07effefff]
[    0.000000] Memory: 3319580K/4191232K available (10494K kernel code, 1306K rwdata, 5756K rodata, 1088K init, 9553K bss, 167140K reserved, 704512K cma-reserved)
[    0.000000] Virtual kernel memory layout:
[    0.000000]     modules : 0xffffff8000000000 - 0xffffff8008000000   (   128 MB)
[    0.000000]     vmalloc : 0xffffff8008000000 - 0xffffffbebfff0000   (   250 GB)
[    0.000000]       .text : 0xffffff8008000000 - 0xffffff8008a40000   ( 10496 KB)
[    0.000000]     .rodata : 0xffffff8008a40000 - 0xffffff8008ff0000   (  5824 KB)
[    0.000000]       .init : 0xffffff8008ff0000 - 0xffffff8009100000   (  1088 KB)
[    0.000000]       .data : 0xffffff8009100000 - 0xffffff8009246808   (  1307 KB)
[    0.000000]        .bss : 0xffffff8009246808 - 0xffffff8009b9aed8   (  9554 KB)
[    0.000000]     fixed   : 0xffffffbefe7fd000 - 0xffffffbefec00000   (  4108 KB)
[    0.000000]     PCI I/O : 0xffffffbefee00000 - 0xffffffbeffe00000   (    16 MB)
[    0.000000]     vmemmap : 0xffffffbf00000000 - 0xffffffc000000000   (     4 GB maximum)
[    0.000000]               0xffffffbf00008000 - 0xffffffbf06000000   (    95 MB actual)
[    0.000000]     memory  : 0xffffffc000200000 - 0xffffffc180000000   (  6142 MB)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=4, Nodes=1
[    0.000000] ftrace: allocating 36277 entries in 142 pages
[    0.000000] Preemptible hierarchical RCU implementation.
[    0.000000]  Tasks RCU enabled.
[    0.000000] NR_IRQS: 64, nr_irqs: 64, preallocated irqs: 0
[    0.000000] parent_rate: 0,  dclk->rate:2666000000, pre_ddr_rate:0, res.a0:139716712
[    0.000000] arch_timer: cp15 timer(s) running at 24.00MHz (virt).
[    0.000000] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0x588fe9dc0, max_idle_ns: 440795202592 ns
[    0.000004] sched_clock: 56 bits at 24MHz, resolution 41ns, wraps every 4398046511097ns
[    0.001194] clocksource: hobot_clocksource: mask: 0xffffffffffffffff max_cycles: 0x1d854df40, max_idle_ns: 3526361616960 ns
[    0.002965] Console: colour dummy device 80x25
[    0.003536] Calibrating delay loop (skipped), value calculated using timer frequency.. 48.00 BogoMIPS (lpj=96000)
[    0.004841] pid_max: default: 32768 minimum: 301
[    0.005496] Security Framework initialized
[    0.006014] AppArmor: AppArmor disabled by boot time parameter
[    0.006857] Mount-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.007724] Mountpoint-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.023768] ASID allocator initialised with 65536 entries
[    0.031765] Hierarchical SRCU implementation.
[    0.063824] smp: Bringing up secondary CPUs ...
[    0.100031] Detected VIPT I-cache on CPU1
[    0.100066] CPU1: Booted secondary processor [410fd034]
[    0.136081] Detected VIPT I-cache on CPU2
[    0.136102] CPU2: Booted secondary processor [410fd034]
[    0.172140] Detected VIPT I-cache on CPU3
[    0.172159] CPU3: Booted secondary processor [410fd034]
[    0.172213] smp: Brought up 1 node, 4 CPUs
[    0.176276] SMP: Total of 4 processors activated.
[    0.176871] CPU features: detected feature: 32-bit EL0 Support
[    0.177689] CPU: All CPU(s) started at EL1
[    0.178217] alternatives: patching kernel code
[    0.179808] devtmpfs: initialized
[    0.188881] random: get_random_u32 called from bucket_table_alloc+0x108/0x270 with crng_init=0
[    0.190467] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 7645041785100000 ns
[    0.191713] futex hash table entries: 1024 (order: 5, 131072 bytes)
[    0.208237] xor: automatically using best checksumming function   32regs
[    0.209171] pinctrl core: initialized pinctrl subsystem
[    0.210403] NET: Registered protocol family 16
[    0.211727] vdso: 2 pages (1 code @ ffffff8008a46000, 1 data @ ffffff8009104000)
[    0.212672] hw-breakpoint: found 6 breakpoint and 4 watchpoint registers.
[    0.214262] DMA: preallocated 256 KiB pool for atomic allocations
[    0.218155] pstore: using zlib compression
[    0.218950] console [pstore-1] enabled
[    0.219547] pstore: Registered ramoops as persistent store backend
[    0.220332] ramoops: attached 0x40000@0x3fc0000, ecc: 0/0
[    0.225305] hobot_dma a1005000.dma: Hobot DMA Engine Driver Probed!!
[    0.239016] SCSI subsystem initialized
[    0.239642] media: Linux media interface: v0.10
[    0.240237] Linux video capture interface: v2.00
[    0.240913] pps_core: LinuxPPS API ver. 1 registered
[    0.241540] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.242716] PTP clock support registered
[    0.243834] ion_dummy: not reserve carveout memory, try to alloc from cma
[    0.380613] Advanced Linux Sound Architecture Driver Initialized.
[    0.381800] usbcore: registered new interface driver usbfs
[    0.382529] usbcore: registered new interface driver hub
[    0.383255] usbcore: registered new device driver usb
[    0.384205] clocksource: Switched to clocksource arch_sys_counter
[    0.431881] VFS: Disk quotas dquot_6.6.0
[    0.432455] VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
[    0.433391] FS-Cache: Loaded
[    0.433876] CacheFiles: Loaded
[    0.439171] NET: Registered protocol family 2
[    0.440096] TCP established hash table entries: 32768 (order: 6, 262144 bytes)
[    0.441242] TCP bind hash table entries: 32768 (order: 7, 524288 bytes)
[    0.442488] TCP: Hash tables configured (established 32768 bind 32768)
[    0.443402] UDP hash table entries: 2048 (order: 4, 65536 bytes)
[    0.444262] UDP-Lite hash table entries: 2048 (order: 4, 65536 bytes)
[    0.445267] NET: Registered protocol family 1
[    0.446104] RPC: Registered named UNIX socket transport module.
[    0.446855] RPC: Registered udp transport module.
[    0.447452] RPC: Registered tcp transport module.
[    0.448051] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.449673] hw perfevents: enabled with armv8_cortex_a53 PMU driver, 7 counters available
[    0.451884] audit: initializing netlink subsys (disabled)
[    0.452689] audit: type=2000 audit(0.448:1): state=initialized audit_enabled=0 res=1
[    0.452936] Initialise system trusted keyrings
[    0.453015] workingset: timestamp_bits=46 max_order=20 bucket_order=0
[    0.456646] zbud: loaded
[    0.458194] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.459053] exFAT: Version 1.2.9
[    0.459534] FS-Cache: Netfs 'nfs' registered for caching
[    0.460815] NFS: Registering the id_resolver key type
[    0.461469] Key type id_resolver registered
[    0.461996] Key type id_legacy registered
[    0.462512] nfs4filelayout_init: NFSv4 File Layout Driver Registering...
[    0.463365] Installing knfsd (copyright (C) 1996 okir@monad.swb.de).
[    0.467478] NET: Registered protocol family 38
[    0.468049] async_tx: api initialized (async)
[    0.468618] Key type asymmetric registered
[    0.469136] Asymmetric key parser 'x509' registered
[    0.469815] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 245)
[    0.470832] io scheduler noop registered
[    0.471484] io scheduler cfq registered (default)
[    0.472079] io scheduler mq-deadline registered
[    0.472810] io scheduler kyber registered
[    0.474016] pinctrl-single a6003170.pinctrl_voltag: 64 pins at pa ffffff8009c4d170 size 8
[    0.475351] pinctrl-single a6004000.pinctrl: 128 pins at pa ffffff8009c61000 size 512
[    0.476603] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: start probe
[    0.477495] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: probe ok
[    0.478369] gpio-x3 a6003000.gpio: x3 gpio probe start!!!
[    0.479059] gpio-x3 a6003000.gpio: x3 gpio add gpiochip start!!!
[    0.479985] gpio-x3 a6003000.gpio: diable all gpio irq
[    0.482245] gpio-x3 a6003000.gpio: irqbase:57
[    0.482797] gpio-x3 a6003000.gpio: x3 irq add start!!!
[    0.483454] irq: Cannot allocate irq_descs @ IRQ57, assuming pre-allocated
[    0.484611] gpio-x3 a6003000.gpio: x3 irq add ok!!!
[    0.485266] gpio-x3 a6003000.gpio: x3 irqchip ops add ok!!!
[    0.485971] gpio-x3 a6003000.gpio: x3 gpio probe ok!!!
[    0.487057] hobot-pwm: hobot-pwmchip0 registered
[    0.487809] hobot-pwm: hobot-pwmchip1 registered
[    0.489166] diag dev [ver:1.1] init done
[    0.490063] hobot_ddr_monitor: LPDDR4 detected
[    0.490829] hobot_ddr_monitor: ddr monitor init finished.
[    0.491226] [vcam] init start
[    0.492307] vcam probe start
[    0.492766] vcam probe end successful
[    0.493227] [vcam] init end
[    0.494153] a5000000.serial: ttyS0 at MMIO 0xa5000000 (irq = 10, base_baud = 12000000) is a hobot-uart
[    0.495365] console [ttyS0] enabled
[    0.495365] console [ttyS0] enabled
[    0.496353] bootconsole [hobot0] disabled
[    0.496353] bootconsole [hobot0] disabled
[    0.497691] hobot-uart a5001000.serial: Failed to create debugfs root directory
[    0.498694] a5001000.serial: ttyS1 at MMIO 0xa5001000 (irq = 11, base_baud = 12000000) is a hobot-uart
[    0.500139] hobot-uart a5003000.serial: Failed to create debugfs root directory
[    0.501165] a5003000.serial: ttyS3 at MMIO 0xa5003000 (irq = 12, base_baud = 12000000) is a hobot-uart
[    0.502710] KGDB: Registered I/O driver kgdboc
[    0.503547] cacheinfo: Unable to detect cache hierarchy for CPU 0
[    0.508994] brd: module loaded
[    0.513557] loop: module loaded
[    0.515074] spi-nand hr_nand.0: GigaDevice SPI NAND was found.
[    0.515834] spi-nand hr_nand.0: 128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
[    0.518476] hobot_spi a5006000.spi: ver: HOBOT-spi_V20.200330 master
[    0.519520] libphy: Fixed MDIO Bus: probed
[    0.520719] st_gmac a5014000.ethernet: found phy-handle subnode
[    0.521557] st_gmac a5014000.ethernet: xj3_mtl_setup, plat->rx-queues-to-use:4, and tx:4
[    0.522742] st_gmac a5014000.ethernet: xj3_probe_config_dt, clk_ptp_rate:250000000
[    0.523744] set mac address 00:11:22:b6:37:9a:
[    0.523747] (using random mac adress)
[    0.524916] (NULL device *): xj3_get_hw_features, tx_fifo_size:16384
[    0.525734] (NULL device *): xj3_get_hw_features, rx_fifo_size:16384
[    0.526551] st_gmac a5014000.ethernet: TSO supported
[    0.527191] st_gmac a5014000.ethernet: TSO feature enabled
[    0.527898] st_gmac a5014000.ethernet: Enable Rx Mitigation via HW Watchdog Timer
[    0.648976] libphy: hobot-mac-mdio: probed
[    0.650533] st_gmac a5014000.ethernet: hobot_eth_probe: probe sucessfully
[    0.651732] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_0v8 not found, using dummy regulator
[    0.652974] dwc3-of-simple b2000000.usb: usb regulator 0v8 enable succeed
[    0.653851] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_3v3 not found, using dummy regulator
[    0.655056] dwc3-of-simple b2000000.usb: usb regulator 3v3 enable succeed
[    0.656595] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    0.658252] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    0.659689] usbcore: registered new interface driver cdc_acm
[    0.660439] cdc_acm: USB Abstract Control Model driver for USB modems and ISDN adapters
[    0.661497] usbcore: registered new interface driver uas
[    0.662217] usbcore: registered new interface driver usb-storage
[    0.663044] usbcore: registered new interface driver usbserial
[    0.663816] usbcore: registered new interface driver usbserial_generic
[    0.664692] usbserial: USB Serial support registered for generic
[    0.665491] usbcore: registered new interface driver usb_serial_simple
[    0.666347] usbserial: USB Serial support registered for carelink
[    0.667148] usbserial: USB Serial support registered for zio
[    0.667893] usbserial: USB Serial support registered for funsoft
[    0.668694] usbserial: USB Serial support registered for flashloader
[    0.669528] usbserial: USB Serial support registered for google
[    0.670310] usbserial: USB Serial support registered for libtransistor
[    0.671168] usbserial: USB Serial support registered for vivopay
[    0.671958] usbserial: USB Serial support registered for moto_modem
[    0.672798] usbserial: USB Serial support registered for motorola_tetra
[    0.673666] usbserial: USB Serial support registered for novatel_gps
[    0.674500] usbserial: USB Serial support registered for hp4x
[    0.675259] usbserial: USB Serial support registered for suunto
[    0.676038] usbserial: USB Serial support registered for siemens_mpi
[    0.676900] usbcore: registered new interface driver rio500
[    0.677728] mousedev: PS/2 mouse device common for all mice
[    0.688782] hobot-rtc a6002000.rtc: rtc core: registered hobot-rtc as rtc0
[    0.689775] i2c /dev entries driver
[    0.690383] hobot-i2c a5009000.i2c: hobot i2c probe start
[    0.691150] hobot-i2c a5009000.i2c: round_rate:96000000
[    0.691827] hobot-i2c a5009000.i2c: I2C bus speed is 400000
[    0.692569] hobot-i2c a5009000.i2c: clkdiv = 0x1d
[    0.693177] hobot-i2c a5009000.i2c: i2c0 diag register....
[    0.694269] hobot-i2c a5009000.i2c: hobot_i2c_0 probe done
[    0.695073] hobot-i2c a500a000.i2c: hobot i2c probe start
[    0.695826] hobot-i2c a500a000.i2c: round_rate:96000000
[    0.696525] hobot-i2c a500a000.i2c: I2C bus speed is 400000
[    0.697244] hobot-i2c a500a000.i2c: clkdiv = 0x1d
[    0.697850] hobot-i2c a500a000.i2c: i2c1 diag register....
[    0.698870] hobot-i2c a500a000.i2c: hobot_i2c_1 probe done
[    0.699823] lirc_dev: IR Remote Control driver registered, major 239
[    0.700662] IR LIRC bridge handler initialized
[    0.701419] sif_mclk clock frequence is 544000000
[    0.702055] mipi_rx0_ipi clock frequence is 544000000
[    0.702744] mipi_rx1_ipi clock frequence is 544000000
[    0.703442] mipi_rx2_ipi clock frequence is 544000000
[    0.704152] mipi_rx3_ipi clock frequence is 544000000
[    0.704892] mipi_tx_ipi clock frequence is 544000000
[    0.705613] mipi_cfg_host clock frequence is 102000000
[    0.706367] pym_mclk clock frequence is 1188000000
[    0.707087] mipi_dev_ref clock frequence is 24000000
[    0.707841] mipi_host_ref clock frequence is 24000000
[    0.708637] sensor0_mclk clock frequence is 37125000
[    0.709414] sensor1_mclk clock frequence is 37125000
[    0.710202] sensor2_mclk clock frequence is 37125000
[    0.711003] sensor3_mclk clock frequence is 37125000
[    0.711642] [FRT:D] x3_ips_probe(0)
[    0.712658] hobot swinfo sel reg ro=0x1 boot dump
[    0.713576] pvt a1009000.pvt: SCRATCH test: 1234abcd, pvt is alive.
[    0.714503] pvt a1009000.pvt: VM Calibrated data detected
[    0.715682] hobot_wdt a1002000.watchdog: watchdog setting [pet:6s bark:11s bite:15s]
[    0.717025] hobot_wdt a1002000.watchdog: Hobot Watchdog Timer at ffffff8009db3000 with timeout 15s
[    0.718377] device-mapper: uevent: version 1.0.3
[    0.719135] device-mapper: ioctl: 4.37.0-ioctl (2017-09-20) initialised: dm-devel@redhat.com
[    0.720368] device-mapper: verity-avb: AVB error handler initialized with vbmeta device:
[    0.722782] Synopsys Designware Multimedia Card Interface Driver
[    0.723782] dwmmc_hobot a5010000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.724640] dwmmc_hobot a5010000.dwmmc: card-detect-delay not found.
[    0.725459] dwmmc_hobot a5010000.dwmmc: data-addr not found.
[    0.726497] mmc_host mmc0: card is non-removable.
[    0.765414] dwmmc_hobot a5011000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.768267] dwmmc_hobot a5011000.dwmmc: card-detect-delay not found.
[    0.769087] dwmmc_hobot a5011000.dwmmc: data-addr not found.
[    0.773857] dwmmc_hobot a5011000.dwmmc: mmc set to fixed voltage 1800
[    0.774920] mmc_host mmc1: card is non-removable.
[    0.872432] dwmmc_hobot a5012000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.873250] dwmmc_hobot a5012000.dwmmc: card-detect-delay not found.
[    0.874083] dwmmc_hobot a5012000.dwmmc: data-addr not found.
[    0.875054] dwmmc_hobot a5012000.dwmmc: Got CD GPIO
[    0.983561] mmc1: queuing unknown CIS tuple 0x80 (2 bytes)
[    0.985761] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.987946] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.991321] mmc1: queuing unknown CIS tuple 0x80 (7 bytes)
[    0.995276] mmc1: queuing unknown CIS tuple 0x81 (9 bytes)
[    1.056509] ledtrig-cpu: registered to indicate activity on CPUs
[    1.057343] hidraw: raw HID events driver (C) Jiri Kosina
[    1.058195] usbcore: registered new interface driver usbhid
[    1.058912] usbhid: USB HID core driver
[    1.059497] logger: created 256K log 'log_main'
[    1.060142] logger: created 256K log 'log_events'
[    1.060825] logger: created 256K log 'log_radio'
[    1.061478] logger: created 256K log 'log_system'
[    1.062505] set dmc devfreq governor to performance
[    1.063138] hobot_dmcfreq_target: dmcfreq->rate:2666000000, target_rate:2666000000
[    1.064111] buf:, powersave_rate:2666000000, dmcfreq->pre_state:0
[    1.070942] usbcore: registered new interface driver snd-usb-audio
[    1.072088] Netfilter messages via NETLINK v0.30.
[    1.072741] ip_set: protocol 6
[    1.073224] ipip: IPv4 and MPLS over IPv4 tunneling driver
[    1.074227] ip_tables: (C) 2000-2006 Netfilter Core Team
[    1.075231] arp_tables: arp_tables: (C) 2002 David S. Miller
[    1.076031] Initializing XFRM netlink socket
[    1.076953] NET: Registered protocol family 10
[    1.078181] Segment Routing with IPv6
[    1.078691] sit: IPv6, IPv4 and MPLS over IPv4 tunneling driver
[    1.079784] NET: Registered protocol family 17
[    1.080466] Key type dns_resolver registered
[    1.082130] Loading compiled-in X.509 certificates
[    1.085640] Loaded X.509 cert 'Build time autogenerated kernel key: 81cb0ef77db2fac76e9588c2120c82422367d268'
[    1.086970] zswap: loaded using pool lzo/zbud
[    1.098203] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    1.099867] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    1.100934] console [netcon0] enabled
[    1.101409] netconsole: network logging started
[    1.102191] hobot-rtc a6002000.rtc: setting system clock to 1970-01-01 00:00:00 UTC (0)
[    1.103386] vps mipi_dphy: probe with x3vio done
[    1.104092] hobot_wdt_test: wdt_test_init: wdt test init
[    1.106816] VCC_CNN0: disabling
[    1.107226] VCC_CNN1: disabling
[    1.108181] vps mipi_host0: ver 140* port0(0:0)
[    1.109123] vps mipi_host1: ver 140* port1(1:0)
[    1.110009] vps mipi_host2: ver 140* port2(0:1)
[    1.110799] vps mipi_host3: ver 140* port3(1:1)
[    1.111629] ALSA device list:
[    1.112014]   No soundcards found.
[    1.112676] md: Skipping autodetection of RAID arrays. (raid=autodetect will force)
[    1.113798] VFS: Cannot open root device "mmcblk2p2" or unknown-block(0,0): error -6
[    1.114791] Please append a correct "root=" boot option; here are the available partitions:
[    1.115865] 0100          102400 ram0
[    1.115867]  (driver?)
[    1.116669] 0101          102400 ram1
[    1.116671]  (driver?)
[    1.117460] 0102          102400 ram2
[    1.117461]  (driver?)
[    1.118249] 0103          102400 ram3
[    1.118251]  (driver?)
[    1.119039] 0104          102400 ram4
[    1.119041]  (driver?)
[    1.119828] 0105          102400 ram5
[    1.119830]  (driver?)
[    1.120679] 0106          102400 ram6
[    1.120681]  (driver?)
[    1.121470] 0107          102400 ram7
[    1.121472]  (driver?)
[    1.122260] 0108          102400 ram8
[    1.122262]  (driver?)
[    1.123049] 0109          102400 ram9
[    1.123051]  (driver?)
[    1.123839] 010a          102400 ram10
[    1.123841]  (driver?)
[    1.124690] 010b          102400 ram11
[    1.124692]  (driver?)
[    1.125492] 010c          102400 ram12
[    1.125493]  (driver?)
[    1.126293] 010d          102400 ram13
[    1.126294]  (driver?)
[    1.127093] 010e          102400 ram14
[    1.127095]  (driver?)
[    1.127894] 010f          102400 ram15
[    1.127896]  (driver?)
[    1.128725] 1f00          131072 mtdblock0
[    1.128727]  (driver?)
[    1.129570] hobot_fusa: set_fusa_error_pin:75 set error pin to 1
[    1.130341] hobot_fusa: fusa errpin not ready
[    1.130345] Kernel panic - not syncing: VFS: Unable to mount root fs on unknown-block(0,0)
[    1.131963] Kernel Offset: disabled
[    1.132415] CPU features: 0x0002004
[    1.132864] Memory Limit: none
[    1.137422] Rebooting in 1 seconds..
[    2.137934] SMP: stopping secondary CPUs
[    2.138442] psci: psci_sys_reset(reboot_mode=0)
NOTICE:  fast_boot:0

S
F
L
O
NOTICE:  efuse cpu_cfg = 0
W
NOTICE:  Booting Trusted Firmware
NOTICE:  BL1: v1.4(release):HR-ROM-Rel-v1.1-141-ga91d4dd-dirty
NOTICE:  BL1: Built : 11:24:44, Oct 23 2019
NOTICE:  boot src: 2
NOTICE:  GigaDev SPI NAND was found.
NOTICE:  Block size: 128 KiB, page size: 2048
NOTICE:  BL1: Booting BL2
Auth pass
NOTICE:  bl1_main exit
SPL normal reset flow
check_reset_state (2): wakeup address = 0x0, hw wakeup status = 0x3, wakeup src=0x100
patch for sys_pll 1200 with 100M eth
SFLOW_INIT
CHIP ID:PCB941/WAFER: W04/ X: X20/ Y: Y36
secondary_jump_to_spl: secure chip flow
X3 SPL : secondary core wake up and jump to spl done (cpu_core_cfg=0)
SFLOW_FIN_HW_A

U-Boot SPL 2018.09-g4ca851534c-dirty (May 11 2022 - 20:09:50 +0800)
SPACC Init - ID: (00000061)
SPL nand boot mode (from strap)
GigaDev SPI NAND was found.
Block size: 128 KiB, page size: 2048
ddr_type = 1 (LPDDR4)
hb_chip_package_type:3
load ddr header src_addr: 100000, load_addr: 802ca020, src_len: a00
find valid ddr image
ddr_hdr.ecc_gran: 0x0
ddr_hdr.ecc_map: 0x0
ddr_hdr.sbr_pattern0: 0x0
ddr_hdr.sbr_pattern1: 0x0
ddr_freq = 05
board id = 31540334
ddr datarate: 3200
### SAMSUNG DDR ###
no ddr pin set
detect part number: 108
detect ddr freq: c80
board id alternative:0x3
index is 12
index is 15
index is 19
hb_ddr_index: 19
ddr_type = 1, ddr_vendor=3, ddr_freq=3200
dram_pll_init
sscg disabled
control load ddrc src_addr: 15ae00, load_addr: 802caa20, src_len: 920
[DDR INFO]      ==ddr_release_info==
[DDR INFO]      VERSION:        develop
[DDR INFO]      BUILD:          2022-05-11-20:09
[DDR INFO]      GIT COMMIT:     4ca851534c1616ace920fdaa000c6fb717c1fb74
[DDR INFO]      GIT TIME:       Wed, 20 Apr 2022 18:28:49 +0800
[DDR INFO]      ==ddr_features==
[DDR INFO]      RDBI:           0
[DDR INFO]      WDBI:           1
[DDR INFO]      InlineECC:      0
[DDR INFO]      DM:             1
[DDR INFO]      DDC:            1
[DDR INFO]      SSCG:           0
[DDR INFO]      BOARD:          XS_ENABLE
[DDR INFO] ddr_controller_cfg done
load ddr phy src_addr: 15b800, load_addr: 802caa20, src_len: 420
ATxSlewRate     : 15f
ATxImpedance    : 7f
TxSlewRate      : 19f
TxOdtDrvStren   : 600
TxImpedanceCtrl : e3f
CalDrvStr0      : 11
VrefInGlobal    : 104
board_type = 4 (CUSTOMER_BOARD)
load dqmap src addr: 15d600, load_addr: 802caa20, src_len: 20
[DDR INFO] dwc_ddrphy_train start
magic = 544f4248
load imem1 src_addr: 11ce00, load_addr: 802caa20, src_len: 8000
load dmem1 src_addr: 15a000, load_addr: 802caa20, src_len: 684
executing 1D fw
load imem2 src_addr: 124e00, load_addr: 802caa20, src_len: 8000
load dmem2 src_addr: 15a800, load_addr: 802caa20, src_len: 564

*******************************************************
p_dmem_lpddr4_2d_16b->MR11_A0:54
p_dmem_lpddr4_2d_16b->MR14_A0:54
p_dmem_lpddr4_2d_16b->MR12_A0:51
p_dmem_lpddr4_2d_16b->MR22_A0:14

p_dmem_lpddr4_2d_16b->MR3_A0:b3
p_dmem_lpddr4_2d_16b->Reserved00:40
p_dmem_lpddr4_2d_16b->Reserved0E:4
p_dmem_lpddr4_2d_16b->Delay_Weight2D:20
p_dmem_lpddr4_2d_16b->Voltage_Weight2D:80
*******************************************************

executing 2D fw
load pie src_addr: 15be00, load_addr: 802caa20, src_len: 11f0
Set QoS.
get_ddr_mr_info:cs_num=1, mr5=0x1, mr8=0x10
no magic in efuse file,bypass efuse
total_sz = 4096
SPL_VERSION:7
uboot partition is uboot_A
load u-boot: src_addr=0x380000, dest_addr=0x4000000, len=2097152
load warm boot spl: addr=0x800, dest_addr=0x80000000, len=31232
load bl31: addr=0x300000, dest_addr=0x0, len=524288
SFLOW_AUTH_BL31
verify signature of header:  verify ok!
verify signature of image:  verify ok!
bypass bpu image
clear keybank!!!!
SFLOW_DBG_EN
Trying to boot from RAM
SPL: bl31 will jump to u-boot or other entry (0x4000000)
SFLOW_CLR_KEY
SFLOW_REG_LD
install_portal copy portal
install_portal call smc and jump to bl31 cold entry(0x0)
hb som type: 5
X3 PI reset VDD_SD done

U-Boot 2018.09-g40785bca (May 27 2022 - 16:30:48 +0800)

Model: Hobot XJ3 Soc Board
DRAM:  system DDR size: 0xffe00000
4 GiB
MMC:   dwmmc@A5010000: 0, dwmmc@A5011000: 1, dwmmc@A5012000: 2 (SD)
Loading Environment from UBI... GigaDevice SPI NAND was found.
128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
*** Warning - bad CRC, using default environment

In:    serial@a5000000
Out:   serial@a5000000
Err:   serial@a5000000
Net:   x3 sdb reset eth phy done

Warning: ethernet@A5014000 (eth0) using random MAC address - ca:75:df:63:b9:ad
eth0: ethernet@A5014000
Disable cnn cores ..
dtb_name:hobot-x3-pi.dtb
base board type: X3 SDB
bootmode: NAND
board_id = 31540334
damaged volume, update marker is setdamaged volume, update marker is setdamaged volume, update marker is sethb_boot_args_cmd_set custom_bootargs 0 ubuntu_boot 0
Hit any key to stop autoboot:  0
enable watchdog success !
switch to partitions #0, OK
mmc2 is current device
Scanning mmc 2:2...
Found U-Boot script /boot/boot.scr
664 bytes read in 2 ms (324.2 KiB/s)
## Executing script at 03c10000
Boot script loaded from devtype:mmc devnum:2 devplist:2
bootargs = console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
Loading fdt file: /boot/hobot/hobot-x3-pi.dtb
69633 bytes read in 8 ms (8.3 MiB/s)
Loading kernel: /boot/Image
19163144 bytes read in 845 ms (21.6 MiB/s)
## Flattened Device Tree blob at 03c00000
   Booting using the fdt blob at 0x3c00000
   Loading Device Tree to 0000000003c00000, end 0000000003c1ffff ... OK
chip_id: ab36300
The address of the fdt is 0x3c00000
Changed status Done
Can't get fdt_addr !!!Orign(MAX) bpu model Reserve Mem Size to 64M!!

Starting kernel ...

[    0.000000] OF: reserved mem: OVERLAP DETECTED!
[    0.000000] image_r5_mem (0x0000000080000000--0x0000000080010000) overlaps with msg_r5_mem (0x000000008000f000--0x0000000080010000)
[    0.000000] Reserved memory: created CMA memory pool at 0x0000000004000000, size 672 MiB
[    0.000000] OF: reserved mem: initialized node ion_cma, compatible id shared-dma-pool
[    0.000000] cma: Reserved 16 MiB at 0x000000007f000000
[    0.000000] On node 0 totalpages: 1047808
[    0.000000]   DMA zone: 8180 pages used for memmap
[    0.000000]   DMA zone: 0 pages reserved
[    0.000000]   DMA zone: 523520 pages, LIFO batch:31
[    0.000000]   Normal zone: 8192 pages used for memmap
[    0.000000]   Normal zone: 524288 pages, LIFO batch:31
[    0.000000] psci: probing for conduit method from DT.
[    0.000000] psci: PSCIv1.1 detected in firmware.
[    0.000000] psci: Using standard PSCI v0.2 function IDs
[    0.000000] psci: MIGRATE_INFO_TYPE not supported.
[    0.000000] psci: SMC Calling Convention v1.1
[    0.000000] percpu: Embedded 25 pages/cpu @ffffffc17ff2a000 s65176 r8192 d29032 u102400
[    0.000000] pcpu-alloc: s65176 r8192 d29032 u102400 alloc=25*4096
[    0.000000] pcpu-alloc: [0] 0 [0] 1 [0] 2 [0] 3
[    0.000000] Detected VIPT I-cache on CPU0
[    0.000000] CPU features: enabling workaround for ARM erratum 845719
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 1031436
[    0.000000] Kernel command line: earlycon loglevel=8 kgdboc=ttyS0 video=hobot:x3sdb-hdmi  console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
[    0.000000] PID hash table entries: 4096 (order: 3, 32768 bytes)
[    0.000000] Dentry cache hash table entries: 524288 (order: 10, 4194304 bytes)
[    0.000000] Inode-cache hash table entries: 262144 (order: 9, 2097152 bytes)
[    0.000000] software IO TLB [mem 0x7afff000-0x7efff000] (64MB) mapped at [ffffffc07afff000-ffffffc07effefff]
[    0.000000] Memory: 3319580K/4191232K available (10494K kernel code, 1306K rwdata, 5756K rodata, 1088K init, 9553K bss, 167140K reserved, 704512K cma-reserved)
[    0.000000] Virtual kernel memory layout:
[    0.000000]     modules : 0xffffff8000000000 - 0xffffff8008000000   (   128 MB)
[    0.000000]     vmalloc : 0xffffff8008000000 - 0xffffffbebfff0000   (   250 GB)
[    0.000000]       .text : 0xffffff8008000000 - 0xffffff8008a40000   ( 10496 KB)
[    0.000000]     .rodata : 0xffffff8008a40000 - 0xffffff8008ff0000   (  5824 KB)
[    0.000000]       .init : 0xffffff8008ff0000 - 0xffffff8009100000   (  1088 KB)
[    0.000000]       .data : 0xffffff8009100000 - 0xffffff8009246808   (  1307 KB)
[    0.000000]        .bss : 0xffffff8009246808 - 0xffffff8009b9aed8   (  9554 KB)
[    0.000000]     fixed   : 0xffffffbefe7fd000 - 0xffffffbefec00000   (  4108 KB)
[    0.000000]     PCI I/O : 0xffffffbefee00000 - 0xffffffbeffe00000   (    16 MB)
[    0.000000]     vmemmap : 0xffffffbf00000000 - 0xffffffc000000000   (     4 GB maximum)
[    0.000000]               0xffffffbf00008000 - 0xffffffbf06000000   (    95 MB actual)
[    0.000000]     memory  : 0xffffffc000200000 - 0xffffffc180000000   (  6142 MB)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=4, Nodes=1
[    0.000000] ftrace: allocating 36277 entries in 142 pages
[    0.000000] Preemptible hierarchical RCU implementation.
[    0.000000]  Tasks RCU enabled.
[    0.000000] NR_IRQS: 64, nr_irqs: 64, preallocated irqs: 0
[    0.000000] parent_rate: 0,  dclk->rate:2666000000, pre_ddr_rate:0, res.a0:139716712
[    0.000000] arch_timer: cp15 timer(s) running at 24.00MHz (virt).
[    0.000000] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0x588fe9dc0, max_idle_ns: 440795202592 ns
[    0.000004] sched_clock: 56 bits at 24MHz, resolution 41ns, wraps every 4398046511097ns
[    0.001196] clocksource: hobot_clocksource: mask: 0xffffffffffffffff max_cycles: 0x1d854df40, max_idle_ns: 3526361616960 ns
[    0.002968] Console: colour dummy device 80x25
[    0.003539] Calibrating delay loop (skipped), value calculated using timer frequency.. 48.00 BogoMIPS (lpj=96000)
[    0.004844] pid_max: default: 32768 minimum: 301
[    0.005499] Security Framework initialized
[    0.006017] AppArmor: AppArmor disabled by boot time parameter
[    0.006860] Mount-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.007728] Mountpoint-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.023770] ASID allocator initialised with 65536 entries
[    0.031767] Hierarchical SRCU implementation.
[    0.063825] smp: Bringing up secondary CPUs ...
[    0.100032] Detected VIPT I-cache on CPU1
[    0.100067] CPU1: Booted secondary processor [410fd034]
[    0.136082] Detected VIPT I-cache on CPU2
[    0.136103] CPU2: Booted secondary processor [410fd034]
[    0.172142] Detected VIPT I-cache on CPU3
[    0.172161] CPU3: Booted secondary processor [410fd034]
[    0.172215] smp: Brought up 1 node, 4 CPUs
[    0.176277] SMP: Total of 4 processors activated.
[    0.176872] CPU features: detected feature: 32-bit EL0 Support
[    0.177690] CPU: All CPU(s) started at EL1
[    0.178218] alternatives: patching kernel code
[    0.179809] devtmpfs: initialized
[    0.188887] random: get_random_u32 called from bucket_table_alloc+0x108/0x270 with crng_init=0
[    0.190471] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 7645041785100000 ns
[    0.191718] futex hash table entries: 1024 (order: 5, 131072 bytes)
[    0.208222] xor: automatically using best checksumming function   32regs
[    0.209164] pinctrl core: initialized pinctrl subsystem
[    0.210394] NET: Registered protocol family 16
[    0.211713] vdso: 2 pages (1 code @ ffffff8008a46000, 1 data @ ffffff8009104000)
[    0.212658] hw-breakpoint: found 6 breakpoint and 4 watchpoint registers.
[    0.214248] DMA: preallocated 256 KiB pool for atomic allocations
[    0.218908] pstore: using zlib compression
[    0.219703] console [pstore-1] enabled
[    0.220299] pstore: Registered ramoops as persistent store backend
[    0.221084] ramoops: attached 0x40000@0x3fc0000, ecc: 0/0
[    0.226094] hobot_dma a1005000.dma: Hobot DMA Engine Driver Probed!!
[    0.240035] SCSI subsystem initialized
[    0.240730] media: Linux media interface: v0.10
[    0.241325] Linux video capture interface: v2.00
[    0.241967] pps_core: LinuxPPS API ver. 1 registered
[    0.242595] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.243770] PTP clock support registered
[    0.245068] ion_dummy: not reserve carveout memory, try to alloc from cma
[    0.381581] Advanced Linux Sound Architecture Driver Initialized.
[    0.382778] usbcore: registered new interface driver usbfs
[    0.383506] usbcore: registered new interface driver hub
[    0.384232] usbcore: registered new device driver usb
[    0.385204] clocksource: Switched to clocksource arch_sys_counter
[    0.432914] VFS: Disk quotas dquot_6.6.0
[    0.433489] VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
[    0.434425] FS-Cache: Loaded
[    0.434929] CacheFiles: Loaded
[    0.440189] NET: Registered protocol family 2
[    0.441108] TCP established hash table entries: 32768 (order: 6, 262144 bytes)
[    0.442240] TCP bind hash table entries: 32768 (order: 7, 524288 bytes)
[    0.443485] TCP: Hash tables configured (established 32768 bind 32768)
[    0.444398] UDP hash table entries: 2048 (order: 4, 65536 bytes)
[    0.445246] UDP-Lite hash table entries: 2048 (order: 4, 65536 bytes)
[    0.446248] NET: Registered protocol family 1
[    0.447046] RPC: Registered named UNIX socket transport module.
[    0.447797] RPC: Registered udp transport module.
[    0.448394] RPC: Registered tcp transport module.
[    0.448993] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.450523] hw perfevents: enabled with armv8_cortex_a53 PMU driver, 7 counters available
[    0.452736] audit: initializing netlink subsys (disabled)
[    0.453520] audit: type=2000 audit(0.452:1): state=initialized audit_enabled=0 res=1
[    0.453778] Initialise system trusted keyrings
[    0.453860] workingset: timestamp_bits=46 max_order=20 bucket_order=0
[    0.457493] zbud: loaded
[    0.459035] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.459895] exFAT: Version 1.2.9
[    0.460374] FS-Cache: Netfs 'nfs' registered for caching
[    0.461533] NFS: Registering the id_resolver key type
[    0.462188] Key type id_resolver registered
[    0.462715] Key type id_legacy registered
[    0.463230] nfs4filelayout_init: NFSv4 File Layout Driver Registering...
[    0.464083] Installing knfsd (copyright (C) 1996 okir@monad.swb.de).
[    0.468177] NET: Registered protocol family 38
[    0.468749] async_tx: api initialized (async)
[    0.469316] Key type asymmetric registered
[    0.469833] Asymmetric key parser 'x509' registered
[    0.470522] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 245)
[    0.471537] io scheduler noop registered
[    0.472200] io scheduler cfq registered (default)
[    0.472795] io scheduler mq-deadline registered
[    0.473403] io scheduler kyber registered
[    0.474594] pinctrl-single a6003170.pinctrl_voltag: 64 pins at pa ffffff8009c4d170 size 8
[    0.475944] pinctrl-single a6004000.pinctrl: 128 pins at pa ffffff8009c61000 size 512
[    0.477150] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: start probe
[    0.478068] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: probe ok
[    0.478953] gpio-x3 a6003000.gpio: x3 gpio probe start!!!
[    0.479642] gpio-x3 a6003000.gpio: x3 gpio add gpiochip start!!!
[    0.480578] gpio-x3 a6003000.gpio: diable all gpio irq
[    0.482851] gpio-x3 a6003000.gpio: irqbase:57
[    0.483403] gpio-x3 a6003000.gpio: x3 irq add start!!!
[    0.484060] irq: Cannot allocate irq_descs @ IRQ57, assuming pre-allocated
[    0.485089] gpio-x3 a6003000.gpio: x3 irq add ok!!!
[    0.485887] gpio-x3 a6003000.gpio: x3 irqchip ops add ok!!!
[    0.486593] gpio-x3 a6003000.gpio: x3 gpio probe ok!!!
[    0.487705] hobot-pwm: hobot-pwmchip0 registered
[    0.488459] hobot-pwm: hobot-pwmchip1 registered
[    0.489823] diag dev [ver:1.1] init done
[    0.490723] hobot_ddr_monitor: LPDDR4 detected
[    0.491479] hobot_ddr_monitor: ddr monitor init finished.
[    0.491865] [vcam] init start
[    0.492926] vcam probe start
[    0.493396] vcam probe end successful
[    0.493858] [vcam] init end
[    0.494768] a5000000.serial: ttyS0 at MMIO 0xa5000000 (irq = 10, base_baud = 12000000) is a hobot-uart
[    0.495991] console [ttyS0] enabled
[    0.495991] console [ttyS0] enabled
[    0.496895] bootconsole [hobot0] disabled
[    0.496895] bootconsole [hobot0] disabled
[    0.498367] hobot-uart a5001000.serial: Failed to create debugfs root directory
[    0.499372] a5001000.serial: ttyS1 at MMIO 0xa5001000 (irq = 11, base_baud = 12000000) is a hobot-uart
[    0.500816] hobot-uart a5003000.serial: Failed to create debugfs root directory
[    0.501828] a5003000.serial: ttyS3 at MMIO 0xa5003000 (irq = 12, base_baud = 12000000) is a hobot-uart
[    0.503364] KGDB: Registered I/O driver kgdboc
[    0.504202] cacheinfo: Unable to detect cache hierarchy for CPU 0
[    0.509787] brd: module loaded
[    0.514359] loop: module loaded
[    0.515874] spi-nand hr_nand.0: GigaDevice SPI NAND was found.
[    0.516633] spi-nand hr_nand.0: 128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
[    0.519370] hobot_spi a5006000.spi: ver: HOBOT-spi_V20.200330 master
[    0.520409] libphy: Fixed MDIO Bus: probed
[    0.521694] st_gmac a5014000.ethernet: found phy-handle subnode
[    0.522530] st_gmac a5014000.ethernet: xj3_mtl_setup, plat->rx-queues-to-use:4, and tx:4
[    0.523713] st_gmac a5014000.ethernet: xj3_probe_config_dt, clk_ptp_rate:250000000
[    0.524717] set mac address 00:11:22:fe:c2:db:
[    0.524720] (using random mac adress)
[    0.525775] (NULL device *): xj3_get_hw_features, tx_fifo_size:16384
[    0.526591] (NULL device *): xj3_get_hw_features, rx_fifo_size:16384
[    0.527409] st_gmac a5014000.ethernet: TSO supported
[    0.528049] st_gmac a5014000.ethernet: TSO feature enabled
[    0.528756] st_gmac a5014000.ethernet: Enable Rx Mitigation via HW Watchdog Timer
[    0.649980] libphy: hobot-mac-mdio: probed
[    0.651537] st_gmac a5014000.ethernet: hobot_eth_probe: probe sucessfully
[    0.652741] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_0v8 not found, using dummy regulator
[    0.653984] dwc3-of-simple b2000000.usb: usb regulator 0v8 enable succeed
[    0.654862] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_3v3 not found, using dummy regulator
[    0.656067] dwc3-of-simple b2000000.usb: usb regulator 3v3 enable succeed
[    0.657607] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    0.659264] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    0.660715] usbcore: registered new interface driver cdc_acm
[    0.661466] cdc_acm: USB Abstract Control Model driver for USB modems and ISDN adapters
[    0.662521] usbcore: registered new interface driver uas
[    0.663238] usbcore: registered new interface driver usb-storage
[    0.664069] usbcore: registered new interface driver usbserial
[    0.664843] usbcore: registered new interface driver usbserial_generic
[    0.665721] usbserial: USB Serial support registered for generic
[    0.666516] usbcore: registered new interface driver usb_serial_simple
[    0.667374] usbserial: USB Serial support registered for carelink
[    0.668177] usbserial: USB Serial support registered for zio
[    0.668922] usbserial: USB Serial support registered for funsoft
[    0.669730] usbserial: USB Serial support registered for flashloader
[    0.670564] usbserial: USB Serial support registered for google
[    0.671343] usbserial: USB Serial support registered for libtransistor
[    0.672199] usbserial: USB Serial support registered for vivopay
[    0.672991] usbserial: USB Serial support registered for moto_modem
[    0.673830] usbserial: USB Serial support registered for motorola_tetra
[    0.674698] usbserial: USB Serial support registered for novatel_gps
[    0.675532] usbserial: USB Serial support registered for hp4x
[    0.676289] usbserial: USB Serial support registered for suunto
[    0.677069] usbserial: USB Serial support registered for siemens_mpi
[    0.677925] usbcore: registered new interface driver rio500
[    0.678755] mousedev: PS/2 mouse device common for all mice
[    0.689799] hobot-rtc a6002000.rtc: rtc core: registered hobot-rtc as rtc0
[    0.690792] i2c /dev entries driver
[    0.691398] hobot-i2c a5009000.i2c: hobot i2c probe start
[    0.692163] hobot-i2c a5009000.i2c: round_rate:96000000
[    0.692841] hobot-i2c a5009000.i2c: I2C bus speed is 400000
[    0.693569] hobot-i2c a5009000.i2c: clkdiv = 0x1d
[    0.694176] hobot-i2c a5009000.i2c: i2c0 diag register....
[    0.695275] hobot-i2c a5009000.i2c: hobot_i2c_0 probe done
[    0.696080] hobot-i2c a500a000.i2c: hobot i2c probe start
[    0.696833] hobot-i2c a500a000.i2c: round_rate:96000000
[    0.697532] hobot-i2c a500a000.i2c: I2C bus speed is 400000
[    0.698250] hobot-i2c a500a000.i2c: clkdiv = 0x1d
[    0.698857] hobot-i2c a500a000.i2c: i2c1 diag register....
[    0.699860] hobot-i2c a500a000.i2c: hobot_i2c_1 probe done
[    0.700822] lirc_dev: IR Remote Control driver registered, major 239
[    0.701662] IR LIRC bridge handler initialized
[    0.702417] sif_mclk clock frequence is 544000000
[    0.703053] mipi_rx0_ipi clock frequence is 544000000
[    0.703741] mipi_rx1_ipi clock frequence is 544000000
[    0.704440] mipi_rx2_ipi clock frequence is 544000000
[    0.705149] mipi_rx3_ipi clock frequence is 544000000
[    0.705879] mipi_tx_ipi clock frequence is 544000000
[    0.706600] mipi_cfg_host clock frequence is 102000000
[    0.707353] pym_mclk clock frequence is 1188000000
[    0.708073] mipi_dev_ref clock frequence is 24000000
[    0.708827] mipi_host_ref clock frequence is 24000000
[    0.709630] sensor0_mclk clock frequence is 37125000
[    0.710408] sensor1_mclk clock frequence is 37125000
[    0.711196] sensor2_mclk clock frequence is 37125000
[    0.711995] sensor3_mclk clock frequence is 37125000
[    0.712634] [FRT:D] x3_ips_probe(0)
[    0.713669] hobot swinfo sel reg ro=0x1 boot dump
[    0.714582] pvt a1009000.pvt: SCRATCH test: 1234abcd, pvt is alive.
[    0.715510] pvt a1009000.pvt: VM Calibrated data detected
[    0.716691] hobot_wdt a1002000.watchdog: watchdog setting [pet:6s bark:11s bite:15s]
[    0.718024] hobot_wdt a1002000.watchdog: Hobot Watchdog Timer at ffffff8009db3000 with timeout 15s
[    0.719374] device-mapper: uevent: version 1.0.3
[    0.720130] device-mapper: ioctl: 4.37.0-ioctl (2017-09-20) initialised: dm-devel@redhat.com
[    0.721300] device-mapper: verity-avb: AVB error handler initialized with vbmeta device:
[    0.723701] Synopsys Designware Multimedia Card Interface Driver
[    0.724698] dwmmc_hobot a5010000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.725579] dwmmc_hobot a5010000.dwmmc: card-detect-delay not found.
[    0.726398] dwmmc_hobot a5010000.dwmmc: data-addr not found.
[    0.727449] mmc_host mmc0: card is non-removable.
[    0.770418] dwmmc_hobot a5011000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.773275] dwmmc_hobot a5011000.dwmmc: card-detect-delay not found.
[    0.774684] dwmmc_hobot a5011000.dwmmc: data-addr not found.
[    0.779458] dwmmc_hobot a5011000.dwmmc: mmc set to fixed voltage 1800
[    0.780527] mmc_host mmc1: card is non-removable.
[    0.877424] dwmmc_hobot a5012000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.878241] dwmmc_hobot a5012000.dwmmc: card-detect-delay not found.
[    0.879074] dwmmc_hobot a5012000.dwmmc: data-addr not found.
[    0.880039] dwmmc_hobot a5012000.dwmmc: Got CD GPIO
[    0.988566] mmc1: queuing unknown CIS tuple 0x80 (2 bytes)
[    0.990759] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.992944] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.996322] mmc1: queuing unknown CIS tuple 0x80 (7 bytes)
[    1.000279] mmc1: queuing unknown CIS tuple 0x81 (9 bytes)
[    1.065502] ledtrig-cpu: registered to indicate activity on CPUs
[    1.066329] hidraw: raw HID events driver (C) Jiri Kosina
[    1.067169] usbcore: registered new interface driver usbhid
[    1.067887] usbhid: USB HID core driver
[    1.068469] logger: created 256K log 'log_main'
[    1.069113] logger: created 256K log 'log_events'
[    1.069804] logger: created 256K log 'log_radio'
[    1.070465] logger: created 256K log 'log_system'
[    1.071519] set dmc devfreq governor to performance
[    1.072163] hobot_dmcfreq_target: dmcfreq->rate:2666000000, target_rate:2666000000
[    1.073144] buf:, powersave_rate:2666000000, dmcfreq->pre_state:0
[    1.080022] usbcore: registered new interface driver snd-usb-audio
[    1.081188] Netfilter messages via NETLINK v0.30.
[    1.081847] ip_set: protocol 6
[    1.082340] ipip: IPv4 and MPLS over IPv4 tunneling driver
[    1.083344] ip_tables: (C) 2000-2006 Netfilter Core Team
[    1.084278] arp_tables: arp_tables: (C) 2002 David S. Miller
[    1.085077] Initializing XFRM netlink socket
[    1.085971] NET: Registered protocol family 10
[    1.087237] Segment Routing with IPv6
[    1.087754] sit: IPv6, IPv4 and MPLS over IPv4 tunneling driver
[    1.088870] NET: Registered protocol family 17
[    1.089526] Key type dns_resolver registered
[    1.091216] Loading compiled-in X.509 certificates
[    1.094744] Loaded X.509 cert 'Build time autogenerated kernel key: 81cb0ef77db2fac76e9588c2120c82422367d268'
[    1.096077] zswap: loaded using pool lzo/zbud
[    1.111397] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    1.113067] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    1.114053] console [netcon0] enabled
[    1.114527] netconsole: network logging started
[    1.115309] hobot-rtc a6002000.rtc: setting system clock to 1970-01-01 00:00:00 UTC (0)
[    1.116500] vps mipi_dphy: probe with x3vio done
[    1.117250] hobot_wdt_test: wdt_test_init: wdt test init
[    1.119952] VCC_CNN0: disabling
[    1.120361] VCC_CNN1: disabling
[    1.121337] vps mipi_host0: ver 140* port0(0:0)
[    1.122255] vps mipi_host1: ver 140* port1(1:0)
[    1.123147] vps mipi_host2: ver 140* port2(0:1)
[    1.123929] vps mipi_host3: ver 140* port3(1:1)
[    1.124766] ALSA device list:
[    1.125151]   No soundcards found.
[    1.125826] md: Skipping autodetection of RAID arrays. (raid=autodetect will force)
[    1.126960] VFS: Cannot open root device "mmcblk2p2" or unknown-block(0,0): error -6
[    1.127954] Please append a correct "root=" boot option; here are the available partitions:
[    1.129028] 0100          102400 ram0
[    1.129030]  (driver?)
[    1.129844] 0101          102400 ram1
[    1.129846]  (driver?)
[    1.130634] 0102          102400 ram2
[    1.130636]  (driver?)
[    1.131425] 0103          102400 ram3
[    1.131426]  (driver?)
[    1.132214] 0104          102400 ram4
[    1.132216]  (driver?)
[    1.133004] 0105          102400 ram5
[    1.133006]  (driver?)
[    1.133851] 0106          102400 ram6
[    1.133853]  (driver?)
[    1.134642] 0107          102400 ram7
[    1.134643]  (driver?)
[    1.135431] 0108          102400 ram8
[    1.135433]  (driver?)
[    1.136221] 0109          102400 ram9
[    1.136223]  (driver?)
[    1.137011] 010a          102400 ram10
[    1.137012]  (driver?)
[    1.137845] 010b          102400 ram11
[    1.137847]  (driver?)
[    1.138646] 010c          102400 ram12
[    1.138648]  (driver?)
[    1.139447] 010d          102400 ram13
[    1.139449]  (driver?)
[    1.140249] 010e          102400 ram14
[    1.140250]  (driver?)
[    1.141049] 010f          102400 ram15
[    1.141051]  (driver?)
[    1.141898] 1f00          131072 mtdblock0
[    1.141900]  (driver?)
[    1.142744] hobot_fusa: set_fusa_error_pin:75 set error pin to 1
[    1.143515] hobot_fusa: fusa errpin not ready
[    1.143519] Kernel panic - not syncing: VFS: Unable to mount root fs on unknown-block(0,0)
[    1.145138] Kernel Offset: disabled
[    1.145589] CPU features: 0x0002004
[    1.146038] Memory Limit: none
[    1.150597] Rebooting in 1 seconds..
[    1.221448] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.222172] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 1
[    1.223625] xhci-hcd xhci-hcd.0.auto: hcc params 0x0220fe6d hci version 0x110 quirks 0x0000000000010010
[    1.224859] xhci-hcd xhci-hcd.0.auto: irq 178, io mem 0xb2000000
[    1.225833] usb usb1: New USB device found, idVendor=1d6b, idProduct=0002, bcdDevice= 4.14
[    1.226896] usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.227825] usb usb1: Product: xHCI Host Controller
[    1.228453] usb usb1: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.229160] usb usb1: SerialNumber: xhci-hcd.0.auto
[    1.230104] hub 1-0:1.0: USB hub found
[    1.230609] hub 1-0:1.0: 1 port detected
[    1.231301] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.232014] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 2
[    1.233003] xhci-hcd xhci-hcd.0.auto: Host supports USB 3.0 SuperSpeed
[    1.233887] usb usb2: We don't know the algorithms for LPM for this host, disabling LPM.
[    1.234992] usb usb2: New USB device found, idVendor=1d6b, idProduct=0003, bcdDevice= 4.14
[    1.236055] usb usb2: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.236983] usb usb2: Product: xHCI Host Controller
[    1.237639] usb usb2: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.238346] usb usb2: SerialNumber: xhci-hcd.0.auto
[    1.239246] hub 2-0:1.0: USB hub found
[    1.239745] hub 2-0:1.0: 1 port detected
[    1.485221] usb 1-1: new high-speed USB device number 2 using xhci-hcd
[    1.637397] usb 1-1: New USB device found, idVendor=1a40, idProduct=0101, bcdDevice= 1.11
[    1.638449] usb 1-1: New USB device strings: Mfr=0, Product=1, SerialNumber=0
[    1.639366] usb 1-1: Product: USB 2.0 Hub
[    1.682055] hub 1-1:1.0: USB hub found
[    1.682572] hub 1-1:1.0: 4 ports detected
[    1.965213] mmc2: new UHS SDR104 SDHC card at address 0001
[    1.966227] mmcblk2: mmc2:0001 SD16G 29.8 GiB
[    1.967838]  mmcblk2: p1 p2
[    2.151109] SMP: stopping secondary CPUs
[    2.151616] psci: psci_sys_reset(reboot_mode=0)
NOTICE:  fast_boot:0

S
F
L
O
NOTICE:  efuse cpu_cfg = 0
W
NOTICE:  Booting Trusted Firmware
NOTICE:  BL1: v1.4(release):HR-ROM-Rel-v1.1-141-ga91d4dd-dirty
NOTICE:  BL1: Built : 11:24:44, Oct 23 2019
NOTICE:  boot src: 2
NOTICE:  GigaDev SPI NAND was found.
NOTICE:  Block size: 128 KiB, page size: 2048
NOTICE:  BL1: Booting BL2
Auth pass
NOTICE:  bl1_main exit
SPL normal reset flow
check_reset_state (2): wakeup address = 0x0, hw wakeup status = 0x3, wakeup src=0x100
patch for sys_pll 1200 with 100M eth
SFLOW_INIT
CHIP ID:PCB941/WAFER: W04/ X: X20/ Y: Y36
secondary_jump_to_spl: secure chip flow
X3 SPL : secondary core wake up and jump to spl done (cpu_core_cfg=0)
SFLOW_FIN_HW_A

U-Boot SPL 2018.09-g4ca851534c-dirty (May 11 2022 - 20:09:50 +0800)
SPACC Init - ID: (00000061)
SPL nand boot mode (from strap)
GigaDev SPI NAND was found.
Block size: 128 KiB, page size: 2048
ddr_type = 1 (LPDDR4)
hb_chip_package_type:3
load ddr header src_addr: 100000, load_addr: 802ca020, src_len: a00
find valid ddr image
ddr_hdr.ecc_gran: 0x0
ddr_hdr.ecc_map: 0x0
ddr_hdr.sbr_pattern0: 0x0
ddr_hdr.sbr_pattern1: 0x0
ddr_freq = 05
board id = 31540334
ddr datarate: 3200
### SAMSUNG DDR ###
no ddr pin set
detect part number: 108
detect ddr freq: c80
board id alternative:0x3
index is 12
index is 15
index is 19
hb_ddr_index: 19
ddr_type = 1, ddr_vendor=3, ddr_freq=3200
dram_pll_init
sscg disabled
control load ddrc src_addr: 15ae00, load_addr: 802caa20, src_len: 920
[DDR INFO]      ==ddr_release_info==
[DDR INFO]      VERSION:        develop
[DDR INFO]      BUILD:          2022-05-11-20:09
[DDR INFO]      GIT COMMIT:     4ca851534c1616ace920fdaa000c6fb717c1fb74
[DDR INFO]      GIT TIME:       Wed, 20 Apr 2022 18:28:49 +0800
[DDR INFO]      ==ddr_features==
[DDR INFO]      RDBI:           0
[DDR INFO]      WDBI:           1
[DDR INFO]      InlineECC:      0
[DDR INFO]      DM:             1
[DDR INFO]      DDC:            1
[DDR INFO]      SSCG:           0
[DDR INFO]      BOARD:          XS_ENABLE
[DDR INFO] ddr_controller_cfg done
load ddr phy src_addr: 15b800, load_addr: 802caa20, src_len: 420
ATxSlewRate     : 15f
ATxImpedance    : 7f
TxSlewRate      : 19f
TxOdtDrvStren   : 600
TxImpedanceCtrl : e3f
CalDrvStr0      : 11
VrefInGlobal    : 104
board_type = 4 (CUSTOMER_BOARD)
load dqmap src addr: 15d600, load_addr: 802caa20, src_len: 20
[DDR INFO] dwc_ddrphy_train start
magic = 544f4248
load imem1 src_addr: 11ce00, load_addr: 802caa20, src_len: 8000
load dmem1 src_addr: 15a000, load_addr: 802caa20, src_len: 684
executing 1D fw
load imem2 src_addr: 124e00, load_addr: 802caa20, src_len: 8000
load dmem2 src_addr: 15a800, load_addr: 802caa20, src_len: 564

*******************************************************
p_dmem_lpddr4_2d_16b->MR11_A0:54
p_dmem_lpddr4_2d_16b->MR14_A0:54
p_dmem_lpddr4_2d_16b->MR12_A0:51
p_dmem_lpddr4_2d_16b->MR22_A0:14

p_dmem_lpddr4_2d_16b->MR3_A0:b3
p_dmem_lpddr4_2d_16b->Reserved00:40
p_dmem_lpddr4_2d_16b->Reserved0E:4
p_dmem_lpddr4_2d_16b->Delay_Weight2D:20
p_dmem_lpddr4_2d_16b->Voltage_Weight2D:80
*******************************************************

executing 2D fw
load pie src_addr: 15be00, load_addr: 802caa20, src_len: 11f0
Set QoS.
get_ddr_mr_info:cs_num=1, mr5=0x1, mr8=0x10
no magic in efuse file,bypass efuse
total_sz = 4096
SPL_VERSION:7
uboot partition is uboot_A
load u-boot: src_addr=0x380000, dest_addr=0x4000000, len=2097152
load warm boot spl: addr=0x800, dest_addr=0x80000000, len=31232
load bl31: addr=0x300000, dest_addr=0x0, len=524288
SFLOW_AUTH_BL31
verify signature of header:  verify ok!
verify signature of image:  verify ok!
bypass bpu image
clear keybank!!!!
SFLOW_DBG_EN
Trying to boot from RAM
SPL: bl31 will jump to u-boot or other entry (0x4000000)
SFLOW_CLR_KEY
SFLOW_REG_LD
install_portal copy portal
install_portal call smc and jump to bl31 cold entry(0x0)
hb som type: 5
X3 PI reset VDD_SD done

U-Boot 2018.09-g40785bca (May 27 2022 - 16:30:48 +0800)

Model: Hobot XJ3 Soc Board
DRAM:  system DDR size: 0xffe00000
4 GiB
MMC:   dwmmc@A5010000: 0, dwmmc@A5011000: 1, dwmmc@A5012000: 2
Loading Environment from UBI... GigaDevice SPI NAND was found.
128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
*** Warning - bad CRC, using default environment

In:    serial@a5000000
Out:   serial@a5000000
Err:   serial@a5000000
Net:   x3 sdb reset eth phy done

Warning: ethernet@A5014000 (eth0) using random MAC address - ea:4d:a8:d5:cc:db
eth0: ethernet@A5014000
Disable cnn cores ..
dtb_name:hobot-x3-pi.dtb
base board type: X3 SDB
bootmode: NAND
board_id = 31540334
damaged volume, update marker is setdamaged volume, update marker is setdamaged volume, update marker is sethb_boot_args_cmd_set custom_bootargs 0 ubuntu_boot 0
Hit any key to stop autoboot:  0
enable watchdog success !
switch to partitions #0, OK
mmc2 is current device
Scanning mmc 2:2...
Found U-Boot script /boot/boot.scr
664 bytes read in 2 ms (324.2 KiB/s)
## Executing script at 03c10000
Boot script loaded from devtype:mmc devnum:2 devplist:2
bootargs = console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
Loading fdt file: /boot/hobot/hobot-x3-pi.dtb
69633 bytes read in 8 ms (8.3 MiB/s)
Loading kernel: /boot/Image
19163144 bytes read in 846 ms (21.6 MiB/s)
## Flattened Device Tree blob at 03c00000
   Booting using the fdt blob at 0x3c00000
   Loading Device Tree to 0000000003c00000, end 0000000003c1ffff ... OK
chip_id: ab36300
The address of the fdt is 0x3c00000
Changed status Done
Can't get fdt_addr !!!Orign(MAX) bpu model Reserve Mem Size to 64M!!

Starting kernel ...

[    0.000000] OF: reserved mem: OVERLAP DETECTED!
[    0.000000] image_r5_mem (0x0000000080000000--0x0000000080010000) overlaps with msg_r5_mem (0x000000008000f000--0x0000000080010000)
[    0.000000] Reserved memory: created CMA memory pool at 0x0000000004000000, size 672 MiB
[    0.000000] OF: reserved mem: initialized node ion_cma, compatible id shared-dma-pool
[    0.000000] cma: Reserved 16 MiB at 0x000000007f000000
[    0.000000] On node 0 totalpages: 1047808
[    0.000000]   DMA zone: 8180 pages used for memmap
[    0.000000]   DMA zone: 0 pages reserved
[    0.000000]   DMA zone: 523520 pages, LIFO batch:31
[    0.000000]   Normal zone: 8192 pages used for memmap
[    0.000000]   Normal zone: 524288 pages, LIFO batch:31
[    0.000000] psci: probing for conduit method from DT.
[    0.000000] psci: PSCIv1.1 detected in firmware.
[    0.000000] psci: Using standard PSCI v0.2 function IDs
[    0.000000] psci: MIGRATE_INFO_TYPE not supported.
[    0.000000] psci: SMC Calling Convention v1.1
[    0.000000] percpu: Embedded 25 pages/cpu @ffffffc17ff2a000 s65176 r8192 d29032 u102400
[    0.000000] pcpu-alloc: s65176 r8192 d29032 u102400 alloc=25*4096
[    0.000000] pcpu-alloc: [0] 0 [0] 1 [0] 2 [0] 3
[    0.000000] Detected VIPT I-cache on CPU0
[    0.000000] CPU features: enabling workaround for ARM erratum 845719
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 1031436
[    0.000000] Kernel command line: earlycon loglevel=8 kgdboc=ttyS0 video=hobot:x3sdb-hdmi  console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
[    0.000000] PID hash table entries: 4096 (order: 3, 32768 bytes)
[    0.000000] Dentry cache hash table entries: 524288 (order: 10, 4194304 bytes)
[    0.000000] Inode-cache hash table entries: 262144 (order: 9, 2097152 bytes)
[    0.000000] software IO TLB [mem 0x7afff000-0x7efff000] (64MB) mapped at [ffffffc07afff000-ffffffc07effefff]
[    0.000000] Memory: 3319580K/4191232K available (10494K kernel code, 1306K rwdata, 5756K rodata, 1088K init, 9553K bss, 167140K reserved, 704512K cma-reserved)
[    0.000000] Virtual kernel memory layout:
[    0.000000]     modules : 0xffffff8000000000 - 0xffffff8008000000   (   128 MB)
[    0.000000]     vmalloc : 0xffffff8008000000 - 0xffffffbebfff0000   (   250 GB)
[    0.000000]       .text : 0xffffff8008000000 - 0xffffff8008a40000   ( 10496 KB)
[    0.000000]     .rodata : 0xffffff8008a40000 - 0xffffff8008ff0000   (  5824 KB)
[    0.000000]       .init : 0xffffff8008ff0000 - 0xffffff8009100000   (  1088 KB)
[    0.000000]       .data : 0xffffff8009100000 - 0xffffff8009246808   (  1307 KB)
[    0.000000]        .bss : 0xffffff8009246808 - 0xffffff8009b9aed8   (  9554 KB)
[    0.000000]     fixed   : 0xffffffbefe7fd000 - 0xffffffbefec00000   (  4108 KB)
[    0.000000]     PCI I/O : 0xffffffbefee00000 - 0xffffffbeffe00000   (    16 MB)
[    0.000000]     vmemmap : 0xffffffbf00000000 - 0xffffffc000000000   (     4 GB maximum)
[    0.000000]               0xffffffbf00008000 - 0xffffffbf06000000   (    95 MB actual)
[    0.000000]     memory  : 0xffffffc000200000 - 0xffffffc180000000   (  6142 MB)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=4, Nodes=1
[    0.000000] ftrace: allocating 36277 entries in 142 pages
[    0.000000] Preemptible hierarchical RCU implementation.
[    0.000000]  Tasks RCU enabled.
[    0.000000] NR_IRQS: 64, nr_irqs: 64, preallocated irqs: 0
[    0.000000] parent_rate: 0,  dclk->rate:2666000000, pre_ddr_rate:0, res.a0:139716712
[    0.000000] arch_timer: cp15 timer(s) running at 24.00MHz (virt).
[    0.000000] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0x588fe9dc0, max_idle_ns: 440795202592 ns
[    0.000004] sched_clock: 56 bits at 24MHz, resolution 41ns, wraps every 4398046511097ns
[    0.001192] clocksource: hobot_clocksource: mask: 0xffffffffffffffff max_cycles: 0x1d854df40, max_idle_ns: 3526361616960 ns
[    0.002965] Console: colour dummy device 80x25
[    0.003537] Calibrating delay loop (skipped), value calculated using timer frequency.. 48.00 BogoMIPS (lpj=96000)
[    0.004842] pid_max: default: 32768 minimum: 301
[    0.005496] Security Framework initialized
[    0.006014] AppArmor: AppArmor disabled by boot time parameter
[    0.006857] Mount-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.007725] Mountpoint-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.023767] ASID allocator initialised with 65536 entries
[    0.031765] Hierarchical SRCU implementation.
[    0.063823] smp: Bringing up secondary CPUs ...
[    0.100030] Detected VIPT I-cache on CPU1
[    0.100064] CPU1: Booted secondary processor [410fd034]
[    0.136080] Detected VIPT I-cache on CPU2
[    0.136101] CPU2: Booted secondary processor [410fd034]
[    0.172140] Detected VIPT I-cache on CPU3
[    0.172160] CPU3: Booted secondary processor [410fd034]
[    0.172213] smp: Brought up 1 node, 4 CPUs
[    0.176276] SMP: Total of 4 processors activated.
[    0.176871] CPU features: detected feature: 32-bit EL0 Support
[    0.177689] CPU: All CPU(s) started at EL1
[    0.178217] alternatives: patching kernel code
[    0.179808] devtmpfs: initialized
[    0.188915] random: get_random_u32 called from bucket_table_alloc+0x108/0x270 with crng_init=0
[    0.190486] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 7645041785100000 ns
[    0.191732] futex hash table entries: 1024 (order: 5, 131072 bytes)
[    0.208269] xor: automatically using best checksumming function   32regs
[    0.209210] pinctrl core: initialized pinctrl subsystem
[    0.210444] NET: Registered protocol family 16
[    0.211764] vdso: 2 pages (1 code @ ffffff8008a46000, 1 data @ ffffff8009104000)
[    0.212709] hw-breakpoint: found 6 breakpoint and 4 watchpoint registers.
[    0.214301] DMA: preallocated 256 KiB pool for atomic allocations
[    0.219120] pstore: using zlib compression
[    0.219916] console [pstore-1] enabled
[    0.220516] pstore: Registered ramoops as persistent store backend
[    0.221301] ramoops: attached 0x40000@0x3fc0000, ecc: 0/0
[    0.226310] hobot_dma a1005000.dma: Hobot DMA Engine Driver Probed!!
[    0.239963] SCSI subsystem initialized
[    0.240752] media: Linux media interface: v0.10
[    0.241348] Linux video capture interface: v2.00
[    0.241981] pps_core: LinuxPPS API ver. 1 registered
[    0.242608] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.243784] PTP clock support registered
[    0.245010] ion_dummy: not reserve carveout memory, try to alloc from cma
[    0.381780] Advanced Linux Sound Architecture Driver Initialized.
[    0.382959] usbcore: registered new interface driver usbfs
[    0.383686] usbcore: registered new interface driver hub
[    0.384418] usbcore: registered new device driver usb
[    0.385387] clocksource: Switched to clocksource arch_sys_counter
[    0.433065] VFS: Disk quotas dquot_6.6.0
[    0.433639] VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
[    0.434585] FS-Cache: Loaded
[    0.435073] CacheFiles: Loaded
[    0.440457] NET: Registered protocol family 2
[    0.441375] TCP established hash table entries: 32768 (order: 6, 262144 bytes)
[    0.442524] TCP bind hash table entries: 32768 (order: 7, 524288 bytes)
[    0.443770] TCP: Hash tables configured (established 32768 bind 32768)
[    0.444685] UDP hash table entries: 2048 (order: 4, 65536 bytes)
[    0.445544] UDP-Lite hash table entries: 2048 (order: 4, 65536 bytes)
[    0.446551] NET: Registered protocol family 1
[    0.447382] RPC: Registered named UNIX socket transport module.
[    0.448133] RPC: Registered udp transport module.
[    0.448730] RPC: Registered tcp transport module.
[    0.449328] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.450836] hw perfevents: enabled with armv8_cortex_a53 PMU driver, 7 counters available
[    0.453064] audit: initializing netlink subsys (disabled)
[    0.453977] audit: type=2000 audit(0.452:1): state=initialized audit_enabled=0 res=1
[    0.454290] Initialise system trusted keyrings
[    0.454366] workingset: timestamp_bits=46 max_order=20 bucket_order=0
[    0.458101] zbud: loaded
[    0.459653] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.460515] exFAT: Version 1.2.9
[    0.460998] FS-Cache: Netfs 'nfs' registered for caching
[    0.462106] NFS: Registering the id_resolver key type
[    0.462759] Key type id_resolver registered
[    0.463286] Key type id_legacy registered
[    0.463801] nfs4filelayout_init: NFSv4 File Layout Driver Registering...
[    0.464655] Installing knfsd (copyright (C) 1996 okir@monad.swb.de).
[    0.468766] NET: Registered protocol family 38
[    0.469337] async_tx: api initialized (async)
[    0.469913] Key type asymmetric registered
[    0.470430] Asymmetric key parser 'x509' registered
[    0.471116] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 245)
[    0.472137] io scheduler noop registered
[    0.472799] io scheduler cfq registered (default)
[    0.473417] io scheduler mq-deadline registered
[    0.473989] io scheduler kyber registered
[    0.475187] pinctrl-single a6003170.pinctrl_voltag: 64 pins at pa ffffff8009c4d170 size 8
[    0.476518] pinctrl-single a6004000.pinctrl: 128 pins at pa ffffff8009c61000 size 512
[    0.477887] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: start probe
[    0.478778] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: probe ok
[    0.479646] gpio-x3 a6003000.gpio: x3 gpio probe start!!!
[    0.480335] gpio-x3 a6003000.gpio: x3 gpio add gpiochip start!!!
[    0.481257] gpio-x3 a6003000.gpio: diable all gpio irq
[    0.483527] gpio-x3 a6003000.gpio: irqbase:57
[    0.484078] gpio-x3 a6003000.gpio: x3 irq add start!!!
[    0.484735] irq: Cannot allocate irq_descs @ IRQ57, assuming pre-allocated
[    0.485779] gpio-x3 a6003000.gpio: x3 irq add ok!!!
[    0.486433] gpio-x3 a6003000.gpio: x3 irqchip ops add ok!!!
[    0.487138] gpio-x3 a6003000.gpio: x3 gpio probe ok!!!
[    0.488237] hobot-pwm: hobot-pwmchip0 registered
[    0.488989] hobot-pwm: hobot-pwmchip1 registered
[    0.490472] diag dev [ver:1.1] init done
[    0.491364] hobot_ddr_monitor: LPDDR4 detected
[    0.492122] hobot_ddr_monitor: ddr monitor init finished.
[    0.492511] [vcam] init start
[    0.493584] vcam probe start
[    0.494049] vcam probe end successful
[    0.494510] [vcam] init end
[    0.495443] a5000000.serial: ttyS0 at MMIO 0xa5000000 (irq = 10, base_baud = 12000000) is a hobot-uart
[    0.496665] console [ttyS0] enabled
[    0.496665] console [ttyS0] enabled
[    0.497583] bootconsole [hobot0] disabled
[    0.497583] bootconsole [hobot0] disabled
[    0.498922] hobot-uart a5001000.serial: Failed to create debugfs root directory
[    0.499926] a5001000.serial: ttyS1 at MMIO 0xa5001000 (irq = 11, base_baud = 12000000) is a hobot-uart
[    0.501369] hobot-uart a5003000.serial: Failed to create debugfs root directory
[    0.502499] a5003000.serial: ttyS3 at MMIO 0xa5003000 (irq = 12, base_baud = 12000000) is a hobot-uart
[    0.504031] KGDB: Registered I/O driver kgdboc
[    0.504873] cacheinfo: Unable to detect cache hierarchy for CPU 0
[    0.510311] brd: module loaded
[    0.514893] loop: module loaded
[    0.516408] spi-nand hr_nand.0: GigaDevice SPI NAND was found.
[    0.517168] spi-nand hr_nand.0: 128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
[    0.519770] hobot_spi a5006000.spi: ver: HOBOT-spi_V20.200330 master
[    0.520812] libphy: Fixed MDIO Bus: probed
[    0.521972] st_gmac a5014000.ethernet: found phy-handle subnode
[    0.522809] st_gmac a5014000.ethernet: xj3_mtl_setup, plat->rx-queues-to-use:4, and tx:4
[    0.523996] st_gmac a5014000.ethernet: xj3_probe_config_dt, clk_ptp_rate:250000000
[    0.524998] set mac address 00:11:22:f4:80:3c:
[    0.525001] (using random mac adress)
[    0.526122] (NULL device *): xj3_get_hw_features, tx_fifo_size:16384
[    0.526939] (NULL device *): xj3_get_hw_features, rx_fifo_size:16384
[    0.527756] st_gmac a5014000.ethernet: TSO supported
[    0.528396] st_gmac a5014000.ethernet: TSO feature enabled
[    0.529103] st_gmac a5014000.ethernet: Enable Rx Mitigation via HW Watchdog Timer
[    0.650191] libphy: hobot-mac-mdio: probed
[    0.651750] st_gmac a5014000.ethernet: hobot_eth_probe: probe sucessfully
[    0.652950] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_0v8 not found, using dummy regulator
[    0.654193] dwc3-of-simple b2000000.usb: usb regulator 0v8 enable succeed
[    0.655070] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_3v3 not found, using dummy regulator
[    0.656283] dwc3-of-simple b2000000.usb: usb regulator 3v3 enable succeed
[    0.657837] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    0.659493] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    0.660929] usbcore: registered new interface driver cdc_acm
[    0.661680] cdc_acm: USB Abstract Control Model driver for USB modems and ISDN adapters
[    0.662739] usbcore: registered new interface driver uas
[    0.663455] usbcore: registered new interface driver usb-storage
[    0.664282] usbcore: registered new interface driver usbserial
[    0.665054] usbcore: registered new interface driver usbserial_generic
[    0.665935] usbserial: USB Serial support registered for generic
[    0.666731] usbcore: registered new interface driver usb_serial_simple
[    0.667590] usbserial: USB Serial support registered for carelink
[    0.668391] usbserial: USB Serial support registered for zio
[    0.669136] usbserial: USB Serial support registered for funsoft
[    0.669937] usbserial: USB Serial support registered for flashloader
[    0.670774] usbserial: USB Serial support registered for google
[    0.671552] usbserial: USB Serial support registered for libtransistor
[    0.672408] usbserial: USB Serial support registered for vivopay
[    0.673198] usbserial: USB Serial support registered for moto_modem
[    0.674039] usbserial: USB Serial support registered for motorola_tetra
[    0.674907] usbserial: USB Serial support registered for novatel_gps
[    0.675743] usbserial: USB Serial support registered for hp4x
[    0.676500] usbserial: USB Serial support registered for suunto
[    0.677278] usbserial: USB Serial support registered for siemens_mpi
[    0.678139] usbcore: registered new interface driver rio500
[    0.678982] mousedev: PS/2 mouse device common for all mice
[    0.690039] hobot-rtc a6002000.rtc: rtc core: registered hobot-rtc as rtc0
[    0.691035] i2c /dev entries driver
[    0.691641] hobot-i2c a5009000.i2c: hobot i2c probe start
[    0.692406] hobot-i2c a5009000.i2c: round_rate:96000000
[    0.693083] hobot-i2c a5009000.i2c: I2C bus speed is 400000
[    0.693824] hobot-i2c a5009000.i2c: clkdiv = 0x1d
[    0.694431] hobot-i2c a5009000.i2c: i2c0 diag register....
[    0.695522] hobot-i2c a5009000.i2c: hobot_i2c_0 probe done
[    0.696327] hobot-i2c a500a000.i2c: hobot i2c probe start
[    0.697081] hobot-i2c a500a000.i2c: round_rate:96000000
[    0.697781] hobot-i2c a500a000.i2c: I2C bus speed is 400000
[    0.698499] hobot-i2c a500a000.i2c: clkdiv = 0x1d
[    0.699106] hobot-i2c a500a000.i2c: i2c1 diag register....
[    0.700116] hobot-i2c a500a000.i2c: hobot_i2c_1 probe done
[    0.701078] lirc_dev: IR Remote Control driver registered, major 239
[    0.701917] IR LIRC bridge handler initialized
[    0.702677] sif_mclk clock frequence is 544000000
[    0.703313] mipi_rx0_ipi clock frequence is 544000000
[    0.704002] mipi_rx1_ipi clock frequence is 544000000
[    0.704701] mipi_rx2_ipi clock frequence is 544000000
[    0.705425] mipi_rx3_ipi clock frequence is 544000000
[    0.706146] mipi_tx_ipi clock frequence is 544000000
[    0.706865] mipi_cfg_host clock frequence is 102000000
[    0.707618] pym_mclk clock frequence is 1188000000
[    0.708338] mipi_dev_ref clock frequence is 24000000
[    0.709091] mipi_host_ref clock frequence is 24000000
[    0.709886] sensor0_mclk clock frequence is 37125000
[    0.710663] sensor1_mclk clock frequence is 37125000
[    0.711451] sensor2_mclk clock frequence is 37125000
[    0.712254] sensor3_mclk clock frequence is 37125000
[    0.712893] [FRT:D] x3_ips_probe(0)
[    0.713914] hobot swinfo sel reg ro=0x1 boot dump
[    0.714824] pvt a1009000.pvt: SCRATCH test: 1234abcd, pvt is alive.
[    0.715748] pvt a1009000.pvt: VM Calibrated data detected
[    0.716929] hobot_wdt a1002000.watchdog: watchdog setting [pet:6s bark:11s bite:15s]
[    0.718279] hobot_wdt a1002000.watchdog: Hobot Watchdog Timer at ffffff8009db3000 with timeout 15s
[    0.719634] device-mapper: uevent: version 1.0.3
[    0.720395] device-mapper: ioctl: 4.37.0-ioctl (2017-09-20) initialised: dm-devel@redhat.com
[    0.721631] device-mapper: verity-avb: AVB error handler initialized with vbmeta device:
[    0.724067] Synopsys Designware Multimedia Card Interface Driver
[    0.725064] dwmmc_hobot a5010000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.725923] dwmmc_hobot a5010000.dwmmc: card-detect-delay not found.
[    0.726742] dwmmc_hobot a5010000.dwmmc: data-addr not found.
[    0.727788] mmc_host mmc0: card is non-removable.
[    0.770597] dwmmc_hobot a5011000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.773445] dwmmc_hobot a5011000.dwmmc: card-detect-delay not found.
[    0.774265] dwmmc_hobot a5011000.dwmmc: data-addr not found.
[    0.779037] dwmmc_hobot a5011000.dwmmc: mmc set to fixed voltage 1800
[    0.780101] mmc_host mmc1: card is non-removable.
[    0.877578] dwmmc_hobot a5012000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.878396] dwmmc_hobot a5012000.dwmmc: card-detect-delay not found.
[    0.879215] dwmmc_hobot a5012000.dwmmc: data-addr not found.
[    0.880196] dwmmc_hobot a5012000.dwmmc: Got CD GPIO
[    0.991736] mmc1: queuing unknown CIS tuple 0x80 (2 bytes)
[    0.993926] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.996111] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.999478] mmc1: queuing unknown CIS tuple 0x80 (7 bytes)
[    1.003433] mmc1: queuing unknown CIS tuple 0x81 (9 bytes)
[    1.053680] ledtrig-cpu: registered to indicate activity on CPUs
[    1.054528] hidraw: raw HID events driver (C) Jiri Kosina
[    1.055396] usbcore: registered new interface driver usbhid
[    1.056120] usbhid: USB HID core driver
[    1.056704] logger: created 256K log 'log_main'
[    1.057351] logger: created 256K log 'log_events'
[    1.058073] logger: created 256K log 'log_radio'
[    1.058729] logger: created 256K log 'log_system'
[    1.059777] set dmc devfreq governor to performance
[    1.060418] hobot_dmcfreq_target: dmcfreq->rate:2666000000, target_rate:2666000000
[    1.061424] buf:, powersave_rate:2666000000, dmcfreq->pre_state:0
[    1.068254] usbcore: registered new interface driver snd-usb-audio
[    1.069442] Netfilter messages via NETLINK v0.30.
[    1.070077] ip_set: protocol 6
[    1.070567] ipip: IPv4 and MPLS over IPv4 tunneling driver
[    1.071588] ip_tables: (C) 2000-2006 Netfilter Core Team
[    1.076653] arp_tables: arp_tables: (C) 2002 David S. Miller
[    1.077485] Initializing XFRM netlink socket
[    1.078358] NET: Registered protocol family 10
[    1.079557] Segment Routing with IPv6
[    1.080065] sit: IPv6, IPv4 and MPLS over IPv4 tunneling driver
[    1.081163] NET: Registered protocol family 17
[    1.081849] Key type dns_resolver registered
[    1.083483] Loading compiled-in X.509 certificates
[    1.086983] Loaded X.509 cert 'Build time autogenerated kernel key: 81cb0ef77db2fac76e9588c2120c82422367d268'
[    1.088317] zswap: loaded using pool lzo/zbud
[    1.099562] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    1.101233] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    1.102274] console [netcon0] enabled
[    1.102750] netconsole: network logging started
[    1.103530] hobot-rtc a6002000.rtc: setting system clock to 1970-01-01 00:00:00 UTC (0)
[    1.104721] vps mipi_dphy: probe with x3vio done
[    1.105461] hobot_wdt_test: wdt_test_init: wdt test init
[    1.108165] VCC_CNN0: disabling
[    1.108574] VCC_CNN1: disabling
[    1.109666] vps mipi_host0: ver 140* port0(0:0)
[    1.110584] vps mipi_host1: ver 140* port1(1:0)
[    1.111472] vps mipi_host2: ver 140* port2(0:1)
[    1.112261] vps mipi_host3: ver 140* port3(1:1)
[    1.113099] ALSA device list:
[    1.113511]   No soundcards found.
[    1.114150] md: Skipping autodetection of RAID arrays. (raid=autodetect will force)
[    1.115285] VFS: Cannot open root device "mmcblk2p2" or unknown-block(0,0): error -6
[    1.116278] Please append a correct "root=" boot option; here are the available partitions:
[    1.117352] 0100          102400 ram0
[    1.117354]  (driver?)
[    1.118189] 0101          102400 ram1
[    1.118192]  (driver?)
[    1.118981] 0102          102400 ram2
[    1.118983]  (driver?)
[    1.119771] 0103          102400 ram3
[    1.119772]  (driver?)
[    1.120560] 0104          102400 ram4
[    1.120562]  (driver?)
[    1.121350] 0105          102400 ram5
[    1.121352]  (driver?)
[    1.122182] 0106          102400 ram6
[    1.122184]  (driver?)
[    1.122972] 0107          102400 ram7
[    1.122974]  (driver?)
[    1.123762] 0108          102400 ram8
[    1.123764]  (driver?)
[    1.124552] 0109          102400 ram9
[    1.124553]  (driver?)
[    1.125341] 010a          102400 ram10
[    1.125343]  (driver?)
[    1.126170] 010b          102400 ram11
[    1.126172]  (driver?)
[    1.126972] 010c          102400 ram12
[    1.126974]  (driver?)
[    1.127773] 010d          102400 ram13
[    1.127775]  (driver?)
[    1.128574] 010e          102400 ram14
[    1.128576]  (driver?)
[    1.129375] 010f          102400 ram15
[    1.129392]  (driver?)
[    1.130195] 1f00          131072 mtdblock0
[    1.130197]  (driver?)
[    1.131040] hobot_fusa: set_fusa_error_pin:75 set error pin to 1
[    1.131811] hobot_fusa: fusa errpin not ready
[    1.131815] Kernel panic - not syncing: VFS: Unable to mount root fs on unknown-block(0,0)
[    1.133433] Kernel Offset: disabled
[    1.133884] CPU features: 0x0002004
[    1.134334] Memory Limit: none
[    1.138874] Rebooting in 1 seconds..
[    1.242596] mmc1: new HSSDIO card at address 0001
[    2.139386] SMP: stopping secondary CPUs
[    2.139893] psci: psci_sys_reset(reboot_mode=0)
NOTICE:  fast_boot:0

S
F
L
O
NOTICE:  efuse cpu_cfg = 0
W
NOTICE:  Booting Trusted Firmware
NOTICE:  BL1: v1.4(release):HR-ROM-Rel-v1.1-141-ga91d4dd-dirty
NOTICE:  BL1: Built : 11:24:44, Oct 23 2019
NOTICE:  boot src: 2
NOTICE:  GigaDev SPI NAND was found.
NOTICE:  Block size: 128 KiB, page size: 2048
NOTICE:  BL1: Booting BL2
Auth pass
NOTICE:  bl1_main exit
SPL normal reset flow
check_reset_state (2): wakeup address = 0x0, hw wakeup status = 0x3, wakeup src=0x100
patch for sys_pll 1200 with 100M eth
SFLOW_INIT
CHIP ID:PCB941/WAFER: W04/ X: X20/ Y: Y36
secondary_jump_to_spl: secure chip flow
X3 SPL : secondary core wake up and jump to spl done (cpu_core_cfg=0)
SFLOW_FIN_HW_A

U-Boot SPL 2018.09-g4ca851534c-dirty (May 11 2022 - 20:09:50 +0800)
SPACC Init - ID: (00000061)
SPL nand boot mode (from strap)
GigaDev SPI NAND was found.
Block size: 128 KiB, page size: 2048
ddr_type = 1 (LPDDR4)
hb_chip_package_type:3
load ddr header src_addr: 100000, load_addr: 802ca020, src_len: a00
find valid ddr image
ddr_hdr.ecc_gran: 0x0
ddr_hdr.ecc_map: 0x0
ddr_hdr.sbr_pattern0: 0x0
ddr_hdr.sbr_pattern1: 0x0
ddr_freq = 05
board id = 31540334
ddr datarate: 3200
### SAMSUNG DDR ###
no ddr pin set
detect part number: 108
detect ddr freq: c80
board id alternative:0x3
index is 12
index is 15
index is 19
hb_ddr_index: 19
ddr_type = 1, ddr_vendor=3, ddr_freq=3200
dram_pll_init
sscg disabled
control load ddrc src_addr: 15ae00, load_addr: 802caa20, src_len: 920
[DDR INFO]      ==ddr_release_info==
[DDR INFO]      VERSION:        develop
[DDR INFO]      BUILD:          2022-05-11-20:09
[DDR INFO]      GIT COMMIT:     4ca851534c1616ace920fdaa000c6fb717c1fb74
[DDR INFO]      GIT TIME:       Wed, 20 Apr 2022 18:28:49 +0800
[DDR INFO]      ==ddr_features==
[DDR INFO]      RDBI:           0
[DDR INFO]      WDBI:           1
[DDR INFO]      InlineECC:      0
[DDR INFO]      DM:             1
[DDR INFO]      DDC:            1
[DDR INFO]      SSCG:           0
[DDR INFO]      BOARD:          XS_ENABLE
[DDR INFO] ddr_controller_cfg done
load ddr phy src_addr: 15b800, load_addr: 802caa20, src_len: 420
ATxSlewRate     : 15f
ATxImpedance    : 7f
TxSlewRate      : 19f
TxOdtDrvStren   : 600
TxImpedanceCtrl : e3f
CalDrvStr0      : 11
VrefInGlobal    : 104
board_type = 4 (CUSTOMER_BOARD)
load dqmap src addr: 15d600, load_addr: 802caa20, src_len: 20
[DDR INFO] dwc_ddrphy_train start
magic = 544f4248
load imem1 src_addr: 11ce00, load_addr: 802caa20, src_len: 8000
load dmem1 src_addr: 15a000, load_addr: 802caa20, src_len: 684
executing 1D fw
load imem2 src_addr: 124e00, load_addr: 802caa20, src_len: 8000
load dmem2 src_addr: 15a800, load_addr: 802caa20, src_len: 564

*******************************************************
p_dmem_lpddr4_2d_16b->MR11_A0:54
p_dmem_lpddr4_2d_16b->MR14_A0:54
p_dmem_lpddr4_2d_16b->MR12_A0:51
p_dmem_lpddr4_2d_16b->MR22_A0:14

p_dmem_lpddr4_2d_16b->MR3_A0:b3
p_dmem_lpddr4_2d_16b->Reserved00:40
p_dmem_lpddr4_2d_16b->Reserved0E:4
p_dmem_lpddr4_2d_16b->Delay_Weight2D:20
p_dmem_lpddr4_2d_16b->Voltage_Weight2D:80
*******************************************************

executing 2D fw
load pie src_addr: 15be00, load_addr: 802caa20, src_len: 11f0
Set QoS.
get_ddr_mr_info:cs_num=1, mr5=0x1, mr8=0x10
no magic in efuse file,bypass efuse
total_sz = 4096
SPL_VERSION:7
uboot partition is uboot_A
load u-boot: src_addr=0x380000, dest_addr=0x4000000, len=2097152
load warm boot spl: addr=0x800, dest_addr=0x80000000, len=31232
load bl31: addr=0x300000, dest_addr=0x0, len=524288
SFLOW_AUTH_BL31
verify signature of header:  verify ok!
verify signature of image:  verify ok!
bypass bpu image
clear keybank!!!!
SFLOW_DBG_EN
Trying to boot from RAM
SPL: bl31 will jump to u-boot or other entry (0x4000000)
SFLOW_CLR_KEY
SFLOW_REG_LD
install_portal copy portal
install_portal call smc and jump to bl31 cold entry(0x0)
hb som type: 5
X3 PI reset VDD_SD done

U-Boot 2018.09-g40785bca (May 27 2022 - 16:30:48 +0800)

Model: Hobot XJ3 Soc Board
DRAM:  system DDR size: 0xffe00000
4 GiB
MMC:   dwmmc@A5010000: 0, dwmmc@A5011000: 1, dwmmc@A5012000: 2 (SD)
Loading Environment from UBI... GigaDevice SPI NAND was found.
128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
*** Warning - bad CRC, using default environment

In:    serial@a5000000
Out:   serial@a5000000
Err:   serial@a5000000
Net:   x3 sdb reset eth phy done

Warning: ethernet@A5014000 (eth0) using random MAC address - 36:e4:fa:1d:ce:03
eth0: ethernet@A5014000
Disable cnn cores ..
dtb_name:hobot-x3-pi.dtb
base board type: X3 SDB
bootmode: NAND
board_id = 31540334
damaged volume, update marker is setdamaged volume, update marker is setdamaged volume, update marker is sethb_boot_args_cmd_set custom_bootargs 0 ubuntu_boot 0
Hit any key to stop autoboot:  0
enable watchdog success !
switch to partitions #0, OK
mmc2 is current device
Scanning mmc 2:2...
Found U-Boot script /boot/boot.scr
664 bytes read in 2 ms (324.2 KiB/s)
## Executing script at 03c10000
Boot script loaded from devtype:mmc devnum:2 devplist:2
bootargs = console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
Loading fdt file: /boot/hobot/hobot-x3-pi.dtb
69633 bytes read in 8 ms (8.3 MiB/s)
Loading kernel: /boot/Image
19163144 bytes read in 845 ms (21.6 MiB/s)
## Flattened Device Tree blob at 03c00000
   Booting using the fdt blob at 0x3c00000
   Loading Device Tree to 0000000003c00000, end 0000000003c1ffff ... OK
chip_id: ab36300
The address of the fdt is 0x3c00000
Changed status Done
Can't get fdt_addr !!!Orign(MAX) bpu model Reserve Mem Size to 64M!!

Starting kernel ...

[    0.000000] OF: reserved mem: OVERLAP DETECTED!
[    0.000000] image_r5_mem (0x0000000080000000--0x0000000080010000) overlaps with msg_r5_mem (0x000000008000f000--0x0000000080010000)
[    0.000000] Reserved memory: created CMA memory pool at 0x0000000004000000, size 672 MiB
[    0.000000] OF: reserved mem: initialized node ion_cma, compatible id shared-dma-pool
[    0.000000] cma: Reserved 16 MiB at 0x000000007f000000
[    0.000000] On node 0 totalpages: 1047808
[    0.000000]   DMA zone: 8180 pages used for memmap
[    0.000000]   DMA zone: 0 pages reserved
[    0.000000]   DMA zone: 523520 pages, LIFO batch:31
[    0.000000]   Normal zone: 8192 pages used for memmap
[    0.000000]   Normal zone: 524288 pages, LIFO batch:31
[    0.000000] psci: probing for conduit method from DT.
[    0.000000] psci: PSCIv1.1 detected in firmware.
[    0.000000] psci: Using standard PSCI v0.2 function IDs
[    0.000000] psci: MIGRATE_INFO_TYPE not supported.
[    0.000000] psci: SMC Calling Convention v1.1
[    0.000000] percpu: Embedded 25 pages/cpu @ffffffc17ff2a000 s65176 r8192 d29032 u102400
[    0.000000] pcpu-alloc: s65176 r8192 d29032 u102400 alloc=25*4096
[    0.000000] pcpu-alloc: [0] 0 [0] 1 [0] 2 [0] 3
[    0.000000] Detected VIPT I-cache on CPU0
[    0.000000] CPU features: enabling workaround for ARM erratum 845719
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 1031436
[    0.000000] Kernel command line: earlycon loglevel=8 kgdboc=ttyS0 video=hobot:x3sdb-hdmi  console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
[    0.000000] PID hash table entries: 4096 (order: 3, 32768 bytes)
[    0.000000] Dentry cache hash table entries: 524288 (order: 10, 4194304 bytes)
[    0.000000] Inode-cache hash table entries: 262144 (order: 9, 2097152 bytes)
[    0.000000] software IO TLB [mem 0x7afff000-0x7efff000] (64MB) mapped at [ffffffc07afff000-ffffffc07effefff]
[    0.000000] Memory: 3319580K/4191232K available (10494K kernel code, 1306K rwdata, 5756K rodata, 1088K init, 9553K bss, 167140K reserved, 704512K cma-reserved)
[    0.000000] Virtual kernel memory layout:
[    0.000000]     modules : 0xffffff8000000000 - 0xffffff8008000000   (   128 MB)
[    0.000000]     vmalloc : 0xffffff8008000000 - 0xffffffbebfff0000   (   250 GB)
[    0.000000]       .text : 0xffffff8008000000 - 0xffffff8008a40000   ( 10496 KB)
[    0.000000]     .rodata : 0xffffff8008a40000 - 0xffffff8008ff0000   (  5824 KB)
[    0.000000]       .init : 0xffffff8008ff0000 - 0xffffff8009100000   (  1088 KB)
[    0.000000]       .data : 0xffffff8009100000 - 0xffffff8009246808   (  1307 KB)
[    0.000000]        .bss : 0xffffff8009246808 - 0xffffff8009b9aed8   (  9554 KB)
[    0.000000]     fixed   : 0xffffffbefe7fd000 - 0xffffffbefec00000   (  4108 KB)
[    0.000000]     PCI I/O : 0xffffffbefee00000 - 0xffffffbeffe00000   (    16 MB)
[    0.000000]     vmemmap : 0xffffffbf00000000 - 0xffffffc000000000   (     4 GB maximum)
[    0.000000]               0xffffffbf00008000 - 0xffffffbf06000000   (    95 MB actual)
[    0.000000]     memory  : 0xffffffc000200000 - 0xffffffc180000000   (  6142 MB)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=4, Nodes=1
[    0.000000] ftrace: allocating 36277 entries in 142 pages
[    0.000000] Preemptible hierarchical RCU implementation.
[    0.000000]  Tasks RCU enabled.
[    0.000000] NR_IRQS: 64, nr_irqs: 64, preallocated irqs: 0
[    0.000000] parent_rate: 0,  dclk->rate:2666000000, pre_ddr_rate:0, res.a0:139716712
[    0.000000] arch_timer: cp15 timer(s) running at 24.00MHz (virt).
[    0.000000] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0x588fe9dc0, max_idle_ns: 440795202592 ns
[    0.000003] sched_clock: 56 bits at 24MHz, resolution 41ns, wraps every 4398046511097ns
[    0.001192] clocksource: hobot_clocksource: mask: 0xffffffffffffffff max_cycles: 0x1d854df40, max_idle_ns: 3526361616960 ns
[    0.002966] Console: colour dummy device 80x25
[    0.003538] Calibrating delay loop (skipped), value calculated using timer frequency.. 48.00 BogoMIPS (lpj=96000)
[    0.004843] pid_max: default: 32768 minimum: 301
[    0.005498] Security Framework initialized
[    0.006016] AppArmor: AppArmor disabled by boot time parameter
[    0.006860] Mount-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.007728] Mountpoint-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.023770] ASID allocator initialised with 65536 entries
[    0.031768] Hierarchical SRCU implementation.
[    0.063827] smp: Bringing up secondary CPUs ...
[    0.100034] Detected VIPT I-cache on CPU1
[    0.100069] CPU1: Booted secondary processor [410fd034]
[    0.136083] Detected VIPT I-cache on CPU2
[    0.136104] CPU2: Booted secondary processor [410fd034]
[    0.172143] Detected VIPT I-cache on CPU3
[    0.172163] CPU3: Booted secondary processor [410fd034]
[    0.172216] smp: Brought up 1 node, 4 CPUs
[    0.176279] SMP: Total of 4 processors activated.
[    0.176874] CPU features: detected feature: 32-bit EL0 Support
[    0.177692] CPU: All CPU(s) started at EL1
[    0.178220] alternatives: patching kernel code
[    0.179807] devtmpfs: initialized
[    0.188908] random: get_random_u32 called from bucket_table_alloc+0x108/0x270 with crng_init=0
[    0.190479] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 7645041785100000 ns
[    0.191725] futex hash table entries: 1024 (order: 5, 131072 bytes)
[    0.208255] xor: automatically using best checksumming function   32regs
[    0.209192] pinctrl core: initialized pinctrl subsystem
[    0.210429] NET: Registered protocol family 16
[    0.211746] vdso: 2 pages (1 code @ ffffff8008a46000, 1 data @ ffffff8009104000)
[    0.212691] hw-breakpoint: found 6 breakpoint and 4 watchpoint registers.
[    0.214282] DMA: preallocated 256 KiB pool for atomic allocations
[    0.218927] pstore: using zlib compression
[    0.219722] console [pstore-1] enabled
[    0.220306] pstore: Registered ramoops as persistent store backend
[    0.221090] ramoops: attached 0x40000@0x3fc0000, ecc: 0/0
[    0.226092] hobot_dma a1005000.dma: Hobot DMA Engine Driver Probed!!
[    0.239806] SCSI subsystem initialized
[    0.240458] media: Linux media interface: v0.10
[    0.241054] Linux video capture interface: v2.00
[    0.241692] pps_core: LinuxPPS API ver. 1 registered
[    0.242319] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.243495] PTP clock support registered
[    0.244800] ion_dummy: not reserve carveout memory, try to alloc from cma
[    0.381300] Advanced Linux Sound Architecture Driver Initialized.
[    0.382463] usbcore: registered new interface driver usbfs
[    0.383194] usbcore: registered new interface driver hub
[    0.383921] usbcore: registered new device driver usb
[    0.384884] clocksource: Switched to clocksource arch_sys_counter
[    0.432546] VFS: Disk quotas dquot_6.6.0
[    0.433119] VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
[    0.434060] FS-Cache: Loaded
[    0.434544] CacheFiles: Loaded
[    0.439861] NET: Registered protocol family 2
[    0.440791] TCP established hash table entries: 32768 (order: 6, 262144 bytes)
[    0.441938] TCP bind hash table entries: 32768 (order: 7, 524288 bytes)
[    0.443186] TCP: Hash tables configured (established 32768 bind 32768)
[    0.444097] UDP hash table entries: 2048 (order: 4, 65536 bytes)
[    0.444955] UDP-Lite hash table entries: 2048 (order: 4, 65536 bytes)
[    0.445963] NET: Registered protocol family 1
[    0.446784] RPC: Registered named UNIX socket transport module.
[    0.447534] RPC: Registered udp transport module.
[    0.448131] RPC: Registered tcp transport module.
[    0.448730] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.450256] hw perfevents: enabled with armv8_cortex_a53 PMU driver, 7 counters available
[    0.452464] audit: initializing netlink subsys (disabled)
[    0.453380] audit: type=2000 audit(0.452:1): state=initialized audit_enabled=0 res=1
[    0.453653] Initialise system trusted keyrings
[    0.453725] workingset: timestamp_bits=46 max_order=20 bucket_order=0
[    0.457357] zbud: loaded
[    0.458921] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.459781] exFAT: Version 1.2.9
[    0.460263] FS-Cache: Netfs 'nfs' registered for caching
[    0.461419] NFS: Registering the id_resolver key type
[    0.462071] Key type id_resolver registered
[    0.462599] Key type id_legacy registered
[    0.463116] nfs4filelayout_init: NFSv4 File Layout Driver Registering...
[    0.463970] Installing knfsd (copyright (C) 1996 okir@monad.swb.de).
[    0.468071] NET: Registered protocol family 38
[    0.468642] async_tx: api initialized (async)
[    0.469224] Key type asymmetric registered
[    0.469742] Asymmetric key parser 'x509' registered
[    0.470425] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 245)
[    0.471442] io scheduler noop registered
[    0.472101] io scheduler cfq registered (default)
[    0.472696] io scheduler mq-deadline registered
[    0.473433] io scheduler kyber registered
[    0.474621] pinctrl-single a6003170.pinctrl_voltag: 64 pins at pa ffffff8009c4d170 size 8
[    0.475954] pinctrl-single a6004000.pinctrl: 128 pins at pa ffffff8009c61000 size 512
[    0.477202] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: start probe
[    0.478095] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: probe ok
[    0.478971] gpio-x3 a6003000.gpio: x3 gpio probe start!!!
[    0.479661] gpio-x3 a6003000.gpio: x3 gpio add gpiochip start!!!
[    0.480583] gpio-x3 a6003000.gpio: diable all gpio irq
[    0.482848] gpio-x3 a6003000.gpio: irqbase:57
[    0.483400] gpio-x3 a6003000.gpio: x3 irq add start!!!
[    0.484057] irq: Cannot allocate irq_descs @ IRQ57, assuming pre-allocated
[    0.485251] gpio-x3 a6003000.gpio: x3 irq add ok!!!
[    0.485906] gpio-x3 a6003000.gpio: x3 irqchip ops add ok!!!
[    0.486612] gpio-x3 a6003000.gpio: x3 gpio probe ok!!!
[    0.487696] hobot-pwm: hobot-pwmchip0 registered
[    0.488448] hobot-pwm: hobot-pwmchip1 registered
[    0.489794] diag dev [ver:1.1] init done
[    0.490692] hobot_ddr_monitor: LPDDR4 detected
[    0.491453] hobot_ddr_monitor: ddr monitor init finished.
[    0.491846] [vcam] init start
[    0.492943] vcam probe start
[    0.493403] vcam probe end successful
[    0.493864] [vcam] init end
[    0.494780] a5000000.serial: ttyS0 at MMIO 0xa5000000 (irq = 10, base_baud = 12000000) is a hobot-uart
[    0.495993] console [ttyS0] enabled
[    0.495993] console [ttyS0] enabled
[    0.496978] bootconsole [hobot0] disabled
[    0.496978] bootconsole [hobot0] disabled
[    0.498306] hobot-uart a5001000.serial: Failed to create debugfs root directory
[    0.499308] a5001000.serial: ttyS1 at MMIO 0xa5001000 (irq = 11, base_baud = 12000000) is a hobot-uart
[    0.500741] hobot-uart a5003000.serial: Failed to create debugfs root directory
[    0.501759] a5003000.serial: ttyS3 at MMIO 0xa5003000 (irq = 12, base_baud = 12000000) is a hobot-uart
[    0.503292] KGDB: Registered I/O driver kgdboc
[    0.504127] cacheinfo: Unable to detect cache hierarchy for CPU 0
[    0.509584] brd: module loaded
[    0.514110] loop: module loaded
[    0.515660] spi-nand hr_nand.0: GigaDevice SPI NAND was found.
[    0.516420] spi-nand hr_nand.0: 128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
[    0.519089] hobot_spi a5006000.spi: ver: HOBOT-spi_V20.200330 master
[    0.520133] libphy: Fixed MDIO Bus: probed
[    0.521504] st_gmac a5014000.ethernet: found phy-handle subnode
[    0.522340] st_gmac a5014000.ethernet: xj3_mtl_setup, plat->rx-queues-to-use:4, and tx:4
[    0.523527] st_gmac a5014000.ethernet: xj3_probe_config_dt, clk_ptp_rate:250000000
[    0.524530] set mac address 00:11:22:84:e2:b6:
[    0.524533] (using random mac adress)
[    0.525720] (NULL device *): xj3_get_hw_features, tx_fifo_size:16384
[    0.526537] (NULL device *): xj3_get_hw_features, rx_fifo_size:16384
[    0.527355] st_gmac a5014000.ethernet: TSO supported
[    0.527995] st_gmac a5014000.ethernet: TSO feature enabled
[    0.528702] st_gmac a5014000.ethernet: Enable Rx Mitigation via HW Watchdog Timer
[    0.649777] libphy: hobot-mac-mdio: probed
[    0.651323] st_gmac a5014000.ethernet: hobot_eth_probe: probe sucessfully
[    0.652520] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_0v8 not found, using dummy regulator
[    0.653762] dwc3-of-simple b2000000.usb: usb regulator 0v8 enable succeed
[    0.654639] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_3v3 not found, using dummy regulator
[    0.655843] dwc3-of-simple b2000000.usb: usb regulator 3v3 enable succeed
[    0.657381] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    0.659037] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    0.660484] usbcore: registered new interface driver cdc_acm
[    0.661233] cdc_acm: USB Abstract Control Model driver for USB modems and ISDN adapters
[    0.662291] usbcore: registered new interface driver uas
[    0.663008] usbcore: registered new interface driver usb-storage
[    0.663835] usbcore: registered new interface driver usbserial
[    0.664606] usbcore: registered new interface driver usbserial_generic
[    0.665483] usbserial: USB Serial support registered for generic
[    0.666285] usbcore: registered new interface driver usb_serial_simple
[    0.667144] usbserial: USB Serial support registered for carelink
[    0.667945] usbserial: USB Serial support registered for zio
[    0.668691] usbserial: USB Serial support registered for funsoft
[    0.669499] usbserial: USB Serial support registered for flashloader
[    0.670334] usbserial: USB Serial support registered for google
[    0.671115] usbserial: USB Serial support registered for libtransistor
[    0.671971] usbserial: USB Serial support registered for vivopay
[    0.672761] usbserial: USB Serial support registered for moto_modem
[    0.673601] usbserial: USB Serial support registered for motorola_tetra
[    0.674469] usbserial: USB Serial support registered for novatel_gps
[    0.675303] usbserial: USB Serial support registered for hp4x
[    0.676062] usbserial: USB Serial support registered for suunto
[    0.676840] usbserial: USB Serial support registered for siemens_mpi
[    0.677694] usbcore: registered new interface driver rio500
[    0.678524] mousedev: PS/2 mouse device common for all mice
[    0.689577] hobot-rtc a6002000.rtc: rtc core: registered hobot-rtc as rtc0
[    0.690572] i2c /dev entries driver
[    0.691179] hobot-i2c a5009000.i2c: hobot i2c probe start
[    0.691942] hobot-i2c a5009000.i2c: round_rate:96000000
[    0.692620] hobot-i2c a5009000.i2c: I2C bus speed is 400000
[    0.693361] hobot-i2c a5009000.i2c: clkdiv = 0x1d
[    0.693968] hobot-i2c a5009000.i2c: i2c0 diag register....
[    0.695057] hobot-i2c a5009000.i2c: hobot_i2c_0 probe done
[    0.695856] hobot-i2c a500a000.i2c: hobot i2c probe start
[    0.696614] hobot-i2c a500a000.i2c: round_rate:96000000
[    0.697314] hobot-i2c a500a000.i2c: I2C bus speed is 400000
[    0.698031] hobot-i2c a500a000.i2c: clkdiv = 0x1d
[    0.698638] hobot-i2c a500a000.i2c: i2c1 diag register....
[    0.699650] hobot-i2c a500a000.i2c: hobot_i2c_1 probe done
[    0.700605] lirc_dev: IR Remote Control driver registered, major 239
[    0.701444] IR LIRC bridge handler initialized
[    0.702207] sif_mclk clock frequence is 544000000
[    0.702843] mipi_rx0_ipi clock frequence is 544000000
[    0.703532] mipi_rx1_ipi clock frequence is 544000000
[    0.704231] mipi_rx2_ipi clock frequence is 544000000
[    0.704951] mipi_rx3_ipi clock frequence is 544000000
[    0.705670] mipi_tx_ipi clock frequence is 544000000
[    0.706390] mipi_cfg_host clock frequence is 102000000
[    0.707144] pym_mclk clock frequence is 1188000000
[    0.707863] mipi_dev_ref clock frequence is 24000000
[    0.708617] mipi_host_ref clock frequence is 24000000
[    0.709412] sensor0_mclk clock frequence is 37125000
[    0.710189] sensor1_mclk clock frequence is 37125000
[    0.710978] sensor2_mclk clock frequence is 37125000
[    0.711777] sensor3_mclk clock frequence is 37125000
[    0.712417] [FRT:D] x3_ips_probe(0)
[    0.713448] hobot swinfo sel reg ro=0x1 boot dump
[    0.714367] pvt a1009000.pvt: SCRATCH test: 1234abcd, pvt is alive.
[    0.715287] pvt a1009000.pvt: VM Calibrated data detected
[    0.716468] hobot_wdt a1002000.watchdog: watchdog setting [pet:6s bark:11s bite:15s]
[    0.717817] hobot_wdt a1002000.watchdog: Hobot Watchdog Timer at ffffff8009db3000 with timeout 15s
[    0.719175] device-mapper: uevent: version 1.0.3
[    0.719938] device-mapper: ioctl: 4.37.0-ioctl (2017-09-20) initialised: dm-devel@redhat.com
[    0.721113] device-mapper: verity-avb: AVB error handler initialized with vbmeta device:
[    0.723593] Synopsys Designware Multimedia Card Interface Driver
[    0.724592] dwmmc_hobot a5010000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.725447] dwmmc_hobot a5010000.dwmmc: card-detect-delay not found.
[    0.726266] dwmmc_hobot a5010000.dwmmc: data-addr not found.
[    0.727293] mmc_host mmc0: card is non-removable.
[    0.766099] dwmmc_hobot a5011000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.768936] dwmmc_hobot a5011000.dwmmc: card-detect-delay not found.
[    0.769755] dwmmc_hobot a5011000.dwmmc: data-addr not found.
[    0.774531] dwmmc_hobot a5011000.dwmmc: mmc set to fixed voltage 1800
[    0.775590] mmc_host mmc1: card is non-removable.
[    0.873079] dwmmc_hobot a5012000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.873903] dwmmc_hobot a5012000.dwmmc: card-detect-delay not found.
[    0.874733] dwmmc_hobot a5012000.dwmmc: data-addr not found.
[    0.875700] dwmmc_hobot a5012000.dwmmc: Got CD GPIO
[    0.986596] mmc1: queuing unknown CIS tuple 0x80 (2 bytes)
[    0.988784] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.990981] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.994360] mmc1: queuing unknown CIS tuple 0x80 (7 bytes)
[    0.998316] mmc1: queuing unknown CIS tuple 0x81 (9 bytes)
[    1.065203] ledtrig-cpu: registered to indicate activity on CPUs
[    1.066029] hidraw: raw HID events driver (C) Jiri Kosina
[    1.066860] usbcore: registered new interface driver usbhid
[    1.067577] usbhid: USB HID core driver
[    1.068170] logger: created 256K log 'log_main'
[    1.068815] logger: created 256K log 'log_events'
[    1.069499] logger: created 256K log 'log_radio'
[    1.070151] logger: created 256K log 'log_system'
[    1.071187] set dmc devfreq governor to performance
[    1.071820] hobot_dmcfreq_target: dmcfreq->rate:2666000000, target_rate:2666000000
[    1.072793] buf:, powersave_rate:2666000000, dmcfreq->pre_state:0
[    1.079625] usbcore: registered new interface driver snd-usb-audio
[    1.080769] Netfilter messages via NETLINK v0.30.
[    1.081418] ip_set: protocol 6
[    1.081901] ipip: IPv4 and MPLS over IPv4 tunneling driver
[    1.082895] ip_tables: (C) 2000-2006 Netfilter Core Team
[    1.083818] arp_tables: arp_tables: (C) 2002 David S. Miller
[    1.084606] Initializing XFRM netlink socket
[    1.085492] NET: Registered protocol family 10
[    1.086724] Segment Routing with IPv6
[    1.087231] sit: IPv6, IPv4 and MPLS over IPv4 tunneling driver
[    1.088325] NET: Registered protocol family 17
[    1.088969] Key type dns_resolver registered
[    1.090612] Loading compiled-in X.509 certificates
[    1.094109] Loaded X.509 cert 'Build time autogenerated kernel key: 81cb0ef77db2fac76e9588c2120c82422367d268'
[    1.095439] zswap: loaded using pool lzo/zbud
[    1.106705] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    1.108367] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    1.109379] console [netcon0] enabled
[    1.109854] netconsole: network logging started
[    1.110635] hobot-rtc a6002000.rtc: setting system clock to 1970-01-01 00:00:00 UTC (0)
[    1.111813] vps mipi_dphy: probe with x3vio done
[    1.112531] hobot_wdt_test: wdt_test_init: wdt test init
[    1.115278] VCC_CNN0: disabling
[    1.115688] VCC_CNN1: disabling
[    1.116640] vps mipi_host0: ver 140* port0(0:0)
[    1.117591] vps mipi_host1: ver 140* port1(1:0)
[    1.118482] vps mipi_host2: ver 140* port2(0:1)
[    1.119270] vps mipi_host3: ver 140* port3(1:1)
[    1.120112] ALSA device list:
[    1.120497]   No soundcards found.
[    1.121185] md: Skipping autodetection of RAID arrays. (raid=autodetect will force)
[    1.122320] VFS: Cannot open root device "mmcblk2p2" or unknown-block(0,0): error -6
[    1.123313] Please append a correct "root=" boot option; here are the available partitions:
[    1.124388] 0100          102400 ram0
[    1.124390]  (driver?)
[    1.125198] 0101          102400 ram1
[    1.125200]  (driver?)
[    1.125989] 0102          102400 ram2
[    1.125991]  (driver?)
[    1.126779] 0103          102400 ram3
[    1.126781]  (driver?)
[    1.127569] 0104          102400 ram4
[    1.127571]  (driver?)
[    1.128358] 0105          102400 ram5
[    1.128360]  (driver?)
[    1.129189] 0106          102400 ram6
[    1.129191]  (driver?)
[    1.129980] 0107          102400 ram7
[    1.129982]  (driver?)
[    1.130769] 0108          102400 ram8
[    1.130771]  (driver?)
[    1.131559] 0109          102400 ram9
[    1.131561]  (driver?)
[    1.132349] 010a          102400 ram10
[    1.132350]  (driver?)
[    1.133165] 010b          102400 ram11
[    1.133167]  (driver?)
[    1.133967] 010c          102400 ram12
[    1.133968]  (driver?)
[    1.134767] 010d          102400 ram13
[    1.134769]  (driver?)
[    1.135568] 010e          102400 ram14
[    1.135570]  (driver?)
[    1.136369] 010f          102400 ram15
[    1.136370]  (driver?)
[    1.137205] 1f00          131072 mtdblock0
[    1.137207]  (driver?)
[    1.138051] hobot_fusa: set_fusa_error_pin:75 set error pin to 1
[    1.138821] hobot_fusa: fusa errpin not ready
[    1.138825] Kernel panic - not syncing: VFS: Unable to mount root fs on unknown-block(0,0)
[    1.140444] Kernel Offset: disabled
[    1.140895] CPU features: 0x0002004
[    1.141344] Memory Limit: none
[    1.145909] Rebooting in 1 seconds..
[    1.217127] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.217849] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 1
[    1.219307] xhci-hcd xhci-hcd.0.auto: hcc params 0x0220fe6d hci version 0x110 quirks 0x0000000000010010
[    1.220543] xhci-hcd xhci-hcd.0.auto: irq 178, io mem 0xb2000000
[    1.221691] usb usb1: New USB device found, idVendor=1d6b, idProduct=0002, bcdDevice= 4.14
[    1.222766] usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.223705] usb usb1: Product: xHCI Host Controller
[    1.224340] usb usb1: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.225061] usb usb1: SerialNumber: xhci-hcd.0.auto
[    1.226276] hub 1-0:1.0: USB hub found
[    1.226804] hub 1-0:1.0: 1 port detected
[    1.227484] mmc1: new HSSDIO card at address 0001
[    1.227585] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.227594] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 2
[    1.227603] xhci-hcd xhci-hcd.0.auto: Host supports USB 3.0 SuperSpeed
[    1.227650] usb usb2: We don't know the algorithms for LPM for this host, disabling LPM.
[    1.227717] usb usb2: New USB device found, idVendor=1d6b, idProduct=0003, bcdDevice= 4.14
[    1.227721] usb usb2: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.227725] usb usb2: Product: xHCI Host Controller
[    1.227728] usb usb2: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.227732] usb usb2: SerialNumber: xhci-hcd.0.auto
[    1.228000] hub 2-0:1.0: USB hub found
[    1.228017] hub 2-0:1.0: 1 port detected
[    1.488891] usb 1-1: new high-speed USB device number 2 using xhci-hcd
[    1.649080] usb 1-1: New USB device found, idVendor=1a40, idProduct=0101, bcdDevice= 1.11
[    1.650140] usb 1-1: New USB device strings: Mfr=0, Product=1, SerialNumber=0
[    1.651057] usb 1-1: Product: USB 2.0 Hub
[    1.707813] hub 1-1:1.0: USB hub found
[    1.708332] hub 1-1:1.0: 4 ports detected
[    1.960893] mmc2: new UHS SDR104 SDHC card at address 0001
[    1.961903] mmcblk2: mmc2:0001 SD16G 29.8 GiB
[    1.963513]  mmcblk2: p1 p2
[    2.146421] SMP: stopping secondary CPUs
[    2.146929] psci: psci_sys_reset(reboot_mode=0)
NOTICE:  fast_boot:0

S
F
L
O
NOTICE:  efuse cpu_cfg = 0
W
NOTICE:  Booting Trusted Firmware
NOTICE:  BL1: v1.4(release):HR-ROM-Rel-v1.1-141-ga91d4dd-dirty
NOTICE:  BL1: Built : 11:24:44, Oct 23 2019
NOTICE:  boot src: 2
NOTICE:  GigaDev SPI NAND was found.
NOTICE:  Block size: 128 KiB, page size: 2048
NOTICE:  BL1: Booting BL2
Auth pass
NOTICE:  bl1_main exit
SPL normal reset flow
check_reset_state (2): wakeup address = 0x0, hw wakeup status = 0x3, wakeup src=0x100
patch for sys_pll 1200 with 100M eth
SFLOW_INIT
CHIP ID:PCB941/WAFER: W04/ X: X20/ Y: Y36
secondary_jump_to_spl: secure chip flow
X3 SPL : secondary core wake up and jump to spl done (cpu_core_cfg=0)
SFLOW_FIN_HW_A

U-Boot SPL 2018.09-g4ca851534c-dirty (May 11 2022 - 20:09:50 +0800)
SPACC Init - ID: (00000061)
SPL nand boot mode (from strap)
GigaDev SPI NAND was found.
Block size: 128 KiB, page size: 2048
ddr_type = 1 (LPDDR4)
hb_chip_package_type:3
load ddr header src_addr: 100000, load_addr: 802ca020, src_len: a00
find valid ddr image
ddr_hdr.ecc_gran: 0x0
ddr_hdr.ecc_map: 0x0
ddr_hdr.sbr_pattern0: 0x0
ddr_hdr.sbr_pattern1: 0x0
ddr_freq = 05
board id = 31540334
ddr datarate: 3200
### SAMSUNG DDR ###
no ddr pin set
detect part number: 108
detect ddr freq: c80
board id alternative:0x3
index is 12
index is 15
index is 19
hb_ddr_index: 19
ddr_type = 1, ddr_vendor=3, ddr_freq=3200
dram_pll_init
sscg disabled
control load ddrc src_addr: 15ae00, load_addr: 802caa20, src_len: 920
[DDR INFO]      ==ddr_release_info==
[DDR INFO]      VERSION:        develop
[DDR INFO]      BUILD:          2022-05-11-20:09
[DDR INFO]      GIT COMMIT:     4ca851534c1616ace920fdaa000c6fb717c1fb74
[DDR INFO]      GIT TIME:       Wed, 20 Apr 2022 18:28:49 +0800
[DDR INFO]      ==ddr_features==
[DDR INFO]      RDBI:           0
[DDR INFO]      WDBI:           1
[DDR INFO]      InlineECC:      0
[DDR INFO]      DM:             1
[DDR INFO]      DDC:            1
[DDR INFO]      SSCG:           0
[DDR INFO]      BOARD:          XS_ENABLE
[DDR INFO] ddr_controller_cfg done
load ddr phy src_addr: 15b800, load_addr: 802caa20, src_len: 420
ATxSlewRate     : 15f
ATxImpedance    : 7f
TxSlewRate      : 19f
TxOdtDrvStren   : 600
TxImpedanceCtrl : e3f
CalDrvStr0      : 11
VrefInGlobal    : 104
board_type = 4 (CUSTOMER_BOARD)
load dqmap src addr: 15d600, load_addr: 802caa20, src_len: 20
[DDR INFO] dwc_ddrphy_train start
magic = 544f4248
load imem1 src_addr: 11ce00, load_addr: 802caa20, src_len: 8000
load dmem1 src_addr: 15a000, load_addr: 802caa20, src_len: 684
executing 1D fw
load imem2 src_addr: 124e00, load_addr: 802caa20, src_len: 8000
load dmem2 src_addr: 15a800, load_addr: 802caa20, src_len: 564

*******************************************************
p_dmem_lpddr4_2d_16b->MR11_A0:54
p_dmem_lpddr4_2d_16b->MR14_A0:54
p_dmem_lpddr4_2d_16b->MR12_A0:51
p_dmem_lpddr4_2d_16b->MR22_A0:14

p_dmem_lpddr4_2d_16b->MR3_A0:b3
p_dmem_lpddr4_2d_16b->Reserved00:40
p_dmem_lpddr4_2d_16b->Reserved0E:4
p_dmem_lpddr4_2d_16b->Delay_Weight2D:20
p_dmem_lpddr4_2d_16b->Voltage_Weight2D:80
*******************************************************

executing 2D fw
load pie src_addr: 15be00, load_addr: 802caa20, src_len: 11f0
Set QoS.
get_ddr_mr_info:cs_num=1, mr5=0x1, mr8=0x10
no magic in efuse file,bypass efuse
total_sz = 4096
SPL_VERSION:7
uboot partition is uboot_A
load u-boot: src_addr=0x380000, dest_addr=0x4000000, len=2097152
load warm boot spl: addr=0x800, dest_addr=0x80000000, len=31232
load bl31: addr=0x300000, dest_addr=0x0, len=524288
SFLOW_AUTH_BL31
verify signature of header:  verify ok!
verify signature of image:  verify ok!
bypass bpu image
clear keybank!!!!
SFLOW_DBG_EN
Trying to boot from RAM
SPL: bl31 will jump to u-boot or other entry (0x4000000)
SFLOW_CLR_KEY
SFLOW_REG_LD
install_portal copy portal
install_portal call smc and jump to bl31 cold entry(0x0)
hb som type: 5
X3 PI reset VDD_SD done

U-Boot 2018.09-g40785bca (May 27 2022 - 16:30:48 +0800)

Model: Hobot XJ3 Soc Board
DRAM:  system DDR size: 0xffe00000
4 GiB
MMC:   dwmmc@A5010000: 0, dwmmc@A5011000: 1, dwmmc@A5012000: 2
Loading Environment from UBI... GigaDevice SPI NAND was found.
128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
*** Warning - bad CRC, using default environment

In:    serial@a5000000
Out:   serial@a5000000
Err:   serial@a5000000
Net:   x3 sdb reset eth phy done

Warning: ethernet@A5014000 (eth0) using random MAC address - 1e:c3:0b:22:eb:bb
eth0: ethernet@A5014000
Disable cnn cores ..
dtb_name:hobot-x3-pi.dtb
base board type: X3 SDB
bootmode: NAND
board_id = 31540334
damaged volume, update marker is setdamaged volume, update marker is setdamaged volume, update marker is sethb_boot_args_cmd_set custom_bootargs 0 ubuntu_boot 0
Hit any key to stop autoboot:  0
enable watchdog success !
switch to partitions #0, OK
mmc2 is current device
Scanning mmc 2:2...
Found U-Boot script /boot/boot.scr
664 bytes read in 2 ms (324.2 KiB/s)
## Executing script at 03c10000
Boot script loaded from devtype:mmc devnum:2 devplist:2
bootargs = console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
Loading fdt file: /boot/hobot/hobot-x3-pi.dtb
69633 bytes read in 7 ms (9.5 MiB/s)
Loading kernel: /boot/Image
19163144 bytes read in 846 ms (21.6 MiB/s)
## Flattened Device Tree blob at 03c00000
   Booting using the fdt blob at 0x3c00000
   Loading Device Tree to 0000000003c00000, end 0000000003c1ffff ... OK
chip_id: ab36300
The address of the fdt is 0x3c00000
Changed status Done
Can't get fdt_addr !!!Orign(MAX) bpu model Reserve Mem Size to 64M!!

Starting kernel ...

[    0.000000] OF: reserved mem: OVERLAP DETECTED!
[    0.000000] image_r5_mem (0x0000000080000000--0x0000000080010000) overlaps with msg_r5_mem (0x000000008000f000--0x0000000080010000)
[    0.000000] Reserved memory: created CMA memory pool at 0x0000000004000000, size 672 MiB
[    0.000000] OF: reserved mem: initialized node ion_cma, compatible id shared-dma-pool
[    0.000000] cma: Reserved 16 MiB at 0x000000007f000000
[    0.000000] On node 0 totalpages: 1047808
[    0.000000]   DMA zone: 8180 pages used for memmap
[    0.000000]   DMA zone: 0 pages reserved
[    0.000000]   DMA zone: 523520 pages, LIFO batch:31
[    0.000000]   Normal zone: 8192 pages used for memmap
[    0.000000]   Normal zone: 524288 pages, LIFO batch:31
[    0.000000] psci: probing for conduit method from DT.
[    0.000000] psci: PSCIv1.1 detected in firmware.
[    0.000000] psci: Using standard PSCI v0.2 function IDs
[    0.000000] psci: MIGRATE_INFO_TYPE not supported.
[    0.000000] psci: SMC Calling Convention v1.1
[    0.000000] percpu: Embedded 25 pages/cpu @ffffffc17ff2a000 s65176 r8192 d29032 u102400
[    0.000000] pcpu-alloc: s65176 r8192 d29032 u102400 alloc=25*4096
[    0.000000] pcpu-alloc: [0] 0 [0] 1 [0] 2 [0] 3
[    0.000000] Detected VIPT I-cache on CPU0
[    0.000000] CPU features: enabling workaround for ARM erratum 845719
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 1031436
[    0.000000] Kernel command line: earlycon loglevel=8 kgdboc=ttyS0 video=hobot:x3sdb-hdmi  console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
[    0.000000] PID hash table entries: 4096 (order: 3, 32768 bytes)
[    0.000000] Dentry cache hash table entries: 524288 (order: 10, 4194304 bytes)
[    0.000000] Inode-cache hash table entries: 262144 (order: 9, 2097152 bytes)
[    0.000000] software IO TLB [mem 0x7afff000-0x7efff000] (64MB) mapped at [ffffffc07afff000-ffffffc07effefff]
[    0.000000] Memory: 3319580K/4191232K available (10494K kernel code, 1306K rwdata, 5756K rodata, 1088K init, 9553K bss, 167140K reserved, 704512K cma-reserved)
[    0.000000] Virtual kernel memory layout:
[    0.000000]     modules : 0xffffff8000000000 - 0xffffff8008000000   (   128 MB)
[    0.000000]     vmalloc : 0xffffff8008000000 - 0xffffffbebfff0000   (   250 GB)
[    0.000000]       .text : 0xffffff8008000000 - 0xffffff8008a40000   ( 10496 KB)
[    0.000000]     .rodata : 0xffffff8008a40000 - 0xffffff8008ff0000   (  5824 KB)
[    0.000000]       .init : 0xffffff8008ff0000 - 0xffffff8009100000   (  1088 KB)
[    0.000000]       .data : 0xffffff8009100000 - 0xffffff8009246808   (  1307 KB)
[    0.000000]        .bss : 0xffffff8009246808 - 0xffffff8009b9aed8   (  9554 KB)
[    0.000000]     fixed   : 0xffffffbefe7fd000 - 0xffffffbefec00000   (  4108 KB)
[    0.000000]     PCI I/O : 0xffffffbefee00000 - 0xffffffbeffe00000   (    16 MB)
[    0.000000]     vmemmap : 0xffffffbf00000000 - 0xffffffc000000000   (     4 GB maximum)
[    0.000000]               0xffffffbf00008000 - 0xffffffbf06000000   (    95 MB actual)
[    0.000000]     memory  : 0xffffffc000200000 - 0xffffffc180000000   (  6142 MB)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=4, Nodes=1
[    0.000000] ftrace: allocating 36277 entries in 142 pages
[    0.000000] Preemptible hierarchical RCU implementation.
[    0.000000]  Tasks RCU enabled.
[    0.000000] NR_IRQS: 64, nr_irqs: 64, preallocated irqs: 0
[    0.000000] parent_rate: 0,  dclk->rate:2666000000, pre_ddr_rate:0, res.a0:139716712
[    0.000000] arch_timer: cp15 timer(s) running at 24.00MHz (virt).
[    0.000000] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0x588fe9dc0, max_idle_ns: 440795202592 ns
[    0.000004] sched_clock: 56 bits at 24MHz, resolution 41ns, wraps every 4398046511097ns
[    0.001194] clocksource: hobot_clocksource: mask: 0xffffffffffffffff max_cycles: 0x1d854df40, max_idle_ns: 3526361616960 ns
[    0.002966] Console: colour dummy device 80x25
[    0.003537] Calibrating delay loop (skipped), value calculated using timer frequency.. 48.00 BogoMIPS (lpj=96000)
[    0.004843] pid_max: default: 32768 minimum: 301
[    0.005498] Security Framework initialized
[    0.006016] AppArmor: AppArmor disabled by boot time parameter
[    0.006858] Mount-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.007726] Mountpoint-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.023767] ASID allocator initialised with 65536 entries
[    0.031765] Hierarchical SRCU implementation.
[    0.063824] smp: Bringing up secondary CPUs ...
[    0.100029] Detected VIPT I-cache on CPU1
[    0.100064] CPU1: Booted secondary processor [410fd034]
[    0.136081] Detected VIPT I-cache on CPU2
[    0.136101] CPU2: Booted secondary processor [410fd034]
[    0.172140] Detected VIPT I-cache on CPU3
[    0.172160] CPU3: Booted secondary processor [410fd034]
[    0.172214] smp: Brought up 1 node, 4 CPUs
[    0.176276] SMP: Total of 4 processors activated.
[    0.176871] CPU features: detected feature: 32-bit EL0 Support
[    0.177689] CPU: All CPU(s) started at EL1
[    0.178217] alternatives: patching kernel code
[    0.179809] devtmpfs: initialized
[    0.188909] random: get_random_u32 called from bucket_table_alloc+0x108/0x270 with crng_init=0
[    0.190482] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 7645041785100000 ns
[    0.191727] futex hash table entries: 1024 (order: 5, 131072 bytes)
[    0.208252] xor: automatically using best checksumming function   32regs
[    0.209190] pinctrl core: initialized pinctrl subsystem
[    0.210423] NET: Registered protocol family 16
[    0.211747] vdso: 2 pages (1 code @ ffffff8008a46000, 1 data @ ffffff8009104000)
[    0.212692] hw-breakpoint: found 6 breakpoint and 4 watchpoint registers.
[    0.214283] DMA: preallocated 256 KiB pool for atomic allocations
[    0.219105] pstore: using zlib compression
[    0.219903] console [pstore-1] enabled
[    0.220491] pstore: Registered ramoops as persistent store backend
[    0.221276] ramoops: attached 0x40000@0x3fc0000, ecc: 0/0
[    0.226274] hobot_dma a1005000.dma: Hobot DMA Engine Driver Probed!!
[    0.243895] SCSI subsystem initialized
[    0.244549] media: Linux media interface: v0.10
[    0.245146] Linux video capture interface: v2.00
[    0.245775] pps_core: LinuxPPS API ver. 1 registered
[    0.246402] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.247577] PTP clock support registered
[    0.248868] ion_dummy: not reserve carveout memory, try to alloc from cma
[    0.385397] Advanced Linux Sound Architecture Driver Initialized.
[    0.386560] usbcore: registered new interface driver usbfs
[    0.387287] usbcore: registered new interface driver hub
[    0.388016] usbcore: registered new device driver usb
[    0.389047] clocksource: Switched to clocksource arch_sys_counter
[    0.436754] VFS: Disk quotas dquot_6.6.0
[    0.437328] VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
[    0.438262] FS-Cache: Loaded
[    0.438744] CacheFiles: Loaded
[    0.444005] NET: Registered protocol family 2
[    0.444932] TCP established hash table entries: 32768 (order: 6, 262144 bytes)
[    0.446078] TCP bind hash table entries: 32768 (order: 7, 524288 bytes)
[    0.447328] TCP: Hash tables configured (established 32768 bind 32768)
[    0.448238] UDP hash table entries: 2048 (order: 4, 65536 bytes)
[    0.449097] UDP-Lite hash table entries: 2048 (order: 4, 65536 bytes)
[    0.450099] NET: Registered protocol family 1
[    0.450936] RPC: Registered named UNIX socket transport module.
[    0.451687] RPC: Registered udp transport module.
[    0.452284] RPC: Registered tcp transport module.
[    0.452883] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.454404] hw perfevents: enabled with armv8_cortex_a53 PMU driver, 7 counters available
[    0.456626] audit: initializing netlink subsys (disabled)
[    0.457434] audit: type=2000 audit(0.456:1): state=initialized audit_enabled=0 res=1
[    0.457701] Initialise system trusted keyrings
[    0.457778] workingset: timestamp_bits=46 max_order=20 bucket_order=0
[    0.461393] zbud: loaded
[    0.462953] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.463813] exFAT: Version 1.2.9
[    0.464294] FS-Cache: Netfs 'nfs' registered for caching
[    0.465425] NFS: Registering the id_resolver key type
[    0.466081] Key type id_resolver registered
[    0.466608] Key type id_legacy registered
[    0.467123] nfs4filelayout_init: NFSv4 File Layout Driver Registering...
[    0.467976] Installing knfsd (copyright (C) 1996 okir@monad.swb.de).
[    0.472058] NET: Registered protocol family 38
[    0.472630] async_tx: api initialized (async)
[    0.473198] Key type asymmetric registered
[    0.473715] Asymmetric key parser 'x509' registered
[    0.474400] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 245)
[    0.475417] io scheduler noop registered
[    0.476071] io scheduler cfq registered (default)
[    0.476667] io scheduler mq-deadline registered
[    0.477339] io scheduler kyber registered
[    0.478531] pinctrl-single a6003170.pinctrl_voltag: 64 pins at pa ffffff8009c4d170 size 8
[    0.479864] pinctrl-single a6004000.pinctrl: 128 pins at pa ffffff8009c61000 size 512
[    0.481122] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: start probe
[    0.482019] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: probe ok
[    0.482897] gpio-x3 a6003000.gpio: x3 gpio probe start!!!
[    0.483587] gpio-x3 a6003000.gpio: x3 gpio add gpiochip start!!!
[    0.484509] gpio-x3 a6003000.gpio: diable all gpio irq
[    0.486896] gpio-x3 a6003000.gpio: irqbase:57
[    0.487449] gpio-x3 a6003000.gpio: x3 irq add start!!!
[    0.488105] irq: Cannot allocate irq_descs @ IRQ57, assuming pre-allocated
[    0.489166] gpio-x3 a6003000.gpio: x3 irq add ok!!!
[    0.489822] gpio-x3 a6003000.gpio: x3 irqchip ops add ok!!!
[    0.490527] gpio-x3 a6003000.gpio: x3 gpio probe ok!!!
[    0.491642] hobot-pwm: hobot-pwmchip0 registered
[    0.492399] hobot-pwm: hobot-pwmchip1 registered
[    0.493764] diag dev [ver:1.1] init done
[    0.494665] hobot_ddr_monitor: LPDDR4 detected
[    0.495451] hobot_ddr_monitor: ddr monitor init finished.
[    0.495849] [vcam] init start
[    0.496908] vcam probe start
[    0.497393] vcam probe end successful
[    0.497855] [vcam] init end
[    0.498777] a5000000.serial: ttyS0 at MMIO 0xa5000000 (irq = 10, base_baud = 12000000) is a hobot-uart
[    0.499990] console [ttyS0] enabled
[    0.499990] console [ttyS0] enabled
[    0.500874] bootconsole [hobot0] disabled
[    0.500874] bootconsole [hobot0] disabled
[    0.502403] hobot-uart a5001000.serial: Failed to create debugfs root directory
[    0.503409] a5001000.serial: ttyS1 at MMIO 0xa5001000 (irq = 11, base_baud = 12000000) is a hobot-uart
[    0.504861] hobot-uart a5003000.serial: Failed to create debugfs root directory
[    0.505865] a5003000.serial: ttyS3 at MMIO 0xa5003000 (irq = 12, base_baud = 12000000) is a hobot-uart
[    0.507391] KGDB: Registered I/O driver kgdboc
[    0.508215] cacheinfo: Unable to detect cache hierarchy for CPU 0
[    0.513726] brd: module loaded
[    0.518256] loop: module loaded
[    0.519758] spi-nand hr_nand.0: GigaDevice SPI NAND was found.
[    0.520518] spi-nand hr_nand.0: 128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
[    0.523143] hobot_spi a5006000.spi: ver: HOBOT-spi_V20.200330 master
[    0.524188] libphy: Fixed MDIO Bus: probed
[    0.525507] st_gmac a5014000.ethernet: found phy-handle subnode
[    0.526342] st_gmac a5014000.ethernet: xj3_mtl_setup, plat->rx-queues-to-use:4, and tx:4
[    0.527525] st_gmac a5014000.ethernet: xj3_probe_config_dt, clk_ptp_rate:250000000
[    0.528530] set mac address 00:11:22:9e:5f:2e:
[    0.528532] (using random mac adress)
[    0.529684] (NULL device *): xj3_get_hw_features, tx_fifo_size:16384
[    0.530501] (NULL device *): xj3_get_hw_features, rx_fifo_size:16384
[    0.531318] st_gmac a5014000.ethernet: TSO supported
[    0.531959] st_gmac a5014000.ethernet: TSO feature enabled
[    0.532665] st_gmac a5014000.ethernet: Enable Rx Mitigation via HW Watchdog Timer
[    0.653749] libphy: hobot-mac-mdio: probed
[    0.655323] st_gmac a5014000.ethernet: hobot_eth_probe: probe sucessfully
[    0.656528] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_0v8 not found, using dummy regulator
[    0.657770] dwc3-of-simple b2000000.usb: usb regulator 0v8 enable succeed
[    0.658647] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_3v3 not found, using dummy regulator
[    0.659849] dwc3-of-simple b2000000.usb: usb regulator 3v3 enable succeed
[    0.661396] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    0.663053] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    0.664493] usbcore: registered new interface driver cdc_acm
[    0.665242] cdc_acm: USB Abstract Control Model driver for USB modems and ISDN adapters
[    0.666301] usbcore: registered new interface driver uas
[    0.667017] usbcore: registered new interface driver usb-storage
[    0.667845] usbcore: registered new interface driver usbserial
[    0.668617] usbcore: registered new interface driver usbserial_generic
[    0.669498] usbserial: USB Serial support registered for generic
[    0.670294] usbcore: registered new interface driver usb_serial_simple
[    0.671151] usbserial: USB Serial support registered for carelink
[    0.671952] usbserial: USB Serial support registered for zio
[    0.672700] usbserial: USB Serial support registered for funsoft
[    0.673508] usbserial: USB Serial support registered for flashloader
[    0.674345] usbserial: USB Serial support registered for google
[    0.675124] usbserial: USB Serial support registered for libtransistor
[    0.675980] usbserial: USB Serial support registered for vivopay
[    0.676770] usbserial: USB Serial support registered for moto_modem
[    0.677609] usbserial: USB Serial support registered for motorola_tetra
[    0.678478] usbserial: USB Serial support registered for novatel_gps
[    0.679315] usbserial: USB Serial support registered for hp4x
[    0.680071] usbserial: USB Serial support registered for suunto
[    0.680851] usbserial: USB Serial support registered for siemens_mpi
[    0.681706] usbcore: registered new interface driver rio500
[    0.682535] mousedev: PS/2 mouse device common for all mice
[    0.693580] hobot-rtc a6002000.rtc: rtc core: registered hobot-rtc as rtc0
[    0.694573] i2c /dev entries driver
[    0.695177] hobot-i2c a5009000.i2c: hobot i2c probe start
[    0.695944] hobot-i2c a5009000.i2c: round_rate:96000000
[    0.696621] hobot-i2c a5009000.i2c: I2C bus speed is 400000
[    0.697359] hobot-i2c a5009000.i2c: clkdiv = 0x1d
[    0.697966] hobot-i2c a5009000.i2c: i2c0 diag register....
[    0.699056] hobot-i2c a5009000.i2c: hobot_i2c_0 probe done
[    0.699858] hobot-i2c a500a000.i2c: hobot i2c probe start
[    0.700611] hobot-i2c a500a000.i2c: round_rate:96000000
[    0.701314] hobot-i2c a500a000.i2c: I2C bus speed is 400000
[    0.702032] hobot-i2c a500a000.i2c: clkdiv = 0x1d
[    0.702638] hobot-i2c a500a000.i2c: i2c1 diag register....
[    0.703651] hobot-i2c a500a000.i2c: hobot_i2c_1 probe done
[    0.704608] lirc_dev: IR Remote Control driver registered, major 239
[    0.705447] IR LIRC bridge handler initialized
[    0.706206] sif_mclk clock frequence is 544000000
[    0.706842] mipi_rx0_ipi clock frequence is 544000000
[    0.707531] mipi_rx1_ipi clock frequence is 544000000
[    0.708230] mipi_rx2_ipi clock frequence is 544000000
[    0.708939] mipi_rx3_ipi clock frequence is 544000000
[    0.709678] mipi_tx_ipi clock frequence is 544000000
[    0.710399] mipi_cfg_host clock frequence is 102000000
[    0.711152] pym_mclk clock frequence is 1188000000
[    0.711875] mipi_dev_ref clock frequence is 24000000
[    0.712628] mipi_host_ref clock frequence is 24000000
[    0.713421] sensor0_mclk clock frequence is 37125000
[    0.714199] sensor1_mclk clock frequence is 37125000
[    0.714987] sensor2_mclk clock frequence is 37125000
[    0.715788] sensor3_mclk clock frequence is 37125000
[    0.716427] [FRT:D] x3_ips_probe(0)
[    0.717454] hobot swinfo sel reg ro=0x1 boot dump
[    0.718366] pvt a1009000.pvt: SCRATCH test: 1234abcd, pvt is alive.
[    0.719291] pvt a1009000.pvt: VM Calibrated data detected
[    0.720470] hobot_wdt a1002000.watchdog: watchdog setting [pet:6s bark:11s bite:15s]
[    0.721810] hobot_wdt a1002000.watchdog: Hobot Watchdog Timer at ffffff8009db3000 with timeout 15s
[    0.723166] device-mapper: uevent: version 1.0.3
[    0.723932] device-mapper: ioctl: 4.37.0-ioctl (2017-09-20) initialised: dm-devel@redhat.com
[    0.725118] device-mapper: verity-avb: AVB error handler initialized with vbmeta device:
[    0.727595] Synopsys Designware Multimedia Card Interface Driver
[    0.728596] dwmmc_hobot a5010000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.729480] dwmmc_hobot a5010000.dwmmc: card-detect-delay not found.
[    0.730299] dwmmc_hobot a5010000.dwmmc: data-addr not found.
[    0.731350] mmc_host mmc0: card is non-removable.
[    0.770254] dwmmc_hobot a5011000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.773096] dwmmc_hobot a5011000.dwmmc: card-detect-delay not found.
[    0.773915] dwmmc_hobot a5011000.dwmmc: data-addr not found.
[    0.778687] dwmmc_hobot a5011000.dwmmc: mmc set to fixed voltage 1800
[    0.779751] mmc_host mmc1: card is non-removable.
[    0.877235] dwmmc_hobot a5012000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.878056] dwmmc_hobot a5012000.dwmmc: card-detect-delay not found.
[    0.878876] dwmmc_hobot a5012000.dwmmc: data-addr not found.
[    0.879858] dwmmc_hobot a5012000.dwmmc: Got CD GPIO
[    0.992446] mmc1: queuing unknown CIS tuple 0x80 (2 bytes)
[    0.994649] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.996844] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    1.000236] mmc1: queuing unknown CIS tuple 0x80 (7 bytes)
[    1.004216] mmc1: queuing unknown CIS tuple 0x81 (9 bytes)
[    1.053344] ledtrig-cpu: registered to indicate activity on CPUs
[    1.054181] hidraw: raw HID events driver (C) Jiri Kosina
[    1.055029] usbcore: registered new interface driver usbhid
[    1.055746] usbhid: USB HID core driver
[    1.056329] logger: created 256K log 'log_main'
[    1.056969] logger: created 256K log 'log_events'
[    1.057658] logger: created 256K log 'log_radio'
[    1.058306] logger: created 256K log 'log_system'
[    1.059326] set dmc devfreq governor to performance
[    1.059959] hobot_dmcfreq_target: dmcfreq->rate:2666000000, target_rate:2666000000
[    1.060932] buf:, powersave_rate:2666000000, dmcfreq->pre_state:0
[    1.067749] usbcore: registered new interface driver snd-usb-audio
[    1.068908] Netfilter messages via NETLINK v0.30.
[    1.069558] ip_set: protocol 6
[    1.070041] ipip: IPv4 and MPLS over IPv4 tunneling driver
[    1.071040] ip_tables: (C) 2000-2006 Netfilter Core Team
[    1.076094] arp_tables: arp_tables: (C) 2002 David S. Miller
[    1.076910] Initializing XFRM netlink socket
[    1.077794] NET: Registered protocol family 10
[    1.079004] Segment Routing with IPv6
[    1.079514] sit: IPv6, IPv4 and MPLS over IPv4 tunneling driver
[    1.080605] NET: Registered protocol family 17
[    1.081258] Key type dns_resolver registered
[    1.082926] Loading compiled-in X.509 certificates
[    1.086435] Loaded X.509 cert 'Build time autogenerated kernel key: 81cb0ef77db2fac76e9588c2120c82422367d268'
[    1.087767] zswap: loaded using pool lzo/zbud
[    1.099191] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    1.100853] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    1.101887] console [netcon0] enabled
[    1.102362] netconsole: network logging started
[    1.103142] hobot-rtc a6002000.rtc: setting system clock to 1970-01-01 00:00:00 UTC (0)
[    1.104329] vps mipi_dphy: probe with x3vio done
[    1.105034] hobot_wdt_test: wdt_test_init: wdt test init
[    1.107863] VCC_CNN0: disabling
[    1.108273] VCC_CNN1: disabling
[    1.109257] vps mipi_host0: ver 140* port0(0:0)
[    1.110168] vps mipi_host1: ver 140* port1(1:0)
[    1.111058] vps mipi_host2: ver 140* port2(0:1)
[    1.111857] vps mipi_host3: ver 140* port3(1:1)
[    1.112691] ALSA device list:
[    1.113112]   No soundcards found.
[    1.113751] md: Skipping autodetection of RAID arrays. (raid=autodetect will force)
[    1.114874] VFS: Cannot open root device "mmcblk2p2" or unknown-block(0,0): error -6
[    1.115868] Please append a correct "root=" boot option; here are the available partitions:
[    1.116942] 0100          102400 ram0
[    1.116944]  (driver?)
[    1.117754] 0101          102400 ram1
[    1.117756]  (driver?)
[    1.118545] 0102          102400 ram2
[    1.118547]  (driver?)
[    1.119335] 0103          102400 ram3
[    1.119337]  (driver?)
[    1.120125] 0104          102400 ram4
[    1.120126]  (driver?)
[    1.120914] 0105          102400 ram5
[    1.120916]  (driver?)
[    1.121774] 0106          102400 ram6
[    1.121776]  (driver?)
[    1.122565] 0107          102400 ram7
[    1.122567]  (driver?)
[    1.123355] 0108          102400 ram8
[    1.123357]  (driver?)
[    1.124145] 0109          102400 ram9
[    1.124146]  (driver?)
[    1.124934] 010a          102400 ram10
[    1.124936]  (driver?)
[    1.125751] 010b          102400 ram11
[    1.125753]  (driver?)
[    1.126553] 010c          102400 ram12
[    1.126555]  (driver?)
[    1.127354] 010d          102400 ram13
[    1.127356]  (driver?)
[    1.128154] 010e          102400 ram14
[    1.128156]  (driver?)
[    1.128955] 010f          102400 ram15
[    1.128957]  (driver?)
[    1.129777] 1f00          131072 mtdblock0
[    1.129780]  (driver?)
[    1.130623] hobot_fusa: set_fusa_error_pin:75 set error pin to 1
[    1.131394] hobot_fusa: fusa errpin not ready
[    1.131397] Kernel panic - not syncing: VFS: Unable to mount root fs on unknown-block(0,0)
[    1.133016] Kernel Offset: disabled
[    1.133467] CPU features: 0x0002004
[    1.133917] Memory Limit: none
[    1.138472] Rebooting in 1 seconds..
[    1.209296] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.210017] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 1
[    1.211474] xhci-hcd xhci-hcd.0.auto: hcc params 0x0220fe6d hci version 0x110 quirks 0x0000000000010010
[    1.212708] xhci-hcd xhci-hcd.0.auto: irq 178, io mem 0xb2000000
[    1.213684] usb usb1: New USB device found, idVendor=1d6b, idProduct=0002, bcdDevice= 4.14
[    1.214747] usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.215676] usb usb1: Product: xHCI Host Controller
[    1.216304] usb usb1: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.217010] usb usb1: SerialNumber: xhci-hcd.0.auto
[    1.217961] hub 1-0:1.0: USB hub found
[    1.218462] hub 1-0:1.0: 1 port detected
[    1.219150] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.219863] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 2
[    1.220852] xhci-hcd xhci-hcd.0.auto: Host supports USB 3.0 SuperSpeed
[    1.221745] usb usb2: We don't know the algorithms for LPM for this host, disabling LPM.
[    1.222852] usb usb2: New USB device found, idVendor=1d6b, idProduct=0003, bcdDevice= 4.14
[    1.223915] usb usb2: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.224843] usb usb2: Product: xHCI Host Controller
[    1.225480] usb usb2: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.226187] usb usb2: SerialNumber: xhci-hcd.0.auto
[    1.227079] hub 2-0:1.0: USB hub found
[    1.227580] hub 2-0:1.0: 1 port detected
[    1.238277] mmc1: new HSSDIO card at address 0001
[    1.473053] usb 1-1: new high-speed USB device number 2 using xhci-hcd
[    1.621242] usb 1-1: New USB device found, idVendor=1a40, idProduct=0101, bcdDevice= 1.11
[    1.622295] usb 1-1: New USB device strings: Mfr=0, Product=1, SerialNumber=0
[    1.623212] usb 1-1: Product: USB 2.0 Hub
[    1.669899] hub 1-1:1.0: USB hub found
[    1.670423] hub 1-1:1.0: 4 ports detected
[    2.138984] SMP: stopping secondary CPUs
[    2.139492] psci: psci_sys_reset(reboot_mode=0)
NOTICE:  fast_boot:0

S
F
L
O
NOTICE:  efuse cpu_cfg = 0
W
NOTICE:  Booting Trusted Firmware
NOTICE:  BL1: v1.4(release):HR-ROM-Rel-v1.1-141-ga91d4dd-dirty
NOTICE:  BL1: Built : 11:24:44, Oct 23 2019
NOTICE:  boot src: 2
NOTICE:  GigaDev SPI NAND was found.
NOTICE:  Block size: 128 KiB, page size: 2048
NOTICE:  BL1: Booting BL2
Auth pass
NOTICE:  bl1_main exit
SPL normal reset flow
check_reset_state (2): wakeup address = 0x0, hw wakeup status = 0x3, wakeup src=0x100
patch for sys_pll 1200 with 100M eth
SFLOW_INIT
CHIP ID:PCB941/WAFER: W04/ X: X20/ Y: Y36
secondary_jump_to_spl: secure chip flow
X3 SPL : secondary core wake up and jump to spl done (cpu_core_cfg=0)
SFLOW_FIN_HW_A

U-Boot SPL 2018.09-g4ca851534c-dirty (May 11 2022 - 20:09:50 +0800)
SPACC Init - ID: (00000061)
SPL nand boot mode (from strap)
GigaDev SPI NAND was found.
Block size: 128 KiB, page size: 2048
ddr_type = 1 (LPDDR4)
hb_chip_package_type:3
load ddr header src_addr: 100000, load_addr: 802ca020, src_len: a00
find valid ddr image
ddr_hdr.ecc_gran: 0x0
ddr_hdr.ecc_map: 0x0
ddr_hdr.sbr_pattern0: 0x0
ddr_hdr.sbr_pattern1: 0x0
ddr_freq = 05
board id = 31540334
ddr datarate: 3200
### SAMSUNG DDR ###
no ddr pin set
detect part number: 108
detect ddr freq: c80
board id alternative:0x3
index is 12
index is 15
index is 19
hb_ddr_index: 19
ddr_type = 1, ddr_vendor=3, ddr_freq=3200
dram_pll_init
sscg disabled
control load ddrc src_addr: 15ae00, load_addr: 802caa20, src_len: 920
[DDR INFO]      ==ddr_release_info==
[DDR INFO]      VERSION:        develop
[DDR INFO]      BUILD:          2022-05-11-20:09
[DDR INFO]      GIT COMMIT:     4ca851534c1616ace920fdaa000c6fb717c1fb74
[DDR INFO]      GIT TIME:       Wed, 20 Apr 2022 18:28:49 +0800
[DDR INFO]      ==ddr_features==
[DDR INFO]      RDBI:           0
[DDR INFO]      WDBI:           1
[DDR INFO]      InlineECC:      0
[DDR INFO]      DM:             1
[DDR INFO]      DDC:            1
[DDR INFO]      SSCG:           0
[DDR INFO]      BOARD:          XS_ENABLE
[DDR INFO] ddr_controller_cfg done
load ddr phy src_addr: 15b800, load_addr: 802caa20, src_len: 420
ATxSlewRate     : 15f
ATxImpedance    : 7f
TxSlewRate      : 19f
TxOdtDrvStren   : 600
TxImpedanceCtrl : e3f
CalDrvStr0      : 11
VrefInGlobal    : 104
board_type = 4 (CUSTOMER_BOARD)
load dqmap src addr: 15d600, load_addr: 802caa20, src_len: 20
[DDR INFO] dwc_ddrphy_train start
magic = 544f4248
load imem1 src_addr: 11ce00, load_addr: 802caa20, src_len: 8000
load dmem1 src_addr: 15a000, load_addr: 802caa20, src_len: 684
executing 1D fw
load imem2 src_addr: 124e00, load_addr: 802caa20, src_len: 8000
load dmem2 src_addr: 15a800, load_addr: 802caa20, src_len: 564

*******************************************************
p_dmem_lpddr4_2d_16b->MR11_A0:54
p_dmem_lpddr4_2d_16b->MR14_A0:54
p_dmem_lpddr4_2d_16b->MR12_A0:51
p_dmem_lpddr4_2d_16b->MR22_A0:14

p_dmem_lpddr4_2d_16b->MR3_A0:b3
p_dmem_lpddr4_2d_16b->Reserved00:40
p_dmem_lpddr4_2d_16b->Reserved0E:4
p_dmem_lpddr4_2d_16b->Delay_Weight2D:20
p_dmem_lpddr4_2d_16b->Voltage_Weight2D:80
*******************************************************

executing 2D fw
load pie src_addr: 15be00, load_addr: 802caa20, src_len: 11f0
Set QoS.
get_ddr_mr_info:cs_num=1, mr5=0x1, mr8=0x10
no magic in efuse file,bypass efuse
total_sz = 4096
SPL_VERSION:7
uboot partition is uboot_A
load u-boot: src_addr=0x380000, dest_addr=0x4000000, len=2097152
load warm boot spl: addr=0x800, dest_addr=0x80000000, len=31232
load bl31: addr=0x300000, dest_addr=0x0, len=524288
SFLOW_AUTH_BL31
verify signature of header:  verify ok!
verify signature of image:  verify ok!
bypass bpu image
clear keybank!!!!
SFLOW_DBG_EN
Trying to boot from RAM
SPL: bl31 will jump to u-boot or other entry (0x4000000)
SFLOW_CLR_KEY
SFLOW_REG_LD
install_portal copy portal
install_portal call smc and jump to bl31 cold entry(0x0)
hb som type: 5
X3 PI reset VDD_SD done

U-Boot 2018.09-g40785bca (May 27 2022 - 16:30:48 +0800)

Model: Hobot XJ3 Soc Board
DRAM:  system DDR size: 0xffe00000
4 GiB
MMC:   dwmmc@A5010000: 0, dwmmc@A5011000: 1, dwmmc@A5012000: 2 (SD)
Loading Environment from UBI... GigaDevice SPI NAND was found.
128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
*** Warning - bad CRC, using default environment

In:    serial@a5000000
Out:   serial@a5000000
Err:   serial@a5000000
Net:   x3 sdb reset eth phy done

Warning: ethernet@A5014000 (eth0) using random MAC address - 46:4c:2c:db:bf:aa
eth0: ethernet@A5014000
Disable cnn cores ..
dtb_name:hobot-x3-pi.dtb
base board type: X3 SDB
bootmode: NAND
board_id = 31540334
damaged volume, update marker is setdamaged volume, update marker is setdamaged volume, update marker is sethb_boot_args_cmd_set custom_bootargs 0 ubuntu_boot 0
Hit any key to stop autoboot:  0
enable watchdog success !
switch to partitions #0, OK
mmc2 is current device
Scanning mmc 2:2...
Found U-Boot script /boot/boot.scr
664 bytes read in 2 ms (324.2 KiB/s)
## Executing script at 03c10000
Boot script loaded from devtype:mmc devnum:2 devplist:2
bootargs = console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
Loading fdt file: /boot/hobot/hobot-x3-pi.dtb
69633 bytes read in 8 ms (8.3 MiB/s)
Loading kernel: /boot/Image
19163144 bytes read in 845 ms (21.6 MiB/s)
## Flattened Device Tree blob at 03c00000
   Booting using the fdt blob at 0x3c00000
   Loading Device Tree to 0000000003c00000, end 0000000003c1ffff ... OK
chip_id: ab36300
The address of the fdt is 0x3c00000
Changed status Done
Can't get fdt_addr !!!Orign(MAX) bpu model Reserve Mem Size to 64M!!

Starting kernel ...

[    0.000000] OF: reserved mem: OVERLAP DETECTED!
[    0.000000] image_r5_mem (0x0000000080000000--0x0000000080010000) overlaps with msg_r5_mem (0x000000008000f000--0x0000000080010000)
[    0.000000] Reserved memory: created CMA memory pool at 0x0000000004000000, size 672 MiB
[    0.000000] OF: reserved mem: initialized node ion_cma, compatible id shared-dma-pool
[    0.000000] cma: Reserved 16 MiB at 0x000000007f000000
[    0.000000] On node 0 totalpages: 1047808
[    0.000000]   DMA zone: 8180 pages used for memmap
[    0.000000]   DMA zone: 0 pages reserved
[    0.000000]   DMA zone: 523520 pages, LIFO batch:31
[    0.000000]   Normal zone: 8192 pages used for memmap
[    0.000000]   Normal zone: 524288 pages, LIFO batch:31
[    0.000000] psci: probing for conduit method from DT.
[    0.000000] psci: PSCIv1.1 detected in firmware.
[    0.000000] psci: Using standard PSCI v0.2 function IDs
[    0.000000] psci: MIGRATE_INFO_TYPE not supported.
[    0.000000] psci: SMC Calling Convention v1.1
[    0.000000] percpu: Embedded 25 pages/cpu @ffffffc17ff2a000 s65176 r8192 d29032 u102400
[    0.000000] pcpu-alloc: s65176 r8192 d29032 u102400 alloc=25*4096
[    0.000000] pcpu-alloc: [0] 0 [0] 1 [0] 2 [0] 3
[    0.000000] Detected VIPT I-cache on CPU0
[    0.000000] CPU features: enabling workaround for ARM erratum 845719
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 1031436
[    0.000000] Kernel command line: earlycon loglevel=8 kgdboc=ttyS0 video=hobot:x3sdb-hdmi  console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
[    0.000000] PID hash table entries: 4096 (order: 3, 32768 bytes)
[    0.000000] Dentry cache hash table entries: 524288 (order: 10, 4194304 bytes)
[    0.000000] Inode-cache hash table entries: 262144 (order: 9, 2097152 bytes)
[    0.000000] software IO TLB [mem 0x7afff000-0x7efff000] (64MB) mapped at [ffffffc07afff000-ffffffc07effefff]
[    0.000000] Memory: 3319580K/4191232K available (10494K kernel code, 1306K rwdata, 5756K rodata, 1088K init, 9553K bss, 167140K reserved, 704512K cma-reserved)
[    0.000000] Virtual kernel memory layout:
[    0.000000]     modules : 0xffffff8000000000 - 0xffffff8008000000   (   128 MB)
[    0.000000]     vmalloc : 0xffffff8008000000 - 0xffffffbebfff0000   (   250 GB)
[    0.000000]       .text : 0xffffff8008000000 - 0xffffff8008a40000   ( 10496 KB)
[    0.000000]     .rodata : 0xffffff8008a40000 - 0xffffff8008ff0000   (  5824 KB)
[    0.000000]       .init : 0xffffff8008ff0000 - 0xffffff8009100000   (  1088 KB)
[    0.000000]       .data : 0xffffff8009100000 - 0xffffff8009246808   (  1307 KB)
[    0.000000]        .bss : 0xffffff8009246808 - 0xffffff8009b9aed8   (  9554 KB)
[    0.000000]     fixed   : 0xffffffbefe7fd000 - 0xffffffbefec00000   (  4108 KB)
[    0.000000]     PCI I/O : 0xffffffbefee00000 - 0xffffffbeffe00000   (    16 MB)
[    0.000000]     vmemmap : 0xffffffbf00000000 - 0xffffffc000000000   (     4 GB maximum)
[    0.000000]               0xffffffbf00008000 - 0xffffffbf06000000   (    95 MB actual)
[    0.000000]     memory  : 0xffffffc000200000 - 0xffffffc180000000   (  6142 MB)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=4, Nodes=1
[    0.000000] ftrace: allocating 36277 entries in 142 pages
[    0.000000] Preemptible hierarchical RCU implementation.
[    0.000000]  Tasks RCU enabled.
[    0.000000] NR_IRQS: 64, nr_irqs: 64, preallocated irqs: 0
[    0.000000] parent_rate: 0,  dclk->rate:2666000000, pre_ddr_rate:0, res.a0:139716712
[    0.000000] arch_timer: cp15 timer(s) running at 24.00MHz (virt).
[    0.000000] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0x588fe9dc0, max_idle_ns: 440795202592 ns
[    0.000003] sched_clock: 56 bits at 24MHz, resolution 41ns, wraps every 4398046511097ns
[    0.001194] clocksource: hobot_clocksource: mask: 0xffffffffffffffff max_cycles: 0x1d854df40, max_idle_ns: 3526361616960 ns
[    0.002966] Console: colour dummy device 80x25
[    0.003537] Calibrating delay loop (skipped), value calculated using timer frequency.. 48.00 BogoMIPS (lpj=96000)
[    0.004844] pid_max: default: 32768 minimum: 301
[    0.005498] Security Framework initialized
[    0.006016] AppArmor: AppArmor disabled by boot time parameter
[    0.006860] Mount-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.007729] Mountpoint-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.023770] ASID allocator initialised with 65536 entries
[    0.031768] Hierarchical SRCU implementation.
[    0.063826] smp: Bringing up secondary CPUs ...
[    0.100033] Detected VIPT I-cache on CPU1
[    0.100068] CPU1: Booted secondary processor [410fd034]
[    0.136084] Detected VIPT I-cache on CPU2
[    0.136104] CPU2: Booted secondary processor [410fd034]
[    0.172143] Detected VIPT I-cache on CPU3
[    0.172162] CPU3: Booted secondary processor [410fd034]
[    0.172216] smp: Brought up 1 node, 4 CPUs
[    0.176279] SMP: Total of 4 processors activated.
[    0.176874] CPU features: detected feature: 32-bit EL0 Support
[    0.177692] CPU: All CPU(s) started at EL1
[    0.178220] alternatives: patching kernel code
[    0.179810] devtmpfs: initialized
[    0.188916] random: get_random_u32 called from bucket_table_alloc+0x108/0x270 with crng_init=0
[    0.190487] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 7645041785100000 ns
[    0.191733] futex hash table entries: 1024 (order: 5, 131072 bytes)
[    0.208212] xor: automatically using best checksumming function   32regs
[    0.209148] pinctrl core: initialized pinctrl subsystem
[    0.210389] NET: Registered protocol family 16
[    0.211712] vdso: 2 pages (1 code @ ffffff8008a46000, 1 data @ ffffff8009104000)
[    0.212658] hw-breakpoint: found 6 breakpoint and 4 watchpoint registers.
[    0.214250] DMA: preallocated 256 KiB pool for atomic allocations
[    0.218650] pstore: using zlib compression
[    0.219444] console [pstore-1] enabled
[    0.220029] pstore: Registered ramoops as persistent store backend
[    0.220813] ramoops: attached 0x40000@0x3fc0000, ecc: 0/0
[    0.225814] hobot_dma a1005000.dma: Hobot DMA Engine Driver Probed!!
[    0.239636] SCSI subsystem initialized
[    0.240269] media: Linux media interface: v0.10
[    0.241010] Linux video capture interface: v2.00
[    0.241652] pps_core: LinuxPPS API ver. 1 registered
[    0.242280] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.243455] PTP clock support registered
[    0.244591] ion_dummy: not reserve carveout memory, try to alloc from cma
[    0.381247] Advanced Linux Sound Architecture Driver Initialized.
[    0.382438] usbcore: registered new interface driver usbfs
[    0.383166] usbcore: registered new interface driver hub
[    0.383893] usbcore: registered new device driver usb
[    0.384841] clocksource: Switched to clocksource arch_sys_counter
[    0.432568] VFS: Disk quotas dquot_6.6.0
[    0.433142] VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
[    0.434079] FS-Cache: Loaded
[    0.434562] CacheFiles: Loaded
[    0.439841] NET: Registered protocol family 2
[    0.440772] TCP established hash table entries: 32768 (order: 6, 262144 bytes)
[    0.441904] TCP bind hash table entries: 32768 (order: 7, 524288 bytes)
[    0.443148] TCP: Hash tables configured (established 32768 bind 32768)
[    0.444056] UDP hash table entries: 2048 (order: 4, 65536 bytes)
[    0.444904] UDP-Lite hash table entries: 2048 (order: 4, 65536 bytes)
[    0.445905] NET: Registered protocol family 1
[    0.446750] RPC: Registered named UNIX socket transport module.
[    0.447501] RPC: Registered udp transport module.
[    0.448098] RPC: Registered tcp transport module.
[    0.448697] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.450223] hw perfevents: enabled with armv8_cortex_a53 PMU driver, 7 counters available
[    0.452434] audit: initializing netlink subsys (disabled)
[    0.453239] audit: type=2000 audit(0.452:1): state=initialized audit_enabled=0 res=1
[    0.453516] Initialise system trusted keyrings
[    0.453593] workingset: timestamp_bits=46 max_order=20 bucket_order=0
[    0.457209] zbud: loaded
[    0.458769] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.459629] exFAT: Version 1.2.9
[    0.460111] FS-Cache: Netfs 'nfs' registered for caching
[    0.461397] NFS: Registering the id_resolver key type
[    0.462052] Key type id_resolver registered
[    0.462579] Key type id_legacy registered
[    0.463094] nfs4filelayout_init: NFSv4 File Layout Driver Registering...
[    0.463947] Installing knfsd (copyright (C) 1996 okir@monad.swb.de).
[    0.468151] NET: Registered protocol family 38
[    0.468724] async_tx: api initialized (async)
[    0.469442] Key type asymmetric registered
[    0.469961] Asymmetric key parser 'x509' registered
[    0.470648] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 245)
[    0.471669] io scheduler noop registered
[    0.472326] io scheduler cfq registered (default)
[    0.472933] io scheduler mq-deadline registered
[    0.473505] io scheduler kyber registered
[    0.474693] pinctrl-single a6003170.pinctrl_voltag: 64 pins at pa ffffff8009c4d170 size 8
[    0.476026] pinctrl-single a6004000.pinctrl: 128 pins at pa ffffff8009c61000 size 512
[    0.477258] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: start probe
[    0.478152] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: probe ok
[    0.479022] gpio-x3 a6003000.gpio: x3 gpio probe start!!!
[    0.479711] gpio-x3 a6003000.gpio: x3 gpio add gpiochip start!!!
[    0.480632] gpio-x3 a6003000.gpio: diable all gpio irq
[    0.483020] gpio-x3 a6003000.gpio: irqbase:57
[    0.483572] gpio-x3 a6003000.gpio: x3 irq add start!!!
[    0.484230] irq: Cannot allocate irq_descs @ IRQ57, assuming pre-allocated
[    0.485288] gpio-x3 a6003000.gpio: x3 irq add ok!!!
[    0.485945] gpio-x3 a6003000.gpio: x3 irqchip ops add ok!!!
[    0.486650] gpio-x3 a6003000.gpio: x3 gpio probe ok!!!
[    0.487760] hobot-pwm: hobot-pwmchip0 registered
[    0.488513] hobot-pwm: hobot-pwmchip1 registered
[    0.489982] diag dev [ver:1.1] init done
[    0.490881] hobot_ddr_monitor: LPDDR4 detected
[    0.491640] hobot_ddr_monitor: ddr monitor init finished.
[    0.492024] [vcam] init start
[    0.493110] vcam probe start
[    0.493572] vcam probe end successful
[    0.494033] [vcam] init end
[    0.494956] a5000000.serial: ttyS0 at MMIO 0xa5000000 (irq = 10, base_baud = 12000000) is a hobot-uart
[    0.496168] console [ttyS0] enabled
[    0.496168] console [ttyS0] enabled
[    0.497083] bootconsole [hobot0] disabled
[    0.497083] bootconsole [hobot0] disabled
[    0.498409] hobot-uart a5001000.serial: Failed to create debugfs root directory
[    0.499410] a5001000.serial: ttyS1 at MMIO 0xa5001000 (irq = 11, base_baud = 12000000) is a hobot-uart
[    0.500876] hobot-uart a5003000.serial: Failed to create debugfs root directory
[    0.501874] a5003000.serial: ttyS3 at MMIO 0xa5003000 (irq = 12, base_baud = 12000000) is a hobot-uart
[    0.503405] KGDB: Registered I/O driver kgdboc
[    0.504236] cacheinfo: Unable to detect cache hierarchy for CPU 0
[    0.509690] brd: module loaded
[    0.514235] loop: module loaded
[    0.515735] spi-nand hr_nand.0: GigaDevice SPI NAND was found.
[    0.516494] spi-nand hr_nand.0: 128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
[    0.519109] hobot_spi a5006000.spi: ver: HOBOT-spi_V20.200330 master
[    0.520152] libphy: Fixed MDIO Bus: probed
[    0.521479] st_gmac a5014000.ethernet: found phy-handle subnode
[    0.522316] st_gmac a5014000.ethernet: xj3_mtl_setup, plat->rx-queues-to-use:4, and tx:4
[    0.523502] st_gmac a5014000.ethernet: xj3_probe_config_dt, clk_ptp_rate:250000000
[    0.524504] set mac address 00:11:22:00:98:5d:
[    0.524507] (using random mac adress)
[    0.525623] (NULL device *): xj3_get_hw_features, tx_fifo_size:16384
[    0.526441] (NULL device *): xj3_get_hw_features, rx_fifo_size:16384
[    0.527258] st_gmac a5014000.ethernet: TSO supported
[    0.527898] st_gmac a5014000.ethernet: TSO feature enabled
[    0.528605] st_gmac a5014000.ethernet: Enable Rx Mitigation via HW Watchdog Timer
[    0.649693] libphy: hobot-mac-mdio: probed
[    0.651255] st_gmac a5014000.ethernet: hobot_eth_probe: probe sucessfully
[    0.652455] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_0v8 not found, using dummy regulator
[    0.653700] dwc3-of-simple b2000000.usb: usb regulator 0v8 enable succeed
[    0.654577] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_3v3 not found, using dummy regulator
[    0.655790] dwc3-of-simple b2000000.usb: usb regulator 3v3 enable succeed
[    0.657341] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    0.658998] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    0.660438] usbcore: registered new interface driver cdc_acm
[    0.661189] cdc_acm: USB Abstract Control Model driver for USB modems and ISDN adapters
[    0.662248] usbcore: registered new interface driver uas
[    0.662965] usbcore: registered new interface driver usb-storage
[    0.663799] usbcore: registered new interface driver usbserial
[    0.664571] usbcore: registered new interface driver usbserial_generic
[    0.665451] usbserial: USB Serial support registered for generic
[    0.666248] usbcore: registered new interface driver usb_serial_simple
[    0.667105] usbserial: USB Serial support registered for carelink
[    0.667906] usbserial: USB Serial support registered for zio
[    0.668651] usbserial: USB Serial support registered for funsoft
[    0.669461] usbserial: USB Serial support registered for flashloader
[    0.670298] usbserial: USB Serial support registered for google
[    0.671076] usbserial: USB Serial support registered for libtransistor
[    0.671932] usbserial: USB Serial support registered for vivopay
[    0.672721] usbserial: USB Serial support registered for moto_modem
[    0.673568] usbserial: USB Serial support registered for motorola_tetra
[    0.674437] usbserial: USB Serial support registered for novatel_gps
[    0.675273] usbserial: USB Serial support registered for hp4x
[    0.676030] usbserial: USB Serial support registered for suunto
[    0.676808] usbserial: USB Serial support registered for siemens_mpi
[    0.677677] usbcore: registered new interface driver rio500
[    0.678510] mousedev: PS/2 mouse device common for all mice
[    0.689561] hobot-rtc a6002000.rtc: rtc core: registered hobot-rtc as rtc0
[    0.690555] i2c /dev entries driver
[    0.691163] hobot-i2c a5009000.i2c: hobot i2c probe start
[    0.691927] hobot-i2c a5009000.i2c: round_rate:96000000
[    0.692605] hobot-i2c a5009000.i2c: I2C bus speed is 400000
[    0.693343] hobot-i2c a5009000.i2c: clkdiv = 0x1d
[    0.693950] hobot-i2c a5009000.i2c: i2c0 diag register....
[    0.695044] hobot-i2c a5009000.i2c: hobot_i2c_0 probe done
[    0.695849] hobot-i2c a500a000.i2c: hobot i2c probe start
[    0.696602] hobot-i2c a500a000.i2c: round_rate:96000000
[    0.697305] hobot-i2c a500a000.i2c: I2C bus speed is 400000
[    0.698023] hobot-i2c a500a000.i2c: clkdiv = 0x1d
[    0.698629] hobot-i2c a500a000.i2c: i2c1 diag register....
[    0.699640] hobot-i2c a500a000.i2c: hobot_i2c_1 probe done
[    0.700599] lirc_dev: IR Remote Control driver registered, major 239
[    0.701437] IR LIRC bridge handler initialized
[    0.702196] sif_mclk clock frequence is 544000000
[    0.702833] mipi_rx0_ipi clock frequence is 544000000
[    0.703521] mipi_rx1_ipi clock frequence is 544000000
[    0.704220] mipi_rx2_ipi clock frequence is 544000000
[    0.704952] mipi_rx3_ipi clock frequence is 544000000
[    0.705673] mipi_tx_ipi clock frequence is 544000000
[    0.706392] mipi_cfg_host clock frequence is 102000000
[    0.707146] pym_mclk clock frequence is 1188000000
[    0.707866] mipi_dev_ref clock frequence is 24000000
[    0.708619] mipi_host_ref clock frequence is 24000000
[    0.709413] sensor0_mclk clock frequence is 37125000
[    0.710189] sensor1_mclk clock frequence is 37125000
[    0.710978] sensor2_mclk clock frequence is 37125000
[    0.711777] sensor3_mclk clock frequence is 37125000
[    0.712416] [FRT:D] x3_ips_probe(0)
[    0.713445] hobot swinfo sel reg ro=0x1 boot dump
[    0.714359] pvt a1009000.pvt: SCRATCH test: 1234abcd, pvt is alive.
[    0.715282] pvt a1009000.pvt: VM Calibrated data detected
[    0.716481] hobot_wdt a1002000.watchdog: watchdog setting [pet:6s bark:11s bite:15s]
[    0.717838] hobot_wdt a1002000.watchdog: Hobot Watchdog Timer at ffffff8009db3000 with timeout 15s
[    0.719191] device-mapper: uevent: version 1.0.3
[    0.719952] device-mapper: ioctl: 4.37.0-ioctl (2017-09-20) initialised: dm-devel@redhat.com
[    0.721164] device-mapper: verity-avb: AVB error handler initialized with vbmeta device:
[    0.723579] Synopsys Designware Multimedia Card Interface Driver
[    0.724577] dwmmc_hobot a5010000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.725428] dwmmc_hobot a5010000.dwmmc: card-detect-delay not found.
[    0.726247] dwmmc_hobot a5010000.dwmmc: data-addr not found.
[    0.727287] mmc_host mmc0: card is non-removable.
[    0.770059] dwmmc_hobot a5011000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.772921] dwmmc_hobot a5011000.dwmmc: card-detect-delay not found.
[    0.774753] dwmmc_hobot a5011000.dwmmc: data-addr not found.
[    0.778858] dwmmc_hobot a5011000.dwmmc: mmc set to fixed voltage 1800
[    0.779920] mmc_host mmc1: card is non-removable.
[    0.877035] dwmmc_hobot a5012000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.877862] dwmmc_hobot a5012000.dwmmc: card-detect-delay not found.
[    0.878680] dwmmc_hobot a5012000.dwmmc: data-addr not found.
[    0.879669] dwmmc_hobot a5012000.dwmmc: Got CD GPIO
[    0.990625] mmc1: queuing unknown CIS tuple 0x80 (2 bytes)
[    0.992821] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.995023] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.998399] mmc1: queuing unknown CIS tuple 0x80 (7 bytes)
[    1.002366] mmc1: queuing unknown CIS tuple 0x81 (9 bytes)
[    1.069140] ledtrig-cpu: registered to indicate activity on CPUs
[    1.069963] hidraw: raw HID events driver (C) Jiri Kosina
[    1.070801] usbcore: registered new interface driver usbhid
[    1.071519] usbhid: USB HID core driver
[    1.072095] logger: created 256K log 'log_main'
[    1.072737] logger: created 256K log 'log_events'
[    1.073420] logger: created 256K log 'log_radio'
[    1.074077] logger: created 256K log 'log_system'
[    1.075105] set dmc devfreq governor to performance
[    1.075738] hobot_dmcfreq_target: dmcfreq->rate:2666000000, target_rate:2666000000
[    1.076710] buf:, powersave_rate:2666000000, dmcfreq->pre_state:0
[    1.083538] usbcore: registered new interface driver snd-usb-audio
[    1.084696] Netfilter messages via NETLINK v0.30.
[    1.085348] ip_set: protocol 6
[    1.085829] ipip: IPv4 and MPLS over IPv4 tunneling driver
[    1.086831] ip_tables: (C) 2000-2006 Netfilter Core Team
[    1.087753] arp_tables: arp_tables: (C) 2002 David S. Miller
[    1.088541] Initializing XFRM netlink socket
[    1.089423] NET: Registered protocol family 10
[    1.090649] Segment Routing with IPv6
[    1.091157] sit: IPv6, IPv4 and MPLS over IPv4 tunneling driver
[    1.092249] NET: Registered protocol family 17
[    1.092904] Key type dns_resolver registered
[    1.094547] Loading compiled-in X.509 certificates
[    1.098062] Loaded X.509 cert 'Build time autogenerated kernel key: 81cb0ef77db2fac76e9588c2120c82422367d268'
[    1.099394] zswap: loaded using pool lzo/zbud
[    1.110653] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    1.112315] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    1.113298] console [netcon0] enabled
[    1.113773] netconsole: network logging started
[    1.114551] hobot-rtc a6002000.rtc: setting system clock to 1970-01-01 00:00:00 UTC (0)
[    1.115733] vps mipi_dphy: probe with x3vio done
[    1.116440] hobot_wdt_test: wdt_test_init: wdt test init
[    1.119169] VCC_CNN0: disabling
[    1.119578] VCC_CNN1: disabling
[    1.120528] vps mipi_host0: ver 140* port0(0:0)
[    1.121499] vps mipi_host1: ver 140* port1(1:0)
[    1.122388] vps mipi_host2: ver 140* port2(0:1)
[    1.123174] vps mipi_host3: ver 140* port3(1:1)
[    1.124007] ALSA device list:
[    1.124393]   No soundcards found.
[    1.125057] md: Skipping autodetection of RAID arrays. (raid=autodetect will force)
[    1.126180] VFS: Cannot open root device "mmcblk2p2" or unknown-block(0,0): error -6
[    1.127174] Please append a correct "root=" boot option; here are the available partitions:
[    1.128248] 0100          102400 ram0
[    1.128250]  (driver?)
[    1.129069] 0101          102400 ram1
[    1.129071]  (driver?)
[    1.129860] 0102          102400 ram2
[    1.129862]  (driver?)
[    1.130650] 0103          102400 ram3
[    1.130652]  (driver?)
[    1.131440] 0104          102400 ram4
[    1.131441]  (driver?)
[    1.132229] 0105          102400 ram5
[    1.132231]  (driver?)
[    1.133059] 0106          102400 ram6
[    1.133061]  (driver?)
[    1.133850] 0107          102400 ram7
[    1.133851]  (driver?)
[    1.134640] 0108          102400 ram8
[    1.134642]  (driver?)
[    1.135429] 0109          102400 ram9
[    1.135431]  (driver?)
[    1.136219] 010a          102400 ram10
[    1.136221]  (driver?)
[    1.137049] 010b          102400 ram11
[    1.137051]  (driver?)
[    1.137851] 010c          102400 ram12
[    1.137852]  (driver?)
[    1.138651] 010d          102400 ram13
[    1.138653]  (driver?)
[    1.139452] 010e          102400 ram14
[    1.139454]  (driver?)
[    1.140253] 010f          102400 ram15
[    1.140255]  (driver?)
[    1.141071] 1f00          131072 mtdblock0
[    1.141073]  (driver?)
[    1.141917] hobot_fusa: set_fusa_error_pin:75 set error pin to 1
[    1.142687] hobot_fusa: fusa errpin not ready
[    1.142691] Kernel panic - not syncing: VFS: Unable to mount root fs on unknown-block(0,0)
[    1.144310] Kernel Offset: disabled
[    1.144761] CPU features: 0x0002004
[    1.145210] Memory Limit: none
[    1.149769] Rebooting in 1 seconds..
[    1.225077] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.225799] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 1
[    1.227257] xhci-hcd xhci-hcd.0.auto: hcc params 0x0220fe6d hci version 0x110 quirks 0x0000000000010010
[    1.228493] xhci-hcd xhci-hcd.0.auto: irq 178, io mem 0xb2000000
[    1.229461] usb usb1: New USB device found, idVendor=1d6b, idProduct=0002, bcdDevice= 4.14
[    1.230059] mmc1: new HSSDIO card at address 0001
[    1.231128] usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.232056] usb usb1: Product: xHCI Host Controller
[    1.232684] usb usb1: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.233399] usb usb1: SerialNumber: xhci-hcd.0.auto
[    1.234330] hub 1-0:1.0: USB hub found
[    1.234833] hub 1-0:1.0: 1 port detected
[    1.235517] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.236231] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 2
[    1.237231] xhci-hcd xhci-hcd.0.auto: Host supports USB 3.0 SuperSpeed
[    1.238107] usb usb2: We don't know the algorithms for LPM for this host, disabling LPM.
[    1.239210] usb usb2: New USB device found, idVendor=1d6b, idProduct=0003, bcdDevice= 4.14
[    1.240273] usb usb2: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.241210] usb usb2: Product: xHCI Host Controller
[    1.241840] usb usb2: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.242546] usb usb2: SerialNumber: xhci-hcd.0.auto
[    1.243442] hub 2-0:1.0: USB hub found
[    1.243942] hub 2-0:1.0: 1 port detected
[    1.492850] usb 1-1: new high-speed USB device number 2 using xhci-hcd
[    1.645041] usb 1-1: New USB device found, idVendor=1a40, idProduct=0101, bcdDevice= 1.11
[    1.646094] usb 1-1: New USB device strings: Mfr=0, Product=1, SerialNumber=0
[    1.647011] usb 1-1: Product: USB 2.0 Hub
[    1.686270] hub 1-1:1.0: USB hub found
[    1.686791] hub 1-1:1.0: 4 ports detected
[    1.964849] mmc2: new UHS SDR104 SDHC card at address 0001
[    1.965864] mmcblk2: mmc2:0001 SD16G 29.8 GiB
[    1.967468]  mmcblk2: p1 p2
[    2.150281] SMP: stopping secondary CPUs
[    2.150789] psci: psci_sys_reset(reboot_mode=0)
NOTICE:  fast_boot:0

S
F
L
O
NOTICE:  efuse cpu_cfg = 0
W
NOTICE:  Booting Trusted Firmware
NOTICE:  BL1: v1.4(release):HR-ROM-Rel-v1.1-141-ga91d4dd-dirty
NOTICE:  BL1: Built : 11:24:44, Oct 23 2019
NOTICE:  boot src: 2
NOTICE:  GigaDev SPI NAND was found.
NOTICE:  Block size: 128 KiB, page size: 2048
NOTICE:  BL1: Booting BL2
Auth pass
NOTICE:  bl1_main exit
SPL normal reset flow
check_reset_state (2): wakeup address = 0x0, hw wakeup status = 0x3, wakeup src=0x100
patch for sys_pll 1200 with 100M eth
SFLOW_INIT
CHIP ID:PCB941/WAFER: W04/ X: X20/ Y: Y36
secondary_jump_to_spl: secure chip flow
X3 SPL : secondary core wake up and jump to spl done (cpu_core_cfg=0)
SFLOW_FIN_HW_A

U-Boot SPL 2018.09-g4ca851534c-dirty (May 11 2022 - 20:09:50 +0800)
SPACC Init - ID: (00000061)
SPL nand boot mode (from strap)
GigaDev SPI NAND was found.
Block size: 128 KiB, page size: 2048
ddr_type = 1 (LPDDR4)
hb_chip_package_type:3
load ddr header src_addr: 100000, load_addr: 802ca020, src_len: a00
find valid ddr image
ddr_hdr.ecc_gran: 0x0
ddr_hdr.ecc_map: 0x0
ddr_hdr.sbr_pattern0: 0x0
ddr_hdr.sbr_pattern1: 0x0
ddr_freq = 05
board id = 31540334
ddr datarate: 3200
### SAMSUNG DDR ###
no ddr pin set
detect part number: 108
detect ddr freq: c80
board id alternative:0x3
index is 12
index is 15
index is 19
hb_ddr_index: 19
ddr_type = 1, ddr_vendor=3, ddr_freq=3200
dram_pll_init
sscg disabled
control load ddrc src_addr: 15ae00, load_addr: 802caa20, src_len: 920
[DDR INFO]      ==ddr_release_info==
[DDR INFO]      VERSION:        develop
[DDR INFO]      BUILD:          2022-05-11-20:09
[DDR INFO]      GIT COMMIT:     4ca851534c1616ace920fdaa000c6fb717c1fb74
[DDR INFO]      GIT TIME:       Wed, 20 Apr 2022 18:28:49 +0800
[DDR INFO]      ==ddr_features==
[DDR INFO]      RDBI:           0
[DDR INFO]      WDBI:           1
[DDR INFO]      InlineECC:      0
[DDR INFO]      DM:             1
[DDR INFO]      DDC:            1
[DDR INFO]      SSCG:           0
[DDR INFO]      BOARD:          XS_ENABLE
[DDR INFO] ddr_controller_cfg done
load ddr phy src_addr: 15b800, load_addr: 802caa20, src_len: 420
ATxSlewRate     : 15f
ATxImpedance    : 7f
TxSlewRate      : 19f
TxOdtDrvStren   : 600
TxImpedanceCtrl : e3f
CalDrvStr0      : 11
VrefInGlobal    : 104
board_type = 4 (CUSTOMER_BOARD)
load dqmap src addr: 15d600, load_addr: 802caa20, src_len: 20
[DDR INFO] dwc_ddrphy_train start
magic = 544f4248
load imem1 src_addr: 11ce00, load_addr: 802caa20, src_len: 8000
load dmem1 src_addr: 15a000, load_addr: 802caa20, src_len: 684
executing 1D fw
load imem2 src_addr: 124e00, load_addr: 802caa20, src_len: 8000
load dmem2 src_addr: 15a800, load_addr: 802caa20, src_len: 564

*******************************************************
p_dmem_lpddr4_2d_16b->MR11_A0:54
p_dmem_lpddr4_2d_16b->MR14_A0:54
p_dmem_lpddr4_2d_16b->MR12_A0:51
p_dmem_lpddr4_2d_16b->MR22_A0:14

p_dmem_lpddr4_2d_16b->MR3_A0:b3
p_dmem_lpddr4_2d_16b->Reserved00:40
p_dmem_lpddr4_2d_16b->Reserved0E:4
p_dmem_lpddr4_2d_16b->Delay_Weight2D:20
p_dmem_lpddr4_2d_16b->Voltage_Weight2D:80
*******************************************************

executing 2D fw
load pie src_addr: 15be00, load_addr: 802caa20, src_len: 11f0
Set QoS.
get_ddr_mr_info:cs_num=1, mr5=0x1, mr8=0x10
no magic in efuse file,bypass efuse
total_sz = 4096
SPL_VERSION:7
uboot partition is uboot_A
load u-boot: src_addr=0x380000, dest_addr=0x4000000, len=2097152
load warm boot spl: addr=0x800, dest_addr=0x80000000, len=31232
load bl31: addr=0x300000, dest_addr=0x0, len=524288
SFLOW_AUTH_BL31
verify signature of header:  verify ok!
verify signature of image:  verify ok!
bypass bpu image
clear keybank!!!!
SFLOW_DBG_EN
Trying to boot from RAM
SPL: bl31 will jump to u-boot or other entry (0x4000000)
SFLOW_CLR_KEY
SFLOW_REG_LD
install_portal copy portal
install_portal call smc and jump to bl31 cold entry(0x0)
hb som type: 5
X3 PI reset VDD_SD done

U-Boot 2018.09-g40785bca (May 27 2022 - 16:30:48 +0800)

Model: Hobot XJ3 Soc Board
DRAM:  system DDR size: 0xffe00000
4 GiB
MMC:   dwmmc@A5010000: 0, dwmmc@A5011000: 1, dwmmc@A5012000: 2
Loading Environment from UBI... GigaDevice SPI NAND was found.
128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
*** Warning - bad CRC, using default environment

In:    serial@a5000000
Out:   serial@a5000000
Err:   serial@a5000000
Net:   x3 sdb reset eth phy done

Warning: ethernet@A5014000 (eth0) using random MAC address - d6:89:09:fa:6f:5f
eth0: ethernet@A5014000
Disable cnn cores ..
dtb_name:hobot-x3-pi.dtb
base board type: X3 SDB
bootmode: NAND
board_id = 31540334
damaged volume, update marker is setdamaged volume, update marker is setdamaged volume, update marker is sethb_boot_args_cmd_set custom_bootargs 0 ubuntu_boot 0
Hit any key to stop autoboot:  0
enable watchdog success !
switch to partitions #0, OK
mmc2 is current device
Scanning mmc 2:2...
Found U-Boot script /boot/boot.scr
664 bytes read in 2 ms (324.2 KiB/s)
## Executing script at 03c10000
Boot script loaded from devtype:mmc devnum:2 devplist:2
bootargs = console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
Loading fdt file: /boot/hobot/hobot-x3-pi.dtb
69633 bytes read in 8 ms (8.3 MiB/s)
Loading kernel: /boot/Image
19163144 bytes read in 845 ms (21.6 MiB/s)
## Flattened Device Tree blob at 03c00000
   Booting using the fdt blob at 0x3c00000
   Loading Device Tree to 0000000003c00000, end 0000000003c1ffff ... OK
chip_id: ab36300
The address of the fdt is 0x3c00000
Changed status Done
Can't get fdt_addr !!!Orign(MAX) bpu model Reserve Mem Size to 64M!!

Starting kernel ...

[    0.000000] OF: reserved mem: OVERLAP DETECTED!
[    0.000000] image_r5_mem (0x0000000080000000--0x0000000080010000) overlaps with msg_r5_mem (0x000000008000f000--0x0000000080010000)
[    0.000000] Reserved memory: created CMA memory pool at 0x0000000004000000, size 672 MiB
[    0.000000] OF: reserved mem: initialized node ion_cma, compatible id shared-dma-pool
[    0.000000] cma: Reserved 16 MiB at 0x000000007f000000
[    0.000000] On node 0 totalpages: 1047808
[    0.000000]   DMA zone: 8180 pages used for memmap
[    0.000000]   DMA zone: 0 pages reserved
[    0.000000]   DMA zone: 523520 pages, LIFO batch:31
[    0.000000]   Normal zone: 8192 pages used for memmap
[    0.000000]   Normal zone: 524288 pages, LIFO batch:31
[    0.000000] psci: probing for conduit method from DT.
[    0.000000] psci: PSCIv1.1 detected in firmware.
[    0.000000] psci: Using standard PSCI v0.2 function IDs
[    0.000000] psci: MIGRATE_INFO_TYPE not supported.
[    0.000000] psci: SMC Calling Convention v1.1
[    0.000000] percpu: Embedded 25 pages/cpu @ffffffc17ff2a000 s65176 r8192 d29032 u102400
[    0.000000] pcpu-alloc: s65176 r8192 d29032 u102400 alloc=25*4096
[    0.000000] pcpu-alloc: [0] 0 [0] 1 [0] 2 [0] 3
[    0.000000] Detected VIPT I-cache on CPU0
[    0.000000] CPU features: enabling workaround for ARM erratum 845719
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 1031436
[    0.000000] Kernel command line: earlycon loglevel=8 kgdboc=ttyS0 video=hobot:x3sdb-hdmi  console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
[    0.000000] PID hash table entries: 4096 (order: 3, 32768 bytes)
[    0.000000] Dentry cache hash table entries: 524288 (order: 10, 4194304 bytes)
[    0.000000] Inode-cache hash table entries: 262144 (order: 9, 2097152 bytes)
[    0.000000] software IO TLB [mem 0x7afff000-0x7efff000] (64MB) mapped at [ffffffc07afff000-ffffffc07effefff]
[    0.000000] Memory: 3319580K/4191232K available (10494K kernel code, 1306K rwdata, 5756K rodata, 1088K init, 9553K bss, 167140K reserved, 704512K cma-reserved)
[    0.000000] Virtual kernel memory layout:
[    0.000000]     modules : 0xffffff8000000000 - 0xffffff8008000000   (   128 MB)
[    0.000000]     vmalloc : 0xffffff8008000000 - 0xffffffbebfff0000   (   250 GB)
[    0.000000]       .text : 0xffffff8008000000 - 0xffffff8008a40000   ( 10496 KB)
[    0.000000]     .rodata : 0xffffff8008a40000 - 0xffffff8008ff0000   (  5824 KB)
[    0.000000]       .init : 0xffffff8008ff0000 - 0xffffff8009100000   (  1088 KB)
[    0.000000]       .data : 0xffffff8009100000 - 0xffffff8009246808   (  1307 KB)
[    0.000000]        .bss : 0xffffff8009246808 - 0xffffff8009b9aed8   (  9554 KB)
[    0.000000]     fixed   : 0xffffffbefe7fd000 - 0xffffffbefec00000   (  4108 KB)
[    0.000000]     PCI I/O : 0xffffffbefee00000 - 0xffffffbeffe00000   (    16 MB)
[    0.000000]     vmemmap : 0xffffffbf00000000 - 0xffffffc000000000   (     4 GB maximum)
[    0.000000]               0xffffffbf00008000 - 0xffffffbf06000000   (    95 MB actual)
[    0.000000]     memory  : 0xffffffc000200000 - 0xffffffc180000000   (  6142 MB)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=4, Nodes=1
[    0.000000] ftrace: allocating 36277 entries in 142 pages
[    0.000000] Preemptible hierarchical RCU implementation.
[    0.000000]  Tasks RCU enabled.
[    0.000000] NR_IRQS: 64, nr_irqs: 64, preallocated irqs: 0
[    0.000000] parent_rate: 0,  dclk->rate:2666000000, pre_ddr_rate:0, res.a0:139716712
[    0.000000] arch_timer: cp15 timer(s) running at 24.00MHz (virt).
[    0.000000] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0x588fe9dc0, max_idle_ns: 440795202592 ns
[    0.000003] sched_clock: 56 bits at 24MHz, resolution 41ns, wraps every 4398046511097ns
[    0.001193] clocksource: hobot_clocksource: mask: 0xffffffffffffffff max_cycles: 0x1d854df40, max_idle_ns: 3526361616960 ns
[    0.002966] Console: colour dummy device 80x25
[    0.003537] Calibrating delay loop (skipped), value calculated using timer frequency.. 48.00 BogoMIPS (lpj=96000)
[    0.004844] pid_max: default: 32768 minimum: 301
[    0.005498] Security Framework initialized
[    0.006016] AppArmor: AppArmor disabled by boot time parameter
[    0.006858] Mount-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.007727] Mountpoint-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.023768] ASID allocator initialised with 65536 entries
[    0.031766] Hierarchical SRCU implementation.
[    0.063825] smp: Bringing up secondary CPUs ...
[    0.100031] Detected VIPT I-cache on CPU1
[    0.100066] CPU1: Booted secondary processor [410fd034]
[    0.136082] Detected VIPT I-cache on CPU2
[    0.136102] CPU2: Booted secondary processor [410fd034]
[    0.172141] Detected VIPT I-cache on CPU3
[    0.172161] CPU3: Booted secondary processor [410fd034]
[    0.172215] smp: Brought up 1 node, 4 CPUs
[    0.176277] SMP: Total of 4 processors activated.
[    0.176872] CPU features: detected feature: 32-bit EL0 Support
[    0.177691] CPU: All CPU(s) started at EL1
[    0.178219] alternatives: patching kernel code
[    0.179809] devtmpfs: initialized
[    0.188879] random: get_random_u32 called from bucket_table_alloc+0x108/0x270 with crng_init=0
[    0.190463] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 7645041785100000 ns
[    0.191710] futex hash table entries: 1024 (order: 5, 131072 bytes)
[    0.208265] xor: automatically using best checksumming function   32regs
[    0.209211] pinctrl core: initialized pinctrl subsystem
[    0.210445] NET: Registered protocol family 16
[    0.211763] vdso: 2 pages (1 code @ ffffff8008a46000, 1 data @ ffffff8009104000)
[    0.212709] hw-breakpoint: found 6 breakpoint and 4 watchpoint registers.
[    0.214298] DMA: preallocated 256 KiB pool for atomic allocations
[    0.219149] pstore: using zlib compression
[    0.219944] console [pstore-1] enabled
[    0.220541] pstore: Registered ramoops as persistent store backend
[    0.221325] ramoops: attached 0x40000@0x3fc0000, ecc: 0/0
[    0.226333] hobot_dma a1005000.dma: Hobot DMA Engine Driver Probed!!
[    0.239806] SCSI subsystem initialized
[    0.240630] media: Linux media interface: v0.10
[    0.241231] Linux video capture interface: v2.00
[    0.241868] pps_core: LinuxPPS API ver. 1 registered
[    0.242496] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.243671] PTP clock support registered
[    0.244940] ion_dummy: not reserve carveout memory, try to alloc from cma
[    0.381520] Advanced Linux Sound Architecture Driver Initialized.
[    0.382681] usbcore: registered new interface driver usbfs
[    0.383408] usbcore: registered new interface driver hub
[    0.384134] usbcore: registered new device driver usb
[    0.385140] clocksource: Switched to clocksource arch_sys_counter
[    0.432812] VFS: Disk quotas dquot_6.6.0
[    0.433385] VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
[    0.434320] FS-Cache: Loaded
[    0.434805] CacheFiles: Loaded
[    0.440145] NET: Registered protocol family 2
[    0.441063] TCP established hash table entries: 32768 (order: 6, 262144 bytes)
[    0.442195] TCP bind hash table entries: 32768 (order: 7, 524288 bytes)
[    0.443450] TCP: Hash tables configured (established 32768 bind 32768)
[    0.444362] UDP hash table entries: 2048 (order: 4, 65536 bytes)
[    0.445209] UDP-Lite hash table entries: 2048 (order: 4, 65536 bytes)
[    0.446211] NET: Registered protocol family 1
[    0.447025] RPC: Registered named UNIX socket transport module.
[    0.447776] RPC: Registered udp transport module.
[    0.448373] RPC: Registered tcp transport module.
[    0.448972] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.450504] hw perfevents: enabled with armv8_cortex_a53 PMU driver, 7 counters available
[    0.452704] audit: initializing netlink subsys (disabled)
[    0.453488] audit: type=2000 audit(0.452:1): state=initialized audit_enabled=0 res=1
[    0.453743] Initialise system trusted keyrings
[    0.453817] workingset: timestamp_bits=46 max_order=20 bucket_order=0
[    0.457397] zbud: loaded
[    0.458936] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.459799] exFAT: Version 1.2.9
[    0.460277] FS-Cache: Netfs 'nfs' registered for caching
[    0.461428] NFS: Registering the id_resolver key type
[    0.462083] Key type id_resolver registered
[    0.462610] Key type id_legacy registered
[    0.463126] nfs4filelayout_init: NFSv4 File Layout Driver Registering...
[    0.463979] Installing knfsd (copyright (C) 1996 okir@monad.swb.de).
[    0.468113] NET: Registered protocol family 38
[    0.468686] async_tx: api initialized (async)
[    0.469250] Key type asymmetric registered
[    0.469767] Asymmetric key parser 'x509' registered
[    0.470452] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 245)
[    0.471468] io scheduler noop registered
[    0.472130] io scheduler cfq registered (default)
[    0.472725] io scheduler mq-deadline registered
[    0.473311] io scheduler kyber registered
[    0.474505] pinctrl-single a6003170.pinctrl_voltag: 64 pins at pa ffffff8009c4d170 size 8
[    0.475856] pinctrl-single a6004000.pinctrl: 128 pins at pa ffffff8009c61000 size 512
[    0.477058] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: start probe
[    0.478103] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: probe ok
[    0.478993] gpio-x3 a6003000.gpio: x3 gpio probe start!!!
[    0.479684] gpio-x3 a6003000.gpio: x3 gpio add gpiochip start!!!
[    0.480610] gpio-x3 a6003000.gpio: diable all gpio irq
[    0.482896] gpio-x3 a6003000.gpio: irqbase:57
[    0.483448] gpio-x3 a6003000.gpio: x3 irq add start!!!
[    0.484105] irq: Cannot allocate irq_descs @ IRQ57, assuming pre-allocated
[    0.485298] gpio-x3 a6003000.gpio: x3 irq add ok!!!
[    0.485956] gpio-x3 a6003000.gpio: x3 irqchip ops add ok!!!
[    0.486661] gpio-x3 a6003000.gpio: x3 gpio probe ok!!!
[    0.487781] hobot-pwm: hobot-pwmchip0 registered
[    0.488536] hobot-pwm: hobot-pwmchip1 registered
[    0.489889] diag dev [ver:1.1] init done
[    0.490790] hobot_ddr_monitor: LPDDR4 detected
[    0.491542] hobot_ddr_monitor: ddr monitor init finished.
[    0.491936] [vcam] init start
[    0.492996] vcam probe start
[    0.493468] vcam probe end successful
[    0.493928] [vcam] init end
[    0.494844] a5000000.serial: ttyS0 at MMIO 0xa5000000 (irq = 10, base_baud = 12000000) is a hobot-uart
[    0.496067] console [ttyS0] enabled
[    0.496067] console [ttyS0] enabled
[    0.496969] bootconsole [hobot0] disabled
[    0.496969] bootconsole [hobot0] disabled
[    0.498484] hobot-uart a5001000.serial: Failed to create debugfs root directory
[    0.499492] a5001000.serial: ttyS1 at MMIO 0xa5001000 (irq = 11, base_baud = 12000000) is a hobot-uart
[    0.500930] hobot-uart a5003000.serial: Failed to create debugfs root directory
[    0.501942] a5003000.serial: ttyS3 at MMIO 0xa5003000 (irq = 12, base_baud = 12000000) is a hobot-uart
[    0.503487] KGDB: Registered I/O driver kgdboc
[    0.504325] cacheinfo: Unable to detect cache hierarchy for CPU 0
[    0.509777] brd: module loaded
[    0.514348] loop: module loaded
[    0.515871] spi-nand hr_nand.0: GigaDevice SPI NAND was found.
[    0.516645] spi-nand hr_nand.0: 128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
[    0.519289] hobot_spi a5006000.spi: ver: HOBOT-spi_V20.200330 master
[    0.520328] libphy: Fixed MDIO Bus: probed
[    0.521643] st_gmac a5014000.ethernet: found phy-handle subnode
[    0.522477] st_gmac a5014000.ethernet: xj3_mtl_setup, plat->rx-queues-to-use:4, and tx:4
[    0.523663] st_gmac a5014000.ethernet: xj3_probe_config_dt, clk_ptp_rate:250000000
[    0.524664] set mac address 00:11:22:ad:8c:a5:
[    0.524667] (using random mac adress)
[    0.525855] (NULL device *): xj3_get_hw_features, tx_fifo_size:16384
[    0.526673] (NULL device *): xj3_get_hw_features, rx_fifo_size:16384
[    0.527491] st_gmac a5014000.ethernet: TSO supported
[    0.528131] st_gmac a5014000.ethernet: TSO feature enabled
[    0.528838] st_gmac a5014000.ethernet: Enable Rx Mitigation via HW Watchdog Timer
[    0.649924] libphy: hobot-mac-mdio: probed
[    0.651483] st_gmac a5014000.ethernet: hobot_eth_probe: probe sucessfully
[    0.652685] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_0v8 not found, using dummy regulator
[    0.653929] dwc3-of-simple b2000000.usb: usb regulator 0v8 enable succeed
[    0.654807] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_3v3 not found, using dummy regulator
[    0.656009] dwc3-of-simple b2000000.usb: usb regulator 3v3 enable succeed
[    0.657553] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    0.659209] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    0.660642] usbcore: registered new interface driver cdc_acm
[    0.661392] cdc_acm: USB Abstract Control Model driver for USB modems and ISDN adapters
[    0.662447] usbcore: registered new interface driver uas
[    0.663168] usbcore: registered new interface driver usb-storage
[    0.664003] usbcore: registered new interface driver usbserial
[    0.664775] usbcore: registered new interface driver usbserial_generic
[    0.665653] usbserial: USB Serial support registered for generic
[    0.666449] usbcore: registered new interface driver usb_serial_simple
[    0.667309] usbserial: USB Serial support registered for carelink
[    0.668110] usbserial: USB Serial support registered for zio
[    0.668855] usbserial: USB Serial support registered for funsoft
[    0.669662] usbserial: USB Serial support registered for flashloader
[    0.670497] usbserial: USB Serial support registered for google
[    0.671275] usbserial: USB Serial support registered for libtransistor
[    0.672134] usbserial: USB Serial support registered for vivopay
[    0.672923] usbserial: USB Serial support registered for moto_modem
[    0.673764] usbserial: USB Serial support registered for motorola_tetra
[    0.674631] usbserial: USB Serial support registered for novatel_gps
[    0.675467] usbserial: USB Serial support registered for hp4x
[    0.676223] usbserial: USB Serial support registered for suunto
[    0.677004] usbserial: USB Serial support registered for siemens_mpi
[    0.677868] usbcore: registered new interface driver rio500
[    0.678703] mousedev: PS/2 mouse device common for all mice
[    0.689753] hobot-rtc a6002000.rtc: rtc core: registered hobot-rtc as rtc0
[    0.690746] i2c /dev entries driver
[    0.691351] hobot-i2c a5009000.i2c: hobot i2c probe start
[    0.692124] hobot-i2c a5009000.i2c: round_rate:96000000
[    0.692802] hobot-i2c a5009000.i2c: I2C bus speed is 400000
[    0.693540] hobot-i2c a5009000.i2c: clkdiv = 0x1d
[    0.694148] hobot-i2c a5009000.i2c: i2c0 diag register....
[    0.695238] hobot-i2c a5009000.i2c: hobot_i2c_0 probe done
[    0.696044] hobot-i2c a500a000.i2c: hobot i2c probe start
[    0.696799] hobot-i2c a500a000.i2c: round_rate:96000000
[    0.697502] hobot-i2c a500a000.i2c: I2C bus speed is 400000
[    0.698220] hobot-i2c a500a000.i2c: clkdiv = 0x1d
[    0.698826] hobot-i2c a500a000.i2c: i2c1 diag register....
[    0.699836] hobot-i2c a500a000.i2c: hobot_i2c_1 probe done
[    0.700798] lirc_dev: IR Remote Control driver registered, major 239
[    0.701637] IR LIRC bridge handler initialized
[    0.702393] sif_mclk clock frequence is 544000000
[    0.703029] mipi_rx0_ipi clock frequence is 544000000
[    0.703718] mipi_rx1_ipi clock frequence is 544000000
[    0.704417] mipi_rx2_ipi clock frequence is 544000000
[    0.705125] mipi_rx3_ipi clock frequence is 544000000
[    0.705865] mipi_tx_ipi clock frequence is 544000000
[    0.706586] mipi_cfg_host clock frequence is 102000000
[    0.707340] pym_mclk clock frequence is 1188000000
[    0.708060] mipi_dev_ref clock frequence is 24000000
[    0.708813] mipi_host_ref clock frequence is 24000000
[    0.709606] sensor0_mclk clock frequence is 37125000
[    0.710387] sensor1_mclk clock frequence is 37125000
[    0.711174] sensor2_mclk clock frequence is 37125000
[    0.711973] sensor3_mclk clock frequence is 37125000
[    0.712613] [FRT:D] x3_ips_probe(0)
[    0.713649] hobot swinfo sel reg ro=0x1 boot dump
[    0.714556] pvt a1009000.pvt: SCRATCH test: 1234abcd, pvt is alive.
[    0.715489] pvt a1009000.pvt: VM Calibrated data detected
[    0.716683] hobot_wdt a1002000.watchdog: watchdog setting [pet:6s bark:11s bite:15s]
[    0.718026] hobot_wdt a1002000.watchdog: Hobot Watchdog Timer at ffffff8009db3000 with timeout 15s
[    0.719374] device-mapper: uevent: version 1.0.3
[    0.720135] device-mapper: ioctl: 4.37.0-ioctl (2017-09-20) initialised: dm-devel@redhat.com
[    0.721341] device-mapper: verity-avb: AVB error handler initialized with vbmeta device:
[    0.723751] Synopsys Designware Multimedia Card Interface Driver
[    0.724750] dwmmc_hobot a5010000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.725610] dwmmc_hobot a5010000.dwmmc: card-detect-delay not found.
[    0.726429] dwmmc_hobot a5010000.dwmmc: data-addr not found.
[    0.727472] mmc_host mmc0: card is non-removable.
[    0.766360] dwmmc_hobot a5011000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.769200] dwmmc_hobot a5011000.dwmmc: card-detect-delay not found.
[    0.770020] dwmmc_hobot a5011000.dwmmc: data-addr not found.
[    0.774789] dwmmc_hobot a5011000.dwmmc: mmc set to fixed voltage 1800
[    0.775851] mmc_host mmc1: card is non-removable.
[    0.873374] dwmmc_hobot a5012000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.874193] dwmmc_hobot a5012000.dwmmc: card-detect-delay not found.
[    0.875023] dwmmc_hobot a5012000.dwmmc: data-addr not found.
[    0.875991] dwmmc_hobot a5012000.dwmmc: Got CD GPIO
[    0.984517] mmc1: queuing unknown CIS tuple 0x80 (2 bytes)
[    0.986723] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.988908] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.992287] mmc1: queuing unknown CIS tuple 0x80 (7 bytes)
[    0.996242] mmc1: queuing unknown CIS tuple 0x81 (9 bytes)
[    1.061426] ledtrig-cpu: registered to indicate activity on CPUs
[    1.062259] hidraw: raw HID events driver (C) Jiri Kosina
[    1.063117] usbcore: registered new interface driver usbhid
[    1.063834] usbhid: USB HID core driver
[    1.064413] logger: created 256K log 'log_main'
[    1.065057] logger: created 256K log 'log_events'
[    1.065738] logger: created 256K log 'log_radio'
[    1.066392] logger: created 256K log 'log_system'
[    1.067417] set dmc devfreq governor to performance
[    1.068050] hobot_dmcfreq_target: dmcfreq->rate:2666000000, target_rate:2666000000
[    1.069023] buf:, powersave_rate:2666000000, dmcfreq->pre_state:0
[    1.075867] usbcore: registered new interface driver snd-usb-audio
[    1.077029] Netfilter messages via NETLINK v0.30.
[    1.077679] ip_set: protocol 6
[    1.078166] ipip: IPv4 and MPLS over IPv4 tunneling driver
[    1.079164] ip_tables: (C) 2000-2006 Netfilter Core Team
[    1.080148] arp_tables: arp_tables: (C) 2002 David S. Miller
[    1.080940] Initializing XFRM netlink socket
[    1.081887] NET: Registered protocol family 10
[    1.083109] Segment Routing with IPv6
[    1.083617] sit: IPv6, IPv4 and MPLS over IPv4 tunneling driver
[    1.084708] NET: Registered protocol family 17
[    1.085360] Key type dns_resolver registered
[    1.086962] Loading compiled-in X.509 certificates
[    1.090473] Loaded X.509 cert 'Build time autogenerated kernel key: 81cb0ef77db2fac76e9588c2120c82422367d268'
[    1.091801] zswap: loaded using pool lzo/zbud
[    1.103147] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    1.104809] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    1.105804] console [netcon0] enabled
[    1.106278] netconsole: network logging started
[    1.107064] hobot-rtc a6002000.rtc: setting system clock to 1970-01-01 00:00:00 UTC (0)
[    1.108244] vps mipi_dphy: probe with x3vio done
[    1.108951] hobot_wdt_test: wdt_test_init: wdt test init
[    1.113846] VCC_CNN0: disabling
[    1.114256] VCC_CNN1: disabling
[    1.115223] vps mipi_host0: ver 140* port0(0:0)
[    1.116128] vps mipi_host1: ver 140* port1(1:0)
[    1.117017] vps mipi_host2: ver 140* port2(0:1)
[    1.117862] vps mipi_host3: ver 140* port3(1:1)
[    1.118702] ALSA device list:
[    1.119086]   No soundcards found.
[    1.119717] md: Skipping autodetection of RAID arrays. (raid=autodetect will force)
[    1.120848] VFS: Cannot open root device "mmcblk2p2" or unknown-block(0,0): error -6
[    1.121865] Please append a correct "root=" boot option; here are the available partitions:
[    1.122940] 0100          102400 ram0
[    1.122942]  (driver?)
[    1.123731] 0101          102400 ram1
[    1.123733]  (driver?)
[    1.124521] 0102          102400 ram2
[    1.124523]  (driver?)
[    1.125363] 0103          102400 ram3
[    1.125365]  (driver?)
[    1.126154] 0104          102400 ram4
[    1.126156]  (driver?)
[    1.126944] 0105          102400 ram5
[    1.126946]  (driver?)
[    1.127734] 0106          102400 ram6
[    1.127736]  (driver?)
[    1.128524] 0107          102400 ram7
[    1.128525]  (driver?)
[    1.129329] 0108          102400 ram8
[    1.129331]  (driver?)
[    1.130120] 0109          102400 ram9
[    1.130121]  (driver?)
[    1.130909] 010a          102400 ram10
[    1.130911]  (driver?)
[    1.131710] 010b          102400 ram11
[    1.131712]  (driver?)
[    1.132511] 010c          102400 ram12
[    1.132513]  (driver?)
[    1.133346] 010d          102400 ram13
[    1.133348]  (driver?)
[    1.134148] 010e          102400 ram14
[    1.134150]  (driver?)
[    1.134949] 010f          102400 ram15
[    1.134951]  (driver?)
[    1.135752] 1f00          131072 mtdblock0
[    1.135754]  (driver?)
[    1.136598] hobot_fusa: set_fusa_error_pin:75 set error pin to 1
[    1.137382] hobot_fusa: fusa errpin not ready
[    1.137386] Kernel panic - not syncing: VFS: Unable to mount root fs on unknown-block(0,0)
[    1.139006] Kernel Offset: disabled
[    1.139457] CPU features: 0x0002004
[    1.139906] Memory Limit: none
[    1.144466] Rebooting in 1 seconds..
[    1.213375] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.214098] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 1
[    1.215559] xhci-hcd xhci-hcd.0.auto: hcc params 0x0220fe6d hci version 0x110 quirks 0x0000000000010010
[    1.216795] xhci-hcd xhci-hcd.0.auto: irq 178, io mem 0xb2000000
[    1.217769] usb usb1: New USB device found, idVendor=1d6b, idProduct=0002, bcdDevice= 4.14
[    1.218832] usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.219761] usb usb1: Product: xHCI Host Controller
[    1.220389] usb usb1: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.221096] usb usb1: SerialNumber: xhci-hcd.0.auto
[    1.222112] hub 1-0:1.0: USB hub found
[    1.222399] mmc1: new HSSDIO card at address 0001
[    1.223220] hub 1-0:1.0: 1 port detected
[    1.223916] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.224630] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 2
[    1.225635] xhci-hcd xhci-hcd.0.auto: Host supports USB 3.0 SuperSpeed
[    1.226511] usb usb2: We don't know the algorithms for LPM for this host, disabling LPM.
[    1.227614] usb usb2: New USB device found, idVendor=1d6b, idProduct=0003, bcdDevice= 4.14
[    1.228677] usb usb2: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.229613] usb usb2: Product: xHCI Host Controller
[    1.230242] usb usb2: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.230948] usb usb2: SerialNumber: xhci-hcd.0.auto
[    1.231854] hub 2-0:1.0: USB hub found
[    1.232355] hub 2-0:1.0: 1 port detected
[    1.489143] usb 1-1: new high-speed USB device number 2 using xhci-hcd
[    1.641332] usb 1-1: New USB device found, idVendor=1a40, idProduct=0101, bcdDevice= 1.11
[    1.642384] usb 1-1: New USB device strings: Mfr=0, Product=1, SerialNumber=0
[    1.643301] usb 1-1: Product: USB 2.0 Hub
[    1.706672] hub 1-1:1.0: USB hub found
[    1.707201] hub 1-1:1.0: 4 ports detected
[    2.144978] SMP: stopping secondary CPUs
[    2.145486] psci: psci_sys_reset(reboot_mode=0)
NOTICE:  fast_boot:0

S
F
L
O
NOTICE:  efuse cpu_cfg = 0
W
NOTICE:  Booting Trusted Firmware
NOTICE:  BL1: v1.4(release):HR-ROM-Rel-v1.1-141-ga91d4dd-dirty
NOTICE:  BL1: Built : 11:24:44, Oct 23 2019
NOTICE:  boot src: 2
NOTICE:  GigaDev SPI NAND was found.
NOTICE:  Block size: 128 KiB, page size: 2048
NOTICE:  BL1: Booting BL2
Auth pass
NOTICE:  bl1_main exit
SPL normal reset flow
check_reset_state (2): wakeup address = 0x0, hw wakeup status = 0x3, wakeup src=0x100
patch for sys_pll 1200 with 100M eth
SFLOW_INIT
CHIP ID:PCB941/WAFER: W04/ X: X20/ Y: Y36
secondary_jump_to_spl: secure chip flow
X3 SPL : secondary core wake up and jump to spl done (cpu_core_cfg=0)
SFLOW_FIN_HW_A

U-Boot SPL 2018.09-g4ca851534c-dirty (May 11 2022 - 20:09:50 +0800)
SPACC Init - ID: (00000061)
SPL nand boot mode (from strap)
GigaDev SPI NAND was found.
Block size: 128 KiB, page size: 2048
ddr_type = 1 (LPDDR4)
hb_chip_package_type:3
load ddr header src_addr: 100000, load_addr: 802ca020, src_len: a00
find valid ddr image
ddr_hdr.ecc_gran: 0x0
ddr_hdr.ecc_map: 0x0
ddr_hdr.sbr_pattern0: 0x0
ddr_hdr.sbr_pattern1: 0x0
ddr_freq = 05
board id = 31540334
ddr datarate: 3200
### SAMSUNG DDR ###
no ddr pin set
detect part number: 108
detect ddr freq: c80
board id alternative:0x3
index is 12
index is 15
index is 19
hb_ddr_index: 19
ddr_type = 1, ddr_vendor=3, ddr_freq=3200
dram_pll_init
sscg disabled
control load ddrc src_addr: 15ae00, load_addr: 802caa20, src_len: 920
[DDR INFO]      ==ddr_release_info==
[DDR INFO]      VERSION:        develop
[DDR INFO]      BUILD:          2022-05-11-20:09
[DDR INFO]      GIT COMMIT:     4ca851534c1616ace920fdaa000c6fb717c1fb74
[DDR INFO]      GIT TIME:       Wed, 20 Apr 2022 18:28:49 +0800
[DDR INFO]      ==ddr_features==
[DDR INFO]      RDBI:           0
[DDR INFO]      WDBI:           1
[DDR INFO]      InlineECC:      0
[DDR INFO]      DM:             1
[DDR INFO]      DDC:            1
[DDR INFO]      SSCG:           0
[DDR INFO]      BOARD:          XS_ENABLE
[DDR INFO] ddr_controller_cfg done
load ddr phy src_addr: 15b800, load_addr: 802caa20, src_len: 420
ATxSlewRate     : 15f
ATxImpedance    : 7f
TxSlewRate      : 19f
TxOdtDrvStren   : 600
TxImpedanceCtrl : e3f
CalDrvStr0      : 11
VrefInGlobal    : 104
board_type = 4 (CUSTOMER_BOARD)
load dqmap src addr: 15d600, load_addr: 802caa20, src_len: 20
[DDR INFO] dwc_ddrphy_train start
magic = 544f4248
load imem1 src_addr: 11ce00, load_addr: 802caa20, src_len: 8000
load dmem1 src_addr: 15a000, load_addr: 802caa20, src_len: 684
executing 1D fw
load imem2 src_addr: 124e00, load_addr: 802caa20, src_len: 8000
load dmem2 src_addr: 15a800, load_addr: 802caa20, src_len: 564

*******************************************************
p_dmem_lpddr4_2d_16b->MR11_A0:54
p_dmem_lpddr4_2d_16b->MR14_A0:54
p_dmem_lpddr4_2d_16b->MR12_A0:51
p_dmem_lpddr4_2d_16b->MR22_A0:14

p_dmem_lpddr4_2d_16b->MR3_A0:b3
p_dmem_lpddr4_2d_16b->Reserved00:40
p_dmem_lpddr4_2d_16b->Reserved0E:4
p_dmem_lpddr4_2d_16b->Delay_Weight2D:20
p_dmem_lpddr4_2d_16b->Voltage_Weight2D:80
*******************************************************

executing 2D fw
load pie src_addr: 15be00, load_addr: 802caa20, src_len: 11f0
Set QoS.
get_ddr_mr_info:cs_num=1, mr5=0x1, mr8=0x10
no magic in efuse file,bypass efuse
total_sz = 4096
SPL_VERSION:7
uboot partition is uboot_A
load u-boot: src_addr=0x380000, dest_addr=0x4000000, len=2097152
load warm boot spl: addr=0x800, dest_addr=0x80000000, len=31232
load bl31: addr=0x300000, dest_addr=0x0, len=524288
SFLOW_AUTH_BL31
verify signature of header:  verify ok!
verify signature of image:  verify ok!
bypass bpu image
clear keybank!!!!
SFLOW_DBG_EN
Trying to boot from RAM
SPL: bl31 will jump to u-boot or other entry (0x4000000)
SFLOW_CLR_KEY
SFLOW_REG_LD
install_portal copy portal
install_portal call smc and jump to bl31 cold entry(0x0)
hb som type: 5
X3 PI reset VDD_SD done

U-Boot 2018.09-g40785bca (May 27 2022 - 16:30:48 +0800)

Model: Hobot XJ3 Soc Board
DRAM:  system DDR size: 0xffe00000
4 GiB
MMC:   dwmmc@A5010000: 0, dwmmc@A5011000: 1, dwmmc@A5012000: 2 (SD)
Loading Environment from UBI... GigaDevice SPI NAND was found.
128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
*** Warning - bad CRC, using default environment

In:    serial@a5000000
Out:   serial@a5000000
Err:   serial@a5000000
Net:   x3 sdb reset eth phy done

Warning: ethernet@A5014000 (eth0) using random MAC address - f2:1f:8e:93:9d:11
eth0: ethernet@A5014000
Disable cnn cores ..
dtb_name:hobot-x3-pi.dtb
base board type: X3 SDB
bootmode: NAND
board_id = 31540334
damaged volume, update marker is setdamaged volume, update marker is setdamaged volume, update marker is sethb_boot_args_cmd_set custom_bootargs 0 ubuntu_boot 0
Hit any key to stop autoboot:  0
enable watchdog success !
switch to partitions #0, OK
mmc2 is current device
Scanning mmc 2:2...
Found U-Boot script /boot/boot.scr
664 bytes read in 2 ms (324.2 KiB/s)
## Executing script at 03c10000
Boot script loaded from devtype:mmc devnum:2 devplist:2
bootargs = console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
Loading fdt file: /boot/hobot/hobot-x3-pi.dtb
69633 bytes read in 8 ms (8.3 MiB/s)
Loading kernel: /boot/Image
19163144 bytes read in 845 ms (21.6 MiB/s)
## Flattened Device Tree blob at 03c00000
   Booting using the fdt blob at 0x3c00000
   Loading Device Tree to 0000000003c00000, end 0000000003c1ffff ... OK
chip_id: ab36300
The address of the fdt is 0x3c00000
Changed status Done
Can't get fdt_addr !!!Orign(MAX) bpu model Reserve Mem Size to 64M!!

Starting kernel ...

[    0.000000] OF: reserved mem: OVERLAP DETECTED!
[    0.000000] image_r5_mem (0x0000000080000000--0x0000000080010000) overlaps with msg_r5_mem (0x000000008000f000--0x0000000080010000)
[    0.000000] Reserved memory: created CMA memory pool at 0x0000000004000000, size 672 MiB
[    0.000000] OF: reserved mem: initialized node ion_cma, compatible id shared-dma-pool
[    0.000000] cma: Reserved 16 MiB at 0x000000007f000000
[    0.000000] On node 0 totalpages: 1047808
[    0.000000]   DMA zone: 8180 pages used for memmap
[    0.000000]   DMA zone: 0 pages reserved
[    0.000000]   DMA zone: 523520 pages, LIFO batch:31
[    0.000000]   Normal zone: 8192 pages used for memmap
[    0.000000]   Normal zone: 524288 pages, LIFO batch:31
[    0.000000] psci: probing for conduit method from DT.
[    0.000000] psci: PSCIv1.1 detected in firmware.
[    0.000000] psci: Using standard PSCI v0.2 function IDs
[    0.000000] psci: MIGRATE_INFO_TYPE not supported.
[    0.000000] psci: SMC Calling Convention v1.1
[    0.000000] percpu: Embedded 25 pages/cpu @ffffffc17ff2a000 s65176 r8192 d29032 u102400
[    0.000000] pcpu-alloc: s65176 r8192 d29032 u102400 alloc=25*4096
[    0.000000] pcpu-alloc: [0] 0 [0] 1 [0] 2 [0] 3
[    0.000000] Detected VIPT I-cache on CPU0
[    0.000000] CPU features: enabling workaround for ARM erratum 845719
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 1031436
[    0.000000] Kernel command line: earlycon loglevel=8 kgdboc=ttyS0 video=hobot:x3sdb-hdmi  console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
[    0.000000] PID hash table entries: 4096 (order: 3, 32768 bytes)
[    0.000000] Dentry cache hash table entries: 524288 (order: 10, 4194304 bytes)
[    0.000000] Inode-cache hash table entries: 262144 (order: 9, 2097152 bytes)
[    0.000000] software IO TLB [mem 0x7afff000-0x7efff000] (64MB) mapped at [ffffffc07afff000-ffffffc07effefff]
[    0.000000] Memory: 3319580K/4191232K available (10494K kernel code, 1306K rwdata, 5756K rodata, 1088K init, 9553K bss, 167140K reserved, 704512K cma-reserved)
[    0.000000] Virtual kernel memory layout:
[    0.000000]     modules : 0xffffff8000000000 - 0xffffff8008000000   (   128 MB)
[    0.000000]     vmalloc : 0xffffff8008000000 - 0xffffffbebfff0000   (   250 GB)
[    0.000000]       .text : 0xffffff8008000000 - 0xffffff8008a40000   ( 10496 KB)
[    0.000000]     .rodata : 0xffffff8008a40000 - 0xffffff8008ff0000   (  5824 KB)
[    0.000000]       .init : 0xffffff8008ff0000 - 0xffffff8009100000   (  1088 KB)
[    0.000000]       .data : 0xffffff8009100000 - 0xffffff8009246808   (  1307 KB)
[    0.000000]        .bss : 0xffffff8009246808 - 0xffffff8009b9aed8   (  9554 KB)
[    0.000000]     fixed   : 0xffffffbefe7fd000 - 0xffffffbefec00000   (  4108 KB)
[    0.000000]     PCI I/O : 0xffffffbefee00000 - 0xffffffbeffe00000   (    16 MB)
[    0.000000]     vmemmap : 0xffffffbf00000000 - 0xffffffc000000000   (     4 GB maximum)
[    0.000000]               0xffffffbf00008000 - 0xffffffbf06000000   (    95 MB actual)
[    0.000000]     memory  : 0xffffffc000200000 - 0xffffffc180000000   (  6142 MB)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=4, Nodes=1
[    0.000000] ftrace: allocating 36277 entries in 142 pages
[    0.000000] Preemptible hierarchical RCU implementation.
[    0.000000]  Tasks RCU enabled.
[    0.000000] NR_IRQS: 64, nr_irqs: 64, preallocated irqs: 0
[    0.000000] parent_rate: 0,  dclk->rate:2666000000, pre_ddr_rate:0, res.a0:139716712
[    0.000000] arch_timer: cp15 timer(s) running at 24.00MHz (virt).
[    0.000000] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0x588fe9dc0, max_idle_ns: 440795202592 ns
[    0.000004] sched_clock: 56 bits at 24MHz, resolution 41ns, wraps every 4398046511097ns
[    0.001191] clocksource: hobot_clocksource: mask: 0xffffffffffffffff max_cycles: 0x1d854df40, max_idle_ns: 3526361616960 ns
[    0.002963] Console: colour dummy device 80x25
[    0.003534] Calibrating delay loop (skipped), value calculated using timer frequency.. 48.00 BogoMIPS (lpj=96000)
[    0.004839] pid_max: default: 32768 minimum: 301
[    0.005494] Security Framework initialized
[    0.006012] AppArmor: AppArmor disabled by boot time parameter
[    0.006855] Mount-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.007724] Mountpoint-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.023765] ASID allocator initialised with 65536 entries
[    0.031763] Hierarchical SRCU implementation.
[    0.063822] smp: Bringing up secondary CPUs ...
[    0.100029] Detected VIPT I-cache on CPU1
[    0.100064] CPU1: Booted secondary processor [410fd034]
[    0.136078] Detected VIPT I-cache on CPU2
[    0.136099] CPU2: Booted secondary processor [410fd034]
[    0.172137] Detected VIPT I-cache on CPU3
[    0.172157] CPU3: Booted secondary processor [410fd034]
[    0.172211] smp: Brought up 1 node, 4 CPUs
[    0.176273] SMP: Total of 4 processors activated.
[    0.176868] CPU features: detected feature: 32-bit EL0 Support
[    0.177686] CPU: All CPU(s) started at EL1
[    0.178214] alternatives: patching kernel code
[    0.179802] devtmpfs: initialized
[    0.188876] random: get_random_u32 called from bucket_table_alloc+0x108/0x270 with crng_init=0
[    0.190453] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 7645041785100000 ns
[    0.191699] futex hash table entries: 1024 (order: 5, 131072 bytes)
[    0.208222] xor: automatically using best checksumming function   32regs
[    0.209159] pinctrl core: initialized pinctrl subsystem
[    0.210396] NET: Registered protocol family 16
[    0.211719] vdso: 2 pages (1 code @ ffffff8008a46000, 1 data @ ffffff8009104000)
[    0.212664] hw-breakpoint: found 6 breakpoint and 4 watchpoint registers.
[    0.214255] DMA: preallocated 256 KiB pool for atomic allocations
[    0.219089] pstore: using zlib compression
[    0.219883] console [pstore-1] enabled
[    0.220479] pstore: Registered ramoops as persistent store backend
[    0.221263] ramoops: attached 0x40000@0x3fc0000, ecc: 0/0
[    0.226264] hobot_dma a1005000.dma: Hobot DMA Engine Driver Probed!!
[    0.239769] SCSI subsystem initialized
[    0.240425] media: Linux media interface: v0.10
[    0.241020] Linux video capture interface: v2.00
[    0.241661] pps_core: LinuxPPS API ver. 1 registered
[    0.242289] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.243464] PTP clock support registered
[    0.244633] ion_dummy: not reserve carveout memory, try to alloc from cma
[    0.381348] Advanced Linux Sound Architecture Driver Initialized.
[    0.382516] usbcore: registered new interface driver usbfs
[    0.383242] usbcore: registered new interface driver hub
[    0.383969] usbcore: registered new device driver usb
[    0.384927] clocksource: Switched to clocksource arch_sys_counter
[    0.432689] VFS: Disk quotas dquot_6.6.0
[    0.433262] VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
[    0.434203] FS-Cache: Loaded
[    0.434689] CacheFiles: Loaded
[    0.440042] NET: Registered protocol family 2
[    0.441010] TCP established hash table entries: 32768 (order: 6, 262144 bytes)
[    0.442129] TCP bind hash table entries: 32768 (order: 7, 524288 bytes)
[    0.443380] TCP: Hash tables configured (established 32768 bind 32768)
[    0.444286] UDP hash table entries: 2048 (order: 4, 65536 bytes)
[    0.445143] UDP-Lite hash table entries: 2048 (order: 4, 65536 bytes)
[    0.446140] NET: Registered protocol family 1
[    0.446977] RPC: Registered named UNIX socket transport module.
[    0.447729] RPC: Registered udp transport module.
[    0.448325] RPC: Registered tcp transport module.
[    0.448946] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.450443] hw perfevents: enabled with armv8_cortex_a53 PMU driver, 7 counters available
[    0.452670] audit: initializing netlink subsys (disabled)
[    0.453624] audit: type=2000 audit(0.452:1): state=initialized audit_enabled=0 res=1
[    0.453906] Initialise system trusted keyrings
[    0.453980] workingset: timestamp_bits=46 max_order=20 bucket_order=0
[    0.457604] zbud: loaded
[    0.459167] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.460026] exFAT: Version 1.2.9
[    0.460506] FS-Cache: Netfs 'nfs' registered for caching
[    0.461796] NFS: Registering the id_resolver key type
[    0.462450] Key type id_resolver registered
[    0.462977] Key type id_legacy registered
[    0.463492] nfs4filelayout_init: NFSv4 File Layout Driver Registering...
[    0.464345] Installing knfsd (copyright (C) 1996 okir@monad.swb.de).
[    0.468406] NET: Registered protocol family 38
[    0.469018] async_tx: api initialized (async)
[    0.469572] Key type asymmetric registered
[    0.470090] Asymmetric key parser 'x509' registered
[    0.470777] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 245)
[    0.471796] io scheduler noop registered
[    0.472453] io scheduler cfq registered (default)
[    0.473070] io scheduler mq-deadline registered
[    0.473643] io scheduler kyber registered
[    0.474835] pinctrl-single a6003170.pinctrl_voltag: 64 pins at pa ffffff8009c4d170 size 8
[    0.476174] pinctrl-single a6004000.pinctrl: 128 pins at pa ffffff8009c61000 size 512
[    0.477559] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: start probe
[    0.478451] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: probe ok
[    0.479324] gpio-x3 a6003000.gpio: x3 gpio probe start!!!
[    0.480015] gpio-x3 a6003000.gpio: x3 gpio add gpiochip start!!!
[    0.480988] gpio-x3 a6003000.gpio: diable all gpio irq
[    0.483239] gpio-x3 a6003000.gpio: irqbase:57
[    0.483791] gpio-x3 a6003000.gpio: x3 irq add start!!!
[    0.484451] irq: Cannot allocate irq_descs @ IRQ57, assuming pre-allocated
[    0.485499] gpio-x3 a6003000.gpio: x3 irq add ok!!!
[    0.486153] gpio-x3 a6003000.gpio: x3 irqchip ops add ok!!!
[    0.486858] gpio-x3 a6003000.gpio: x3 gpio probe ok!!!
[    0.487967] hobot-pwm: hobot-pwmchip0 registered
[    0.488719] hobot-pwm: hobot-pwmchip1 registered
[    0.490102] diag dev [ver:1.1] init done
[    0.490997] hobot_ddr_monitor: LPDDR4 detected
[    0.491757] hobot_ddr_monitor: ddr monitor init finished.
[    0.492154] [vcam] init start
[    0.493301] vcam probe start
[    0.493769] vcam probe end successful
[    0.494229] [vcam] init end
[    0.495155] a5000000.serial: ttyS0 at MMIO 0xa5000000 (irq = 10, base_baud = 12000000) is a hobot-uart
[    0.496366] console [ttyS0] enabled
[    0.496366] console [ttyS0] enabled
[    0.497268] bootconsole [hobot0] disabled
[    0.497268] bootconsole [hobot0] disabled
[    0.498591] hobot-uart a5001000.serial: Failed to create debugfs root directory
[    0.499594] a5001000.serial: ttyS1 at MMIO 0xa5001000 (irq = 11, base_baud = 12000000) is a hobot-uart
[    0.501165] hobot-uart a5003000.serial: Failed to create debugfs root directory
[    0.502166] a5003000.serial: ttyS3 at MMIO 0xa5003000 (irq = 12, base_baud = 12000000) is a hobot-uart
[    0.503692] KGDB: Registered I/O driver kgdboc
[    0.504521] cacheinfo: Unable to detect cache hierarchy for CPU 0
[    0.509991] brd: module loaded
[    0.514589] loop: module loaded
[    0.516123] spi-nand hr_nand.0: GigaDevice SPI NAND was found.
[    0.516883] spi-nand hr_nand.0: 128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
[    0.519567] hobot_spi a5006000.spi: ver: HOBOT-spi_V20.200330 master
[    0.520610] libphy: Fixed MDIO Bus: probed
[    0.521947] st_gmac a5014000.ethernet: found phy-handle subnode
[    0.522783] st_gmac a5014000.ethernet: xj3_mtl_setup, plat->rx-queues-to-use:4, and tx:4
[    0.523967] st_gmac a5014000.ethernet: xj3_probe_config_dt, clk_ptp_rate:250000000
[    0.524986] set mac address 00:11:22:22:a4:83:
[    0.524988] (using random mac adress)
[    0.526032] (NULL device *): xj3_get_hw_features, tx_fifo_size:16384
[    0.526849] (NULL device *): xj3_get_hw_features, rx_fifo_size:16384
[    0.527666] st_gmac a5014000.ethernet: TSO supported
[    0.528306] st_gmac a5014000.ethernet: TSO feature enabled
[    0.529114] st_gmac a5014000.ethernet: Enable Rx Mitigation via HW Watchdog Timer
[    0.650183] libphy: hobot-mac-mdio: probed
[    0.651738] st_gmac a5014000.ethernet: hobot_eth_probe: probe sucessfully
[    0.652958] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_0v8 not found, using dummy regulator
[    0.654179] dwc3-of-simple b2000000.usb: usb regulator 0v8 enable succeed
[    0.655056] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_3v3 not found, using dummy regulator
[    0.656268] dwc3-of-simple b2000000.usb: usb regulator 3v3 enable succeed
[    0.657814] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    0.659471] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    0.660907] usbcore: registered new interface driver cdc_acm
[    0.661661] cdc_acm: USB Abstract Control Model driver for USB modems and ISDN adapters
[    0.662720] usbcore: registered new interface driver uas
[    0.663436] usbcore: registered new interface driver usb-storage
[    0.664262] usbcore: registered new interface driver usbserial
[    0.665056] usbcore: registered new interface driver usbserial_generic
[    0.665917] usbserial: USB Serial support registered for generic
[    0.666712] usbcore: registered new interface driver usb_serial_simple
[    0.667569] usbserial: USB Serial support registered for carelink
[    0.668370] usbserial: USB Serial support registered for zio
[    0.669136] usbserial: USB Serial support registered for funsoft
[    0.669928] usbserial: USB Serial support registered for flashloader
[    0.670762] usbserial: USB Serial support registered for google
[    0.671543] usbserial: USB Serial support registered for libtransistor
[    0.672399] usbserial: USB Serial support registered for vivopay
[    0.673211] usbserial: USB Serial support registered for moto_modem
[    0.674034] usbserial: USB Serial support registered for motorola_tetra
[    0.674902] usbserial: USB Serial support registered for novatel_gps
[    0.675736] usbserial: USB Serial support registered for hp4x
[    0.676496] usbserial: USB Serial support registered for suunto
[    0.677295] usbserial: USB Serial support registered for siemens_mpi
[    0.678140] usbcore: registered new interface driver rio500
[    0.678969] mousedev: PS/2 mouse device common for all mice
[    0.690014] hobot-rtc a6002000.rtc: rtc core: registered hobot-rtc as rtc0
[    0.691008] i2c /dev entries driver
[    0.691620] hobot-i2c a5009000.i2c: hobot i2c probe start
[    0.692383] hobot-i2c a5009000.i2c: round_rate:96000000
[    0.693082] hobot-i2c a5009000.i2c: I2C bus speed is 400000
[    0.693800] hobot-i2c a5009000.i2c: clkdiv = 0x1d
[    0.694407] hobot-i2c a5009000.i2c: i2c0 diag register....
[    0.695501] hobot-i2c a5009000.i2c: hobot_i2c_0 probe done
[    0.696304] hobot-i2c a500a000.i2c: hobot i2c probe start
[    0.697086] hobot-i2c a500a000.i2c: round_rate:96000000
[    0.697763] hobot-i2c a500a000.i2c: I2C bus speed is 400000
[    0.698480] hobot-i2c a500a000.i2c: clkdiv = 0x1d
[    0.699086] hobot-i2c a500a000.i2c: i2c1 diag register....
[    0.700096] hobot-i2c a500a000.i2c: hobot_i2c_1 probe done
[    0.701076] lirc_dev: IR Remote Control driver registered, major 239
[    0.701894] IR LIRC bridge handler initialized
[    0.702644] sif_mclk clock frequence is 544000000
[    0.703281] mipi_rx0_ipi clock frequence is 544000000
[    0.703972] mipi_rx1_ipi clock frequence is 544000000
[    0.704672] mipi_rx2_ipi clock frequence is 544000000
[    0.705404] mipi_rx3_ipi clock frequence is 544000000
[    0.706125] mipi_tx_ipi clock frequence is 544000000
[    0.706846] mipi_cfg_host clock frequence is 102000000
[    0.707599] pym_mclk clock frequence is 1188000000
[    0.708319] mipi_dev_ref clock frequence is 24000000
[    0.709094] mipi_host_ref clock frequence is 24000000
[    0.709871] sensor0_mclk clock frequence is 37125000
[    0.710646] sensor1_mclk clock frequence is 37125000
[    0.711435] sensor2_mclk clock frequence is 37125000
[    0.712234] sensor3_mclk clock frequence is 37125000
[    0.712873] [FRT:D] x3_ips_probe(0)
[    0.713908] hobot swinfo sel reg ro=0x1 boot dump
[    0.714822] pvt a1009000.pvt: SCRATCH test: 1234abcd, pvt is alive.
[    0.715745] pvt a1009000.pvt: VM Calibrated data detected
[    0.716958] hobot_wdt a1002000.watchdog: watchdog setting [pet:6s bark:11s bite:15s]
[    0.718281] hobot_wdt a1002000.watchdog: Hobot Watchdog Timer at ffffff8009db3000 with timeout 15s
[    0.719635] device-mapper: uevent: version 1.0.3
[    0.720394] device-mapper: ioctl: 4.37.0-ioctl (2017-09-20) initialised: dm-devel@redhat.com
[    0.721597] device-mapper: verity-avb: AVB error handler initialized with vbmeta device:
[    0.724009] Synopsys Designware Multimedia Card Interface Driver
[    0.725046] dwmmc_hobot a5010000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.725872] dwmmc_hobot a5010000.dwmmc: card-detect-delay not found.
[    0.726691] dwmmc_hobot a5010000.dwmmc: data-addr not found.
[    0.727733] mmc_host mmc0: card is non-removable.
[    0.766144] dwmmc_hobot a5011000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.768976] dwmmc_hobot a5011000.dwmmc: card-detect-delay not found.
[    0.769803] dwmmc_hobot a5011000.dwmmc: data-addr not found.
[    0.774576] dwmmc_hobot a5011000.dwmmc: mmc set to fixed voltage 1800
[    0.775635] mmc_host mmc1: card is non-removable.
[    0.873115] dwmmc_hobot a5012000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.873934] dwmmc_hobot a5012000.dwmmc: card-detect-delay not found.
[    0.874770] dwmmc_hobot a5012000.dwmmc: data-addr not found.
[    0.875736] dwmmc_hobot a5012000.dwmmc: Got CD GPIO
[    0.986688] mmc1: queuing unknown CIS tuple 0x80 (2 bytes)
[    0.988883] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.991085] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.994461] mmc1: queuing unknown CIS tuple 0x80 (7 bytes)
[    0.998425] mmc1: queuing unknown CIS tuple 0x81 (9 bytes)
[    1.065265] ledtrig-cpu: registered to indicate activity on CPUs
[    1.066100] hidraw: raw HID events driver (C) Jiri Kosina
[    1.066976] usbcore: registered new interface driver usbhid
[    1.067700] usbhid: USB HID core driver
[    1.068315] logger: created 256K log 'log_main'
[    1.068992] logger: created 256K log 'log_events'
[    1.069669] logger: created 256K log 'log_radio'
[    1.070334] logger: created 256K log 'log_system'
[    1.071390] set dmc devfreq governor to performance
[    1.072039] hobot_dmcfreq_target: dmcfreq->rate:2666000000, target_rate:2666000000
[    1.073051] buf:, powersave_rate:2666000000, dmcfreq->pre_state:0
[    1.079924] usbcore: registered new interface driver snd-usb-audio
[    1.081158] Netfilter messages via NETLINK v0.30.
[    1.081800] ip_set: protocol 6
[    1.082296] ipip: IPv4 and MPLS over IPv4 tunneling driver
[    1.083324] ip_tables: (C) 2000-2006 Netfilter Core Team
[    1.084260] arp_tables: arp_tables: (C) 2002 David S. Miller
[    1.085088] Initializing XFRM netlink socket
[    1.085981] NET: Registered protocol family 10
[    1.087262] Segment Routing with IPv6
[    1.087770] sit: IPv6, IPv4 and MPLS over IPv4 tunneling driver
[    1.088875] NET: Registered protocol family 17
[    1.089559] Key type dns_resolver registered
[    1.091185] Loading compiled-in X.509 certificates
[    1.094699] Loaded X.509 cert 'Build time autogenerated kernel key: 81cb0ef77db2fac76e9588c2120c82422367d268'
[    1.096030] zswap: loaded using pool lzo/zbud
[    1.107309] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    1.108991] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    1.109963] console [netcon0] enabled
[    1.110438] netconsole: network logging started
[    1.111220] hobot-rtc a6002000.rtc: setting system clock to 1970-01-01 00:00:00 UTC (0)
[    1.112404] vps mipi_dphy: probe with x3vio done
[    1.113272] hobot_wdt_test: wdt_test_init: wdt test init
[    1.115988] VCC_CNN0: disabling
[    1.116398] VCC_CNN1: disabling
[    1.117378] vps mipi_host0: ver 140* port0(0:0)
[    1.118285] vps mipi_host1: ver 140* port1(1:0)
[    1.119178] vps mipi_host2: ver 140* port2(0:1)
[    1.119967] vps mipi_host3: ver 140* port3(1:1)
[    1.120801] ALSA device list:
[    1.121198]   No soundcards found.
[    1.121835] md: Skipping autodetection of RAID arrays. (raid=autodetect will force)
[    1.122970] VFS: Cannot open root device "mmcblk2p2" or unknown-block(0,0): error -6
[    1.123964] Please append a correct "root=" boot option; here are the available partitions:
[    1.125066] 0100          102400 ram0
[    1.125068]  (driver?)
[    1.125858] 0101          102400 ram1
[    1.125860]  (driver?)
[    1.126648] 0102          102400 ram2
[    1.126650]  (driver?)
[    1.127438] 0103          102400 ram3
[    1.127440]  (driver?)
[    1.128228] 0104          102400 ram4
[    1.128230]  (driver?)
[    1.129062] 0105          102400 ram5
[    1.129064]  (driver?)
[    1.129853] 0106          102400 ram6
[    1.129854]  (driver?)
[    1.130643] 0107          102400 ram7
[    1.130644]  (driver?)
[    1.131432] 0108          102400 ram8
[    1.131434]  (driver?)
[    1.132222] 0109          102400 ram9
[    1.132224]  (driver?)
[    1.133038] 010a          102400 ram10
[    1.133040]  (driver?)
[    1.133840] 010b          102400 ram11
[    1.133842]  (driver?)
[    1.134641] 010c          102400 ram12
[    1.134643]  (driver?)
[    1.135442] 010d          102400 ram13
[    1.135444]  (driver?)
[    1.136243] 010e          102400 ram14
[    1.136245]  (driver?)
[    1.137075] 010f          102400 ram15
[    1.137077]  (driver?)
[    1.137879] 1f00          131072 mtdblock0
[    1.137881]  (driver?)
[    1.138725] hobot_fusa: set_fusa_error_pin:75 set error pin to 1
[    1.139495] hobot_fusa: fusa errpin not ready
[    1.139499] Kernel panic - not syncing: VFS: Unable to mount root fs on unknown-block(0,0)
[    1.141118] Kernel Offset: disabled
[    1.141569] CPU features: 0x0002004
[    1.142019] Memory Limit: none
[    1.146578] Rebooting in 1 seconds..
[    1.217176] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.217898] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 1
[    1.219354] xhci-hcd xhci-hcd.0.auto: hcc params 0x0220fe6d hci version 0x110 quirks 0x0000000000010010
[    1.220589] xhci-hcd xhci-hcd.0.auto: irq 178, io mem 0xb2000000
[    1.221565] usb usb1: New USB device found, idVendor=1d6b, idProduct=0002, bcdDevice= 4.14
[    1.222628] usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.223557] usb usb1: Product: xHCI Host Controller
[    1.224186] usb usb1: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.224892] usb usb1: SerialNumber: xhci-hcd.0.auto
[    1.225848] hub 1-0:1.0: USB hub found
[    1.226350] hub 1-0:1.0: 1 port detected
[    1.227038] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.227751] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 2
[    1.228742] xhci-hcd xhci-hcd.0.auto: Host supports USB 3.0 SuperSpeed
[    1.229634] usb usb2: We don't know the algorithms for LPM for this host, disabling LPM.
[    1.230736] usb usb2: New USB device found, idVendor=1d6b, idProduct=0003, bcdDevice= 4.14
[    1.231799] usb usb2: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.232727] usb usb2: Product: xHCI Host Controller
[    1.233365] usb usb2: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.234073] usb usb2: SerialNumber: xhci-hcd.0.auto
[    1.234147] mmc1: new HSSDIO card at address 0001
[    1.235586] hub 2-0:1.0: USB hub found
[    1.236090] hub 2-0:1.0: 1 port detected
[    1.480936] usb 1-1: new high-speed USB device number 2 using xhci-hcd
[    1.629121] usb 1-1: New USB device found, idVendor=1a40, idProduct=0101, bcdDevice= 1.11
[    1.630173] usb 1-1: New USB device strings: Mfr=0, Product=1, SerialNumber=0
[    1.631091] usb 1-1: Product: USB 2.0 Hub
[    1.677799] hub 1-1:1.0: USB hub found
[    1.678317] hub 1-1:1.0: 4 ports detected
[    1.964938] mmc2: new UHS SDR104 SDHC card at address 0001
[    1.965965] mmcblk2: mmc2:0001 SD16G 29.8 GiB
[    1.967574]  mmcblk2: p1 p2
[    2.147091] SMP: stopping secondary CPUs
[    2.147599] psci: psci_sys_reset(reboot_mode=0)
NOTICE:  fast_boot:0

S
F
L
O
NOTICE:  efuse cpu_cfg = 0
W
NOTICE:  Booting Trusted Firmware
NOTICE:  BL1: v1.4(release):HR-ROM-Rel-v1.1-141-ga91d4dd-dirty
NOTICE:  BL1: Built : 11:24:44, Oct 23 2019
NOTICE:  boot src: 2
NOTICE:  GigaDev SPI NAND was found.
NOTICE:  Block size: 128 KiB, page size: 2048
NOTICE:  BL1: Booting BL2
Auth pass
NOTICE:  bl1_main exit
SPL normal reset flow
check_reset_state (2): wakeup address = 0x0, hw wakeup status = 0x3, wakeup src=0x100
patch for sys_pll 1200 with 100M eth
SFLOW_INIT
CHIP ID:PCB941/WAFER: W04/ X: X20/ Y: Y36
secondary_jump_to_spl: secure chip flow
X3 SPL : secondary core wake up and jump to spl done (cpu_core_cfg=0)
SFLOW_FIN_HW_A

U-Boot SPL 2018.09-g4ca851534c-dirty (May 11 2022 - 20:09:50 +0800)
SPACC Init - ID: (00000061)
SPL nand boot mode (from strap)
GigaDev SPI NAND was found.
Block size: 128 KiB, page size: 2048
ddr_type = 1 (LPDDR4)
hb_chip_package_type:3
load ddr header src_addr: 100000, load_addr: 802ca020, src_len: a00
find valid ddr image
ddr_hdr.ecc_gran: 0x0
ddr_hdr.ecc_map: 0x0
ddr_hdr.sbr_pattern0: 0x0
ddr_hdr.sbr_pattern1: 0x0
ddr_freq = 05
board id = 31540334
ddr datarate: 3200
### SAMSUNG DDR ###
no ddr pin set
detect part number: 108
detect ddr freq: c80
board id alternative:0x3
index is 12
index is 15
index is 19
hb_ddr_index: 19
ddr_type = 1, ddr_vendor=3, ddr_freq=3200
dram_pll_init
sscg disabled
control load ddrc src_addr: 15ae00, load_addr: 802caa20, src_len: 920
[DDR INFO]      ==ddr_release_info==
[DDR INFO]      VERSION:        develop
[DDR INFO]      BUILD:          2022-05-11-20:09
[DDR INFO]      GIT COMMIT:     4ca851534c1616ace920fdaa000c6fb717c1fb74
[DDR INFO]      GIT TIME:       Wed, 20 Apr 2022 18:28:49 +0800
[DDR INFO]      ==ddr_features==
[DDR INFO]      RDBI:           0
[DDR INFO]      WDBI:           1
[DDR INFO]      InlineECC:      0
[DDR INFO]      DM:             1
[DDR INFO]      DDC:            1
[DDR INFO]      SSCG:           0
[DDR INFO]      BOARD:          XS_ENABLE
[DDR INFO] ddr_controller_cfg done
load ddr phy src_addr: 15b800, load_addr: 802caa20, src_len: 420
ATxSlewRate     : 15f
ATxImpedance    : 7f
TxSlewRate      : 19f
TxOdtDrvStren   : 600
TxImpedanceCtrl : e3f
CalDrvStr0      : 11
VrefInGlobal    : 104
board_type = 4 (CUSTOMER_BOARD)
load dqmap src addr: 15d600, load_addr: 802caa20, src_len: 20
[DDR INFO] dwc_ddrphy_train start
magic = 544f4248
load imem1 src_addr: 11ce00, load_addr: 802caa20, src_len: 8000
load dmem1 src_addr: 15a000, load_addr: 802caa20, src_len: 684
executing 1D fw
load imem2 src_addr: 124e00, load_addr: 802caa20, src_len: 8000
load dmem2 src_addr: 15a800, load_addr: 802caa20, src_len: 564

*******************************************************
p_dmem_lpddr4_2d_16b->MR11_A0:54
p_dmem_lpddr4_2d_16b->MR14_A0:54
p_dmem_lpddr4_2d_16b->MR12_A0:51
p_dmem_lpddr4_2d_16b->MR22_A0:14

p_dmem_lpddr4_2d_16b->MR3_A0:b3
p_dmem_lpddr4_2d_16b->Reserved00:40
p_dmem_lpddr4_2d_16b->Reserved0E:4
p_dmem_lpddr4_2d_16b->Delay_Weight2D:20
p_dmem_lpddr4_2d_16b->Voltage_Weight2D:80
*******************************************************

executing 2D fw
load pie src_addr: 15be00, load_addr: 802caa20, src_len: 11f0
Set QoS.
get_ddr_mr_info:cs_num=1, mr5=0x1, mr8=0x10
no magic in efuse file,bypass efuse
total_sz = 4096
SPL_VERSION:7
uboot partition is uboot_A
load u-boot: src_addr=0x380000, dest_addr=0x4000000, len=2097152
load warm boot spl: addr=0x800, dest_addr=0x80000000, len=31232
load bl31: addr=0x300000, dest_addr=0x0, len=524288
SFLOW_AUTH_BL31
verify signature of header:  verify ok!
verify signature of image:  verify ok!
bypass bpu image
clear keybank!!!!
SFLOW_DBG_EN
Trying to boot from RAM
SPL: bl31 will jump to u-boot or other entry (0x4000000)
SFLOW_CLR_KEY
SFLOW_REG_LD
install_portal copy portal
install_portal call smc and jump to bl31 cold entry(0x0)
hb som type: 5
X3 PI reset VDD_SD done

U-Boot 2018.09-g40785bca (May 27 2022 - 16:30:48 +0800)

Model: Hobot XJ3 Soc Board
DRAM:  system DDR size: 0xffe00000
4 GiB
MMC:   dwmmc@A5010000: 0, dwmmc@A5011000: 1, dwmmc@A5012000: 2
Loading Environment from UBI... GigaDevice SPI NAND was found.
128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
*** Warning - bad CRC, using default environment

In:    serial@a5000000
Out:   serial@a5000000
Err:   serial@a5000000
Net:   x3 sdb reset eth phy done

Warning: ethernet@A5014000 (eth0) using random MAC address - 0e:52:2b:57:9c:d6
eth0: ethernet@A5014000
Disable cnn cores ..
dtb_name:hobot-x3-pi.dtb
base board type: X3 SDB
bootmode: NAND
board_id = 31540334
damaged volume, update marker is setdamaged volume, update marker is setdamaged volume, update marker is sethb_boot_args_cmd_set custom_bootargs 0 ubuntu_boot 0
Hit any key to stop autoboot:  0
enable watchdog success !
switch to partitions #0, OK
mmc2 is current device
Scanning mmc 2:2...
Found U-Boot script /boot/boot.scr
664 bytes read in 1 ms (648.4 KiB/s)
## Executing script at 03c10000
Boot script loaded from devtype:mmc devnum:2 devplist:2
bootargs = console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
Loading fdt file: /boot/hobot/hobot-x3-pi.dtb
69633 bytes read in 8 ms (8.3 MiB/s)
Loading kernel: /boot/Image
19163144 bytes read in 845 ms (21.6 MiB/s)
## Flattened Device Tree blob at 03c00000
   Booting using the fdt blob at 0x3c00000
   Loading Device Tree to 0000000003c00000, end 0000000003c1ffff ... OK
chip_id: ab36300
The address of the fdt is 0x3c00000
Changed status Done
Can't get fdt_addr !!!Orign(MAX) bpu model Reserve Mem Size to 64M!!

Starting kernel ...

[    0.000000] OF: reserved mem: OVERLAP DETECTED!
[    0.000000] image_r5_mem (0x0000000080000000--0x0000000080010000) overlaps with msg_r5_mem (0x000000008000f000--0x0000000080010000)
[    0.000000] Reserved memory: created CMA memory pool at 0x0000000004000000, size 672 MiB
[    0.000000] OF: reserved mem: initialized node ion_cma, compatible id shared-dma-pool
[    0.000000] cma: Reserved 16 MiB at 0x000000007f000000
[    0.000000] On node 0 totalpages: 1047808
[    0.000000]   DMA zone: 8180 pages used for memmap
[    0.000000]   DMA zone: 0 pages reserved
[    0.000000]   DMA zone: 523520 pages, LIFO batch:31
[    0.000000]   Normal zone: 8192 pages used for memmap
[    0.000000]   Normal zone: 524288 pages, LIFO batch:31
[    0.000000] psci: probing for conduit method from DT.
[    0.000000] psci: PSCIv1.1 detected in firmware.
[    0.000000] psci: Using standard PSCI v0.2 function IDs
[    0.000000] psci: MIGRATE_INFO_TYPE not supported.
[    0.000000] psci: SMC Calling Convention v1.1
[    0.000000] percpu: Embedded 25 pages/cpu @ffffffc17ff2a000 s65176 r8192 d29032 u102400
[    0.000000] pcpu-alloc: s65176 r8192 d29032 u102400 alloc=25*4096
[    0.000000] pcpu-alloc: [0] 0 [0] 1 [0] 2 [0] 3
[    0.000000] Detected VIPT I-cache on CPU0
[    0.000000] CPU features: enabling workaround for ARM erratum 845719
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 1031436
[    0.000000] Kernel command line: earlycon loglevel=8 kgdboc=ttyS0 video=hobot:x3sdb-hdmi  console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
[    0.000000] PID hash table entries: 4096 (order: 3, 32768 bytes)
[    0.000000] Dentry cache hash table entries: 524288 (order: 10, 4194304 bytes)
[    0.000000] Inode-cache hash table entries: 262144 (order: 9, 2097152 bytes)
[    0.000000] software IO TLB [mem 0x7afff000-0x7efff000] (64MB) mapped at [ffffffc07afff000-ffffffc07effefff]
[    0.000000] Memory: 3319580K/4191232K available (10494K kernel code, 1306K rwdata, 5756K rodata, 1088K init, 9553K bss, 167140K reserved, 704512K cma-reserved)
[    0.000000] Virtual kernel memory layout:
[    0.000000]     modules : 0xffffff8000000000 - 0xffffff8008000000   (   128 MB)
[    0.000000]     vmalloc : 0xffffff8008000000 - 0xffffffbebfff0000   (   250 GB)
[    0.000000]       .text : 0xffffff8008000000 - 0xffffff8008a40000   ( 10496 KB)
[    0.000000]     .rodata : 0xffffff8008a40000 - 0xffffff8008ff0000   (  5824 KB)
[    0.000000]       .init : 0xffffff8008ff0000 - 0xffffff8009100000   (  1088 KB)
[    0.000000]       .data : 0xffffff8009100000 - 0xffffff8009246808   (  1307 KB)
[    0.000000]        .bss : 0xffffff8009246808 - 0xffffff8009b9aed8   (  9554 KB)
[    0.000000]     fixed   : 0xffffffbefe7fd000 - 0xffffffbefec00000   (  4108 KB)
[    0.000000]     PCI I/O : 0xffffffbefee00000 - 0xffffffbeffe00000   (    16 MB)
[    0.000000]     vmemmap : 0xffffffbf00000000 - 0xffffffc000000000   (     4 GB maximum)
[    0.000000]               0xffffffbf00008000 - 0xffffffbf06000000   (    95 MB actual)
[    0.000000]     memory  : 0xffffffc000200000 - 0xffffffc180000000   (  6142 MB)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=4, Nodes=1
[    0.000000] ftrace: allocating 36277 entries in 142 pages
[    0.000000] Preemptible hierarchical RCU implementation.
[    0.000000]  Tasks RCU enabled.
[    0.000000] NR_IRQS: 64, nr_irqs: 64, preallocated irqs: 0
[    0.000000] parent_rate: 0,  dclk->rate:2666000000, pre_ddr_rate:0, res.a0:139716712
[    0.000000] arch_timer: cp15 timer(s) running at 24.00MHz (virt).
[    0.000000] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0x588fe9dc0, max_idle_ns: 440795202592 ns
[    0.000003] sched_clock: 56 bits at 24MHz, resolution 41ns, wraps every 4398046511097ns
[    0.001194] clocksource: hobot_clocksource: mask: 0xffffffffffffffff max_cycles: 0x1d854df40, max_idle_ns: 3526361616960 ns
[    0.002968] Console: colour dummy device 80x25
[    0.003539] Calibrating delay loop (skipped), value calculated using timer frequency.. 48.00 BogoMIPS (lpj=96000)
[    0.004845] pid_max: default: 32768 minimum: 301
[    0.005498] Security Framework initialized
[    0.006016] AppArmor: AppArmor disabled by boot time parameter
[    0.006860] Mount-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.007728] Mountpoint-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.023769] ASID allocator initialised with 65536 entries
[    0.031767] Hierarchical SRCU implementation.
[    0.063827] smp: Bringing up secondary CPUs ...
[    0.100034] Detected VIPT I-cache on CPU1
[    0.100069] CPU1: Booted secondary processor [410fd034]
[    0.136083] Detected VIPT I-cache on CPU2
[    0.136104] CPU2: Booted secondary processor [410fd034]
[    0.172143] Detected VIPT I-cache on CPU3
[    0.172163] CPU3: Booted secondary processor [410fd034]
[    0.172217] smp: Brought up 1 node, 4 CPUs
[    0.176280] SMP: Total of 4 processors activated.
[    0.176874] CPU features: detected feature: 32-bit EL0 Support
[    0.177693] CPU: All CPU(s) started at EL1
[    0.178222] alternatives: patching kernel code
[    0.179810] devtmpfs: initialized
[    0.188916] random: get_random_u32 called from bucket_table_alloc+0x108/0x270 with crng_init=0
[    0.190487] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 7645041785100000 ns
[    0.191732] futex hash table entries: 1024 (order: 5, 131072 bytes)
[    0.208305] xor: automatically using best checksumming function   32regs
[    0.209244] pinctrl core: initialized pinctrl subsystem
[    0.210477] NET: Registered protocol family 16
[    0.211800] vdso: 2 pages (1 code @ ffffff8008a46000, 1 data @ ffffff8009104000)
[    0.212744] hw-breakpoint: found 6 breakpoint and 4 watchpoint registers.
[    0.214332] DMA: preallocated 256 KiB pool for atomic allocations
[    0.219155] pstore: using zlib compression
[    0.219950] console [pstore-1] enabled
[    0.220550] pstore: Registered ramoops as persistent store backend
[    0.221335] ramoops: attached 0x40000@0x3fc0000, ecc: 0/0
[    0.226343] hobot_dma a1005000.dma: Hobot DMA Engine Driver Probed!!
[    0.239189] SCSI subsystem initialized
[    0.239815] media: Linux media interface: v0.10
[    0.240449] Linux video capture interface: v2.00
[    0.241099] pps_core: LinuxPPS API ver. 1 registered
[    0.241727] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.242903] PTP clock support registered
[    0.244037] ion_dummy: not reserve carveout memory, try to alloc from cma
[    0.380905] Advanced Linux Sound Architecture Driver Initialized.
[    0.382097] usbcore: registered new interface driver usbfs
[    0.382825] usbcore: registered new interface driver hub
[    0.383554] usbcore: registered new device driver usb
[    0.384501] clocksource: Switched to clocksource arch_sys_counter
[    0.432198] VFS: Disk quotas dquot_6.6.0
[    0.432780] VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
[    0.433717] FS-Cache: Loaded
[    0.434199] CacheFiles: Loaded
[    0.439460] NET: Registered protocol family 2
[    0.440382] TCP established hash table entries: 32768 (order: 6, 262144 bytes)
[    0.441528] TCP bind hash table entries: 32768 (order: 7, 524288 bytes)
[    0.442776] TCP: Hash tables configured (established 32768 bind 32768)
[    0.443686] UDP hash table entries: 2048 (order: 4, 65536 bytes)
[    0.444542] UDP-Lite hash table entries: 2048 (order: 4, 65536 bytes)
[    0.445542] NET: Registered protocol family 1
[    0.446364] RPC: Registered named UNIX socket transport module.
[    0.447115] RPC: Registered udp transport module.
[    0.447712] RPC: Registered tcp transport module.
[    0.448311] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.449822] hw perfevents: enabled with armv8_cortex_a53 PMU driver, 7 counters available
[    0.452047] audit: initializing netlink subsys (disabled)
[    0.452854] audit: type=2000 audit(0.448:1): state=initialized audit_enabled=0 res=1
[    0.453135] Initialise system trusted keyrings
[    0.453204] workingset: timestamp_bits=46 max_order=20 bucket_order=0
[    0.456990] zbud: loaded
[    0.458542] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.459402] exFAT: Version 1.2.9
[    0.459882] FS-Cache: Netfs 'nfs' registered for caching
[    0.461013] NFS: Registering the id_resolver key type
[    0.461665] Key type id_resolver registered
[    0.462192] Key type id_legacy registered
[    0.462710] nfs4filelayout_init: NFSv4 File Layout Driver Registering...
[    0.463563] Installing knfsd (copyright (C) 1996 okir@monad.swb.de).
[    0.467652] NET: Registered protocol family 38
[    0.468223] async_tx: api initialized (async)
[    0.468809] Key type asymmetric registered
[    0.469327] Asymmetric key parser 'x509' registered
[    0.470009] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 245)
[    0.471027] io scheduler noop registered
[    0.471681] io scheduler cfq registered (default)
[    0.472276] io scheduler mq-deadline registered
[    0.473000] io scheduler kyber registered
[    0.474208] pinctrl-single a6003170.pinctrl_voltag: 64 pins at pa ffffff8009c4d170 size 8
[    0.475549] pinctrl-single a6004000.pinctrl: 128 pins at pa ffffff8009c61000 size 512
[    0.476798] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: start probe
[    0.477690] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: probe ok
[    0.478559] gpio-x3 a6003000.gpio: x3 gpio probe start!!!
[    0.479249] gpio-x3 a6003000.gpio: x3 gpio add gpiochip start!!!
[    0.480168] gpio-x3 a6003000.gpio: diable all gpio irq
[    0.482428] gpio-x3 a6003000.gpio: irqbase:57
[    0.482980] gpio-x3 a6003000.gpio: x3 irq add start!!!
[    0.483636] irq: Cannot allocate irq_descs @ IRQ57, assuming pre-allocated
[    0.484832] gpio-x3 a6003000.gpio: x3 irq add ok!!!
[    0.485487] gpio-x3 a6003000.gpio: x3 irqchip ops add ok!!!
[    0.486193] gpio-x3 a6003000.gpio: x3 gpio probe ok!!!
[    0.487276] hobot-pwm: hobot-pwmchip0 registered
[    0.488027] hobot-pwm: hobot-pwmchip1 registered
[    0.489391] diag dev [ver:1.1] init done
[    0.490291] hobot_ddr_monitor: LPDDR4 detected
[    0.491067] hobot_ddr_monitor: ddr monitor init finished.
[    0.491455] [vcam] init start
[    0.492545] vcam probe start
[    0.492998] vcam probe end successful
[    0.493459] [vcam] init end
[    0.494382] a5000000.serial: ttyS0 at MMIO 0xa5000000 (irq = 10, base_baud = 12000000) is a hobot-uart
[    0.495603] console [ttyS0] enabled
[    0.495603] console [ttyS0] enabled
[    0.496644] bootconsole [hobot0] disabled
[    0.496644] bootconsole [hobot0] disabled
[    0.497974] hobot-uart a5001000.serial: Failed to create debugfs root directory
[    0.498981] a5001000.serial: ttyS1 at MMIO 0xa5001000 (irq = 11, base_baud = 12000000) is a hobot-uart
[    0.500426] hobot-uart a5003000.serial: Failed to create debugfs root directory
[    0.501446] a5003000.serial: ttyS3 at MMIO 0xa5003000 (irq = 12, base_baud = 12000000) is a hobot-uart
[    0.502983] KGDB: Registered I/O driver kgdboc
[    0.503819] cacheinfo: Unable to detect cache hierarchy for CPU 0
[    0.509271] brd: module loaded
[    0.513803] loop: module loaded
[    0.515306] spi-nand hr_nand.0: GigaDevice SPI NAND was found.
[    0.516065] spi-nand hr_nand.0: 128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
[    0.518667] hobot_spi a5006000.spi: ver: HOBOT-spi_V20.200330 master
[    0.519707] libphy: Fixed MDIO Bus: probed
[    0.520916] st_gmac a5014000.ethernet: found phy-handle subnode
[    0.521752] st_gmac a5014000.ethernet: xj3_mtl_setup, plat->rx-queues-to-use:4, and tx:4
[    0.522936] st_gmac a5014000.ethernet: xj3_probe_config_dt, clk_ptp_rate:250000000
[    0.523938] set mac address 00:11:22:15:52:c2:
[    0.523941] (using random mac adress)
[    0.525086] (NULL device *): xj3_get_hw_features, tx_fifo_size:16384
[    0.525903] (NULL device *): xj3_get_hw_features, rx_fifo_size:16384
[    0.526721] st_gmac a5014000.ethernet: TSO supported
[    0.527362] st_gmac a5014000.ethernet: TSO feature enabled
[    0.528068] st_gmac a5014000.ethernet: Enable Rx Mitigation via HW Watchdog Timer
[    0.649156] libphy: hobot-mac-mdio: probed
[    0.650688] st_gmac a5014000.ethernet: hobot_eth_probe: probe sucessfully
[    0.651886] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_0v8 not found, using dummy regulator
[    0.653132] dwc3-of-simple b2000000.usb: usb regulator 0v8 enable succeed
[    0.654010] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_3v3 not found, using dummy regulator
[    0.655211] dwc3-of-simple b2000000.usb: usb regulator 3v3 enable succeed
[    0.656753] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    0.658410] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    0.659847] usbcore: registered new interface driver cdc_acm
[    0.660596] cdc_acm: USB Abstract Control Model driver for USB modems and ISDN adapters
[    0.661654] usbcore: registered new interface driver uas
[    0.662371] usbcore: registered new interface driver usb-storage
[    0.663198] usbcore: registered new interface driver usbserial
[    0.663972] usbcore: registered new interface driver usbserial_generic
[    0.664852] usbserial: USB Serial support registered for generic
[    0.665648] usbcore: registered new interface driver usb_serial_simple
[    0.666505] usbserial: USB Serial support registered for carelink
[    0.667306] usbserial: USB Serial support registered for zio
[    0.668051] usbserial: USB Serial support registered for funsoft
[    0.668852] usbserial: USB Serial support registered for flashloader
[    0.669688] usbserial: USB Serial support registered for google
[    0.670467] usbserial: USB Serial support registered for libtransistor
[    0.671323] usbserial: USB Serial support registered for vivopay
[    0.672113] usbserial: USB Serial support registered for moto_modem
[    0.672953] usbserial: USB Serial support registered for motorola_tetra
[    0.673821] usbserial: USB Serial support registered for novatel_gps
[    0.674658] usbserial: USB Serial support registered for hp4x
[    0.675417] usbserial: USB Serial support registered for suunto
[    0.676195] usbserial: USB Serial support registered for siemens_mpi
[    0.677057] usbcore: registered new interface driver rio500
[    0.677889] mousedev: PS/2 mouse device common for all mice
[    0.688937] hobot-rtc a6002000.rtc: rtc core: registered hobot-rtc as rtc0
[    0.689929] i2c /dev entries driver
[    0.690535] hobot-i2c a5009000.i2c: hobot i2c probe start
[    0.691304] hobot-i2c a5009000.i2c: round_rate:96000000
[    0.691981] hobot-i2c a5009000.i2c: I2C bus speed is 400000
[    0.692722] hobot-i2c a5009000.i2c: clkdiv = 0x1d
[    0.693329] hobot-i2c a5009000.i2c: i2c0 diag register....
[    0.694418] hobot-i2c a5009000.i2c: hobot_i2c_0 probe done
[    0.695218] hobot-i2c a500a000.i2c: hobot i2c probe start
[    0.695971] hobot-i2c a500a000.i2c: round_rate:96000000
[    0.696670] hobot-i2c a500a000.i2c: I2C bus speed is 400000
[    0.697388] hobot-i2c a500a000.i2c: clkdiv = 0x1d
[    0.697994] hobot-i2c a500a000.i2c: i2c1 diag register....
[    0.699013] hobot-i2c a500a000.i2c: hobot_i2c_1 probe done
[    0.699972] lirc_dev: IR Remote Control driver registered, major 239
[    0.700814] IR LIRC bridge handler initialized
[    0.701567] sif_mclk clock frequence is 544000000
[    0.702203] mipi_rx0_ipi clock frequence is 544000000
[    0.702891] mipi_rx1_ipi clock frequence is 544000000
[    0.703591] mipi_rx2_ipi clock frequence is 544000000
[    0.704300] mipi_rx3_ipi clock frequence is 544000000
[    0.705040] mipi_tx_ipi clock frequence is 544000000
[    0.705760] mipi_cfg_host clock frequence is 102000000
[    0.706514] pym_mclk clock frequence is 1188000000
[    0.707241] mipi_dev_ref clock frequence is 24000000
[    0.707995] mipi_host_ref clock frequence is 24000000
[    0.708792] sensor0_mclk clock frequence is 37125000
[    0.709569] sensor1_mclk clock frequence is 37125000
[    0.710358] sensor2_mclk clock frequence is 37125000
[    0.711158] sensor3_mclk clock frequence is 37125000
[    0.711797] [FRT:D] x3_ips_probe(0)
[    0.712851] hobot swinfo sel reg ro=0x1 boot dump
[    0.713763] pvt a1009000.pvt: SCRATCH test: 1234abcd, pvt is alive.
[    0.714687] pvt a1009000.pvt: VM Calibrated data detected
[    0.715880] hobot_wdt a1002000.watchdog: watchdog setting [pet:6s bark:11s bite:15s]
[    0.717228] hobot_wdt a1002000.watchdog: Hobot Watchdog Timer at ffffff8009db3000 with timeout 15s
[    0.718584] device-mapper: uevent: version 1.0.3
[    0.719341] device-mapper: ioctl: 4.37.0-ioctl (2017-09-20) initialised: dm-devel@redhat.com
[    0.720524] device-mapper: verity-avb: AVB error handler initialized with vbmeta device:
[    0.722954] Synopsys Designware Multimedia Card Interface Driver
[    0.723952] dwmmc_hobot a5010000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.724862] dwmmc_hobot a5010000.dwmmc: card-detect-delay not found.
[    0.725681] dwmmc_hobot a5010000.dwmmc: data-addr not found.
[    0.726723] mmc_host mmc0: card is non-removable.
[    0.765704] dwmmc_hobot a5011000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.768550] dwmmc_hobot a5011000.dwmmc: card-detect-delay not found.
[    0.769378] dwmmc_hobot a5011000.dwmmc: data-addr not found.
[    0.774147] dwmmc_hobot a5011000.dwmmc: mmc set to fixed voltage 1800
[    0.775206] mmc_host mmc1: card is non-removable.
[    0.872740] dwmmc_hobot a5012000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.873558] dwmmc_hobot a5012000.dwmmc: card-detect-delay not found.
[    0.874391] dwmmc_hobot a5012000.dwmmc: data-addr not found.
[    0.875361] dwmmc_hobot a5012000.dwmmc: Got CD GPIO
[    0.983861] mmc1: queuing unknown CIS tuple 0x80 (2 bytes)
[    0.986059] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.988241] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.991618] mmc1: queuing unknown CIS tuple 0x80 (7 bytes)
[    0.995573] mmc1: queuing unknown CIS tuple 0x81 (9 bytes)
[    1.060795] ledtrig-cpu: registered to indicate activity on CPUs
[    1.061624] hidraw: raw HID events driver (C) Jiri Kosina
[    1.062452] usbcore: registered new interface driver usbhid
[    1.063169] usbhid: USB HID core driver
[    1.063746] logger: created 256K log 'log_main'
[    1.064388] logger: created 256K log 'log_events'
[    1.065075] logger: created 256K log 'log_radio'
[    1.065725] logger: created 256K log 'log_system'
[    1.066759] set dmc devfreq governor to performance
[    1.067392] hobot_dmcfreq_target: dmcfreq->rate:2666000000, target_rate:2666000000
[    1.068364] buf:, powersave_rate:2666000000, dmcfreq->pre_state:0
[    1.075193] usbcore: registered new interface driver snd-usb-audio
[    1.076333] Netfilter messages via NETLINK v0.30.
[    1.076983] ip_set: protocol 6
[    1.077466] ipip: IPv4 and MPLS over IPv4 tunneling driver
[    1.078473] ip_tables: (C) 2000-2006 Netfilter Core Team
[    1.079394] arp_tables: arp_tables: (C) 2002 David S. Miller
[    1.080181] Initializing XFRM netlink socket
[    1.081060] NET: Registered protocol family 10
[    1.082296] Segment Routing with IPv6
[    1.082806] sit: IPv6, IPv4 and MPLS over IPv4 tunneling driver
[    1.083906] NET: Registered protocol family 17
[    1.084558] Key type dns_resolver registered
[    1.086196] Loading compiled-in X.509 certificates
[    1.089717] Loaded X.509 cert 'Build time autogenerated kernel key: 81cb0ef77db2fac76e9588c2120c82422367d268'
[    1.091051] zswap: loaded using pool lzo/zbud
[    1.102318] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    1.103990] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    1.105003] console [netcon0] enabled
[    1.105478] netconsole: network logging started
[    1.106258] hobot-rtc a6002000.rtc: setting system clock to 1970-01-01 00:00:00 UTC (0)
[    1.107446] vps mipi_dphy: probe with x3vio done
[    1.108165] hobot_wdt_test: wdt_test_init: wdt test init
[    1.110955] VCC_CNN0: disabling
[    1.111365] VCC_CNN1: disabling
[    1.112326] vps mipi_host0: ver 140* port0(0:0)
[    1.113275] vps mipi_host1: ver 140* port1(1:0)
[    1.114174] vps mipi_host2: ver 140* port2(0:1)
[    1.114965] vps mipi_host3: ver 140* port3(1:1)
[    1.115796] ALSA device list:
[    1.116181]   No soundcards found.
[    1.116834] md: Skipping autodetection of RAID arrays. (raid=autodetect will force)
[    1.117969] VFS: Cannot open root device "mmcblk2p2" or unknown-block(0,0): error -6
[    1.118962] Please append a correct "root=" boot option; here are the available partitions:
[    1.120037] 0100          102400 ram0
[    1.120039]  (driver?)
[    1.120869] 0101          102400 ram1
[    1.120871]  (driver?)
[    1.121660] 0102          102400 ram2
[    1.121661]  (driver?)
[    1.122450] 0103          102400 ram3
[    1.122451]  (driver?)
[    1.123239] 0104          102400 ram4
[    1.123241]  (driver?)
[    1.124029] 0105          102400 ram5
[    1.124031]  (driver?)
[    1.124894] 0106          102400 ram6
[    1.124896]  (driver?)
[    1.125685] 0107          102400 ram7
[    1.125687]  (driver?)
[    1.126475] 0108          102400 ram8
[    1.126477]  (driver?)
[    1.127265] 0109          102400 ram9
[    1.127266]  (driver?)
[    1.128054] 010a          102400 ram10
[    1.128056]  (driver?)
[    1.128887] 010b          102400 ram11
[    1.128889]  (driver?)
[    1.129688] 010c          102400 ram12
[    1.129690]  (driver?)
[    1.130489] 010d          102400 ram13
[    1.130491]  (driver?)
[    1.131290] 010e          102400 ram14
[    1.131291]  (driver?)
[    1.132090] 010f          102400 ram15
[    1.132092]  (driver?)
[    1.132911] 1f00          131072 mtdblock0
[    1.132913]  (driver?)
[    1.133756] hobot_fusa: set_fusa_error_pin:75 set error pin to 1
[    1.134527] hobot_fusa: fusa errpin not ready
[    1.134530] Kernel panic - not syncing: VFS: Unable to mount root fs on unknown-block(0,0)
[    1.136149] Kernel Offset: disabled
[    1.136600] CPU features: 0x0002004
[    1.137050] Memory Limit: none
[    1.141601] Rebooting in 1 seconds..
[    2.142113] SMP: stopping secondary CPUs
[    2.142621] psci: psci_sys_reset(reboot_mode=0)
NOTICE:  fast_boot:0

S
F
L
O
NOTICE:  efuse cpu_cfg = 0
W
NOTICE:  Booting Trusted Firmware
NOTICE:  BL1: v1.4(release):HR-ROM-Rel-v1.1-141-ga91d4dd-dirty
NOTICE:  BL1: Built : 11:24:44, Oct 23 2019
NOTICE:  boot src: 2
NOTICE:  GigaDev SPI NAND was found.
NOTICE:  Block size: 128 KiB, page size: 2048
NOTICE:  BL1: Booting BL2
Auth pass
NOTICE:  bl1_main exit
SPL normal reset flow
check_reset_state (2): wakeup address = 0x0, hw wakeup status = 0x3, wakeup src=0x100
patch for sys_pll 1200 with 100M eth
SFLOW_INIT
CHIP ID:PCB941/WAFER: W04/ X: X20/ Y: Y36
secondary_jump_to_spl: secure chip flow
X3 SPL : secondary core wake up and jump to spl done (cpu_core_cfg=0)
SFLOW_FIN_HW_A

U-Boot SPL 2018.09-g4ca851534c-dirty (May 11 2022 - 20:09:50 +0800)
SPACC Init - ID: (00000061)
SPL nand boot mode (from strap)
GigaDev SPI NAND was found.
Block size: 128 KiB, page size: 2048
ddr_type = 1 (LPDDR4)
hb_chip_package_type:3
load ddr header src_addr: 100000, load_addr: 802ca020, src_len: a00
find valid ddr image
ddr_hdr.ecc_gran: 0x0
ddr_hdr.ecc_map: 0x0
ddr_hdr.sbr_pattern0: 0x0
ddr_hdr.sbr_pattern1: 0x0
ddr_freq = 05
board id = 31540334
ddr datarate: 3200
### SAMSUNG DDR ###
no ddr pin set
detect part number: 108
detect ddr freq: c80
board id alternative:0x3
index is 12
index is 15
index is 19
hb_ddr_index: 19
ddr_type = 1, ddr_vendor=3, ddr_freq=3200
dram_pll_init
sscg disabled
control load ddrc src_addr: 15ae00, load_addr: 802caa20, src_len: 920
[DDR INFO]      ==ddr_release_info==
[DDR INFO]      VERSION:        develop
[DDR INFO]      BUILD:          2022-05-11-20:09
[DDR INFO]      GIT COMMIT:     4ca851534c1616ace920fdaa000c6fb717c1fb74
[DDR INFO]      GIT TIME:       Wed, 20 Apr 2022 18:28:49 +0800
[DDR INFO]      ==ddr_features==
[DDR INFO]      RDBI:           0
[DDR INFO]      WDBI:           1
[DDR INFO]      InlineECC:      0
[DDR INFO]      DM:             1
[DDR INFO]      DDC:            1
[DDR INFO]      SSCG:           0
[DDR INFO]      BOARD:          XS_ENABLE
[DDR INFO] ddr_controller_cfg done
load ddr phy src_addr: 15b800, load_addr: 802caa20, src_len: 420
ATxSlewRate     : 15f
ATxImpedance    : 7f
TxSlewRate      : 19f
TxOdtDrvStren   : 600
TxImpedanceCtrl : e3f
CalDrvStr0      : 11
VrefInGlobal    : 104
board_type = 4 (CUSTOMER_BOARD)
load dqmap src addr: 15d600, load_addr: 802caa20, src_len: 20
[DDR INFO] dwc_ddrphy_train start
magic = 544f4248
load imem1 src_addr: 11ce00, load_addr: 802caa20, src_len: 8000
load dmem1 src_addr: 15a000, load_addr: 802caa20, src_len: 684
executing 1D fw
load imem2 src_addr: 124e00, load_addr: 802caa20, src_len: 8000
load dmem2 src_addr: 15a800, load_addr: 802caa20, src_len: 564

*******************************************************
p_dmem_lpddr4_2d_16b->MR11_A0:54
p_dmem_lpddr4_2d_16b->MR14_A0:54
p_dmem_lpddr4_2d_16b->MR12_A0:51
p_dmem_lpddr4_2d_16b->MR22_A0:14

p_dmem_lpddr4_2d_16b->MR3_A0:b3
p_dmem_lpddr4_2d_16b->Reserved00:40
p_dmem_lpddr4_2d_16b->Reserved0E:4
p_dmem_lpddr4_2d_16b->Delay_Weight2D:20
p_dmem_lpddr4_2d_16b->Voltage_Weight2D:80
*******************************************************

executing 2D fw
load pie src_addr: 15be00, load_addr: 802caa20, src_len: 11f0
Set QoS.
get_ddr_mr_info:cs_num=1, mr5=0x1, mr8=0x10
no magic in efuse file,bypass efuse
total_sz = 4096
SPL_VERSION:7
uboot partition is uboot_A
load u-boot: src_addr=0x380000, dest_addr=0x4000000, len=2097152
load warm boot spl: addr=0x800, dest_addr=0x80000000, len=31232
load bl31: addr=0x300000, dest_addr=0x0, len=524288
SFLOW_AUTH_BL31
verify signature of header:  verify ok!
verify signature of image:  verify ok!
bypass bpu image
clear keybank!!!!
SFLOW_DBG_EN
Trying to boot from RAM
SPL: bl31 will jump to u-boot or other entry (0x4000000)
SFLOW_CLR_KEY
SFLOW_REG_LD
install_portal copy portal
install_portal call smc and jump to bl31 cold entry(0x0)
hb som type: 5
X3 PI reset VDD_SD done

U-Boot 2018.09-g40785bca (May 27 2022 - 16:30:48 +0800)

Model: Hobot XJ3 Soc Board
DRAM:  system DDR size: 0xffe00000
4 GiB
MMC:   dwmmc@A5010000: 0, dwmmc@A5011000: 1, dwmmc@A5012000: 2 (SD)
Loading Environment from UBI... GigaDevice SPI NAND was found.
128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
*** Warning - bad CRC, using default environment

In:    serial@a5000000
Out:   serial@a5000000
Err:   serial@a5000000
Net:   x3 sdb reset eth phy done

Warning: ethernet@A5014000 (eth0) using random MAC address - 46:d6:4e:f1:c5:34
eth0: ethernet@A5014000
Disable cnn cores ..
dtb_name:hobot-x3-pi.dtb
base board type: X3 SDB
bootmode: NAND
board_id = 31540334
damaged volume, update marker is setdamaged volume, update marker is setdamaged volume, update marker is sethb_boot_args_cmd_set custom_bootargs 0 ubuntu_boot 0
Hit any key to stop autoboot:  0
enable watchdog success !
switch to partitions #0, OK
mmc2 is current device
Scanning mmc 2:2...
Found U-Boot script /boot/boot.scr
664 bytes read in 2 ms (324.2 KiB/s)
## Executing script at 03c10000
Boot script loaded from devtype:mmc devnum:2 devplist:2
bootargs = console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
Loading fdt file: /boot/hobot/hobot-x3-pi.dtb
69633 bytes read in 7 ms (9.5 MiB/s)
Loading kernel: /boot/Image
19163144 bytes read in 846 ms (21.6 MiB/s)
## Flattened Device Tree blob at 03c00000
   Booting using the fdt blob at 0x3c00000
   Loading Device Tree to 0000000003c00000, end 0000000003c1ffff ... OK
chip_id: ab36300
The address of the fdt is 0x3c00000
Changed status Done
Can't get fdt_addr !!!Orign(MAX) bpu model Reserve Mem Size to 64M!!

Starting kernel ...

[    0.000000] OF: reserved mem: OVERLAP DETECTED!
[    0.000000] image_r5_mem (0x0000000080000000--0x0000000080010000) overlaps with msg_r5_mem (0x000000008000f000--0x0000000080010000)
[    0.000000] Reserved memory: created CMA memory pool at 0x0000000004000000, size 672 MiB
[    0.000000] OF: reserved mem: initialized node ion_cma, compatible id shared-dma-pool
[    0.000000] cma: Reserved 16 MiB at 0x000000007f000000
[    0.000000] On node 0 totalpages: 1047808
[    0.000000]   DMA zone: 8180 pages used for memmap
[    0.000000]   DMA zone: 0 pages reserved
[    0.000000]   DMA zone: 523520 pages, LIFO batch:31
[    0.000000]   Normal zone: 8192 pages used for memmap
[    0.000000]   Normal zone: 524288 pages, LIFO batch:31
[    0.000000] psci: probing for conduit method from DT.
[    0.000000] psci: PSCIv1.1 detected in firmware.
[    0.000000] psci: Using standard PSCI v0.2 function IDs
[    0.000000] psci: MIGRATE_INFO_TYPE not supported.
[    0.000000] psci: SMC Calling Convention v1.1
[    0.000000] percpu: Embedded 25 pages/cpu @ffffffc17ff2a000 s65176 r8192 d29032 u102400
[    0.000000] pcpu-alloc: s65176 r8192 d29032 u102400 alloc=25*4096
[    0.000000] pcpu-alloc: [0] 0 [0] 1 [0] 2 [0] 3
[    0.000000] Detected VIPT I-cache on CPU0
[    0.000000] CPU features: enabling workaround for ARM erratum 845719
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 1031436
[    0.000000] Kernel command line: earlycon loglevel=8 kgdboc=ttyS0 video=hobot:x3sdb-hdmi  console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
[    0.000000] PID hash table entries: 4096 (order: 3, 32768 bytes)
[    0.000000] Dentry cache hash table entries: 524288 (order: 10, 4194304 bytes)
[    0.000000] Inode-cache hash table entries: 262144 (order: 9, 2097152 bytes)
[    0.000000] software IO TLB [mem 0x7afff000-0x7efff000] (64MB) mapped at [ffffffc07afff000-ffffffc07effefff]
[    0.000000] Memory: 3319580K/4191232K available (10494K kernel code, 1306K rwdata, 5756K rodata, 1088K init, 9553K bss, 167140K reserved, 704512K cma-reserved)
[    0.000000] Virtual kernel memory layout:
[    0.000000]     modules : 0xffffff8000000000 - 0xffffff8008000000   (   128 MB)
[    0.000000]     vmalloc : 0xffffff8008000000 - 0xffffffbebfff0000   (   250 GB)
[    0.000000]       .text : 0xffffff8008000000 - 0xffffff8008a40000   ( 10496 KB)
[    0.000000]     .rodata : 0xffffff8008a40000 - 0xffffff8008ff0000   (  5824 KB)
[    0.000000]       .init : 0xffffff8008ff0000 - 0xffffff8009100000   (  1088 KB)
[    0.000000]       .data : 0xffffff8009100000 - 0xffffff8009246808   (  1307 KB)
[    0.000000]        .bss : 0xffffff8009246808 - 0xffffff8009b9aed8   (  9554 KB)
[    0.000000]     fixed   : 0xffffffbefe7fd000 - 0xffffffbefec00000   (  4108 KB)
[    0.000000]     PCI I/O : 0xffffffbefee00000 - 0xffffffbeffe00000   (    16 MB)
[    0.000000]     vmemmap : 0xffffffbf00000000 - 0xffffffc000000000   (     4 GB maximum)
[    0.000000]               0xffffffbf00008000 - 0xffffffbf06000000   (    95 MB actual)
[    0.000000]     memory  : 0xffffffc000200000 - 0xffffffc180000000   (  6142 MB)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=4, Nodes=1
[    0.000000] ftrace: allocating 36277 entries in 142 pages
[    0.000000] Preemptible hierarchical RCU implementation.
[    0.000000]  Tasks RCU enabled.
[    0.000000] NR_IRQS: 64, nr_irqs: 64, preallocated irqs: 0
[    0.000000] parent_rate: 0,  dclk->rate:2666000000, pre_ddr_rate:0, res.a0:139716712
[    0.000000] arch_timer: cp15 timer(s) running at 24.00MHz (virt).
[    0.000000] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0x588fe9dc0, max_idle_ns: 440795202592 ns
[    0.000003] sched_clock: 56 bits at 24MHz, resolution 41ns, wraps every 4398046511097ns
[    0.001194] clocksource: hobot_clocksource: mask: 0xffffffffffffffff max_cycles: 0x1d854df40, max_idle_ns: 3526361616960 ns
[    0.002970] Console: colour dummy device 80x25
[    0.003541] Calibrating delay loop (skipped), value calculated using timer frequency.. 48.00 BogoMIPS (lpj=96000)
[    0.004847] pid_max: default: 32768 minimum: 301
[    0.005502] Security Framework initialized
[    0.006020] AppArmor: AppArmor disabled by boot time parameter
[    0.006863] Mount-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.007731] Mountpoint-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.023774] ASID allocator initialised with 65536 entries
[    0.031772] Hierarchical SRCU implementation.
[    0.063830] smp: Bringing up secondary CPUs ...
[    0.100036] Detected VIPT I-cache on CPU1
[    0.100071] CPU1: Booted secondary processor [410fd034]
[    0.136087] Detected VIPT I-cache on CPU2
[    0.136107] CPU2: Booted secondary processor [410fd034]
[    0.172145] Detected VIPT I-cache on CPU3
[    0.172165] CPU3: Booted secondary processor [410fd034]
[    0.172218] smp: Brought up 1 node, 4 CPUs
[    0.176281] SMP: Total of 4 processors activated.
[    0.176876] CPU features: detected feature: 32-bit EL0 Support
[    0.177694] CPU: All CPU(s) started at EL1
[    0.178222] alternatives: patching kernel code
[    0.179815] devtmpfs: initialized
[    0.188909] random: get_random_u32 called from bucket_table_alloc+0x108/0x270 with crng_init=0
[    0.190497] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 7645041785100000 ns
[    0.191743] futex hash table entries: 1024 (order: 5, 131072 bytes)
[    0.208241] xor: automatically using best checksumming function   32regs
[    0.209177] pinctrl core: initialized pinctrl subsystem
[    0.210419] NET: Registered protocol family 16
[    0.211741] vdso: 2 pages (1 code @ ffffff8008a46000, 1 data @ ffffff8009104000)
[    0.212686] hw-breakpoint: found 6 breakpoint and 4 watchpoint registers.
[    0.214277] DMA: preallocated 256 KiB pool for atomic allocations
[    0.218925] pstore: using zlib compression
[    0.219720] console [pstore-1] enabled
[    0.220320] pstore: Registered ramoops as persistent store backend
[    0.221105] ramoops: attached 0x40000@0x3fc0000, ecc: 0/0
[    0.226097] hobot_dma a1005000.dma: Hobot DMA Engine Driver Probed!!
[    0.239896] SCSI subsystem initialized
[    0.240593] media: Linux media interface: v0.10
[    0.241189] Linux video capture interface: v2.00
[    0.241823] pps_core: LinuxPPS API ver. 1 registered
[    0.242451] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.243626] PTP clock support registered
[    0.244799] ion_dummy: not reserve carveout memory, try to alloc from cma
[    0.381539] Advanced Linux Sound Architecture Driver Initialized.
[    0.382702] usbcore: registered new interface driver usbfs
[    0.383429] usbcore: registered new interface driver hub
[    0.384157] usbcore: registered new device driver usb
[    0.385147] clocksource: Switched to clocksource arch_sys_counter
[    0.432785] VFS: Disk quotas dquot_6.6.0
[    0.433359] VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
[    0.434294] FS-Cache: Loaded
[    0.434778] CacheFiles: Loaded
[    0.440082] NET: Registered protocol family 2
[    0.441008] TCP established hash table entries: 32768 (order: 6, 262144 bytes)
[    0.442154] TCP bind hash table entries: 32768 (order: 7, 524288 bytes)
[    0.443402] TCP: Hash tables configured (established 32768 bind 32768)
[    0.444311] UDP hash table entries: 2048 (order: 4, 65536 bytes)
[    0.445171] UDP-Lite hash table entries: 2048 (order: 4, 65536 bytes)
[    0.446171] NET: Registered protocol family 1
[    0.447006] RPC: Registered named UNIX socket transport module.
[    0.447758] RPC: Registered udp transport module.
[    0.448355] RPC: Registered tcp transport module.
[    0.448953] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.450590] hw perfevents: enabled with armv8_cortex_a53 PMU driver, 7 counters available
[    0.452803] audit: initializing netlink subsys (disabled)
[    0.453611] audit: type=2000 audit(0.452:1): state=initialized audit_enabled=0 res=1
[    0.453920] Initialise system trusted keyrings
[    0.454000] workingset: timestamp_bits=46 max_order=20 bucket_order=0
[    0.457765] zbud: loaded
[    0.459335] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.460196] exFAT: Version 1.2.9
[    0.460676] FS-Cache: Netfs 'nfs' registered for caching
[    0.461814] NFS: Registering the id_resolver key type
[    0.462471] Key type id_resolver registered
[    0.462998] Key type id_legacy registered
[    0.463514] nfs4filelayout_init: NFSv4 File Layout Driver Registering...
[    0.464368] Installing knfsd (copyright (C) 1996 okir@monad.swb.de).
[    0.468519] NET: Registered protocol family 38
[    0.469090] async_tx: api initialized (async)
[    0.469661] Key type asymmetric registered
[    0.470178] Asymmetric key parser 'x509' registered
[    0.470857] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 245)
[    0.471873] io scheduler noop registered
[    0.472531] io scheduler cfq registered (default)
[    0.473126] io scheduler mq-deadline registered
[    0.473748] io scheduler kyber registered
[    0.474933] pinctrl-single a6003170.pinctrl_voltag: 64 pins at pa ffffff8009c4d170 size 8
[    0.476273] pinctrl-single a6004000.pinctrl: 128 pins at pa ffffff8009c61000 size 512
[    0.477522] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: start probe
[    0.478412] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: probe ok
[    0.479281] gpio-x3 a6003000.gpio: x3 gpio probe start!!!
[    0.479971] gpio-x3 a6003000.gpio: x3 gpio add gpiochip start!!!
[    0.480901] gpio-x3 a6003000.gpio: diable all gpio irq
[    0.483170] gpio-x3 a6003000.gpio: irqbase:57
[    0.483722] gpio-x3 a6003000.gpio: x3 irq add start!!!
[    0.484378] irq: Cannot allocate irq_descs @ IRQ57, assuming pre-allocated
[    0.485559] gpio-x3 a6003000.gpio: x3 irq add ok!!!
[    0.486214] gpio-x3 a6003000.gpio: x3 irqchip ops add ok!!!
[    0.486919] gpio-x3 a6003000.gpio: x3 gpio probe ok!!!
[    0.488011] hobot-pwm: hobot-pwmchip0 registered
[    0.488765] hobot-pwm: hobot-pwmchip1 registered
[    0.490114] diag dev [ver:1.1] init done
[    0.491017] hobot_ddr_monitor: LPDDR4 detected
[    0.491787] hobot_ddr_monitor: ddr monitor init finished.
[    0.492173] [vcam] init start
[    0.493251] vcam probe start
[    0.493711] vcam probe end successful
[    0.494172] [vcam] init end
[    0.495077] a5000000.serial: ttyS0 at MMIO 0xa5000000 (irq = 10, base_baud = 12000000) is a hobot-uart
[    0.496289] console [ttyS0] enabled
[    0.496289] console [ttyS0] enabled
[    0.497363] bootconsole [hobot0] disabled
[    0.497363] bootconsole [hobot0] disabled
[    0.498715] hobot-uart a5001000.serial: Failed to create debugfs root directory
[    0.499720] a5001000.serial: ttyS1 at MMIO 0xa5001000 (irq = 11, base_baud = 12000000) is a hobot-uart
[    0.501214] hobot-uart a5003000.serial: Failed to create debugfs root directory
[    0.502218] a5003000.serial: ttyS3 at MMIO 0xa5003000 (irq = 12, base_baud = 12000000) is a hobot-uart
[    0.503754] KGDB: Registered I/O driver kgdboc
[    0.504603] cacheinfo: Unable to detect cache hierarchy for CPU 0
[    0.510065] brd: module loaded
[    0.514623] loop: module loaded
[    0.516136] spi-nand hr_nand.0: GigaDevice SPI NAND was found.
[    0.516896] spi-nand hr_nand.0: 128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
[    0.519511] hobot_spi a5006000.spi: ver: HOBOT-spi_V20.200330 master
[    0.520555] libphy: Fixed MDIO Bus: probed
[    0.521830] st_gmac a5014000.ethernet: found phy-handle subnode
[    0.522668] st_gmac a5014000.ethernet: xj3_mtl_setup, plat->rx-queues-to-use:4, and tx:4
[    0.523854] st_gmac a5014000.ethernet: xj3_probe_config_dt, clk_ptp_rate:250000000
[    0.524856] set mac address 00:11:22:63:e2:c0:
[    0.524859] (using random mac adress)
[    0.525979] (NULL device *): xj3_get_hw_features, tx_fifo_size:16384
[    0.526796] (NULL device *): xj3_get_hw_features, rx_fifo_size:16384
[    0.527614] st_gmac a5014000.ethernet: TSO supported
[    0.528254] st_gmac a5014000.ethernet: TSO feature enabled
[    0.528961] st_gmac a5014000.ethernet: Enable Rx Mitigation via HW Watchdog Timer
[    0.650051] libphy: hobot-mac-mdio: probed
[    0.651606] st_gmac a5014000.ethernet: hobot_eth_probe: probe sucessfully
[    0.652806] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_0v8 not found, using dummy regulator
[    0.654049] dwc3-of-simple b2000000.usb: usb regulator 0v8 enable succeed
[    0.654926] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_3v3 not found, using dummy regulator
[    0.656140] dwc3-of-simple b2000000.usb: usb regulator 3v3 enable succeed
[    0.657686] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    0.659342] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    0.660770] usbcore: registered new interface driver cdc_acm
[    0.661520] cdc_acm: USB Abstract Control Model driver for USB modems and ISDN adapters
[    0.662579] usbcore: registered new interface driver uas
[    0.663296] usbcore: registered new interface driver usb-storage
[    0.664122] usbcore: registered new interface driver usbserial
[    0.664896] usbcore: registered new interface driver usbserial_generic
[    0.665775] usbserial: USB Serial support registered for generic
[    0.666572] usbcore: registered new interface driver usb_serial_simple
[    0.667429] usbserial: USB Serial support registered for carelink
[    0.668230] usbserial: USB Serial support registered for zio
[    0.668975] usbserial: USB Serial support registered for funsoft
[    0.669783] usbserial: USB Serial support registered for flashloader
[    0.670617] usbserial: USB Serial support registered for google
[    0.671398] usbserial: USB Serial support registered for libtransistor
[    0.672254] usbserial: USB Serial support registered for vivopay
[    0.673044] usbserial: USB Serial support registered for moto_modem
[    0.673883] usbserial: USB Serial support registered for motorola_tetra
[    0.674752] usbserial: USB Serial support registered for novatel_gps
[    0.675586] usbserial: USB Serial support registered for hp4x
[    0.676345] usbserial: USB Serial support registered for suunto
[    0.677125] usbserial: USB Serial support registered for siemens_mpi
[    0.677990] usbcore: registered new interface driver rio500
[    0.678822] mousedev: PS/2 mouse device common for all mice
[    0.689869] hobot-rtc a6002000.rtc: rtc core: registered hobot-rtc as rtc0
[    0.690862] i2c /dev entries driver
[    0.691468] hobot-i2c a5009000.i2c: hobot i2c probe start
[    0.692232] hobot-i2c a5009000.i2c: round_rate:96000000
[    0.692909] hobot-i2c a5009000.i2c: I2C bus speed is 400000
[    0.693647] hobot-i2c a5009000.i2c: clkdiv = 0x1d
[    0.694254] hobot-i2c a5009000.i2c: i2c0 diag register....
[    0.695364] hobot-i2c a5009000.i2c: hobot_i2c_0 probe done
[    0.696170] hobot-i2c a500a000.i2c: hobot i2c probe start
[    0.696924] hobot-i2c a500a000.i2c: round_rate:96000000
[    0.697626] hobot-i2c a500a000.i2c: I2C bus speed is 400000
[    0.698344] hobot-i2c a500a000.i2c: clkdiv = 0x1d
[    0.698951] hobot-i2c a500a000.i2c: i2c1 diag register....
[    0.699961] hobot-i2c a500a000.i2c: hobot_i2c_1 probe done
[    0.700919] lirc_dev: IR Remote Control driver registered, major 239
[    0.701759] IR LIRC bridge handler initialized
[    0.702516] sif_mclk clock frequence is 544000000
[    0.703152] mipi_rx0_ipi clock frequence is 544000000
[    0.703841] mipi_rx1_ipi clock frequence is 544000000
[    0.704539] mipi_rx2_ipi clock frequence is 544000000
[    0.705269] mipi_rx3_ipi clock frequence is 544000000
[    0.705990] mipi_tx_ipi clock frequence is 544000000
[    0.706710] mipi_cfg_host clock frequence is 102000000
[    0.707464] pym_mclk clock frequence is 1188000000
[    0.708185] mipi_dev_ref clock frequence is 24000000
[    0.708938] mipi_host_ref clock frequence is 24000000
[    0.709731] sensor0_mclk clock frequence is 37125000
[    0.710508] sensor1_mclk clock frequence is 37125000
[    0.711294] sensor2_mclk clock frequence is 37125000
[    0.712097] sensor3_mclk clock frequence is 37125000
[    0.712737] [FRT:D] x3_ips_probe(0)
[    0.713766] hobot swinfo sel reg ro=0x1 boot dump
[    0.714676] pvt a1009000.pvt: SCRATCH test: 1234abcd, pvt is alive.
[    0.715598] pvt a1009000.pvt: VM Calibrated data detected
[    0.716781] hobot_wdt a1002000.watchdog: watchdog setting [pet:6s bark:11s bite:15s]
[    0.718116] hobot_wdt a1002000.watchdog: Hobot Watchdog Timer at ffffff8009db3000 with timeout 15s
[    0.719469] device-mapper: uevent: version 1.0.3
[    0.720231] device-mapper: ioctl: 4.37.0-ioctl (2017-09-20) initialised: dm-devel@redhat.com
[    0.721436] device-mapper: verity-avb: AVB error handler initialized with vbmeta device:
[    0.723839] Synopsys Designware Multimedia Card Interface Driver
[    0.724838] dwmmc_hobot a5010000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.725688] dwmmc_hobot a5010000.dwmmc: card-detect-delay not found.
[    0.726507] dwmmc_hobot a5010000.dwmmc: data-addr not found.
[    0.727547] mmc_host mmc0: card is non-removable.
[    0.766370] dwmmc_hobot a5011000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.769201] dwmmc_hobot a5011000.dwmmc: card-detect-delay not found.
[    0.770021] dwmmc_hobot a5011000.dwmmc: data-addr not found.
[    0.774800] dwmmc_hobot a5011000.dwmmc: mmc set to fixed voltage 1800
[    0.775860] mmc_host mmc1: card is non-removable.
[    0.873337] dwmmc_hobot a5012000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.874153] dwmmc_hobot a5012000.dwmmc: card-detect-delay not found.
[    0.874983] dwmmc_hobot a5012000.dwmmc: data-addr not found.
[    0.875947] dwmmc_hobot a5012000.dwmmc: Got CD GPIO
[    0.986843] mmc1: queuing unknown CIS tuple 0x80 (2 bytes)
[    0.989030] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.991228] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.994594] mmc1: queuing unknown CIS tuple 0x80 (7 bytes)
[    0.998548] mmc1: queuing unknown CIS tuple 0x81 (9 bytes)
[    1.065454] ledtrig-cpu: registered to indicate activity on CPUs
[    1.066282] hidraw: raw HID events driver (C) Jiri Kosina
[    1.067115] usbcore: registered new interface driver usbhid
[    1.067832] usbhid: USB HID core driver
[    1.068417] logger: created 256K log 'log_main'
[    1.069061] logger: created 256K log 'log_events'
[    1.069744] logger: created 256K log 'log_radio'
[    1.070393] logger: created 256K log 'log_system'
[    1.071430] set dmc devfreq governor to performance
[    1.072063] hobot_dmcfreq_target: dmcfreq->rate:2666000000, target_rate:2666000000
[    1.073035] buf:, powersave_rate:2666000000, dmcfreq->pre_state:0
[    1.079865] usbcore: registered new interface driver snd-usb-audio
[    1.081014] Netfilter messages via NETLINK v0.30.
[    1.081662] ip_set: protocol 6
[    1.082148] ipip: IPv4 and MPLS over IPv4 tunneling driver
[    1.083145] ip_tables: (C) 2000-2006 Netfilter Core Team
[    1.084064] arp_tables: arp_tables: (C) 2002 David S. Miller
[    1.084854] Initializing XFRM netlink socket
[    1.085728] NET: Registered protocol family 10
[    1.086961] Segment Routing with IPv6
[    1.087471] sit: IPv6, IPv4 and MPLS over IPv4 tunneling driver
[    1.088567] NET: Registered protocol family 17
[    1.089213] Key type dns_resolver registered
[    1.090859] Loading compiled-in X.509 certificates
[    1.094363] Loaded X.509 cert 'Build time autogenerated kernel key: 81cb0ef77db2fac76e9588c2120c82422367d268'
[    1.095696] zswap: loaded using pool lzo/zbud
[    1.107006] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    1.108668] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    1.109673] console [netcon0] enabled
[    1.110148] netconsole: network logging started
[    1.110927] hobot-rtc a6002000.rtc: setting system clock to 1970-01-01 00:00:00 UTC (0)
[    1.112104] vps mipi_dphy: probe with x3vio done
[    1.112807] hobot_wdt_test: wdt_test_init: wdt test init
[    1.115555] VCC_CNN0: disabling
[    1.115964] VCC_CNN1: disabling
[    1.116929] vps mipi_host0: ver 140* port0(0:0)
[    1.117868] vps mipi_host1: ver 140* port1(1:0)
[    1.118755] vps mipi_host2: ver 140* port2(0:1)
[    1.119546] vps mipi_host3: ver 140* port3(1:1)
[    1.120381] ALSA device list:
[    1.120766]   No soundcards found.
[    1.121435] md: Skipping autodetection of RAID arrays. (raid=autodetect will force)
[    1.122557] VFS: Cannot open root device "mmcblk2p2" or unknown-block(0,0): error -6
[    1.123551] Please append a correct "root=" boot option; here are the available partitions:
[    1.124625] 0100          102400 ram0
[    1.124627]  (driver?)
[    1.125435] 0101          102400 ram1
[    1.125437]  (driver?)
[    1.126226] 0102          102400 ram2
[    1.126228]  (driver?)
[    1.127016] 0103          102400 ram3
[    1.127018]  (driver?)
[    1.127806] 0104          102400 ram4
[    1.127807]  (driver?)
[    1.128595] 0105          102400 ram5
[    1.128597]  (driver?)
[    1.129428] 0106          102400 ram6
[    1.129430]  (driver?)
[    1.130219] 0107          102400 ram7
[    1.130221]  (driver?)
[    1.131009] 0108          102400 ram8
[    1.131011]  (driver?)
[    1.131799] 0109          102400 ram9
[    1.131801]  (driver?)
[    1.132589] 010a          102400 ram10
[    1.132590]  (driver?)
[    1.133404] 010b          102400 ram11
[    1.133406]  (driver?)
[    1.134206] 010c          102400 ram12
[    1.134207]  (driver?)
[    1.135007] 010d          102400 ram13
[    1.135008]  (driver?)
[    1.135807] 010e          102400 ram14
[    1.135809]  (driver?)
[    1.136608] 010f          102400 ram15
[    1.136610]  (driver?)
[    1.137429] 1f00          131072 mtdblock0
[    1.137431]  (driver?)
[    1.138275] hobot_fusa: set_fusa_error_pin:75 set error pin to 1
[    1.139045] hobot_fusa: fusa errpin not ready
[    1.139049] Kernel panic - not syncing: VFS: Unable to mount root fs on unknown-block(0,0)
[    1.140668] Kernel Offset: disabled
[    1.141119] CPU features: 0x0002004
[    1.141568] Memory Limit: none
[    1.146138] Rebooting in 1 seconds..
[    1.217389] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.218111] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 1
[    1.219571] xhci-hcd xhci-hcd.0.auto: hcc params 0x0220fe6d hci version 0x110 quirks 0x0000000000010010
[    1.220804] xhci-hcd xhci-hcd.0.auto: irq 178, io mem 0xb2000000
[    1.222104] usb usb1: New USB device found, idVendor=1d6b, idProduct=0002, bcdDevice= 4.14
[    1.223182] usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.224126] usb usb1: Product: xHCI Host Controller
[    1.224755] usb usb1: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.225472] usb usb1: SerialNumber: xhci-hcd.0.auto
[    1.226714] hub 1-0:1.0: USB hub found
[    1.227247] hub 1-0:1.0: 1 port detected
[    1.227955] mmc1: new HSSDIO card at address 0001
[    1.228847] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.229575] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 2
[    1.230566] xhci-hcd xhci-hcd.0.auto: Host supports USB 3.0 SuperSpeed
[    1.231442] usb usb2: We don't know the algorithms for LPM for this host, disabling LPM.
[    1.232546] usb usb2: New USB device found, idVendor=1d6b, idProduct=0003, bcdDevice= 4.14
[    1.233619] usb usb2: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.234547] usb usb2: Product: xHCI Host Controller
[    1.235176] usb usb2: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.235882] usb usb2: SerialNumber: xhci-hcd.0.auto
[    1.236788] hub 2-0:1.0: USB hub found
[    1.237323] hub 2-0:1.0: 1 port detected
[    1.481166] usb 1-1: new high-speed USB device number 2 using xhci-hcd
[    1.629343] usb 1-1: New USB device found, idVendor=1a40, idProduct=0101, bcdDevice= 1.11
[    1.630395] usb 1-1: New USB device strings: Mfr=0, Product=1, SerialNumber=0
[    1.631312] usb 1-1: Product: USB 2.0 Hub
[    1.679606] hub 1-1:1.0: USB hub found
[    1.680124] hub 1-1:1.0: 4 ports detected
[    1.961160] mmc2: new UHS SDR104 SDHC card at address 0001
[    1.962183] mmcblk2: mmc2:0001 SD16G 29.8 GiB
[    1.963792]  mmcblk2: p1 p2
[    2.146651] SMP: stopping secondary CPUs
[    2.147159] psci: psci_sys_reset(reboot_mode=0)
NOTICE:  fast_boot:0

S
F
L
O
NOTICE:  efuse cpu_cfg = 0
W
NOTICE:  Booting Trusted Firmware
NOTICE:  BL1: v1.4(release):HR-ROM-Rel-v1.1-141-ga91d4dd-dirty
NOTICE:  BL1: Built : 11:24:44, Oct 23 2019
NOTICE:  boot src: 2
NOTICE:  GigaDev SPI NAND was found.
NOTICE:  Block size: 128 KiB, page size: 2048
NOTICE:  BL1: Booting BL2
Auth pass
NOTICE:  bl1_main exit
SPL normal reset flow
check_reset_state (2): wakeup address = 0x0, hw wakeup status = 0x3, wakeup src=0x100
patch for sys_pll 1200 with 100M eth
SFLOW_INIT
CHIP ID:PCB941/WAFER: W04/ X: X20/ Y: Y36
secondary_jump_to_spl: secure chip flow
X3 SPL : secondary core wake up and jump to spl done (cpu_core_cfg=0)
SFLOW_FIN_HW_A

U-Boot SPL 2018.09-g4ca851534c-dirty (May 11 2022 - 20:09:50 +0800)
SPACC Init - ID: (00000061)
SPL nand boot mode (from strap)
GigaDev SPI NAND was found.
Block size: 128 KiB, page size: 2048
ddr_type = 1 (LPDDR4)
hb_chip_package_type:3
load ddr header src_addr: 100000, load_addr: 802ca020, src_len: a00
find valid ddr image
ddr_hdr.ecc_gran: 0x0
ddr_hdr.ecc_map: 0x0
ddr_hdr.sbr_pattern0: 0x0
ddr_hdr.sbr_pattern1: 0x0
ddr_freq = 05
board id = 31540334
ddr datarate: 3200
### SAMSUNG DDR ###
no ddr pin set
detect part number: 108
detect ddr freq: c80
board id alternative:0x3
index is 12
index is 15
index is 19
hb_ddr_index: 19
ddr_type = 1, ddr_vendor=3, ddr_freq=3200
dram_pll_init
sscg disabled
control load ddrc src_addr: 15ae00, load_addr: 802caa20, src_len: 920
[DDR INFO]      ==ddr_release_info==
[DDR INFO]      VERSION:        develop
[DDR INFO]      BUILD:          2022-05-11-20:09
[DDR INFO]      GIT COMMIT:     4ca851534c1616ace920fdaa000c6fb717c1fb74
[DDR INFO]      GIT TIME:       Wed, 20 Apr 2022 18:28:49 +0800
[DDR INFO]      ==ddr_features==
[DDR INFO]      RDBI:           0
[DDR INFO]      WDBI:           1
[DDR INFO]      InlineECC:      0
[DDR INFO]      DM:             1
[DDR INFO]      DDC:            1
[DDR INFO]      SSCG:           0
[DDR INFO]      BOARD:          XS_ENABLE
[DDR INFO] ddr_controller_cfg done
load ddr phy src_addr: 15b800, load_addr: 802caa20, src_len: 420
ATxSlewRate     : 15f
ATxImpedance    : 7f
TxSlewRate      : 19f
TxOdtDrvStren   : 600
TxImpedanceCtrl : e3f
CalDrvStr0      : 11
VrefInGlobal    : 104
board_type = 4 (CUSTOMER_BOARD)
load dqmap src addr: 15d600, load_addr: 802caa20, src_len: 20
[DDR INFO] dwc_ddrphy_train start
magic = 544f4248
load imem1 src_addr: 11ce00, load_addr: 802caa20, src_len: 8000
load dmem1 src_addr: 15a000, load_addr: 802caa20, src_len: 684
executing 1D fw
load imem2 src_addr: 124e00, load_addr: 802caa20, src_len: 8000
load dmem2 src_addr: 15a800, load_addr: 802caa20, src_len: 564

*******************************************************
p_dmem_lpddr4_2d_16b->MR11_A0:54
p_dmem_lpddr4_2d_16b->MR14_A0:54
p_dmem_lpddr4_2d_16b->MR12_A0:51
p_dmem_lpddr4_2d_16b->MR22_A0:14

p_dmem_lpddr4_2d_16b->MR3_A0:b3
p_dmem_lpddr4_2d_16b->Reserved00:40
p_dmem_lpddr4_2d_16b->Reserved0E:4
p_dmem_lpddr4_2d_16b->Delay_Weight2D:20
p_dmem_lpddr4_2d_16b->Voltage_Weight2D:80
*******************************************************

executing 2D fw
load pie src_addr: 15be00, load_addr: 802caa20, src_len: 11f0
Set QoS.
get_ddr_mr_info:cs_num=1, mr5=0x1, mr8=0x10
no magic in efuse file,bypass efuse
total_sz = 4096
SPL_VERSION:7
uboot partition is uboot_A
load u-boot: src_addr=0x380000, dest_addr=0x4000000, len=2097152
load warm boot spl: addr=0x800, dest_addr=0x80000000, len=31232
load bl31: addr=0x300000, dest_addr=0x0, len=524288
SFLOW_AUTH_BL31
verify signature of header:  verify ok!
verify signature of image:  verify ok!
bypass bpu image
clear keybank!!!!
SFLOW_DBG_EN
Trying to boot from RAM
SPL: bl31 will jump to u-boot or other entry (0x4000000)
SFLOW_CLR_KEY
SFLOW_REG_LD
install_portal copy portal
install_portal call smc and jump to bl31 cold entry(0x0)
hb som type: 5
X3 PI reset VDD_SD done

U-Boot 2018.09-g40785bca (May 27 2022 - 16:30:48 +0800)

Model: Hobot XJ3 Soc Board
DRAM:  system DDR size: 0xffe00000
4 GiB
MMC:   dwmmc@A5010000: 0, dwmmc@A5011000: 1, dwmmc@A5012000: 2
Loading Environment from UBI... GigaDevice SPI NAND was found.
128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
*** Warning - bad CRC, using default environment

In:    serial@a5000000
Out:   serial@a5000000
Err:   serial@a5000000
Net:   x3 sdb reset eth phy done

Warning: ethernet@A5014000 (eth0) using random MAC address - d6:94:19:bb:8d:5c
eth0: ethernet@A5014000
Disable cnn cores ..
dtb_name:hobot-x3-pi.dtb
base board type: X3 SDB
bootmode: NAND
board_id = 31540334
damaged volume, update marker is setdamaged volume, update marker is setdamaged volume, update marker is sethb_boot_args_cmd_set custom_bootargs 0 ubuntu_boot 0
Hit any key to stop autoboot:  0
enable watchdog success !
switch to partitions #0, OK
mmc2 is current device
Scanning mmc 2:2...
Found U-Boot script /boot/boot.scr
664 bytes read in 2 ms (324.2 KiB/s)
## Executing script at 03c10000
Boot script loaded from devtype:mmc devnum:2 devplist:2
bootargs = console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
Loading fdt file: /boot/hobot/hobot-x3-pi.dtb
69633 bytes read in 8 ms (8.3 MiB/s)
Loading kernel: /boot/Image
19163144 bytes read in 845 ms (21.6 MiB/s)
## Flattened Device Tree blob at 03c00000
   Booting using the fdt blob at 0x3c00000
   Loading Device Tree to 0000000003c00000, end 0000000003c1ffff ... OK
chip_id: ab36300
The address of the fdt is 0x3c00000
Changed status Done
Can't get fdt_addr !!!Orign(MAX) bpu model Reserve Mem Size to 64M!!

Starting kernel ...

[    0.000000] OF: reserved mem: OVERLAP DETECTED!
[    0.000000] image_r5_mem (0x0000000080000000--0x0000000080010000) overlaps with msg_r5_mem (0x000000008000f000--0x0000000080010000)
[    0.000000] Reserved memory: created CMA memory pool at 0x0000000004000000, size 672 MiB
[    0.000000] OF: reserved mem: initialized node ion_cma, compatible id shared-dma-pool
[    0.000000] cma: Reserved 16 MiB at 0x000000007f000000
[    0.000000] On node 0 totalpages: 1047808
[    0.000000]   DMA zone: 8180 pages used for memmap
[    0.000000]   DMA zone: 0 pages reserved
[    0.000000]   DMA zone: 523520 pages, LIFO batch:31
[    0.000000]   Normal zone: 8192 pages used for memmap
[    0.000000]   Normal zone: 524288 pages, LIFO batch:31
[    0.000000] psci: probing for conduit method from DT.
[    0.000000] psci: PSCIv1.1 detected in firmware.
[    0.000000] psci: Using standard PSCI v0.2 function IDs
[    0.000000] psci: MIGRATE_INFO_TYPE not supported.
[    0.000000] psci: SMC Calling Convention v1.1
[    0.000000] percpu: Embedded 25 pages/cpu @ffffffc17ff2a000 s65176 r8192 d29032 u102400
[    0.000000] pcpu-alloc: s65176 r8192 d29032 u102400 alloc=25*4096
[    0.000000] pcpu-alloc: [0] 0 [0] 1 [0] 2 [0] 3
[    0.000000] Detected VIPT I-cache on CPU0
[    0.000000] CPU features: enabling workaround for ARM erratum 845719
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 1031436
[    0.000000] Kernel command line: earlycon loglevel=8 kgdboc=ttyS0 video=hobot:x3sdb-hdmi  console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
[    0.000000] PID hash table entries: 4096 (order: 3, 32768 bytes)
[    0.000000] Dentry cache hash table entries: 524288 (order: 10, 4194304 bytes)
[    0.000000] Inode-cache hash table entries: 262144 (order: 9, 2097152 bytes)
[    0.000000] software IO TLB [mem 0x7afff000-0x7efff000] (64MB) mapped at [ffffffc07afff000-ffffffc07effefff]
[    0.000000] Memory: 3319580K/4191232K available (10494K kernel code, 1306K rwdata, 5756K rodata, 1088K init, 9553K bss, 167140K reserved, 704512K cma-reserved)
[    0.000000] Virtual kernel memory layout:
[    0.000000]     modules : 0xffffff8000000000 - 0xffffff8008000000   (   128 MB)
[    0.000000]     vmalloc : 0xffffff8008000000 - 0xffffffbebfff0000   (   250 GB)
[    0.000000]       .text : 0xffffff8008000000 - 0xffffff8008a40000   ( 10496 KB)
[    0.000000]     .rodata : 0xffffff8008a40000 - 0xffffff8008ff0000   (  5824 KB)
[    0.000000]       .init : 0xffffff8008ff0000 - 0xffffff8009100000   (  1088 KB)
[    0.000000]       .data : 0xffffff8009100000 - 0xffffff8009246808   (  1307 KB)
[    0.000000]        .bss : 0xffffff8009246808 - 0xffffff8009b9aed8   (  9554 KB)
[    0.000000]     fixed   : 0xffffffbefe7fd000 - 0xffffffbefec00000   (  4108 KB)
[    0.000000]     PCI I/O : 0xffffffbefee00000 - 0xffffffbeffe00000   (    16 MB)
[    0.000000]     vmemmap : 0xffffffbf00000000 - 0xffffffc000000000   (     4 GB maximum)
[    0.000000]               0xffffffbf00008000 - 0xffffffbf06000000   (    95 MB actual)
[    0.000000]     memory  : 0xffffffc000200000 - 0xffffffc180000000   (  6142 MB)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=4, Nodes=1
[    0.000000] ftrace: allocating 36277 entries in 142 pages
[    0.000000] Preemptible hierarchical RCU implementation.
[    0.000000]  Tasks RCU enabled.
[    0.000000] NR_IRQS: 64, nr_irqs: 64, preallocated irqs: 0
[    0.000000] parent_rate: 0,  dclk->rate:2666000000, pre_ddr_rate:0, res.a0:139716712
[    0.000000] arch_timer: cp15 timer(s) running at 24.00MHz (virt).
[    0.000000] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0x588fe9dc0, max_idle_ns: 440795202592 ns
[    0.000004] sched_clock: 56 bits at 24MHz, resolution 41ns, wraps every 4398046511097ns
[    0.001195] clocksource: hobot_clocksource: mask: 0xffffffffffffffff max_cycles: 0x1d854df40, max_idle_ns: 3526361616960 ns
[    0.002969] Console: colour dummy device 80x25
[    0.003539] Calibrating delay loop (skipped), value calculated using timer frequency.. 48.00 BogoMIPS (lpj=96000)
[    0.004845] pid_max: default: 32768 minimum: 301
[    0.005501] Security Framework initialized
[    0.006019] AppArmor: AppArmor disabled by boot time parameter
[    0.006861] Mount-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.007729] Mountpoint-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.023772] ASID allocator initialised with 65536 entries
[    0.031768] Hierarchical SRCU implementation.
[    0.063826] smp: Bringing up secondary CPUs ...
[    0.100035] Detected VIPT I-cache on CPU1
[    0.100069] CPU1: Booted secondary processor [410fd034]
[    0.136084] Detected VIPT I-cache on CPU2
[    0.136105] CPU2: Booted secondary processor [410fd034]
[    0.172143] Detected VIPT I-cache on CPU3
[    0.172163] CPU3: Booted secondary processor [410fd034]
[    0.172217] smp: Brought up 1 node, 4 CPUs
[    0.176279] SMP: Total of 4 processors activated.
[    0.176873] CPU features: detected feature: 32-bit EL0 Support
[    0.177691] CPU: All CPU(s) started at EL1
[    0.178219] alternatives: patching kernel code
[    0.179807] devtmpfs: initialized
[    0.188899] random: get_random_u32 called from bucket_table_alloc+0x108/0x270 with crng_init=0
[    0.190486] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 7645041785100000 ns
[    0.191732] futex hash table entries: 1024 (order: 5, 131072 bytes)
[    0.208245] xor: automatically using best checksumming function   32regs
[    0.209184] pinctrl core: initialized pinctrl subsystem
[    0.210423] NET: Registered protocol family 16
[    0.211744] vdso: 2 pages (1 code @ ffffff8008a46000, 1 data @ ffffff8009104000)
[    0.212689] hw-breakpoint: found 6 breakpoint and 4 watchpoint registers.
[    0.214279] DMA: preallocated 256 KiB pool for atomic allocations
[    0.219116] pstore: using zlib compression
[    0.219910] console [pstore-1] enabled
[    0.220508] pstore: Registered ramoops as persistent store backend
[    0.221293] ramoops: attached 0x40000@0x3fc0000, ecc: 0/0
[    0.226306] hobot_dma a1005000.dma: Hobot DMA Engine Driver Probed!!
[    0.239973] SCSI subsystem initialized
[    0.240646] media: Linux media interface: v0.10
[    0.241242] Linux video capture interface: v2.00
[    0.241882] pps_core: LinuxPPS API ver. 1 registered
[    0.242510] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.243685] PTP clock support registered
[    0.244969] ion_dummy: not reserve carveout memory, try to alloc from cma
[    0.385329] Advanced Linux Sound Architecture Driver Initialized.
[    0.386517] usbcore: registered new interface driver usbfs
[    0.387244] usbcore: registered new interface driver hub
[    0.387971] usbcore: registered new device driver usb
[    0.388944] clocksource: Switched to clocksource arch_sys_counter
[    0.436679] VFS: Disk quotas dquot_6.6.0
[    0.437252] VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
[    0.438188] FS-Cache: Loaded
[    0.438672] CacheFiles: Loaded
[    0.444035] NET: Registered protocol family 2
[    0.445001] TCP established hash table entries: 32768 (order: 6, 262144 bytes)
[    0.446118] TCP bind hash table entries: 32768 (order: 7, 524288 bytes)
[    0.447399] TCP: Hash tables configured (established 32768 bind 32768)
[    0.448309] UDP hash table entries: 2048 (order: 4, 65536 bytes)
[    0.449164] UDP-Lite hash table entries: 2048 (order: 4, 65536 bytes)
[    0.450165] NET: Registered protocol family 1
[    0.450971] RPC: Registered named UNIX socket transport module.
[    0.451722] RPC: Registered udp transport module.
[    0.452319] RPC: Registered tcp transport module.
[    0.452918] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.454552] hw perfevents: enabled with armv8_cortex_a53 PMU driver, 7 counters available
[    0.456763] audit: initializing netlink subsys (disabled)
[    0.457555] audit: type=2000 audit(0.456:1): state=initialized audit_enabled=0 res=1
[    0.457817] Initialise system trusted keyrings
[    0.457896] workingset: timestamp_bits=46 max_order=20 bucket_order=0
[    0.461603] zbud: loaded
[    0.463161] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.464020] exFAT: Version 1.2.9
[    0.464500] FS-Cache: Netfs 'nfs' registered for caching
[    0.465783] NFS: Registering the id_resolver key type
[    0.466438] Key type id_resolver registered
[    0.466965] Key type id_legacy registered
[    0.467481] nfs4filelayout_init: NFSv4 File Layout Driver Registering...
[    0.468334] Installing knfsd (copyright (C) 1996 okir@monad.swb.de).
[    0.472436] NET: Registered protocol family 38
[    0.473162] async_tx: api initialized (async)
[    0.473715] Key type asymmetric registered
[    0.474233] Asymmetric key parser 'x509' registered
[    0.474919] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 245)
[    0.475937] io scheduler noop registered
[    0.476593] io scheduler cfq registered (default)
[    0.477201] io scheduler mq-deadline registered
[    0.477773] io scheduler kyber registered
[    0.478969] pinctrl-single a6003170.pinctrl_voltag: 64 pins at pa ffffff8009c4d170 size 8
[    0.480319] pinctrl-single a6004000.pinctrl: 128 pins at pa ffffff8009c61000 size 512
[    0.481547] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: start probe
[    0.482435] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: probe ok
[    0.483302] gpio-x3 a6003000.gpio: x3 gpio probe start!!!
[    0.483994] gpio-x3 a6003000.gpio: x3 gpio add gpiochip start!!!
[    0.484915] gpio-x3 a6003000.gpio: diable all gpio irq
[    0.487315] gpio-x3 a6003000.gpio: irqbase:57
[    0.487867] gpio-x3 a6003000.gpio: x3 irq add start!!!
[    0.488524] irq: Cannot allocate irq_descs @ IRQ57, assuming pre-allocated
[    0.489570] gpio-x3 a6003000.gpio: x3 irq add ok!!!
[    0.490225] gpio-x3 a6003000.gpio: x3 irqchip ops add ok!!!
[    0.490930] gpio-x3 a6003000.gpio: x3 gpio probe ok!!!
[    0.492036] hobot-pwm: hobot-pwmchip0 registered
[    0.492790] hobot-pwm: hobot-pwmchip1 registered
[    0.494142] diag dev [ver:1.1] init done
[    0.495047] hobot_ddr_monitor: LPDDR4 detected
[    0.495814] hobot_ddr_monitor: ddr monitor init finished.
[    0.496211] [vcam] init start
[    0.497384] vcam probe start
[    0.497847] vcam probe end successful
[    0.498307] [vcam] init end
[    0.499242] a5000000.serial: ttyS0 at MMIO 0xa5000000 (irq = 10, base_baud = 12000000) is a hobot-uart
[    0.500466] console [ttyS0] enabled
[    0.500466] console [ttyS0] enabled
[    0.501394] bootconsole [hobot0] disabled
[    0.501394] bootconsole [hobot0] disabled
[    0.502718] hobot-uart a5001000.serial: Failed to create debugfs root directory
[    0.503720] a5001000.serial: ttyS1 at MMIO 0xa5001000 (irq = 11, base_baud = 12000000) is a hobot-uart
[    0.505195] hobot-uart a5003000.serial: Failed to create debugfs root directory
[    0.506191] a5003000.serial: ttyS3 at MMIO 0xa5003000 (irq = 12, base_baud = 12000000) is a hobot-uart
[    0.507709] KGDB: Registered I/O driver kgdboc
[    0.508552] cacheinfo: Unable to detect cache hierarchy for CPU 0
[    0.514030] brd: module loaded
[    0.518564] loop: module loaded
[    0.520072] spi-nand hr_nand.0: GigaDevice SPI NAND was found.
[    0.520832] spi-nand hr_nand.0: 128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
[    0.523460] hobot_spi a5006000.spi: ver: HOBOT-spi_V20.200330 master
[    0.524505] libphy: Fixed MDIO Bus: probed
[    0.525870] st_gmac a5014000.ethernet: found phy-handle subnode
[    0.526709] st_gmac a5014000.ethernet: xj3_mtl_setup, plat->rx-queues-to-use:4, and tx:4
[    0.527895] st_gmac a5014000.ethernet: xj3_probe_config_dt, clk_ptp_rate:250000000
[    0.528896] set mac address 00:11:22:f6:eb:1d:
[    0.528898] (using random mac adress)
[    0.529954] (NULL device *): xj3_get_hw_features, tx_fifo_size:16384
[    0.530771] (NULL device *): xj3_get_hw_features, rx_fifo_size:16384
[    0.531588] st_gmac a5014000.ethernet: TSO supported
[    0.532228] st_gmac a5014000.ethernet: TSO feature enabled
[    0.532935] st_gmac a5014000.ethernet: Enable Rx Mitigation via HW Watchdog Timer
[    0.654004] libphy: hobot-mac-mdio: probed
[    0.655542] st_gmac a5014000.ethernet: hobot_eth_probe: probe sucessfully
[    0.656744] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_0v8 not found, using dummy regulator
[    0.657986] dwc3-of-simple b2000000.usb: usb regulator 0v8 enable succeed
[    0.658863] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_3v3 not found, using dummy regulator
[    0.660065] dwc3-of-simple b2000000.usb: usb regulator 3v3 enable succeed
[    0.661599] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    0.663256] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    0.664693] usbcore: registered new interface driver cdc_acm
[    0.665444] cdc_acm: USB Abstract Control Model driver for USB modems and ISDN adapters
[    0.666500] usbcore: registered new interface driver uas
[    0.667218] usbcore: registered new interface driver usb-storage
[    0.668046] usbcore: registered new interface driver usbserial
[    0.668818] usbcore: registered new interface driver usbserial_generic
[    0.669696] usbserial: USB Serial support registered for generic
[    0.670493] usbcore: registered new interface driver usb_serial_simple
[    0.671350] usbserial: USB Serial support registered for carelink
[    0.672150] usbserial: USB Serial support registered for zio
[    0.672895] usbserial: USB Serial support registered for funsoft
[    0.673706] usbserial: USB Serial support registered for flashloader
[    0.674540] usbserial: USB Serial support registered for google
[    0.675318] usbserial: USB Serial support registered for libtransistor
[    0.676173] usbserial: USB Serial support registered for vivopay
[    0.676982] usbserial: USB Serial support registered for moto_modem
[    0.677806] usbserial: USB Serial support registered for motorola_tetra
[    0.678676] usbserial: USB Serial support registered for novatel_gps
[    0.679510] usbserial: USB Serial support registered for hp4x
[    0.680266] usbserial: USB Serial support registered for suunto
[    0.681065] usbserial: USB Serial support registered for siemens_mpi
[    0.681910] usbcore: registered new interface driver rio500
[    0.682748] mousedev: PS/2 mouse device common for all mice
[    0.693804] hobot-rtc a6002000.rtc: rtc core: registered hobot-rtc as rtc0
[    0.694796] i2c /dev entries driver
[    0.695403] hobot-i2c a5009000.i2c: hobot i2c probe start
[    0.696171] hobot-i2c a5009000.i2c: round_rate:96000000
[    0.696848] hobot-i2c a5009000.i2c: I2C bus speed is 400000
[    0.697590] hobot-i2c a5009000.i2c: clkdiv = 0x1d
[    0.698197] hobot-i2c a5009000.i2c: i2c0 diag register....
[    0.699288] hobot-i2c a5009000.i2c: hobot_i2c_0 probe done
[    0.700092] hobot-i2c a500a000.i2c: hobot i2c probe start
[    0.700847] hobot-i2c a500a000.i2c: round_rate:96000000
[    0.701546] hobot-i2c a500a000.i2c: I2C bus speed is 400000
[    0.702264] hobot-i2c a500a000.i2c: clkdiv = 0x1d
[    0.702870] hobot-i2c a500a000.i2c: i2c1 diag register....
[    0.703884] hobot-i2c a500a000.i2c: hobot_i2c_1 probe done
[    0.704842] lirc_dev: IR Remote Control driver registered, major 239
[    0.705680] IR LIRC bridge handler initialized
[    0.706437] sif_mclk clock frequence is 544000000
[    0.707073] mipi_rx0_ipi clock frequence is 544000000
[    0.707762] mipi_rx1_ipi clock frequence is 544000000
[    0.708461] mipi_rx2_ipi clock frequence is 544000000
[    0.709189] mipi_rx3_ipi clock frequence is 544000000
[    0.709910] mipi_tx_ipi clock frequence is 544000000
[    0.710630] mipi_cfg_host clock frequence is 102000000
[    0.711382] pym_mclk clock frequence is 1188000000
[    0.712104] mipi_dev_ref clock frequence is 24000000
[    0.712857] mipi_host_ref clock frequence is 24000000
[    0.713648] sensor0_mclk clock frequence is 37125000
[    0.714428] sensor1_mclk clock frequence is 37125000
[    0.715216] sensor2_mclk clock frequence is 37125000
[    0.716015] sensor3_mclk clock frequence is 37125000
[    0.716655] [FRT:D] x3_ips_probe(0)
[    0.717674] hobot swinfo sel reg ro=0x1 boot dump
[    0.718586] pvt a1009000.pvt: SCRATCH test: 1234abcd, pvt is alive.
[    0.719512] pvt a1009000.pvt: VM Calibrated data detected
[    0.720691] hobot_wdt a1002000.watchdog: watchdog setting [pet:6s bark:11s bite:15s]
[    0.722032] hobot_wdt a1002000.watchdog: Hobot Watchdog Timer at ffffff8009db3000 with timeout 15s
[    0.723384] device-mapper: uevent: version 1.0.3
[    0.724145] device-mapper: ioctl: 4.37.0-ioctl (2017-09-20) initialised: dm-devel@redhat.com
[    0.725371] device-mapper: verity-avb: AVB error handler initialized with vbmeta device:
[    0.727782] Synopsys Designware Multimedia Card Interface Driver
[    0.728783] dwmmc_hobot a5010000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.729644] dwmmc_hobot a5010000.dwmmc: card-detect-delay not found.
[    0.730464] dwmmc_hobot a5010000.dwmmc: data-addr not found.
[    0.731504] mmc_host mmc0: card is non-removable.
[    0.770152] dwmmc_hobot a5011000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.772995] dwmmc_hobot a5011000.dwmmc: card-detect-delay not found.
[    0.773814] dwmmc_hobot a5011000.dwmmc: data-addr not found.
[    0.778583] dwmmc_hobot a5011000.dwmmc: mmc set to fixed voltage 1800
[    0.779646] mmc_host mmc1: card is non-removable.
[    0.877162] dwmmc_hobot a5012000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.878002] dwmmc_hobot a5012000.dwmmc: card-detect-delay not found.
[    0.878845] dwmmc_hobot a5012000.dwmmc: data-addr not found.
[    0.879817] dwmmc_hobot a5012000.dwmmc: Got CD GPIO
[    0.990773] mmc1: queuing unknown CIS tuple 0x80 (2 bytes)
[    0.992969] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.995163] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.998536] mmc1: queuing unknown CIS tuple 0x80 (7 bytes)
[    1.002503] mmc1: queuing unknown CIS tuple 0x81 (9 bytes)
[    1.069245] ledtrig-cpu: registered to indicate activity on CPUs
[    1.070085] hidraw: raw HID events driver (C) Jiri Kosina
[    1.070921] usbcore: registered new interface driver usbhid
[    1.071638] usbhid: USB HID core driver
[    1.072219] logger: created 256K log 'log_main'
[    1.072867] logger: created 256K log 'log_events'
[    1.073560] logger: created 256K log 'log_radio'
[    1.074219] logger: created 256K log 'log_system'
[    1.075265] set dmc devfreq governor to performance
[    1.075898] hobot_dmcfreq_target: dmcfreq->rate:2666000000, target_rate:2666000000
[    1.076870] buf:, powersave_rate:2666000000, dmcfreq->pre_state:0
[    1.083722] usbcore: registered new interface driver snd-usb-audio
[    1.084907] Netfilter messages via NETLINK v0.30.
[    1.085564] ip_set: protocol 6
[    1.086064] ipip: IPv4 and MPLS over IPv4 tunneling driver
[    1.087092] ip_tables: (C) 2000-2006 Netfilter Core Team
[    1.088146] arp_tables: arp_tables: (C) 2002 David S. Miller
[    1.088952] Initializing XFRM netlink socket
[    1.089819] NET: Registered protocol family 10
[    1.091050] Segment Routing with IPv6
[    1.091558] sit: IPv6, IPv4 and MPLS over IPv4 tunneling driver
[    1.092654] NET: Registered protocol family 17
[    1.093326] Key type dns_resolver registered
[    1.094993] Loading compiled-in X.509 certificates
[    1.098499] Loaded X.509 cert 'Build time autogenerated kernel key: 81cb0ef77db2fac76e9588c2120c82422367d268'
[    1.099832] zswap: loaded using pool lzo/zbud
[    1.111086] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    1.112748] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    1.113749] console [netcon0] enabled
[    1.114224] netconsole: network logging started
[    1.115007] hobot-rtc a6002000.rtc: setting system clock to 1970-01-01 00:00:00 UTC (0)
[    1.116187] vps mipi_dphy: probe with x3vio done
[    1.116889] hobot_wdt_test: wdt_test_init: wdt test init
[    1.119642] VCC_CNN0: disabling
[    1.120052] VCC_CNN1: disabling
[    1.121034] vps mipi_host0: ver 140* port0(0:0)
[    1.121960] vps mipi_host1: ver 140* port1(1:0)
[    1.122855] vps mipi_host2: ver 140* port2(0:1)
[    1.123641] vps mipi_host3: ver 140* port3(1:1)
[    1.124476] ALSA device list:
[    1.124861]   No soundcards found.
[    1.125553] md: Skipping autodetection of RAID arrays. (raid=autodetect will force)
[    1.126676] VFS: Cannot open root device "mmcblk2p2" or unknown-block(0,0): error -6
[    1.127670] Please append a correct "root=" boot option; here are the available partitions:
[    1.128744] 0100          102400 ram0
[    1.128746]  (driver?)
[    1.129559] 0101          102400 ram1
[    1.129561]  (driver?)
[    1.130350] 0102          102400 ram2
[    1.130352]  (driver?)
[    1.131140] 0103          102400 ram3
[    1.131141]  (driver?)
[    1.131929] 0104          102400 ram4
[    1.131931]  (driver?)
[    1.132719] 0105          102400 ram5
[    1.132721]  (driver?)
[    1.133546] 0106          102400 ram6
[    1.133548]  (driver?)
[    1.134336] 0107          102400 ram7
[    1.134338]  (driver?)
[    1.135127] 0108          102400 ram8
[    1.135128]  (driver?)
[    1.135916] 0109          102400 ram9
[    1.135918]  (driver?)
[    1.136705] 010a          102400 ram10
[    1.136707]  (driver?)
[    1.137548] 010b          102400 ram11
[    1.137550]  (driver?)
[    1.138350] 010c          102400 ram12
[    1.138352]  (driver?)
[    1.139151] 010d          102400 ram13
[    1.139153]  (driver?)
[    1.139952] 010e          102400 ram14
[    1.139953]  (driver?)
[    1.140752] 010f          102400 ram15
[    1.140754]  (driver?)
[    1.141573] 1f00          131072 mtdblock0
[    1.141576]  (driver?)
[    1.142419] hobot_fusa: set_fusa_error_pin:75 set error pin to 1
[    1.143190] hobot_fusa: fusa errpin not ready
[    1.143194] Kernel panic - not syncing: VFS: Unable to mount root fs on unknown-block(0,0)
[    1.144813] Kernel Offset: disabled
[    1.145264] CPU features: 0x0002004
[    1.145713] Memory Limit: none
[    1.150239] Rebooting in 1 seconds..
[    1.242161] mmc1: new HSSDIO card at address 0001
[    2.150750] SMP: stopping secondary CPUs
[    2.151258] psci: psci_sys_reset(reboot_mode=0)
NOTICE:  fast_boot:0

S
F
L
O
NOTICE:  efuse cpu_cfg = 0
W
NOTICE:  Booting Trusted Firmware
NOTICE:  BL1: v1.4(release):HR-ROM-Rel-v1.1-141-ga91d4dd-dirty
NOTICE:  BL1: Built : 11:24:44, Oct 23 2019
NOTICE:  boot src: 2
NOTICE:  GigaDev SPI NAND was found.
NOTICE:  Block size: 128 KiB, page size: 2048
NOTICE:  BL1: Booting BL2
Auth pass
NOTICE:  bl1_main exit
SPL normal reset flow
check_reset_state (2): wakeup address = 0x0, hw wakeup status = 0x3, wakeup src=0x100
patch for sys_pll 1200 with 100M eth
SFLOW_INIT
CHIP ID:PCB941/WAFER: W04/ X: X20/ Y: Y36
secondary_jump_to_spl: secure chip flow
X3 SPL : secondary core wake up and jump to spl done (cpu_core_cfg=0)
SFLOW_FIN_HW_A

U-Boot SPL 2018.09-g4ca851534c-dirty (May 11 2022 - 20:09:50 +0800)
SPACC Init - ID: (00000061)
SPL nand boot mode (from strap)
GigaDev SPI NAND was found.
Block size: 128 KiB, page size: 2048
ddr_type = 1 (LPDDR4)
hb_chip_package_type:3
load ddr header src_addr: 100000, load_addr: 802ca020, src_len: a00
find valid ddr image
ddr_hdr.ecc_gran: 0x0
ddr_hdr.ecc_map: 0x0
ddr_hdr.sbr_pattern0: 0x0
ddr_hdr.sbr_pattern1: 0x0
ddr_freq = 05
board id = 31540334
ddr datarate: 3200
### SAMSUNG DDR ###
no ddr pin set
detect part number: 108
detect ddr freq: c80
board id alternative:0x3
index is 12
index is 15
index is 19
hb_ddr_index: 19
ddr_type = 1, ddr_vendor=3, ddr_freq=3200
dram_pll_init
sscg disabled
control load ddrc src_addr: 15ae00, load_addr: 802caa20, src_len: 920
[DDR INFO]      ==ddr_release_info==
[DDR INFO]      VERSION:        develop
[DDR INFO]      BUILD:          2022-05-11-20:09
[DDR INFO]      GIT COMMIT:     4ca851534c1616ace920fdaa000c6fb717c1fb74
[DDR INFO]      GIT TIME:       Wed, 20 Apr 2022 18:28:49 +0800
[DDR INFO]      ==ddr_features==
[DDR INFO]      RDBI:           0
[DDR INFO]      WDBI:           1
[DDR INFO]      InlineECC:      0
[DDR INFO]      DM:             1
[DDR INFO]      DDC:            1
[DDR INFO]      SSCG:           0
[DDR INFO]      BOARD:          XS_ENABLE
[DDR INFO] ddr_controller_cfg done
load ddr phy src_addr: 15b800, load_addr: 802caa20, src_len: 420
ATxSlewRate     : 15f
ATxImpedance    : 7f
TxSlewRate      : 19f
TxOdtDrvStren   : 600
TxImpedanceCtrl : e3f
CalDrvStr0      : 11
VrefInGlobal    : 104
board_type = 4 (CUSTOMER_BOARD)
load dqmap src addr: 15d600, load_addr: 802caa20, src_len: 20
[DDR INFO] dwc_ddrphy_train start
magic = 544f4248
load imem1 src_addr: 11ce00, load_addr: 802caa20, src_len: 8000
load dmem1 src_addr: 15a000, load_addr: 802caa20, src_len: 684
executing 1D fw
load imem2 src_addr: 124e00, load_addr: 802caa20, src_len: 8000
load dmem2 src_addr: 15a800, load_addr: 802caa20, src_len: 564

*******************************************************
p_dmem_lpddr4_2d_16b->MR11_A0:54
p_dmem_lpddr4_2d_16b->MR14_A0:54
p_dmem_lpddr4_2d_16b->MR12_A0:51
p_dmem_lpddr4_2d_16b->MR22_A0:14

p_dmem_lpddr4_2d_16b->MR3_A0:b3
p_dmem_lpddr4_2d_16b->Reserved00:40
p_dmem_lpddr4_2d_16b->Reserved0E:4
p_dmem_lpddr4_2d_16b->Delay_Weight2D:20
p_dmem_lpddr4_2d_16b->Voltage_Weight2D:80
*******************************************************

executing 2D fw
load pie src_addr: 15be00, load_addr: 802caa20, src_len: 11f0
Set QoS.
get_ddr_mr_info:cs_num=1, mr5=0x1, mr8=0x10
no magic in efuse file,bypass efuse
total_sz = 4096
SPL_VERSION:7
uboot partition is uboot_A
load u-boot: src_addr=0x380000, dest_addr=0x4000000, len=2097152
load warm boot spl: addr=0x800, dest_addr=0x80000000, len=31232
load bl31: addr=0x300000, dest_addr=0x0, len=524288
SFLOW_AUTH_BL31
verify signature of header:  verify ok!
verify signature of image:  verify ok!
bypass bpu image
clear keybank!!!!
SFLOW_DBG_EN
Trying to boot from RAM
SPL: bl31 will jump to u-boot or other entry (0x4000000)
SFLOW_CLR_KEY
SFLOW_REG_LD
install_portal copy portal
install_portal call smc and jump to bl31 cold entry(0x0)
hb som type: 5
X3 PI reset VDD_SD done

U-Boot 2018.09-g40785bca (May 27 2022 - 16:30:48 +0800)

Model: Hobot XJ3 Soc Board
DRAM:  system DDR size: 0xffe00000
4 GiB
MMC:   dwmmc@A5010000: 0, dwmmc@A5011000: 1, dwmmc@A5012000: 2 (SD)
Loading Environment from UBI... GigaDevice SPI NAND was found.
128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
*** Warning - bad CRC, using default environment

In:    serial@a5000000
Out:   serial@a5000000
Err:   serial@a5000000
Net:   x3 sdb reset eth phy done

Warning: ethernet@A5014000 (eth0) using random MAC address - c6:96:e7:55:d7:ff
eth0: ethernet@A5014000
Disable cnn cores ..
dtb_name:hobot-x3-pi.dtb
base board type: X3 SDB
bootmode: NAND
board_id = 31540334
damaged volume, update marker is setdamaged volume, update marker is setdamaged volume, update marker is sethb_boot_args_cmd_set custom_bootargs 0 ubuntu_boot 0
Hit any key to stop autoboot:  0
enable watchdog success !
switch to partitions #0, OK
mmc2 is current device
Scanning mmc 2:2...
Found U-Boot script /boot/boot.scr
664 bytes read in 2 ms (324.2 KiB/s)
## Executing script at 03c10000
Boot script loaded from devtype:mmc devnum:2 devplist:2
bootargs = console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
Loading fdt file: /boot/hobot/hobot-x3-pi.dtb
69633 bytes read in 8 ms (8.3 MiB/s)
Loading kernel: /boot/Image
19163144 bytes read in 845 ms (21.6 MiB/s)
## Flattened Device Tree blob at 03c00000
   Booting using the fdt blob at 0x3c00000
   Loading Device Tree to 0000000003c00000, end 0000000003c1ffff ... OK
chip_id: ab36300
The address of the fdt is 0x3c00000
Changed status Done
Can't get fdt_addr !!!Orign(MAX) bpu model Reserve Mem Size to 64M!!

Starting kernel ...

[    0.000000] OF: reserved mem: OVERLAP DETECTED!
[    0.000000] image_r5_mem (0x0000000080000000--0x0000000080010000) overlaps with msg_r5_mem (0x000000008000f000--0x0000000080010000)
[    0.000000] Reserved memory: created CMA memory pool at 0x0000000004000000, size 672 MiB
[    0.000000] OF: reserved mem: initialized node ion_cma, compatible id shared-dma-pool
[    0.000000] cma: Reserved 16 MiB at 0x000000007f000000
[    0.000000] On node 0 totalpages: 1047808
[    0.000000]   DMA zone: 8180 pages used for memmap
[    0.000000]   DMA zone: 0 pages reserved
[    0.000000]   DMA zone: 523520 pages, LIFO batch:31
[    0.000000]   Normal zone: 8192 pages used for memmap
[    0.000000]   Normal zone: 524288 pages, LIFO batch:31
[    0.000000] psci: probing for conduit method from DT.
[    0.000000] psci: PSCIv1.1 detected in firmware.
[    0.000000] psci: Using standard PSCI v0.2 function IDs
[    0.000000] psci: MIGRATE_INFO_TYPE not supported.
[    0.000000] psci: SMC Calling Convention v1.1
[    0.000000] percpu: Embedded 25 pages/cpu @ffffffc17ff2a000 s65176 r8192 d29032 u102400
[    0.000000] pcpu-alloc: s65176 r8192 d29032 u102400 alloc=25*4096
[    0.000000] pcpu-alloc: [0] 0 [0] 1 [0] 2 [0] 3
[    0.000000] Detected VIPT I-cache on CPU0
[    0.000000] CPU features: enabling workaround for ARM erratum 845719
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 1031436
[    0.000000] Kernel command line: earlycon loglevel=8 kgdboc=ttyS0 video=hobot:x3sdb-hdmi  console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
[    0.000000] PID hash table entries: 4096 (order: 3, 32768 bytes)
[    0.000000] Dentry cache hash table entries: 524288 (order: 10, 4194304 bytes)
[    0.000000] Inode-cache hash table entries: 262144 (order: 9, 2097152 bytes)
[    0.000000] software IO TLB [mem 0x7afff000-0x7efff000] (64MB) mapped at [ffffffc07afff000-ffffffc07effefff]
[    0.000000] Memory: 3319580K/4191232K available (10494K kernel code, 1306K rwdata, 5756K rodata, 1088K init, 9553K bss, 167140K reserved, 704512K cma-reserved)
[    0.000000] Virtual kernel memory layout:
[    0.000000]     modules : 0xffffff8000000000 - 0xffffff8008000000   (   128 MB)
[    0.000000]     vmalloc : 0xffffff8008000000 - 0xffffffbebfff0000   (   250 GB)
[    0.000000]       .text : 0xffffff8008000000 - 0xffffff8008a40000   ( 10496 KB)
[    0.000000]     .rodata : 0xffffff8008a40000 - 0xffffff8008ff0000   (  5824 KB)
[    0.000000]       .init : 0xffffff8008ff0000 - 0xffffff8009100000   (  1088 KB)
[    0.000000]       .data : 0xffffff8009100000 - 0xffffff8009246808   (  1307 KB)
[    0.000000]        .bss : 0xffffff8009246808 - 0xffffff8009b9aed8   (  9554 KB)
[    0.000000]     fixed   : 0xffffffbefe7fd000 - 0xffffffbefec00000   (  4108 KB)
[    0.000000]     PCI I/O : 0xffffffbefee00000 - 0xffffffbeffe00000   (    16 MB)
[    0.000000]     vmemmap : 0xffffffbf00000000 - 0xffffffc000000000   (     4 GB maximum)
[    0.000000]               0xffffffbf00008000 - 0xffffffbf06000000   (    95 MB actual)
[    0.000000]     memory  : 0xffffffc000200000 - 0xffffffc180000000   (  6142 MB)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=4, Nodes=1
[    0.000000] ftrace: allocating 36277 entries in 142 pages
[    0.000000] Preemptible hierarchical RCU implementation.
[    0.000000]  Tasks RCU enabled.
[    0.000000] NR_IRQS: 64, nr_irqs: 64, preallocated irqs: 0
[    0.000000] parent_rate: 0,  dclk->rate:2666000000, pre_ddr_rate:0, res.a0:139716712
[    0.000000] arch_timer: cp15 timer(s) running at 24.00MHz (virt).
[    0.000000] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0x588fe9dc0, max_idle_ns: 440795202592 ns
[    0.000003] sched_clock: 56 bits at 24MHz, resolution 41ns, wraps every 4398046511097ns
[    0.001191] clocksource: hobot_clocksource: mask: 0xffffffffffffffff max_cycles: 0x1d854df40, max_idle_ns: 3526361616960 ns
[    0.002965] Console: colour dummy device 80x25
[    0.003536] Calibrating delay loop (skipped), value calculated using timer frequency.. 48.00 BogoMIPS (lpj=96000)
[    0.004842] pid_max: default: 32768 minimum: 301
[    0.005495] Security Framework initialized
[    0.006013] AppArmor: AppArmor disabled by boot time parameter
[    0.006855] Mount-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.007724] Mountpoint-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.023766] ASID allocator initialised with 65536 entries
[    0.031763] Hierarchical SRCU implementation.
[    0.063822] smp: Bringing up secondary CPUs ...
[    0.100030] Detected VIPT I-cache on CPU1
[    0.100065] CPU1: Booted secondary processor [410fd034]
[    0.136078] Detected VIPT I-cache on CPU2
[    0.136098] CPU2: Booted secondary processor [410fd034]
[    0.172139] Detected VIPT I-cache on CPU3
[    0.172159] CPU3: Booted secondary processor [410fd034]
[    0.172213] smp: Brought up 1 node, 4 CPUs
[    0.176276] SMP: Total of 4 processors activated.
[    0.176870] CPU features: detected feature: 32-bit EL0 Support
[    0.177689] CPU: All CPU(s) started at EL1
[    0.178218] alternatives: patching kernel code
[    0.179804] devtmpfs: initialized
[    0.188893] random: get_random_u32 called from bucket_table_alloc+0x108/0x270 with crng_init=0
[    0.190479] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 7645041785100000 ns
[    0.191725] futex hash table entries: 1024 (order: 5, 131072 bytes)
[    0.208284] xor: automatically using best checksumming function   32regs
[    0.209224] pinctrl core: initialized pinctrl subsystem
[    0.210456] NET: Registered protocol family 16
[    0.211781] vdso: 2 pages (1 code @ ffffff8008a46000, 1 data @ ffffff8009104000)
[    0.212726] hw-breakpoint: found 6 breakpoint and 4 watchpoint registers.
[    0.214317] DMA: preallocated 256 KiB pool for atomic allocations
[    0.218959] pstore: using zlib compression
[    0.219754] console [pstore-1] enabled
[    0.220364] pstore: Registered ramoops as persistent store backend
[    0.221149] ramoops: attached 0x40000@0x3fc0000, ecc: 0/0
[    0.226153] hobot_dma a1005000.dma: Hobot DMA Engine Driver Probed!!
[    0.239892] SCSI subsystem initialized
[    0.240592] media: Linux media interface: v0.10
[    0.241188] Linux video capture interface: v2.00
[    0.241825] pps_core: LinuxPPS API ver. 1 registered
[    0.242453] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.243628] PTP clock support registered
[    0.244800] ion_dummy: not reserve carveout memory, try to alloc from cma
[    0.381579] Advanced Linux Sound Architecture Driver Initialized.
[    0.382776] usbcore: registered new interface driver usbfs
[    0.383504] usbcore: registered new interface driver hub
[    0.384232] usbcore: registered new device driver usb
[    0.385244] clocksource: Switched to clocksource arch_sys_counter
[    0.432958] VFS: Disk quotas dquot_6.6.0
[    0.433530] VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
[    0.434471] FS-Cache: Loaded
[    0.434956] CacheFiles: Loaded
[    0.440247] NET: Registered protocol family 2
[    0.441177] TCP established hash table entries: 32768 (order: 6, 262144 bytes)
[    0.442310] TCP bind hash table entries: 32768 (order: 7, 524288 bytes)
[    0.443554] TCP: Hash tables configured (established 32768 bind 32768)
[    0.444464] UDP hash table entries: 2048 (order: 4, 65536 bytes)
[    0.445310] UDP-Lite hash table entries: 2048 (order: 4, 65536 bytes)
[    0.446312] NET: Registered protocol family 1
[    0.447140] RPC: Registered named UNIX socket transport module.
[    0.447891] RPC: Registered udp transport module.
[    0.448488] RPC: Registered tcp transport module.
[    0.449087] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.450613] hw perfevents: enabled with armv8_cortex_a53 PMU driver, 7 counters available
[    0.452823] audit: initializing netlink subsys (disabled)
[    0.453621] audit: type=2000 audit(0.452:1): state=initialized audit_enabled=0 res=1
[    0.453883] Initialise system trusted keyrings
[    0.453962] workingset: timestamp_bits=46 max_order=20 bucket_order=0
[    0.457571] zbud: loaded
[    0.459113] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.459971] exFAT: Version 1.2.9
[    0.460455] FS-Cache: Netfs 'nfs' registered for caching
[    0.461603] NFS: Registering the id_resolver key type
[    0.462258] Key type id_resolver registered
[    0.462785] Key type id_legacy registered
[    0.463300] nfs4filelayout_init: NFSv4 File Layout Driver Registering...
[    0.464153] Installing knfsd (copyright (C) 1996 okir@monad.swb.de).
[    0.468289] NET: Registered protocol family 38
[    0.468860] async_tx: api initialized (async)
[    0.469446] Key type asymmetric registered
[    0.469964] Asymmetric key parser 'x509' registered
[    0.470646] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 245)
[    0.471657] io scheduler noop registered
[    0.472314] io scheduler cfq registered (default)
[    0.472909] io scheduler mq-deadline registered
[    0.473494] io scheduler kyber registered
[    0.474681] pinctrl-single a6003170.pinctrl_voltag: 64 pins at pa ffffff8009c4d170 size 8
[    0.476021] pinctrl-single a6004000.pinctrl: 128 pins at pa ffffff8009c61000 size 512
[    0.477227] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: start probe
[    0.478264] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: probe ok
[    0.479144] gpio-x3 a6003000.gpio: x3 gpio probe start!!!
[    0.479834] gpio-x3 a6003000.gpio: x3 gpio add gpiochip start!!!
[    0.480756] gpio-x3 a6003000.gpio: diable all gpio irq
[    0.483038] gpio-x3 a6003000.gpio: irqbase:57
[    0.483590] gpio-x3 a6003000.gpio: x3 irq add start!!!
[    0.484246] irq: Cannot allocate irq_descs @ IRQ57, assuming pre-allocated
[    0.485448] gpio-x3 a6003000.gpio: x3 irq add ok!!!
[    0.486105] gpio-x3 a6003000.gpio: x3 irqchip ops add ok!!!
[    0.486811] gpio-x3 a6003000.gpio: x3 gpio probe ok!!!
[    0.487917] hobot-pwm: hobot-pwmchip0 registered
[    0.488671] hobot-pwm: hobot-pwmchip1 registered
[    0.490054] diag dev [ver:1.1] init done
[    0.490954] hobot_ddr_monitor: LPDDR4 detected
[    0.491714] hobot_ddr_monitor: ddr monitor init finished.
[    0.492105] [vcam] init start
[    0.493165] vcam probe start
[    0.493662] vcam probe end successful
[    0.494123] [vcam] init end
[    0.495047] a5000000.serial: ttyS0 at MMIO 0xa5000000 (irq = 10, base_baud = 12000000) is a hobot-uart
[    0.496258] console [ttyS0] enabled
[    0.496258] console [ttyS0] enabled
[    0.497141] bootconsole [hobot0] disabled
[    0.497141] bootconsole [hobot0] disabled
[    0.498611] hobot-uart a5001000.serial: Failed to create debugfs root directory
[    0.499616] a5001000.serial: ttyS1 at MMIO 0xa5001000 (irq = 11, base_baud = 12000000) is a hobot-uart
[    0.501058] hobot-uart a5003000.serial: Failed to create debugfs root directory
[    0.502081] a5003000.serial: ttyS3 at MMIO 0xa5003000 (irq = 12, base_baud = 12000000) is a hobot-uart
[    0.503618] KGDB: Registered I/O driver kgdboc
[    0.504447] cacheinfo: Unable to detect cache hierarchy for CPU 0
[    0.509890] brd: module loaded
[    0.514431] loop: module loaded
[    0.515984] spi-nand hr_nand.0: GigaDevice SPI NAND was found.
[    0.516744] spi-nand hr_nand.0: 128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
[    0.519356] hobot_spi a5006000.spi: ver: HOBOT-spi_V20.200330 master
[    0.520398] libphy: Fixed MDIO Bus: probed
[    0.521590] st_gmac a5014000.ethernet: found phy-handle subnode
[    0.522429] st_gmac a5014000.ethernet: xj3_mtl_setup, plat->rx-queues-to-use:4, and tx:4
[    0.523614] st_gmac a5014000.ethernet: xj3_probe_config_dt, clk_ptp_rate:250000000
[    0.524616] set mac address 00:11:22:3d:1d:46:
[    0.524619] (using random mac adress)
[    0.525795] (NULL device *): xj3_get_hw_features, tx_fifo_size:16384
[    0.526612] (NULL device *): xj3_get_hw_features, rx_fifo_size:16384
[    0.527430] st_gmac a5014000.ethernet: TSO supported
[    0.528070] st_gmac a5014000.ethernet: TSO feature enabled
[    0.528777] st_gmac a5014000.ethernet: Enable Rx Mitigation via HW Watchdog Timer
[    0.649866] libphy: hobot-mac-mdio: probed
[    0.651393] st_gmac a5014000.ethernet: hobot_eth_probe: probe sucessfully
[    0.652595] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_0v8 not found, using dummy regulator
[    0.653837] dwc3-of-simple b2000000.usb: usb regulator 0v8 enable succeed
[    0.654714] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_3v3 not found, using dummy regulator
[    0.655916] dwc3-of-simple b2000000.usb: usb regulator 3v3 enable succeed
[    0.657465] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    0.659122] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    0.660568] usbcore: registered new interface driver cdc_acm
[    0.661319] cdc_acm: USB Abstract Control Model driver for USB modems and ISDN adapters
[    0.662375] usbcore: registered new interface driver uas
[    0.663093] usbcore: registered new interface driver usb-storage
[    0.663923] usbcore: registered new interface driver usbserial
[    0.664695] usbcore: registered new interface driver usbserial_generic
[    0.665573] usbserial: USB Serial support registered for generic
[    0.666369] usbcore: registered new interface driver usb_serial_simple
[    0.667225] usbserial: USB Serial support registered for carelink
[    0.668026] usbserial: USB Serial support registered for zio
[    0.668774] usbserial: USB Serial support registered for funsoft
[    0.669582] usbserial: USB Serial support registered for flashloader
[    0.670416] usbserial: USB Serial support registered for google
[    0.671195] usbserial: USB Serial support registered for libtransistor
[    0.672050] usbserial: USB Serial support registered for vivopay
[    0.672841] usbserial: USB Serial support registered for moto_modem
[    0.673683] usbserial: USB Serial support registered for motorola_tetra
[    0.674550] usbserial: USB Serial support registered for novatel_gps
[    0.675384] usbserial: USB Serial support registered for hp4x
[    0.676140] usbserial: USB Serial support registered for suunto
[    0.676918] usbserial: USB Serial support registered for siemens_mpi
[    0.677788] usbcore: registered new interface driver rio500
[    0.678621] mousedev: PS/2 mouse device common for all mice
[    0.689666] hobot-rtc a6002000.rtc: rtc core: registered hobot-rtc as rtc0
[    0.690658] i2c /dev entries driver
[    0.691269] hobot-i2c a5009000.i2c: hobot i2c probe start
[    0.692035] hobot-i2c a5009000.i2c: round_rate:96000000
[    0.692713] hobot-i2c a5009000.i2c: I2C bus speed is 400000
[    0.693454] hobot-i2c a5009000.i2c: clkdiv = 0x1d
[    0.694061] hobot-i2c a5009000.i2c: i2c0 diag register....
[    0.695155] hobot-i2c a5009000.i2c: hobot_i2c_0 probe done
[    0.695958] hobot-i2c a500a000.i2c: hobot i2c probe start
[    0.696711] hobot-i2c a500a000.i2c: round_rate:96000000
[    0.697410] hobot-i2c a500a000.i2c: I2C bus speed is 400000
[    0.698128] hobot-i2c a500a000.i2c: clkdiv = 0x1d
[    0.698734] hobot-i2c a500a000.i2c: i2c1 diag register....
[    0.699745] hobot-i2c a500a000.i2c: hobot_i2c_1 probe done
[    0.700705] lirc_dev: IR Remote Control driver registered, major 239
[    0.701548] IR LIRC bridge handler initialized
[    0.702302] sif_mclk clock frequence is 544000000
[    0.702938] mipi_rx0_ipi clock frequence is 544000000
[    0.703626] mipi_rx1_ipi clock frequence is 544000000
[    0.704328] mipi_rx2_ipi clock frequence is 544000000
[    0.705037] mipi_rx3_ipi clock frequence is 544000000
[    0.705777] mipi_tx_ipi clock frequence is 544000000
[    0.706497] mipi_cfg_host clock frequence is 102000000
[    0.707250] pym_mclk clock frequence is 1188000000
[    0.707971] mipi_dev_ref clock frequence is 24000000
[    0.708725] mipi_host_ref clock frequence is 24000000
[    0.709518] sensor0_mclk clock frequence is 37125000
[    0.710296] sensor1_mclk clock frequence is 37125000
[    0.711085] sensor2_mclk clock frequence is 37125000
[    0.711885] sensor3_mclk clock frequence is 37125000
[    0.712524] [FRT:D] x3_ips_probe(0)
[    0.713548] hobot swinfo sel reg ro=0x1 boot dump
[    0.714470] pvt a1009000.pvt: SCRATCH test: 1234abcd, pvt is alive.
[    0.715397] pvt a1009000.pvt: VM Calibrated data detected
[    0.716575] hobot_wdt a1002000.watchdog: watchdog setting [pet:6s bark:11s bite:15s]
[    0.717923] hobot_wdt a1002000.watchdog: Hobot Watchdog Timer at ffffff8009db3000 with timeout 15s
[    0.719282] device-mapper: uevent: version 1.0.3
[    0.720047] device-mapper: ioctl: 4.37.0-ioctl (2017-09-20) initialised: dm-devel@redhat.com
[    0.721202] device-mapper: verity-avb: AVB error handler initialized with vbmeta device:
[    0.723620] Synopsys Designware Multimedia Card Interface Driver
[    0.724619] dwmmc_hobot a5010000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.725479] dwmmc_hobot a5010000.dwmmc: card-detect-delay not found.
[    0.726298] dwmmc_hobot a5010000.dwmmc: data-addr not found.
[    0.727348] mmc_host mmc0: card is non-removable.
[    0.766469] dwmmc_hobot a5011000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.769302] dwmmc_hobot a5011000.dwmmc: card-detect-delay not found.
[    0.770122] dwmmc_hobot a5011000.dwmmc: data-addr not found.
[    0.774898] dwmmc_hobot a5011000.dwmmc: mmc set to fixed voltage 1800
[    0.775958] mmc_host mmc1: card is non-removable.
[    0.873445] dwmmc_hobot a5012000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.874262] dwmmc_hobot a5012000.dwmmc: card-detect-delay not found.
[    0.875093] dwmmc_hobot a5012000.dwmmc: data-addr not found.
[    0.876058] dwmmc_hobot a5012000.dwmmc: Got CD GPIO
[    0.986961] mmc1: queuing unknown CIS tuple 0x80 (2 bytes)
[    0.989149] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.991344] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.994708] mmc1: queuing unknown CIS tuple 0x80 (7 bytes)
[    0.998664] mmc1: queuing unknown CIS tuple 0x81 (9 bytes)
[    1.065538] ledtrig-cpu: registered to indicate activity on CPUs
[    1.066368] hidraw: raw HID events driver (C) Jiri Kosina
[    1.067201] usbcore: registered new interface driver usbhid
[    1.067918] usbhid: USB HID core driver
[    1.068501] logger: created 256K log 'log_main'
[    1.069141] logger: created 256K log 'log_events'
[    1.069824] logger: created 256K log 'log_radio'
[    1.070477] logger: created 256K log 'log_system'
[    1.071511] set dmc devfreq governor to performance
[    1.072144] hobot_dmcfreq_target: dmcfreq->rate:2666000000, target_rate:2666000000
[    1.073117] buf:, powersave_rate:2666000000, dmcfreq->pre_state:0
[    1.079960] usbcore: registered new interface driver snd-usb-audio
[    1.081118] Netfilter messages via NETLINK v0.30.
[    1.081757] ip_set: protocol 6
[    1.082239] ipip: IPv4 and MPLS over IPv4 tunneling driver
[    1.083230] ip_tables: (C) 2000-2006 Netfilter Core Team
[    1.084152] arp_tables: arp_tables: (C) 2002 David S. Miller
[    1.084940] Initializing XFRM netlink socket
[    1.085821] NET: Registered protocol family 10
[    1.087052] Segment Routing with IPv6
[    1.087562] sit: IPv6, IPv4 and MPLS over IPv4 tunneling driver
[    1.088649] NET: Registered protocol family 17
[    1.089316] Key type dns_resolver registered
[    1.090960] Loading compiled-in X.509 certificates
[    1.094476] Loaded X.509 cert 'Build time autogenerated kernel key: 81cb0ef77db2fac76e9588c2120c82422367d268'
[    1.095808] zswap: loaded using pool lzo/zbud
[    1.107132] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    1.108793] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    1.109817] console [netcon0] enabled
[    1.110291] netconsole: network logging started
[    1.111073] hobot-rtc a6002000.rtc: setting system clock to 1970-01-01 00:00:00 UTC (0)
[    1.112255] vps mipi_dphy: probe with x3vio done
[    1.112961] hobot_wdt_test: wdt_test_init: wdt test init
[    1.115816] VCC_CNN0: disabling
[    1.116225] VCC_CNN1: disabling
[    1.117182] vps mipi_host0: ver 140* port0(0:0)
[    1.118123] vps mipi_host1: ver 140* port1(1:0)
[    1.119013] vps mipi_host2: ver 140* port2(0:1)
[    1.119797] vps mipi_host3: ver 140* port3(1:1)
[    1.120629] ALSA device list:
[    1.121013]   No soundcards found.
[    1.121694] md: Skipping autodetection of RAID arrays. (raid=autodetect will force)
[    1.122816] VFS: Cannot open root device "mmcblk2p2" or unknown-block(0,0): error -6
[    1.123809] Please append a correct "root=" boot option; here are the available partitions:
[    1.124883] 0100          102400 ram0
[    1.124886]  (driver?)
[    1.125694] 0101          102400 ram1
[    1.125696]  (driver?)
[    1.126485] 0102          102400 ram2
[    1.126487]  (driver?)
[    1.127275] 0103          102400 ram3
[    1.127277]  (driver?)
[    1.128064] 0104          102400 ram4
[    1.128066]  (driver?)
[    1.128854] 0105          102400 ram5
[    1.128856]  (driver?)
[    1.129705] 0106          102400 ram6
[    1.129707]  (driver?)
[    1.130497] 0107          102400 ram7
[    1.130498]  (driver?)
[    1.131286] 0108          102400 ram8
[    1.131288]  (driver?)
[    1.132076] 0109          102400 ram9
[    1.132078]  (driver?)
[    1.132866] 010a          102400 ram10
[    1.132868]  (driver?)
[    1.133683] 010b          102400 ram11
[    1.133685]  (driver?)
[    1.134485] 010c          102400 ram12
[    1.134486]  (driver?)
[    1.135285] 010d          102400 ram13
[    1.135287]  (driver?)
[    1.136086] 010e          102400 ram14
[    1.136088]  (driver?)
[    1.136887] 010f          102400 ram15
[    1.136889]  (driver?)
[    1.137710] 1f00          131072 mtdblock0
[    1.137712]  (driver?)
[    1.138555] hobot_fusa: set_fusa_error_pin:75 set error pin to 1
[    1.139326] hobot_fusa: fusa errpin not ready
[    1.139330] Kernel panic - not syncing: VFS: Unable to mount root fs on unknown-block(0,0)
[    1.140949] Kernel Offset: disabled
[    1.141400] CPU features: 0x0002004
[    1.141849] Memory Limit: none
[    1.146411] Rebooting in 1 seconds..
[    1.181252] dwmmc_hobot a5012000.dwmmc: Unexpected interrupt latency
[    1.193246] dwmmc_hobot a5011000.dwmmc: Unexpected interrupt latency
[    1.217486] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.218204] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 1
[    1.219662] xhci-hcd xhci-hcd.0.auto: hcc params 0x0220fe6d hci version 0x110 quirks 0x0000000000010010
[    1.220897] xhci-hcd xhci-hcd.0.auto: irq 178, io mem 0xb2000000
[    1.221872] usb usb1: New USB device found, idVendor=1d6b, idProduct=0002, bcdDevice= 4.14
[    1.222936] usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.223864] usb usb1: Product: xHCI Host Controller
[    1.224493] usb usb1: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.225199] usb usb1: SerialNumber: xhci-hcd.0.auto
[    1.226159] hub 1-0:1.0: USB hub found
[    1.226661] hub 1-0:1.0: 1 port detected
[    1.227349] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.228063] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 2
[    1.229053] xhci-hcd xhci-hcd.0.auto: Host supports USB 3.0 SuperSpeed
[    1.229943] usb usb2: We don't know the algorithms for LPM for this host, disabling LPM.
[    1.231052] usb usb2: New USB device found, idVendor=1d6b, idProduct=0003, bcdDevice= 4.14
[    1.232115] usb usb2: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.233043] usb usb2: Product: xHCI Host Controller
[    1.233686] usb usb2: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.234393] usb usb2: SerialNumber: xhci-hcd.0.auto
[    1.235291] hub 2-0:1.0: USB hub found
[    1.235791] hub 2-0:1.0: 1 port detected
[    2.146924] SMP: stopping secondary CPUs
[    2.147432] psci: psci_sys_reset(reboot_mode=0)
NOTICE:  fast_boot:0

S
F
L
O
NOTICE:  efuse cpu_cfg = 0
W
NOTICE:  Booting Trusted Firmware
NOTICE:  BL1: v1.4(release):HR-ROM-Rel-v1.1-141-ga91d4dd-dirty
NOTICE:  BL1: Built : 11:24:44, Oct 23 2019
NOTICE:  boot src: 2
NOTICE:  GigaDev SPI NAND was found.
NOTICE:  Block size: 128 KiB, page size: 2048
NOTICE:  BL1: Booting BL2
Auth pass
NOTICE:  bl1_main exit
SPL normal reset flow
check_reset_state (2): wakeup address = 0x0, hw wakeup status = 0x3, wakeup src=0x100
patch for sys_pll 1200 with 100M eth
SFLOW_INIT
CHIP ID:PCB941/WAFER: W04/ X: X20/ Y: Y36
secondary_jump_to_spl: secure chip flow
X3 SPL : secondary core wake up and jump to spl done (cpu_core_cfg=0)
SFLOW_FIN_HW_A

U-Boot SPL 2018.09-g4ca851534c-dirty (May 11 2022 - 20:09:50 +0800)
SPACC Init - ID: (00000061)
SPL nand boot mode (from strap)
GigaDev SPI NAND was found.
Block size: 128 KiB, page size: 2048
ddr_type = 1 (LPDDR4)
hb_chip_package_type:3
load ddr header src_addr: 100000, load_addr: 802ca020, src_len: a00
find valid ddr image
ddr_hdr.ecc_gran: 0x0
ddr_hdr.ecc_map: 0x0
ddr_hdr.sbr_pattern0: 0x0
ddr_hdr.sbr_pattern1: 0x0
ddr_freq = 05
board id = 31540334
ddr datarate: 3200
### SAMSUNG DDR ###
no ddr pin set
detect part number: 108
detect ddr freq: c80
board id alternative:0x3
index is 12
index is 15
index is 19
hb_ddr_index: 19
ddr_type = 1, ddr_vendor=3, ddr_freq=3200
dram_pll_init
sscg disabled
control load ddrc src_addr: 15ae00, load_addr: 802caa20, src_len: 920
[DDR INFO]      ==ddr_release_info==
[DDR INFO]      VERSION:        develop
[DDR INFO]      BUILD:          2022-05-11-20:09
[DDR INFO]      GIT COMMIT:     4ca851534c1616ace920fdaa000c6fb717c1fb74
[DDR INFO]      GIT TIME:       Wed, 20 Apr 2022 18:28:49 +0800
[DDR INFO]      ==ddr_features==
[DDR INFO]      RDBI:           0
[DDR INFO]      WDBI:           1
[DDR INFO]      InlineECC:      0
[DDR INFO]      DM:             1
[DDR INFO]      DDC:            1
[DDR INFO]      SSCG:           0
[DDR INFO]      BOARD:          XS_ENABLE
[DDR INFO] ddr_controller_cfg done
load ddr phy src_addr: 15b800, load_addr: 802caa20, src_len: 420
ATxSlewRate     : 15f
ATxImpedance    : 7f
TxSlewRate      : 19f
TxOdtDrvStren   : 600
TxImpedanceCtrl : e3f
CalDrvStr0      : 11
VrefInGlobal    : 104
board_type = 4 (CUSTOMER_BOARD)
load dqmap src addr: 15d600, load_addr: 802caa20, src_len: 20
[DDR INFO] dwc_ddrphy_train start
magic = 544f4248
load imem1 src_addr: 11ce00, load_addr: 802caa20, src_len: 8000
load dmem1 src_addr: 15a000, load_addr: 802caa20, src_len: 684
executing 1D fw
load imem2 src_addr: 124e00, load_addr: 802caa20, src_len: 8000
load dmem2 src_addr: 15a800, load_addr: 802caa20, src_len: 564

*******************************************************
p_dmem_lpddr4_2d_16b->MR11_A0:54
p_dmem_lpddr4_2d_16b->MR14_A0:54
p_dmem_lpddr4_2d_16b->MR12_A0:51
p_dmem_lpddr4_2d_16b->MR22_A0:14

p_dmem_lpddr4_2d_16b->MR3_A0:b3
p_dmem_lpddr4_2d_16b->Reserved00:40
p_dmem_lpddr4_2d_16b->Reserved0E:4
p_dmem_lpddr4_2d_16b->Delay_Weight2D:20
p_dmem_lpddr4_2d_16b->Voltage_Weight2D:80
*******************************************************

executing 2D fw
load pie src_addr: 15be00, load_addr: 802caa20, src_len: 11f0
Set QoS.
get_ddr_mr_info:cs_num=1, mr5=0x1, mr8=0x10
no magic in efuse file,bypass efuse
total_sz = 4096
SPL_VERSION:7
uboot partition is uboot_A
load u-boot: src_addr=0x380000, dest_addr=0x4000000, len=2097152
load warm boot spl: addr=0x800, dest_addr=0x80000000, len=31232
load bl31: addr=0x300000, dest_addr=0x0, len=524288
SFLOW_AUTH_BL31
verify signature of header:  verify ok!
verify signature of image:  verify ok!
bypass bpu image
clear keybank!!!!
SFLOW_DBG_EN
Trying to boot from RAM
SPL: bl31 will jump to u-boot or other entry (0x4000000)
SFLOW_CLR_KEY
SFLOW_REG_LD
install_portal copy portal
install_portal call smc and jump to bl31 cold entry(0x0)
hb som type: 5
X3 PI reset VDD_SD done

U-Boot 2018.09-g40785bca (May 27 2022 - 16:30:48 +0800)

Model: Hobot XJ3 Soc Board
DRAM:  system DDR size: 0xffe00000
4 GiB
MMC:   dwmmc@A5010000: 0, dwmmc@A5011000: 1, dwmmc@A5012000: 2 (SD)
Loading Environment from UBI... GigaDevice SPI NAND was found.
128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
*** Warning - bad CRC, using default environment

In:    serial@a5000000
Out:   serial@a5000000
Err:   serial@a5000000
Net:   x3 sdb reset eth phy done

Warning: ethernet@A5014000 (eth0) using random MAC address - 6a:38:03:7e:5e:b9
eth0: ethernet@A5014000
Disable cnn cores ..
dtb_name:hobot-x3-pi.dtb
base board type: X3 SDB
bootmode: NAND
board_id = 31540334
damaged volume, update marker is setdamaged volume, update marker is setdamaged volume, update marker is sethb_boot_args_cmd_set custom_bootargs 0 ubuntu_boot 0
Hit any key to stop autoboot:  0
enable watchdog success !
switch to partitions #0, OK
mmc2 is current device
Scanning mmc 2:2...
Found U-Boot script /boot/boot.scr
664 bytes read in 2 ms (324.2 KiB/s)
## Executing script at 03c10000
Boot script loaded from devtype:mmc devnum:2 devplist:2
bootargs = console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
Loading fdt file: /boot/hobot/hobot-x3-pi.dtb
69633 bytes read in 8 ms (8.3 MiB/s)
Loading kernel: /boot/Image
19163144 bytes read in 846 ms (21.6 MiB/s)
## Flattened Device Tree blob at 03c00000
   Booting using the fdt blob at 0x3c00000
   Loading Device Tree to 0000000003c00000, end 0000000003c1ffff ... OK
chip_id: ab36300
The address of the fdt is 0x3c00000
Changed status Done
Can't get fdt_addr !!!Orign(MAX) bpu model Reserve Mem Size to 64M!!

Starting kernel ...

[    0.000000] OF: reserved mem: OVERLAP DETECTED!
[    0.000000] image_r5_mem (0x0000000080000000--0x0000000080010000) overlaps with msg_r5_mem (0x000000008000f000--0x0000000080010000)
[    0.000000] Reserved memory: created CMA memory pool at 0x0000000004000000, size 672 MiB
[    0.000000] OF: reserved mem: initialized node ion_cma, compatible id shared-dma-pool
[    0.000000] cma: Reserved 16 MiB at 0x000000007f000000
[    0.000000] On node 0 totalpages: 1047808
[    0.000000]   DMA zone: 8180 pages used for memmap
[    0.000000]   DMA zone: 0 pages reserved
[    0.000000]   DMA zone: 523520 pages, LIFO batch:31
[    0.000000]   Normal zone: 8192 pages used for memmap
[    0.000000]   Normal zone: 524288 pages, LIFO batch:31
[    0.000000] psci: probing for conduit method from DT.
[    0.000000] psci: PSCIv1.1 detected in firmware.
[    0.000000] psci: Using standard PSCI v0.2 function IDs
[    0.000000] psci: MIGRATE_INFO_TYPE not supported.
[    0.000000] psci: SMC Calling Convention v1.1
[    0.000000] percpu: Embedded 25 pages/cpu @ffffffc17ff2a000 s65176 r8192 d29032 u102400
[    0.000000] pcpu-alloc: s65176 r8192 d29032 u102400 alloc=25*4096
[    0.000000] pcpu-alloc: [0] 0 [0] 1 [0] 2 [0] 3
[    0.000000] Detected VIPT I-cache on CPU0
[    0.000000] CPU features: enabling workaround for ARM erratum 845719
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 1031436
[    0.000000] Kernel command line: earlycon loglevel=8 kgdboc=ttyS0 video=hobot:x3sdb-hdmi  console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
[    0.000000] PID hash table entries: 4096 (order: 3, 32768 bytes)
[    0.000000] Dentry cache hash table entries: 524288 (order: 10, 4194304 bytes)
[    0.000000] Inode-cache hash table entries: 262144 (order: 9, 2097152 bytes)
[    0.000000] software IO TLB [mem 0x7afff000-0x7efff000] (64MB) mapped at [ffffffc07afff000-ffffffc07effefff]
[    0.000000] Memory: 3319580K/4191232K available (10494K kernel code, 1306K rwdata, 5756K rodata, 1088K init, 9553K bss, 167140K reserved, 704512K cma-reserved)
[    0.000000] Virtual kernel memory layout:
[    0.000000]     modules : 0xffffff8000000000 - 0xffffff8008000000   (   128 MB)
[    0.000000]     vmalloc : 0xffffff8008000000 - 0xffffffbebfff0000   (   250 GB)
[    0.000000]       .text : 0xffffff8008000000 - 0xffffff8008a40000   ( 10496 KB)
[    0.000000]     .rodata : 0xffffff8008a40000 - 0xffffff8008ff0000   (  5824 KB)
[    0.000000]       .init : 0xffffff8008ff0000 - 0xffffff8009100000   (  1088 KB)
[    0.000000]       .data : 0xffffff8009100000 - 0xffffff8009246808   (  1307 KB)
[    0.000000]        .bss : 0xffffff8009246808 - 0xffffff8009b9aed8   (  9554 KB)
[    0.000000]     fixed   : 0xffffffbefe7fd000 - 0xffffffbefec00000   (  4108 KB)
[    0.000000]     PCI I/O : 0xffffffbefee00000 - 0xffffffbeffe00000   (    16 MB)
[    0.000000]     vmemmap : 0xffffffbf00000000 - 0xffffffc000000000   (     4 GB maximum)
[    0.000000]               0xffffffbf00008000 - 0xffffffbf06000000   (    95 MB actual)
[    0.000000]     memory  : 0xffffffc000200000 - 0xffffffc180000000   (  6142 MB)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=4, Nodes=1
[    0.000000] ftrace: allocating 36277 entries in 142 pages
[    0.000000] Preemptible hierarchical RCU implementation.
[    0.000000]  Tasks RCU enabled.
[    0.000000] NR_IRQS: 64, nr_irqs: 64, preallocated irqs: 0
[    0.000000] parent_rate: 0,  dclk->rate:2666000000, pre_ddr_rate:0, res.a0:139716712
[    0.000000] arch_timer: cp15 timer(s) running at 24.00MHz (virt).
[    0.000000] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0x588fe9dc0, max_idle_ns: 440795202592 ns
[    0.000004] sched_clock: 56 bits at 24MHz, resolution 41ns, wraps every 4398046511097ns
[    0.001194] clocksource: hobot_clocksource: mask: 0xffffffffffffffff max_cycles: 0x1d854df40, max_idle_ns: 3526361616960 ns
[    0.002966] Console: colour dummy device 80x25
[    0.003537] Calibrating delay loop (skipped), value calculated using timer frequency.. 48.00 BogoMIPS (lpj=96000)
[    0.004843] pid_max: default: 32768 minimum: 301
[    0.005498] Security Framework initialized
[    0.006017] AppArmor: AppArmor disabled by boot time parameter
[    0.006859] Mount-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.007727] Mountpoint-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.023770] ASID allocator initialised with 65536 entries
[    0.031767] Hierarchical SRCU implementation.
[    0.063826] smp: Bringing up secondary CPUs ...
[    0.100031] Detected VIPT I-cache on CPU1
[    0.100066] CPU1: Booted secondary processor [410fd034]
[    0.136083] Detected VIPT I-cache on CPU2
[    0.136104] CPU2: Booted secondary processor [410fd034]
[    0.172143] Detected VIPT I-cache on CPU3
[    0.172163] CPU3: Booted secondary processor [410fd034]
[    0.172216] smp: Brought up 1 node, 4 CPUs
[    0.176279] SMP: Total of 4 processors activated.
[    0.176874] CPU features: detected feature: 32-bit EL0 Support
[    0.177692] CPU: All CPU(s) started at EL1
[    0.178220] alternatives: patching kernel code
[    0.179809] devtmpfs: initialized
[    0.188879] random: get_random_u32 called from bucket_table_alloc+0x108/0x270 with crng_init=0
[    0.190463] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 7645041785100000 ns
[    0.191709] futex hash table entries: 1024 (order: 5, 131072 bytes)
[    0.208230] xor: automatically using best checksumming function   32regs
[    0.209166] pinctrl core: initialized pinctrl subsystem
[    0.210404] NET: Registered protocol family 16
[    0.211721] vdso: 2 pages (1 code @ ffffff8008a46000, 1 data @ ffffff8009104000)
[    0.212666] hw-breakpoint: found 6 breakpoint and 4 watchpoint registers.
[    0.214257] DMA: preallocated 256 KiB pool for atomic allocations
[    0.219060] pstore: using zlib compression
[    0.219856] console [pstore-1] enabled
[    0.220454] pstore: Registered ramoops as persistent store backend
[    0.221239] ramoops: attached 0x40000@0x3fc0000, ecc: 0/0
[    0.226243] hobot_dma a1005000.dma: Hobot DMA Engine Driver Probed!!
[    0.240014] SCSI subsystem initialized
[    0.240674] media: Linux media interface: v0.10
[    0.241270] Linux video capture interface: v2.00
[    0.241901] pps_core: LinuxPPS API ver. 1 registered
[    0.242529] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.243704] PTP clock support registered
[    0.245020] ion_dummy: not reserve carveout memory, try to alloc from cma
[    0.381719] Advanced Linux Sound Architecture Driver Initialized.
[    0.382919] usbcore: registered new interface driver usbfs
[    0.383647] usbcore: registered new interface driver hub
[    0.384374] usbcore: registered new device driver usb
[    0.385334] clocksource: Switched to clocksource arch_sys_counter
[    0.433035] VFS: Disk quotas dquot_6.6.0
[    0.433614] VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
[    0.434549] FS-Cache: Loaded
[    0.435034] CacheFiles: Loaded
[    0.440274] NET: Registered protocol family 2
[    0.441198] TCP established hash table entries: 32768 (order: 6, 262144 bytes)
[    0.442344] TCP bind hash table entries: 32768 (order: 7, 524288 bytes)
[    0.443591] TCP: Hash tables configured (established 32768 bind 32768)
[    0.444501] UDP hash table entries: 2048 (order: 4, 65536 bytes)
[    0.445366] UDP-Lite hash table entries: 2048 (order: 4, 65536 bytes)
[    0.446370] NET: Registered protocol family 1
[    0.447197] RPC: Registered named UNIX socket transport module.
[    0.447948] RPC: Registered udp transport module.
[    0.448545] RPC: Registered tcp transport module.
[    0.449144] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.450671] hw perfevents: enabled with armv8_cortex_a53 PMU driver, 7 counters available
[    0.452881] audit: initializing netlink subsys (disabled)
[    0.453677] audit: type=2000 audit(0.452:1): state=initialized audit_enabled=0 res=1
[    0.453988] Initialise system trusted keyrings
[    0.454062] workingset: timestamp_bits=46 max_order=20 bucket_order=0
[    0.457753] zbud: loaded
[    0.459325] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.460186] exFAT: Version 1.2.9
[    0.460665] FS-Cache: Netfs 'nfs' registered for caching
[    0.461833] NFS: Registering the id_resolver key type
[    0.462487] Key type id_resolver registered
[    0.463014] Key type id_legacy registered
[    0.463529] nfs4filelayout_init: NFSv4 File Layout Driver Registering...
[    0.464383] Installing knfsd (copyright (C) 1996 okir@monad.swb.de).
[    0.468526] NET: Registered protocol family 38
[    0.469100] async_tx: api initialized (async)
[    0.469664] Key type asymmetric registered
[    0.470182] Asymmetric key parser 'x509' registered
[    0.470868] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 245)
[    0.471893] io scheduler noop registered
[    0.472551] io scheduler cfq registered (default)
[    0.473147] io scheduler mq-deadline registered
[    0.473732] io scheduler kyber registered
[    0.474922] pinctrl-single a6003170.pinctrl_voltag: 64 pins at pa ffffff8009c4d170 size 8
[    0.476262] pinctrl-single a6004000.pinctrl: 128 pins at pa ffffff8009c61000 size 512
[    0.477657] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: start probe
[    0.478564] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: probe ok
[    0.479443] gpio-x3 a6003000.gpio: x3 gpio probe start!!!
[    0.480132] gpio-x3 a6003000.gpio: x3 gpio add gpiochip start!!!
[    0.481057] gpio-x3 a6003000.gpio: diable all gpio irq
[    0.483314] gpio-x3 a6003000.gpio: irqbase:57
[    0.483866] gpio-x3 a6003000.gpio: x3 irq add start!!!
[    0.484526] irq: Cannot allocate irq_descs @ IRQ57, assuming pre-allocated
[    0.485573] gpio-x3 a6003000.gpio: x3 irq add ok!!!
[    0.486227] gpio-x3 a6003000.gpio: x3 irqchip ops add ok!!!
[    0.486932] gpio-x3 a6003000.gpio: x3 gpio probe ok!!!
[    0.488039] hobot-pwm: hobot-pwmchip0 registered
[    0.488792] hobot-pwm: hobot-pwmchip1 registered
[    0.490284] diag dev [ver:1.1] init done
[    0.491177] hobot_ddr_monitor: LPDDR4 detected
[    0.491947] hobot_ddr_monitor: ddr monitor init finished.
[    0.492333] [vcam] init start
[    0.493521] vcam probe start
[    0.493992] vcam probe end successful
[    0.494453] [vcam] init end
[    0.495384] a5000000.serial: ttyS0 at MMIO 0xa5000000 (irq = 10, base_baud = 12000000) is a hobot-uart
[    0.496596] console [ttyS0] enabled
[    0.496596] console [ttyS0] enabled
[    0.497503] bootconsole [hobot0] disabled
[    0.497503] bootconsole [hobot0] disabled
[    0.498823] hobot-uart a5001000.serial: Failed to create debugfs root directory
[    0.499823] a5001000.serial: ttyS1 at MMIO 0xa5001000 (irq = 11, base_baud = 12000000) is a hobot-uart
[    0.501261] hobot-uart a5003000.serial: Failed to create debugfs root directory
[    0.502374] a5003000.serial: ttyS3 at MMIO 0xa5003000 (irq = 12, base_baud = 12000000) is a hobot-uart
[    0.503915] KGDB: Registered I/O driver kgdboc
[    0.504749] cacheinfo: Unable to detect cache hierarchy for CPU 0
[    0.510182] brd: module loaded
[    0.514740] loop: module loaded
[    0.516290] spi-nand hr_nand.0: GigaDevice SPI NAND was found.
[    0.517050] spi-nand hr_nand.0: 128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
[    0.519702] hobot_spi a5006000.spi: ver: HOBOT-spi_V20.200330 master
[    0.520747] libphy: Fixed MDIO Bus: probed
[    0.522049] st_gmac a5014000.ethernet: found phy-handle subnode
[    0.522886] st_gmac a5014000.ethernet: xj3_mtl_setup, plat->rx-queues-to-use:4, and tx:4
[    0.524070] st_gmac a5014000.ethernet: xj3_probe_config_dt, clk_ptp_rate:250000000
[    0.525072] set mac address 00:11:22:60:fd:87:
[    0.525075] (using random mac adress)
[    0.526219] (NULL device *): xj3_get_hw_features, tx_fifo_size:16384
[    0.527037] (NULL device *): xj3_get_hw_features, rx_fifo_size:16384
[    0.527855] st_gmac a5014000.ethernet: TSO supported
[    0.528495] st_gmac a5014000.ethernet: TSO feature enabled
[    0.529201] st_gmac a5014000.ethernet: Enable Rx Mitigation via HW Watchdog Timer
[    0.650292] libphy: hobot-mac-mdio: probed
[    0.651854] st_gmac a5014000.ethernet: hobot_eth_probe: probe sucessfully
[    0.653050] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_0v8 not found, using dummy regulator
[    0.654294] dwc3-of-simple b2000000.usb: usb regulator 0v8 enable succeed
[    0.655172] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_3v3 not found, using dummy regulator
[    0.656377] dwc3-of-simple b2000000.usb: usb regulator 3v3 enable succeed
[    0.657916] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    0.659572] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    0.661006] usbcore: registered new interface driver cdc_acm
[    0.661757] cdc_acm: USB Abstract Control Model driver for USB modems and ISDN adapters
[    0.662814] usbcore: registered new interface driver uas
[    0.663534] usbcore: registered new interface driver usb-storage
[    0.664362] usbcore: registered new interface driver usbserial
[    0.665134] usbcore: registered new interface driver usbserial_generic
[    0.666013] usbserial: USB Serial support registered for generic
[    0.666811] usbcore: registered new interface driver usb_serial_simple
[    0.667668] usbserial: USB Serial support registered for carelink
[    0.668469] usbserial: USB Serial support registered for zio
[    0.669214] usbserial: USB Serial support registered for funsoft
[    0.670022] usbserial: USB Serial support registered for flashloader
[    0.670856] usbserial: USB Serial support registered for google
[    0.671637] usbserial: USB Serial support registered for libtransistor
[    0.672494] usbserial: USB Serial support registered for vivopay
[    0.673284] usbserial: USB Serial support registered for moto_modem
[    0.674125] usbserial: USB Serial support registered for motorola_tetra
[    0.674993] usbserial: USB Serial support registered for novatel_gps
[    0.675827] usbserial: USB Serial support registered for hp4x
[    0.676586] usbserial: USB Serial support registered for suunto
[    0.677374] usbserial: USB Serial support registered for siemens_mpi
[    0.678219] usbcore: registered new interface driver rio500
[    0.679046] mousedev: PS/2 mouse device common for all mice
[    0.690096] hobot-rtc a6002000.rtc: rtc core: registered hobot-rtc as rtc0
[    0.691091] i2c /dev entries driver
[    0.691700] hobot-i2c a5009000.i2c: hobot i2c probe start
[    0.692465] hobot-i2c a5009000.i2c: round_rate:96000000
[    0.693143] hobot-i2c a5009000.i2c: I2C bus speed is 400000
[    0.693881] hobot-i2c a5009000.i2c: clkdiv = 0x1d
[    0.694488] hobot-i2c a5009000.i2c: i2c0 diag register....
[    0.695589] hobot-i2c a5009000.i2c: hobot_i2c_0 probe done
[    0.696392] hobot-i2c a500a000.i2c: hobot i2c probe start
[    0.697143] hobot-i2c a500a000.i2c: round_rate:96000000
[    0.697843] hobot-i2c a500a000.i2c: I2C bus speed is 400000
[    0.698561] hobot-i2c a500a000.i2c: clkdiv = 0x1d
[    0.699167] hobot-i2c a500a000.i2c: i2c1 diag register....
[    0.700184] hobot-i2c a500a000.i2c: hobot_i2c_1 probe done
[    0.701141] lirc_dev: IR Remote Control driver registered, major 239
[    0.701970] IR LIRC bridge handler initialized
[    0.702721] sif_mclk clock frequence is 544000000
[    0.703358] mipi_rx0_ipi clock frequence is 544000000
[    0.704046] mipi_rx1_ipi clock frequence is 544000000
[    0.704744] mipi_rx2_ipi clock frequence is 544000000
[    0.705475] mipi_rx3_ipi clock frequence is 544000000
[    0.706196] mipi_tx_ipi clock frequence is 544000000
[    0.706916] mipi_cfg_host clock frequence is 102000000
[    0.707671] pym_mclk clock frequence is 1188000000
[    0.708391] mipi_dev_ref clock frequence is 24000000
[    0.709145] mipi_host_ref clock frequence is 24000000
[    0.709938] sensor0_mclk clock frequence is 37125000
[    0.710718] sensor1_mclk clock frequence is 37125000
[    0.711507] sensor2_mclk clock frequence is 37125000
[    0.712308] sensor3_mclk clock frequence is 37125000
[    0.712947] [FRT:D] x3_ips_probe(0)
[    0.713972] hobot swinfo sel reg ro=0x1 boot dump
[    0.714883] pvt a1009000.pvt: SCRATCH test: 1234abcd, pvt is alive.
[    0.715808] pvt a1009000.pvt: VM Calibrated data detected
[    0.716993] hobot_wdt a1002000.watchdog: watchdog setting [pet:6s bark:11s bite:15s]
[    0.718337] hobot_wdt a1002000.watchdog: Hobot Watchdog Timer at ffffff8009db3000 with timeout 15s
[    0.719686] device-mapper: uevent: version 1.0.3
[    0.720446] device-mapper: ioctl: 4.37.0-ioctl (2017-09-20) initialised: dm-devel@redhat.com
[    0.721679] device-mapper: verity-avb: AVB error handler initialized with vbmeta device:
[    0.724089] Synopsys Designware Multimedia Card Interface Driver
[    0.725089] dwmmc_hobot a5010000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.725949] dwmmc_hobot a5010000.dwmmc: card-detect-delay not found.
[    0.726768] dwmmc_hobot a5010000.dwmmc: data-addr not found.
[    0.727811] mmc_host mmc0: card is non-removable.
[    0.770549] dwmmc_hobot a5011000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.773386] dwmmc_hobot a5011000.dwmmc: card-detect-delay not found.
[    0.774206] dwmmc_hobot a5011000.dwmmc: data-addr not found.
[    0.778974] dwmmc_hobot a5011000.dwmmc: mmc set to fixed voltage 1800
[    0.780038] mmc_host mmc1: card is non-removable.
[    0.877536] dwmmc_hobot a5012000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.878376] dwmmc_hobot a5012000.dwmmc: card-detect-delay not found.
[    0.879219] dwmmc_hobot a5012000.dwmmc: data-addr not found.
[    0.880189] dwmmc_hobot a5012000.dwmmc: Got CD GPIO
[    0.991142] mmc1: queuing unknown CIS tuple 0x80 (2 bytes)
[    0.993339] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.995532] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.998908] mmc1: queuing unknown CIS tuple 0x80 (7 bytes)
[    1.002875] mmc1: queuing unknown CIS tuple 0x81 (9 bytes)
[    1.069663] ledtrig-cpu: registered to indicate activity on CPUs
[    1.070518] hidraw: raw HID events driver (C) Jiri Kosina
[    1.071388] usbcore: registered new interface driver usbhid
[    1.072111] usbhid: USB HID core driver
[    1.072693] logger: created 256K log 'log_main'
[    1.073373] logger: created 256K log 'log_events'
[    1.074037] logger: created 256K log 'log_radio'
[    1.074687] logger: created 256K log 'log_system'
[    1.075723] set dmc devfreq governor to performance
[    1.076356] hobot_dmcfreq_target: dmcfreq->rate:2666000000, target_rate:2666000000
[    1.077350] buf:, powersave_rate:2666000000, dmcfreq->pre_state:0
[    1.084163] usbcore: registered new interface driver snd-usb-audio
[    1.085314] Netfilter messages via NETLINK v0.30.
[    1.085981] ip_set: protocol 6
[    1.086465] ipip: IPv4 and MPLS over IPv4 tunneling driver
[    1.087472] ip_tables: (C) 2000-2006 Netfilter Core Team
[    1.088386] arp_tables: arp_tables: (C) 2002 David S. Miller
[    1.089176] Initializing XFRM netlink socket
[    1.090054] NET: Registered protocol family 10
[    1.091309] Segment Routing with IPv6
[    1.091820] sit: IPv6, IPv4 and MPLS over IPv4 tunneling driver
[    1.092912] NET: Registered protocol family 17
[    1.093580] Key type dns_resolver registered
[    1.095197] Loading compiled-in X.509 certificates
[    1.098707] Loaded X.509 cert 'Build time autogenerated kernel key: 81cb0ef77db2fac76e9588c2120c82422367d268'
[    1.100037] zswap: loaded using pool lzo/zbud
[    1.111298] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    1.112959] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    1.113981] console [netcon0] enabled
[    1.114457] netconsole: network logging started
[    1.115236] hobot-rtc a6002000.rtc: setting system clock to 1970-01-01 00:00:00 UTC (0)
[    1.116420] vps mipi_dphy: probe with x3vio done
[    1.117125] hobot_wdt_test: wdt_test_init: wdt test init
[    1.119871] VCC_CNN0: disabling
[    1.120281] VCC_CNN1: disabling
[    1.121247] vps mipi_host0: ver 140* port0(0:0)
[    1.122187] vps mipi_host1: ver 140* port1(1:0)
[    1.123074] vps mipi_host2: ver 140* port2(0:1)
[    1.123862] vps mipi_host3: ver 140* port3(1:1)
[    1.124695] ALSA device list:
[    1.125080]   No soundcards found.
[    1.125763] md: Skipping autodetection of RAID arrays. (raid=autodetect will force)
[    1.126884] VFS: Cannot open root device "mmcblk2p2" or unknown-block(0,0): error -6
[    1.127877] Please append a correct "root=" boot option; here are the available partitions:
[    1.128951] 0100          102400 ram0
[    1.128953]  (driver?)
[    1.129762] 0101          102400 ram1
[    1.129764]  (driver?)
[    1.130553] 0102          102400 ram2
[    1.130555]  (driver?)
[    1.131343] 0103          102400 ram3
[    1.131345]  (driver?)
[    1.132133] 0104          102400 ram4
[    1.132135]  (driver?)
[    1.132923] 0105          102400 ram5
[    1.132924]  (driver?)
[    1.133755] 0106          102400 ram6
[    1.133758]  (driver?)
[    1.134546] 0107          102400 ram7
[    1.134548]  (driver?)
[    1.135336] 0108          102400 ram8
[    1.135338]  (driver?)
[    1.136126] 0109          102400 ram9
[    1.136128]  (driver?)
[    1.136916] 010a          102400 ram10
[    1.136917]  (driver?)
[    1.137746] 010b          102400 ram11
[    1.137748]  (driver?)
[    1.138547] 010c          102400 ram12
[    1.138549]  (driver?)
[    1.139348] 010d          102400 ram13
[    1.139349]  (driver?)
[    1.140148] 010e          102400 ram14
[    1.140150]  (driver?)
[    1.140949] 010f          102400 ram15
[    1.140951]  (driver?)
[    1.141773] 1f00          131072 mtdblock0
[    1.141775]  (driver?)
[    1.142619] hobot_fusa: set_fusa_error_pin:75 set error pin to 1
[    1.143389] hobot_fusa: fusa errpin not ready
[    1.143393] Kernel panic - not syncing: VFS: Unable to mount root fs on unknown-block(0,0)
[    1.145012] Kernel Offset: disabled
[    1.145463] CPU features: 0x0002004
[    1.145912] Memory Limit: none
[    1.150468] Rebooting in 1 seconds..
[    1.221579] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.222300] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 1
[    1.223757] xhci-hcd xhci-hcd.0.auto: hcc params 0x0220fe6d hci version 0x110 quirks 0x0000000000010010
[    1.224993] xhci-hcd xhci-hcd.0.auto: irq 178, io mem 0xb2000000
[    1.225971] usb usb1: New USB device found, idVendor=1d6b, idProduct=0002, bcdDevice= 4.14
[    1.227035] usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.227963] usb usb1: Product: xHCI Host Controller
[    1.228592] usb usb1: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.229298] usb usb1: SerialNumber: xhci-hcd.0.auto
[    1.230253] hub 1-0:1.0: USB hub found
[    1.230556] mmc1: new HSSDIO card at address 0001
[    1.231359] hub 1-0:1.0: 1 port detected
[    1.232053] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.232768] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 2
[    1.233776] xhci-hcd xhci-hcd.0.auto: Host supports USB 3.0 SuperSpeed
[    1.234651] usb usb2: We don't know the algorithms for LPM for this host, disabling LPM.
[    1.235755] usb usb2: New USB device found, idVendor=1d6b, idProduct=0003, bcdDevice= 4.14
[    1.236818] usb usb2: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.237756] usb usb2: Product: xHCI Host Controller
[    1.238385] usb usb2: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.239091] usb usb2: SerialNumber: xhci-hcd.0.auto
[    1.240000] hub 2-0:1.0: USB hub found
[    1.240500] hub 2-0:1.0: 1 port detected
[    1.485343] usb 1-1: new high-speed USB device number 2 using xhci-hcd
[    1.633528] usb 1-1: New USB device found, idVendor=1a40, idProduct=0101, bcdDevice= 1.11
[    1.634581] usb 1-1: New USB device strings: Mfr=0, Product=1, SerialNumber=0
[    1.635498] usb 1-1: Product: USB 2.0 Hub
[    1.682815] hub 1-1:1.0: USB hub found
[    1.683335] hub 1-1:1.0: 4 ports detected
[    1.969345] mmc2: new UHS SDR104 SDHC card at address 0001
[    1.970374] mmcblk2: mmc2:0001 SD16G 29.8 GiB
[    1.971977]  mmcblk2: p1 p2
[    2.150979] SMP: stopping secondary CPUs
[    2.151487] psci: psci_sys_reset(reboot_mode=0)
NOTICE:  fast_boot:0

S
F
L
O
NOTICE:  efuse cpu_cfg = 0
W
NOTICE:  Booting Trusted Firmware
NOTICE:  BL1: v1.4(release):HR-ROM-Rel-v1.1-141-ga91d4dd-dirty
NOTICE:  BL1: Built : 11:24:44, Oct 23 2019
NOTICE:  boot src: 2
NOTICE:  GigaDev SPI NAND was found.
NOTICE:  Block size: 128 KiB, page size: 2048
NOTICE:  BL1: Booting BL2
Auth pass
NOTICE:  bl1_main exit
SPL normal reset flow
check_reset_state (2): wakeup address = 0x0, hw wakeup status = 0x3, wakeup src=0x100
patch for sys_pll 1200 with 100M eth
SFLOW_INIT
CHIP ID:PCB941/WAFER: W04/ X: X20/ Y: Y36
secondary_jump_to_spl: secure chip flow
X3 SPL : secondary core wake up and jump to spl done (cpu_core_cfg=0)
SFLOW_FIN_HW_A

U-Boot SPL 2018.09-g4ca851534c-dirty (May 11 2022 - 20:09:50 +0800)
SPACC Init - ID: (00000061)
SPL nand boot mode (from strap)
GigaDev SPI NAND was found.
Block size: 128 KiB, page size: 2048
ddr_type = 1 (LPDDR4)
hb_chip_package_type:3
load ddr header src_addr: 100000, load_addr: 802ca020, src_len: a00
find valid ddr image
ddr_hdr.ecc_gran: 0x0
ddr_hdr.ecc_map: 0x0
ddr_hdr.sbr_pattern0: 0x0
ddr_hdr.sbr_pattern1: 0x0
ddr_freq = 05
board id = 31540334
ddr datarate: 3200
### SAMSUNG DDR ###
no ddr pin set
detect part number: 108
detect ddr freq: c80
board id alternative:0x3
index is 12
index is 15
index is 19
hb_ddr_index: 19
ddr_type = 1, ddr_vendor=3, ddr_freq=3200
dram_pll_init
sscg disabled
control load ddrc src_addr: 15ae00, load_addr: 802caa20, src_len: 920
[DDR INFO]      ==ddr_release_info==
[DDR INFO]      VERSION:        develop
[DDR INFO]      BUILD:          2022-05-11-20:09
[DDR INFO]      GIT COMMIT:     4ca851534c1616ace920fdaa000c6fb717c1fb74
[DDR INFO]      GIT TIME:       Wed, 20 Apr 2022 18:28:49 +0800
[DDR INFO]      ==ddr_features==
[DDR INFO]      RDBI:           0
[DDR INFO]      WDBI:           1
[DDR INFO]      InlineECC:      0
[DDR INFO]      DM:             1
[DDR INFO]      DDC:            1
[DDR INFO]      SSCG:           0
[DDR INFO]      BOARD:          XS_ENABLE
[DDR INFO] ddr_controller_cfg done
load ddr phy src_addr: 15b800, load_addr: 802caa20, src_len: 420
ATxSlewRate     : 15f
ATxImpedance    : 7f
TxSlewRate      : 19f
TxOdtDrvStren   : 600
TxImpedanceCtrl : e3f
CalDrvStr0      : 11
VrefInGlobal    : 104
board_type = 4 (CUSTOMER_BOARD)
load dqmap src addr: 15d600, load_addr: 802caa20, src_len: 20
[DDR INFO] dwc_ddrphy_train start
magic = 544f4248
load imem1 src_addr: 11ce00, load_addr: 802caa20, src_len: 8000
load dmem1 src_addr: 15a000, load_addr: 802caa20, src_len: 684
executing 1D fw
load imem2 src_addr: 124e00, load_addr: 802caa20, src_len: 8000
load dmem2 src_addr: 15a800, load_addr: 802caa20, src_len: 564

*******************************************************
p_dmem_lpddr4_2d_16b->MR11_A0:54
p_dmem_lpddr4_2d_16b->MR14_A0:54
p_dmem_lpddr4_2d_16b->MR12_A0:51
p_dmem_lpddr4_2d_16b->MR22_A0:14

p_dmem_lpddr4_2d_16b->MR3_A0:b3
p_dmem_lpddr4_2d_16b->Reserved00:40
p_dmem_lpddr4_2d_16b->Reserved0E:4
p_dmem_lpddr4_2d_16b->Delay_Weight2D:20
p_dmem_lpddr4_2d_16b->Voltage_Weight2D:80
*******************************************************

executing 2D fw
load pie src_addr: 15be00, load_addr: 802caa20, src_len: 11f0
Set QoS.
get_ddr_mr_info:cs_num=1, mr5=0x1, mr8=0x10
no magic in efuse file,bypass efuse
total_sz = 4096
SPL_VERSION:7
uboot partition is uboot_A
load u-boot: src_addr=0x380000, dest_addr=0x4000000, len=2097152
load warm boot spl: addr=0x800, dest_addr=0x80000000, len=31232
load bl31: addr=0x300000, dest_addr=0x0, len=524288
SFLOW_AUTH_BL31
verify signature of header:  verify ok!
verify signature of image:  verify ok!
bypass bpu image
clear keybank!!!!
SFLOW_DBG_EN
Trying to boot from RAM
SPL: bl31 will jump to u-boot or other entry (0x4000000)
SFLOW_CLR_KEY
SFLOW_REG_LD
install_portal copy portal
install_portal call smc and jump to bl31 cold entry(0x0)
hb som type: 5
X3 PI reset VDD_SD done

U-Boot 2018.09-g40785bca (May 27 2022 - 16:30:48 +0800)

Model: Hobot XJ3 Soc Board
DRAM:  system DDR size: 0xffe00000
4 GiB
MMC:   dwmmc@A5010000: 0, dwmmc@A5011000: 1, dwmmc@A5012000: 2
Loading Environment from UBI... GigaDevice SPI NAND was found.
128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
*** Warning - bad CRC, using default environment

In:    serial@a5000000
Out:   serial@a5000000
Err:   serial@a5000000
Net:   x3 sdb reset eth phy done

Warning: ethernet@A5014000 (eth0) using random MAC address - 6a:1d:81:c5:db:ac
eth0: ethernet@A5014000
Disable cnn cores ..
dtb_name:hobot-x3-pi.dtb
base board type: X3 SDB
bootmode: NAND
board_id = 31540334
damaged volume, update marker is setdamaged volume, update marker is setdamaged volume, update marker is sethb_boot_args_cmd_set custom_bootargs 0 ubuntu_boot 0
Hit any key to stop autoboot:  0
enable watchdog success !
switch to partitions #0, OK
mmc2 is current device
Scanning mmc 2:2...
Found U-Boot script /boot/boot.scr
664 bytes read in 2 ms (324.2 KiB/s)
## Executing script at 03c10000
Boot script loaded from devtype:mmc devnum:2 devplist:2
bootargs = console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
Loading fdt file: /boot/hobot/hobot-x3-pi.dtb
69633 bytes read in 8 ms (8.3 MiB/s)
Loading kernel: /boot/Image
19163144 bytes read in 845 ms (21.6 MiB/s)
## Flattened Device Tree blob at 03c00000
   Booting using the fdt blob at 0x3c00000
   Loading Device Tree to 0000000003c00000, end 0000000003c1ffff ... OK
chip_id: ab36300
The address of the fdt is 0x3c00000
Changed status Done
Can't get fdt_addr !!!Orign(MAX) bpu model Reserve Mem Size to 64M!!

Starting kernel ...

[    0.000000] OF: reserved mem: OVERLAP DETECTED!
[    0.000000] image_r5_mem (0x0000000080000000--0x0000000080010000) overlaps with msg_r5_mem (0x000000008000f000--0x0000000080010000)
[    0.000000] Reserved memory: created CMA memory pool at 0x0000000004000000, size 672 MiB
[    0.000000] OF: reserved mem: initialized node ion_cma, compatible id shared-dma-pool
[    0.000000] cma: Reserved 16 MiB at 0x000000007f000000
[    0.000000] On node 0 totalpages: 1047808
[    0.000000]   DMA zone: 8180 pages used for memmap
[    0.000000]   DMA zone: 0 pages reserved
[    0.000000]   DMA zone: 523520 pages, LIFO batch:31
[    0.000000]   Normal zone: 8192 pages used for memmap
[    0.000000]   Normal zone: 524288 pages, LIFO batch:31
[    0.000000] psci: probing for conduit method from DT.
[    0.000000] psci: PSCIv1.1 detected in firmware.
[    0.000000] psci: Using standard PSCI v0.2 function IDs
[    0.000000] psci: MIGRATE_INFO_TYPE not supported.
[    0.000000] psci: SMC Calling Convention v1.1
[    0.000000] percpu: Embedded 25 pages/cpu @ffffffc17ff2a000 s65176 r8192 d29032 u102400
[    0.000000] pcpu-alloc: s65176 r8192 d29032 u102400 alloc=25*4096
[    0.000000] pcpu-alloc: [0] 0 [0] 1 [0] 2 [0] 3
[    0.000000] Detected VIPT I-cache on CPU0
[    0.000000] CPU features: enabling workaround for ARM erratum 845719
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 1031436
[    0.000000] Kernel command line: earlycon loglevel=8 kgdboc=ttyS0 video=hobot:x3sdb-hdmi  console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
[    0.000000] PID hash table entries: 4096 (order: 3, 32768 bytes)
[    0.000000] Dentry cache hash table entries: 524288 (order: 10, 4194304 bytes)
[    0.000000] Inode-cache hash table entries: 262144 (order: 9, 2097152 bytes)
[    0.000000] software IO TLB [mem 0x7afff000-0x7efff000] (64MB) mapped at [ffffffc07afff000-ffffffc07effefff]
[    0.000000] Memory: 3319580K/4191232K available (10494K kernel code, 1306K rwdata, 5756K rodata, 1088K init, 9553K bss, 167140K reserved, 704512K cma-reserved)
[    0.000000] Virtual kernel memory layout:
[    0.000000]     modules : 0xffffff8000000000 - 0xffffff8008000000   (   128 MB)
[    0.000000]     vmalloc : 0xffffff8008000000 - 0xffffffbebfff0000   (   250 GB)
[    0.000000]       .text : 0xffffff8008000000 - 0xffffff8008a40000   ( 10496 KB)
[    0.000000]     .rodata : 0xffffff8008a40000 - 0xffffff8008ff0000   (  5824 KB)
[    0.000000]       .init : 0xffffff8008ff0000 - 0xffffff8009100000   (  1088 KB)
[    0.000000]       .data : 0xffffff8009100000 - 0xffffff8009246808   (  1307 KB)
[    0.000000]        .bss : 0xffffff8009246808 - 0xffffff8009b9aed8   (  9554 KB)
[    0.000000]     fixed   : 0xffffffbefe7fd000 - 0xffffffbefec00000   (  4108 KB)
[    0.000000]     PCI I/O : 0xffffffbefee00000 - 0xffffffbeffe00000   (    16 MB)
[    0.000000]     vmemmap : 0xffffffbf00000000 - 0xffffffc000000000   (     4 GB maximum)
[    0.000000]               0xffffffbf00008000 - 0xffffffbf06000000   (    95 MB actual)
[    0.000000]     memory  : 0xffffffc000200000 - 0xffffffc180000000   (  6142 MB)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=4, Nodes=1
[    0.000000] ftrace: allocating 36277 entries in 142 pages
[    0.000000] Preemptible hierarchical RCU implementation.
[    0.000000]  Tasks RCU enabled.
[    0.000000] NR_IRQS: 64, nr_irqs: 64, preallocated irqs: 0
[    0.000000] parent_rate: 0,  dclk->rate:2666000000, pre_ddr_rate:0, res.a0:139716712
[    0.000000] arch_timer: cp15 timer(s) running at 24.00MHz (virt).
[    0.000000] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0x588fe9dc0, max_idle_ns: 440795202592 ns
[    0.000003] sched_clock: 56 bits at 24MHz, resolution 41ns, wraps every 4398046511097ns
[    0.001192] clocksource: hobot_clocksource: mask: 0xffffffffffffffff max_cycles: 0x1d854df40, max_idle_ns: 3526361616960 ns
[    0.002963] Console: colour dummy device 80x25
[    0.003535] Calibrating delay loop (skipped), value calculated using timer frequency.. 48.00 BogoMIPS (lpj=96000)
[    0.004840] pid_max: default: 32768 minimum: 301
[    0.005496] Security Framework initialized
[    0.006014] AppArmor: AppArmor disabled by boot time parameter
[    0.006857] Mount-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.007724] Mountpoint-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.023767] ASID allocator initialised with 65536 entries
[    0.031765] Hierarchical SRCU implementation.
[    0.063824] smp: Bringing up secondary CPUs ...
[    0.100031] Detected VIPT I-cache on CPU1
[    0.100066] CPU1: Booted secondary processor [410fd034]
[    0.136081] Detected VIPT I-cache on CPU2
[    0.136102] CPU2: Booted secondary processor [410fd034]
[    0.172140] Detected VIPT I-cache on CPU3
[    0.172160] CPU3: Booted secondary processor [410fd034]
[    0.172214] smp: Brought up 1 node, 4 CPUs
[    0.176277] SMP: Total of 4 processors activated.
[    0.176871] CPU features: detected feature: 32-bit EL0 Support
[    0.177690] CPU: All CPU(s) started at EL1
[    0.178219] alternatives: patching kernel code
[    0.179809] devtmpfs: initialized
[    0.188890] random: get_random_u32 called from bucket_table_alloc+0x108/0x270 with crng_init=0
[    0.190476] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 7645041785100000 ns
[    0.191722] futex hash table entries: 1024 (order: 5, 131072 bytes)
[    0.208255] xor: automatically using best checksumming function   32regs
[    0.209194] pinctrl core: initialized pinctrl subsystem
[    0.210424] NET: Registered protocol family 16
[    0.211746] vdso: 2 pages (1 code @ ffffff8008a46000, 1 data @ ffffff8009104000)
[    0.212691] hw-breakpoint: found 6 breakpoint and 4 watchpoint registers.
[    0.214279] DMA: preallocated 256 KiB pool for atomic allocations
[    0.218388] pstore: using zlib compression
[    0.219183] console [pstore-1] enabled
[    0.219779] pstore: Registered ramoops as persistent store backend
[    0.220564] ramoops: attached 0x40000@0x3fc0000, ecc: 0/0
[    0.225536] hobot_dma a1005000.dma: Hobot DMA Engine Driver Probed!!
[    0.239311] SCSI subsystem initialized
[    0.239945] media: Linux media interface: v0.10
[    0.240700] Linux video capture interface: v2.00
[    0.241341] pps_core: LinuxPPS API ver. 1 registered
[    0.241968] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.243144] PTP clock support registered
[    0.244280] ion_dummy: not reserve carveout memory, try to alloc from cma
[    0.381014] Advanced Linux Sound Architecture Driver Initialized.
[    0.382232] usbcore: registered new interface driver usbfs
[    0.382959] usbcore: registered new interface driver hub
[    0.383686] usbcore: registered new device driver usb
[    0.384632] clocksource: Switched to clocksource arch_sys_counter
[    0.432338] VFS: Disk quotas dquot_6.6.0
[    0.432909] VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
[    0.433851] FS-Cache: Loaded
[    0.434333] CacheFiles: Loaded
[    0.439604] NET: Registered protocol family 2
[    0.440525] TCP established hash table entries: 32768 (order: 6, 262144 bytes)
[    0.441670] TCP bind hash table entries: 32768 (order: 7, 524288 bytes)
[    0.442920] TCP: Hash tables configured (established 32768 bind 32768)
[    0.443833] UDP hash table entries: 2048 (order: 4, 65536 bytes)
[    0.444691] UDP-Lite hash table entries: 2048 (order: 4, 65536 bytes)
[    0.445691] NET: Registered protocol family 1
[    0.446527] RPC: Registered named UNIX socket transport module.
[    0.447278] RPC: Registered udp transport module.
[    0.447875] RPC: Registered tcp transport module.
[    0.448474] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.450114] hw perfevents: enabled with armv8_cortex_a53 PMU driver, 7 counters available
[    0.452323] audit: initializing netlink subsys (disabled)
[    0.453129] audit: type=2000 audit(0.448:1): state=initialized audit_enabled=0 res=1
[    0.453376] Initialise system trusted keyrings
[    0.453454] workingset: timestamp_bits=46 max_order=20 bucket_order=0
[    0.457209] zbud: loaded
[    0.458762] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.459622] exFAT: Version 1.2.9
[    0.460101] FS-Cache: Netfs 'nfs' registered for caching
[    0.461339] NFS: Registering the id_resolver key type
[    0.461992] Key type id_resolver registered
[    0.462519] Key type id_legacy registered
[    0.463034] nfs4filelayout_init: NFSv4 File Layout Driver Registering...
[    0.463888] Installing knfsd (copyright (C) 1996 okir@monad.swb.de).
[    0.467984] NET: Registered protocol family 38
[    0.468557] async_tx: api initialized (async)
[    0.469135] Key type asymmetric registered
[    0.469653] Asymmetric key parser 'x509' registered
[    0.470340] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 245)
[    0.471358] io scheduler noop registered
[    0.472012] io scheduler cfq registered (default)
[    0.472608] io scheduler mq-deadline registered
[    0.473350] io scheduler kyber registered
[    0.474544] pinctrl-single a6003170.pinctrl_voltag: 64 pins at pa ffffff8009c4d170 size 8
[    0.475883] pinctrl-single a6004000.pinctrl: 128 pins at pa ffffff8009c61000 size 512
[    0.477109] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: start probe
[    0.478003] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: probe ok
[    0.478871] gpio-x3 a6003000.gpio: x3 gpio probe start!!!
[    0.479561] gpio-x3 a6003000.gpio: x3 gpio add gpiochip start!!!
[    0.480484] gpio-x3 a6003000.gpio: diable all gpio irq
[    0.482745] gpio-x3 a6003000.gpio: irqbase:57
[    0.483296] gpio-x3 a6003000.gpio: x3 irq add start!!!
[    0.483953] irq: Cannot allocate irq_descs @ IRQ57, assuming pre-allocated
[    0.485181] gpio-x3 a6003000.gpio: x3 irq add ok!!!
[    0.485839] gpio-x3 a6003000.gpio: x3 irqchip ops add ok!!!
[    0.486544] gpio-x3 a6003000.gpio: x3 gpio probe ok!!!
[    0.487626] hobot-pwm: hobot-pwmchip0 registered
[    0.488376] hobot-pwm: hobot-pwmchip1 registered
[    0.489719] diag dev [ver:1.1] init done
[    0.490613] hobot_ddr_monitor: LPDDR4 detected
[    0.491368] hobot_ddr_monitor: ddr monitor init finished.
[    0.491750] [vcam] init start
[    0.492824] vcam probe start
[    0.493283] vcam probe end successful
[    0.493744] [vcam] init end
[    0.494663] a5000000.serial: ttyS0 at MMIO 0xa5000000 (irq = 10, base_baud = 12000000) is a hobot-uart
[    0.495877] console [ttyS0] enabled
[    0.495877] console [ttyS0] enabled
[    0.496850] bootconsole [hobot0] disabled
[    0.496850] bootconsole [hobot0] disabled
[    0.498183] hobot-uart a5001000.serial: Failed to create debugfs root directory
[    0.499186] a5001000.serial: ttyS1 at MMIO 0xa5001000 (irq = 11, base_baud = 12000000) is a hobot-uart
[    0.500656] hobot-uart a5003000.serial: Failed to create debugfs root directory
[    0.501654] a5003000.serial: ttyS3 at MMIO 0xa5003000 (irq = 12, base_baud = 12000000) is a hobot-uart
[    0.503192] KGDB: Registered I/O driver kgdboc
[    0.504021] cacheinfo: Unable to detect cache hierarchy for CPU 0
[    0.509487] brd: module loaded
[    0.514060] loop: module loaded
[    0.515618] spi-nand hr_nand.0: GigaDevice SPI NAND was found.
[    0.516393] spi-nand hr_nand.0: 128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
[    0.519118] hobot_spi a5006000.spi: ver: HOBOT-spi_V20.200330 master
[    0.520163] libphy: Fixed MDIO Bus: probed
[    0.521413] st_gmac a5014000.ethernet: found phy-handle subnode
[    0.522248] st_gmac a5014000.ethernet: xj3_mtl_setup, plat->rx-queues-to-use:4, and tx:4
[    0.523432] st_gmac a5014000.ethernet: xj3_probe_config_dt, clk_ptp_rate:250000000
[    0.524435] set mac address 00:11:22:d7:bc:7b:
[    0.524437] (using random mac adress)
[    0.525547] (NULL device *): xj3_get_hw_features, tx_fifo_size:16384
[    0.526364] (NULL device *): xj3_get_hw_features, rx_fifo_size:16384
[    0.527181] st_gmac a5014000.ethernet: TSO supported
[    0.527821] st_gmac a5014000.ethernet: TSO feature enabled
[    0.528527] st_gmac a5014000.ethernet: Enable Rx Mitigation via HW Watchdog Timer
[    0.649613] libphy: hobot-mac-mdio: probed
[    0.651159] st_gmac a5014000.ethernet: hobot_eth_probe: probe sucessfully
[    0.652358] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_0v8 not found, using dummy regulator
[    0.653599] dwc3-of-simple b2000000.usb: usb regulator 0v8 enable succeed
[    0.654477] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_3v3 not found, using dummy regulator
[    0.655690] dwc3-of-simple b2000000.usb: usb regulator 3v3 enable succeed
[    0.657234] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    0.658891] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    0.660321] usbcore: registered new interface driver cdc_acm
[    0.661071] cdc_acm: USB Abstract Control Model driver for USB modems and ISDN adapters
[    0.662128] usbcore: registered new interface driver uas
[    0.662848] usbcore: registered new interface driver usb-storage
[    0.663678] usbcore: registered new interface driver usbserial
[    0.664450] usbcore: registered new interface driver usbserial_generic
[    0.665326] usbserial: USB Serial support registered for generic
[    0.666123] usbcore: registered new interface driver usb_serial_simple
[    0.666979] usbserial: USB Serial support registered for carelink
[    0.667782] usbserial: USB Serial support registered for zio
[    0.668527] usbserial: USB Serial support registered for funsoft
[    0.669335] usbserial: USB Serial support registered for flashloader
[    0.670169] usbserial: USB Serial support registered for google
[    0.670947] usbserial: USB Serial support registered for libtransistor
[    0.671804] usbserial: USB Serial support registered for vivopay
[    0.672596] usbserial: USB Serial support registered for moto_modem
[    0.673435] usbserial: USB Serial support registered for motorola_tetra
[    0.674302] usbserial: USB Serial support registered for novatel_gps
[    0.675136] usbserial: USB Serial support registered for hp4x
[    0.675893] usbserial: USB Serial support registered for suunto
[    0.676680] usbserial: USB Serial support registered for siemens_mpi
[    0.677527] usbcore: registered new interface driver rio500
[    0.678356] mousedev: PS/2 mouse device common for all mice
[    0.689403] hobot-rtc a6002000.rtc: rtc core: registered hobot-rtc as rtc0
[    0.690394] i2c /dev entries driver
[    0.691003] hobot-i2c a5009000.i2c: hobot i2c probe start
[    0.691766] hobot-i2c a5009000.i2c: round_rate:96000000
[    0.692443] hobot-i2c a5009000.i2c: I2C bus speed is 400000
[    0.693184] hobot-i2c a5009000.i2c: clkdiv = 0x1d
[    0.693792] hobot-i2c a5009000.i2c: i2c0 diag register....
[    0.694898] hobot-i2c a5009000.i2c: hobot_i2c_0 probe done
[    0.695701] hobot-i2c a500a000.i2c: hobot i2c probe start
[    0.696458] hobot-i2c a500a000.i2c: round_rate:96000000
[    0.697156] hobot-i2c a500a000.i2c: I2C bus speed is 400000
[    0.697874] hobot-i2c a500a000.i2c: clkdiv = 0x1d
[    0.698480] hobot-i2c a500a000.i2c: i2c1 diag register....
[    0.699505] hobot-i2c a500a000.i2c: hobot_i2c_1 probe done
[    0.700468] lirc_dev: IR Remote Control driver registered, major 239
[    0.701308] IR LIRC bridge handler initialized
[    0.702066] sif_mclk clock frequence is 544000000
[    0.702704] mipi_rx0_ipi clock frequence is 544000000
[    0.703393] mipi_rx1_ipi clock frequence is 544000000
[    0.704091] mipi_rx2_ipi clock frequence is 544000000
[    0.704820] mipi_rx3_ipi clock frequence is 544000000
[    0.705540] mipi_tx_ipi clock frequence is 544000000
[    0.706260] mipi_cfg_host clock frequence is 102000000
[    0.707013] pym_mclk clock frequence is 1188000000
[    0.707733] mipi_dev_ref clock frequence is 24000000
[    0.708486] mipi_host_ref clock frequence is 24000000
[    0.709281] sensor0_mclk clock frequence is 37125000
[    0.710059] sensor1_mclk clock frequence is 37125000
[    0.710845] sensor2_mclk clock frequence is 37125000
[    0.711646] sensor3_mclk clock frequence is 37125000
[    0.712285] [FRT:D] x3_ips_probe(0)
[    0.713313] hobot swinfo sel reg ro=0x1 boot dump
[    0.714227] pvt a1009000.pvt: SCRATCH test: 1234abcd, pvt is alive.
[    0.715151] pvt a1009000.pvt: VM Calibrated data detected
[    0.716324] hobot_wdt a1002000.watchdog: watchdog setting [pet:6s bark:11s bite:15s]
[    0.717676] hobot_wdt a1002000.watchdog: Hobot Watchdog Timer at ffffff8009db3000 with timeout 15s
[    0.719030] device-mapper: uevent: version 1.0.3
[    0.719793] device-mapper: ioctl: 4.37.0-ioctl (2017-09-20) initialised: dm-devel@redhat.com
[    0.720975] device-mapper: verity-avb: AVB error handler initialized with vbmeta device:
[    0.723377] Synopsys Designware Multimedia Card Interface Driver
[    0.724376] dwmmc_hobot a5010000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.725233] dwmmc_hobot a5010000.dwmmc: card-detect-delay not found.
[    0.726051] dwmmc_hobot a5010000.dwmmc: data-addr not found.
[    0.727090] mmc_host mmc0: card is non-removable.
[    0.765844] dwmmc_hobot a5011000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.768684] dwmmc_hobot a5011000.dwmmc: card-detect-delay not found.
[    0.769504] dwmmc_hobot a5011000.dwmmc: data-addr not found.
[    0.774273] dwmmc_hobot a5011000.dwmmc: mmc set to fixed voltage 1800
[    0.775333] mmc_host mmc1: card is non-removable.
[    0.872837] dwmmc_hobot a5012000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.873678] dwmmc_hobot a5012000.dwmmc: card-detect-delay not found.
[    0.874519] dwmmc_hobot a5012000.dwmmc: data-addr not found.
[    0.875487] dwmmc_hobot a5012000.dwmmc: Got CD GPIO
[    0.986443] mmc1: queuing unknown CIS tuple 0x80 (2 bytes)
[    0.988641] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.990833] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.994209] mmc1: queuing unknown CIS tuple 0x80 (7 bytes)
[    0.998176] mmc1: queuing unknown CIS tuple 0x81 (9 bytes)
[    1.064961] ledtrig-cpu: registered to indicate activity on CPUs
[    1.065814] hidraw: raw HID events driver (C) Jiri Kosina
[    1.066687] usbcore: registered new interface driver usbhid
[    1.067411] usbhid: USB HID core driver
[    1.067993] logger: created 256K log 'log_main'
[    1.068670] logger: created 256K log 'log_events'
[    1.069338] logger: created 256K log 'log_radio'
[    1.069991] logger: created 256K log 'log_system'
[    1.071012] set dmc devfreq governor to performance
[    1.071645] hobot_dmcfreq_target: dmcfreq->rate:2666000000, target_rate:2666000000
[    1.072617] buf:, powersave_rate:2666000000, dmcfreq->pre_state:0
[    1.079439] usbcore: registered new interface driver snd-usb-audio
[    1.080582] Netfilter messages via NETLINK v0.30.
[    1.081248] ip_set: protocol 6
[    1.081732] ipip: IPv4 and MPLS over IPv4 tunneling driver
[    1.082732] ip_tables: (C) 2000-2006 Netfilter Core Team
[    1.083659] arp_tables: arp_tables: (C) 2002 David S. Miller
[    1.084447] Initializing XFRM netlink socket
[    1.085333] NET: Registered protocol family 10
[    1.086552] Segment Routing with IPv6
[    1.087061] sit: IPv6, IPv4 and MPLS over IPv4 tunneling driver
[    1.088151] NET: Registered protocol family 17
[    1.088829] Key type dns_resolver registered
[    1.090473] Loading compiled-in X.509 certificates
[    1.093980] Loaded X.509 cert 'Build time autogenerated kernel key: 81cb0ef77db2fac76e9588c2120c82422367d268'
[    1.095314] zswap: loaded using pool lzo/zbud
[    1.106656] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    1.108319] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    1.109370] console [netcon0] enabled
[    1.109845] netconsole: network logging started
[    1.110626] hobot-rtc a6002000.rtc: setting system clock to 1970-01-01 00:00:00 UTC (0)
[    1.111816] vps mipi_dphy: probe with x3vio done
[    1.112524] hobot_wdt_test: wdt_test_init: wdt test init
[    1.115277] VCC_CNN0: disabling
[    1.115687] VCC_CNN1: disabling
[    1.116668] vps mipi_host0: ver 140* port0(0:0)
[    1.117598] vps mipi_host1: ver 140* port1(1:0)
[    1.118493] vps mipi_host2: ver 140* port2(0:1)
[    1.119285] vps mipi_host3: ver 140* port3(1:1)
[    1.120119] ALSA device list:
[    1.120503]   No soundcards found.
[    1.121158] md: Skipping autodetection of RAID arrays. (raid=autodetect will force)
[    1.122296] VFS: Cannot open root device "mmcblk2p2" or unknown-block(0,0): error -6
[    1.123290] Please append a correct "root=" boot option; here are the available partitions:
[    1.124364] 0100          102400 ram0
[    1.124366]  (driver?)
[    1.125189] 0101          102400 ram1
[    1.125191]  (driver?)
[    1.125980] 0102          102400 ram2
[    1.125981]  (driver?)
[    1.126769] 0103          102400 ram3
[    1.126771]  (driver?)
[    1.127559] 0104          102400 ram4
[    1.127561]  (driver?)
[    1.128348] 0105          102400 ram5
[    1.128350]  (driver?)
[    1.129179] 0106          102400 ram6
[    1.129181]  (driver?)
[    1.129969] 0107          102400 ram7
[    1.129971]  (driver?)
[    1.130759] 0108          102400 ram8
[    1.130761]  (driver?)
[    1.131548] 0109          102400 ram9
[    1.131550]  (driver?)
[    1.132338] 010a          102400 ram10
[    1.132340]  (driver?)
[    1.133173] 010b          102400 ram11
[    1.133175]  (driver?)
[    1.133975] 010c          102400 ram12
[    1.133977]  (driver?)
[    1.134776] 010d          102400 ram13
[    1.134777]  (driver?)
[    1.135576] 010e          102400 ram14
[    1.135578]  (driver?)
[    1.136377] 010f          102400 ram15
[    1.136378]  (driver?)
[    1.137196] 1f00          131072 mtdblock0
[    1.137198]  (driver?)
[    1.138042] hobot_fusa: set_fusa_error_pin:75 set error pin to 1
[    1.138812] hobot_fusa: fusa errpin not ready
[    1.138816] Kernel panic - not syncing: VFS: Unable to mount root fs on unknown-block(0,0)
[    1.140435] Kernel Offset: disabled
[    1.140886] CPU features: 0x0002004
[    1.141335] Memory Limit: none
[    1.145893] Rebooting in 1 seconds..
[    1.216880] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.217602] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 1
[    1.219062] xhci-hcd xhci-hcd.0.auto: hcc params 0x0220fe6d hci version 0x110 quirks 0x0000000000010010
[    1.220296] xhci-hcd xhci-hcd.0.auto: irq 178, io mem 0xb2000000
[    1.221262] usb usb1: New USB device found, idVendor=1d6b, idProduct=0002, bcdDevice= 4.14
[    1.222326] usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.223254] usb usb1: Product: xHCI Host Controller
[    1.223883] usb usb1: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.224589] usb usb1: SerialNumber: xhci-hcd.0.auto
[    1.225545] hub 1-0:1.0: USB hub found
[    1.226048] hub 1-0:1.0: 1 port detected
[    1.226734] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.227447] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 2
[    1.228435] xhci-hcd xhci-hcd.0.auto: Host supports USB 3.0 SuperSpeed
[    1.230577] mmc1: new HSSDIO card at address 0001
[    1.231413] usb usb2: We don't know the algorithms for LPM for this host, disabling LPM.
[    1.232518] usb usb2: New USB device found, idVendor=1d6b, idProduct=0003, bcdDevice= 4.14
[    1.233590] usb usb2: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.234519] usb usb2: Product: xHCI Host Controller
[    1.235148] usb usb2: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.235853] usb usb2: SerialNumber: xhci-hcd.0.auto
[    1.236773] hub 2-0:1.0: USB hub found
[    1.237274] hub 2-0:1.0: 1 port detected
[    1.480645] usb 1-1: new high-speed USB device number 2 using xhci-hcd
[    1.628836] usb 1-1: New USB device found, idVendor=1a40, idProduct=0101, bcdDevice= 1.11
[    1.629888] usb 1-1: New USB device strings: Mfr=0, Product=1, SerialNumber=0
[    1.630805] usb 1-1: Product: USB 2.0 Hub
[    1.679569] hub 1-1:1.0: USB hub found
[    1.680088] hub 1-1:1.0: 4 ports detected
[    2.085879] mmc2: new UHS SDR104 SDHC card at address 0001
[    2.086894] mmcblk2: mmc2:0001 SD16G 29.8 GiB
[    2.088513]  mmcblk2: p1 p2
[    2.146404] SMP: stopping secondary CPUs
[    2.146913] psci: psci_sys_reset(reboot_mode=0)
NOTICE:  fast_boot:0

S
F
L
O
NOTICE:  efuse cpu_cfg = 0
W
NOTICE:  Booting Trusted Firmware
NOTICE:  BL1: v1.4(release):HR-ROM-Rel-v1.1-141-ga91d4dd-dirty
NOTICE:  BL1: Built : 11:24:44, Oct 23 2019
NOTICE:  boot src: 2
NOTICE:  GigaDev SPI NAND was found.
NOTICE:  Block size: 128 KiB, page size: 2048
NOTICE:  BL1: Booting BL2
Auth pass
NOTICE:  bl1_main exit
SPL normal reset flow
check_reset_state (2): wakeup address = 0x0, hw wakeup status = 0x3, wakeup src=0x100
patch for sys_pll 1200 with 100M eth
SFLOW_INIT
CHIP ID:PCB941/WAFER: W04/ X: X20/ Y: Y36
secondary_jump_to_spl: secure chip flow
X3 SPL : secondary core wake up and jump to spl done (cpu_core_cfg=0)
SFLOW_FIN_HW_A

U-Boot SPL 2018.09-g4ca851534c-dirty (May 11 2022 - 20:09:50 +0800)
SPACC Init - ID: (00000061)
SPL nand boot mode (from strap)
GigaDev SPI NAND was found.
Block size: 128 KiB, page size: 2048
ddr_type = 1 (LPDDR4)
hb_chip_package_type:3
load ddr header src_addr: 100000, load_addr: 802ca020, src_len: a00
find valid ddr image
ddr_hdr.ecc_gran: 0x0
ddr_hdr.ecc_map: 0x0
ddr_hdr.sbr_pattern0: 0x0
ddr_hdr.sbr_pattern1: 0x0
ddr_freq = 05
board id = 31540334
ddr datarate: 3200
### SAMSUNG DDR ###
no ddr pin set
detect part number: 108
detect ddr freq: c80
board id alternative:0x3
index is 12
index is 15
index is 19
hb_ddr_index: 19
ddr_type = 1, ddr_vendor=3, ddr_freq=3200
dram_pll_init
sscg disabled
control load ddrc src_addr: 15ae00, load_addr: 802caa20, src_len: 920
[DDR INFO]      ==ddr_release_info==
[DDR INFO]      VERSION:        develop
[DDR INFO]      BUILD:          2022-05-11-20:09
[DDR INFO]      GIT COMMIT:     4ca851534c1616ace920fdaa000c6fb717c1fb74
[DDR INFO]      GIT TIME:       Wed, 20 Apr 2022 18:28:49 +0800
[DDR INFO]      ==ddr_features==
[DDR INFO]      RDBI:           0
[DDR INFO]      WDBI:           1
[DDR INFO]      InlineECC:      0
[DDR INFO]      DM:             1
[DDR INFO]      DDC:            1
[DDR INFO]      SSCG:           0
[DDR INFO]      BOARD:          XS_ENABLE
[DDR INFO] ddr_controller_cfg done
load ddr phy src_addr: 15b800, load_addr: 802caa20, src_len: 420
ATxSlewRate     : 15f
ATxImpedance    : 7f
TxSlewRate      : 19f
TxOdtDrvStren   : 600
TxImpedanceCtrl : e3f
CalDrvStr0      : 11
VrefInGlobal    : 104
board_type = 4 (CUSTOMER_BOARD)
load dqmap src addr: 15d600, load_addr: 802caa20, src_len: 20
[DDR INFO] dwc_ddrphy_train start
magic = 544f4248
load imem1 src_addr: 11ce00, load_addr: 802caa20, src_len: 8000
load dmem1 src_addr: 15a000, load_addr: 802caa20, src_len: 684
executing 1D fw
load imem2 src_addr: 124e00, load_addr: 802caa20, src_len: 8000
load dmem2 src_addr: 15a800, load_addr: 802caa20, src_len: 564

*******************************************************
p_dmem_lpddr4_2d_16b->MR11_A0:54
p_dmem_lpddr4_2d_16b->MR14_A0:54
p_dmem_lpddr4_2d_16b->MR12_A0:51
p_dmem_lpddr4_2d_16b->MR22_A0:14

p_dmem_lpddr4_2d_16b->MR3_A0:b3
p_dmem_lpddr4_2d_16b->Reserved00:40
p_dmem_lpddr4_2d_16b->Reserved0E:4
p_dmem_lpddr4_2d_16b->Delay_Weight2D:20
p_dmem_lpddr4_2d_16b->Voltage_Weight2D:80
*******************************************************

executing 2D fw
load pie src_addr: 15be00, load_addr: 802caa20, src_len: 11f0
Set QoS.
get_ddr_mr_info:cs_num=1, mr5=0x1, mr8=0x10
no magic in efuse file,bypass efuse
total_sz = 4096
SPL_VERSION:7
uboot partition is uboot_A
load u-boot: src_addr=0x380000, dest_addr=0x4000000, len=2097152
load warm boot spl: addr=0x800, dest_addr=0x80000000, len=31232
load bl31: addr=0x300000, dest_addr=0x0, len=524288
SFLOW_AUTH_BL31
verify signature of header:  verify ok!
verify signature of image:  verify ok!
bypass bpu image
clear keybank!!!!
SFLOW_DBG_EN
Trying to boot from RAM
SPL: bl31 will jump to u-boot or other entry (0x4000000)
SFLOW_CLR_KEY
SFLOW_REG_LD
install_portal copy portal
install_portal call smc and jump to bl31 cold entry(0x0)
hb som type: 5
X3 PI reset VDD_SD done

U-Boot 2018.09-g40785bca (May 27 2022 - 16:30:48 +0800)

Model: Hobot XJ3 Soc Board
DRAM:  system DDR size: 0xffe00000
4 GiB
MMC:   dwmmc@A5010000: 0, dwmmc@A5011000: 1, dwmmc@A5012000: 2
Loading Environment from UBI... GigaDevice SPI NAND was found.
128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
*** Warning - bad CRC, using default environment

In:    serial@a5000000
Out:   serial@a5000000
Err:   serial@a5000000
Net:   x3 sdb reset eth phy done

Warning: ethernet@A5014000 (eth0) using random MAC address - 02:b4:ad:5f:21:b5
eth0: ethernet@A5014000
Disable cnn cores ..
dtb_name:hobot-x3-pi.dtb
base board type: X3 SDB
bootmode: NAND
board_id = 31540334
damaged volume, update marker is setdamaged volume, update marker is setdamaged volume, update marker is sethb_boot_args_cmd_set custom_bootargs 0 ubuntu_boot 0
Hit any key to stop autoboot:  0
enable watchdog success !
switch to partitions #0, OK
mmc2 is current device
Scanning mmc 2:2...
Found U-Boot script /boot/boot.scr
664 bytes read in 1 ms (648.4 KiB/s)
## Executing script at 03c10000
Boot script loaded from devtype:mmc devnum:2 devplist:2
bootargs = console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
Loading fdt file: /boot/hobot/hobot-x3-pi.dtb
69633 bytes read in 8 ms (8.3 MiB/s)
Loading kernel: /boot/Image
19163144 bytes read in 845 ms (21.6 MiB/s)
## Flattened Device Tree blob at 03c00000
   Booting using the fdt blob at 0x3c00000
   Loading Device Tree to 0000000003c00000, end 0000000003c1ffff ... OK
chip_id: ab36300
The address of the fdt is 0x3c00000
Changed status Done
Can't get fdt_addr !!!Orign(MAX) bpu model Reserve Mem Size to 64M!!

Starting kernel ...

[    0.000000] OF: reserved mem: OVERLAP DETECTED!
[    0.000000] image_r5_mem (0x0000000080000000--0x0000000080010000) overlaps with msg_r5_mem (0x000000008000f000--0x0000000080010000)
[    0.000000] Reserved memory: created CMA memory pool at 0x0000000004000000, size 672 MiB
[    0.000000] OF: reserved mem: initialized node ion_cma, compatible id shared-dma-pool
[    0.000000] cma: Reserved 16 MiB at 0x000000007f000000
[    0.000000] On node 0 totalpages: 1047808
[    0.000000]   DMA zone: 8180 pages used for memmap
[    0.000000]   DMA zone: 0 pages reserved
[    0.000000]   DMA zone: 523520 pages, LIFO batch:31
[    0.000000]   Normal zone: 8192 pages used for memmap
[    0.000000]   Normal zone: 524288 pages, LIFO batch:31
[    0.000000] psci: probing for conduit method from DT.
[    0.000000] psci: PSCIv1.1 detected in firmware.
[    0.000000] psci: Using standard PSCI v0.2 function IDs
[    0.000000] psci: MIGRATE_INFO_TYPE not supported.
[    0.000000] psci: SMC Calling Convention v1.1
[    0.000000] percpu: Embedded 25 pages/cpu @ffffffc17ff2a000 s65176 r8192 d29032 u102400
[    0.000000] pcpu-alloc: s65176 r8192 d29032 u102400 alloc=25*4096
[    0.000000] pcpu-alloc: [0] 0 [0] 1 [0] 2 [0] 3
[    0.000000] Detected VIPT I-cache on CPU0
[    0.000000] CPU features: enabling workaround for ARM erratum 845719
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 1031436
[    0.000000] Kernel command line: earlycon loglevel=8 kgdboc=ttyS0 video=hobot:x3sdb-hdmi  console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
[    0.000000] PID hash table entries: 4096 (order: 3, 32768 bytes)
[    0.000000] Dentry cache hash table entries: 524288 (order: 10, 4194304 bytes)
[    0.000000] Inode-cache hash table entries: 262144 (order: 9, 2097152 bytes)
[    0.000000] software IO TLB [mem 0x7afff000-0x7efff000] (64MB) mapped at [ffffffc07afff000-ffffffc07effefff]
[    0.000000] Memory: 3319580K/4191232K available (10494K kernel code, 1306K rwdata, 5756K rodata, 1088K init, 9553K bss, 167140K reserved, 704512K cma-reserved)
[    0.000000] Virtual kernel memory layout:
[    0.000000]     modules : 0xffffff8000000000 - 0xffffff8008000000   (   128 MB)
[    0.000000]     vmalloc : 0xffffff8008000000 - 0xffffffbebfff0000   (   250 GB)
[    0.000000]       .text : 0xffffff8008000000 - 0xffffff8008a40000   ( 10496 KB)
[    0.000000]     .rodata : 0xffffff8008a40000 - 0xffffff8008ff0000   (  5824 KB)
[    0.000000]       .init : 0xffffff8008ff0000 - 0xffffff8009100000   (  1088 KB)
[    0.000000]       .data : 0xffffff8009100000 - 0xffffff8009246808   (  1307 KB)
[    0.000000]        .bss : 0xffffff8009246808 - 0xffffff8009b9aed8   (  9554 KB)
[    0.000000]     fixed   : 0xffffffbefe7fd000 - 0xffffffbefec00000   (  4108 KB)
[    0.000000]     PCI I/O : 0xffffffbefee00000 - 0xffffffbeffe00000   (    16 MB)
[    0.000000]     vmemmap : 0xffffffbf00000000 - 0xffffffc000000000   (     4 GB maximum)
[    0.000000]               0xffffffbf00008000 - 0xffffffbf06000000   (    95 MB actual)
[    0.000000]     memory  : 0xffffffc000200000 - 0xffffffc180000000   (  6142 MB)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=4, Nodes=1
[    0.000000] ftrace: allocating 36277 entries in 142 pages
[    0.000000] Preemptible hierarchical RCU implementation.
[    0.000000]  Tasks RCU enabled.
[    0.000000] NR_IRQS: 64, nr_irqs: 64, preallocated irqs: 0
[    0.000000] parent_rate: 0,  dclk->rate:2666000000, pre_ddr_rate:0, res.a0:139716712
[    0.000000] arch_timer: cp15 timer(s) running at 24.00MHz (virt).
[    0.000000] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0x588fe9dc0, max_idle_ns: 440795202592 ns
[    0.000004] sched_clock: 56 bits at 24MHz, resolution 41ns, wraps every 4398046511097ns
[    0.001195] clocksource: hobot_clocksource: mask: 0xffffffffffffffff max_cycles: 0x1d854df40, max_idle_ns: 3526361616960 ns
[    0.002968] Console: colour dummy device 80x25
[    0.003539] Calibrating delay loop (skipped), value calculated using timer frequency.. 48.00 BogoMIPS (lpj=96000)
[    0.004845] pid_max: default: 32768 minimum: 301
[    0.005500] Security Framework initialized
[    0.006018] AppArmor: AppArmor disabled by boot time parameter
[    0.006861] Mount-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.007729] Mountpoint-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.023772] ASID allocator initialised with 65536 entries
[    0.031769] Hierarchical SRCU implementation.
[    0.063829] smp: Bringing up secondary CPUs ...
[    0.100035] Detected VIPT I-cache on CPU1
[    0.100069] CPU1: Booted secondary processor [410fd034]
[    0.136084] Detected VIPT I-cache on CPU2
[    0.136105] CPU2: Booted secondary processor [410fd034]
[    0.172144] Detected VIPT I-cache on CPU3
[    0.172164] CPU3: Booted secondary processor [410fd034]
[    0.172217] smp: Brought up 1 node, 4 CPUs
[    0.176280] SMP: Total of 4 processors activated.
[    0.176874] CPU features: detected feature: 32-bit EL0 Support
[    0.177693] CPU: All CPU(s) started at EL1
[    0.178221] alternatives: patching kernel code
[    0.179810] devtmpfs: initialized
[    0.188912] random: get_random_u32 called from bucket_table_alloc+0x108/0x270 with crng_init=0
[    0.190483] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 7645041785100000 ns
[    0.191728] futex hash table entries: 1024 (order: 5, 131072 bytes)
[    0.208254] xor: automatically using best checksumming function   32regs
[    0.209192] pinctrl core: initialized pinctrl subsystem
[    0.210421] NET: Registered protocol family 16
[    0.211741] vdso: 2 pages (1 code @ ffffff8008a46000, 1 data @ ffffff8009104000)
[    0.212685] hw-breakpoint: found 6 breakpoint and 4 watchpoint registers.
[    0.214274] DMA: preallocated 256 KiB pool for atomic allocations
[    0.219100] pstore: using zlib compression
[    0.219897] console [pstore-1] enabled
[    0.220497] pstore: Registered ramoops as persistent store backend
[    0.221282] ramoops: attached 0x40000@0x3fc0000, ecc: 0/0
[    0.226288] hobot_dma a1005000.dma: Hobot DMA Engine Driver Probed!!
[    0.240033] SCSI subsystem initialized
[    0.240694] media: Linux media interface: v0.10
[    0.241288] Linux video capture interface: v2.00
[    0.241937] pps_core: LinuxPPS API ver. 1 registered
[    0.242565] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.243741] PTP clock support registered
[    0.244944] ion_dummy: not reserve carveout memory, try to alloc from cma
[    0.381541] Advanced Linux Sound Architecture Driver Initialized.
[    0.382732] usbcore: registered new interface driver usbfs
[    0.383460] usbcore: registered new interface driver hub
[    0.384192] usbcore: registered new device driver usb
[    0.385158] clocksource: Switched to clocksource arch_sys_counter
[    0.432910] VFS: Disk quotas dquot_6.6.0
[    0.433493] VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
[    0.434430] FS-Cache: Loaded
[    0.434920] CacheFiles: Loaded
[    0.440251] NET: Registered protocol family 2
[    0.441224] TCP established hash table entries: 32768 (order: 6, 262144 bytes)
[    0.442344] TCP bind hash table entries: 32768 (order: 7, 524288 bytes)
[    0.443589] TCP: Hash tables configured (established 32768 bind 32768)
[    0.444495] UDP hash table entries: 2048 (order: 4, 65536 bytes)
[    0.445353] UDP-Lite hash table entries: 2048 (order: 4, 65536 bytes)
[    0.446355] NET: Registered protocol family 1
[    0.447184] RPC: Registered named UNIX socket transport module.
[    0.447935] RPC: Registered udp transport module.
[    0.448532] RPC: Registered tcp transport module.
[    0.449131] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.450638] hw perfevents: enabled with armv8_cortex_a53 PMU driver, 7 counters available
[    0.452850] audit: initializing netlink subsys (disabled)
[    0.453657] audit: type=2000 audit(0.452:1): state=initialized audit_enabled=0 res=1
[    0.453971] Initialise system trusted keyrings
[    0.454048] workingset: timestamp_bits=46 max_order=20 bucket_order=0
[    0.457762] zbud: loaded
[    0.459320] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.460178] exFAT: Version 1.2.9
[    0.460659] FS-Cache: Netfs 'nfs' registered for caching
[    0.461787] NFS: Registering the id_resolver key type
[    0.462441] Key type id_resolver registered
[    0.462968] Key type id_legacy registered
[    0.463484] nfs4filelayout_init: NFSv4 File Layout Driver Registering...
[    0.464337] Installing knfsd (copyright (C) 1996 okir@monad.swb.de).
[    0.468583] NET: Registered protocol family 38
[    0.469199] async_tx: api initialized (async)
[    0.469753] Key type asymmetric registered
[    0.470271] Asymmetric key parser 'x509' registered
[    0.470965] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 245)
[    0.471984] io scheduler noop registered
[    0.472637] io scheduler cfq registered (default)
[    0.473382] io scheduler mq-deadline registered
[    0.473954] io scheduler kyber registered
[    0.475153] pinctrl-single a6003170.pinctrl_voltag: 64 pins at pa ffffff8009c4d170 size 8
[    0.476491] pinctrl-single a6004000.pinctrl: 128 pins at pa ffffff8009c61000 size 512
[    0.477734] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: start probe
[    0.478629] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: probe ok
[    0.479500] gpio-x3 a6003000.gpio: x3 gpio probe start!!!
[    0.480189] gpio-x3 a6003000.gpio: x3 gpio add gpiochip start!!!
[    0.481112] gpio-x3 a6003000.gpio: diable all gpio irq
[    0.483370] gpio-x3 a6003000.gpio: irqbase:57
[    0.483922] gpio-x3 a6003000.gpio: x3 irq add start!!!
[    0.484579] irq: Cannot allocate irq_descs @ IRQ57, assuming pre-allocated
[    0.485665] gpio-x3 a6003000.gpio: x3 irq add ok!!!
[    0.486320] gpio-x3 a6003000.gpio: x3 irqchip ops add ok!!!
[    0.487026] gpio-x3 a6003000.gpio: x3 gpio probe ok!!!
[    0.488104] hobot-pwm: hobot-pwmchip0 registered
[    0.488853] hobot-pwm: hobot-pwmchip1 registered
[    0.490256] diag dev [ver:1.1] init done
[    0.491155] hobot_ddr_monitor: LPDDR4 detected
[    0.491945] hobot_ddr_monitor: ddr monitor init finished.
[    0.492350] [vcam] init start
[    0.493447] vcam probe start
[    0.493896] vcam probe end successful
[    0.494356] [vcam] init end
[    0.495272] a5000000.serial: ttyS0 at MMIO 0xa5000000 (irq = 10, base_baud = 12000000) is a hobot-uart
[    0.496482] console [ttyS0] enabled
[    0.496482] console [ttyS0] enabled
[    0.497381] bootconsole [hobot0] disabled
[    0.497381] bootconsole [hobot0] disabled
[    0.498696] hobot-uart a5001000.serial: Failed to create debugfs root directory
[    0.499693] a5001000.serial: ttyS1 at MMIO 0xa5001000 (irq = 11, base_baud = 12000000) is a hobot-uart
[    0.501124] hobot-uart a5003000.serial: Failed to create debugfs root directory
[    0.502276] a5003000.serial: ttyS3 at MMIO 0xa5003000 (irq = 12, base_baud = 12000000) is a hobot-uart
[    0.503809] KGDB: Registered I/O driver kgdboc
[    0.504639] cacheinfo: Unable to detect cache hierarchy for CPU 0
[    0.510122] brd: module loaded
[    0.514707] loop: module loaded
[    0.516268] spi-nand hr_nand.0: GigaDevice SPI NAND was found.
[    0.517028] spi-nand hr_nand.0: 128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
[    0.519738] hobot_spi a5006000.spi: ver: HOBOT-spi_V20.200330 master
[    0.520780] libphy: Fixed MDIO Bus: probed
[    0.522090] st_gmac a5014000.ethernet: found phy-handle subnode
[    0.522925] st_gmac a5014000.ethernet: xj3_mtl_setup, plat->rx-queues-to-use:4, and tx:4
[    0.524108] st_gmac a5014000.ethernet: xj3_probe_config_dt, clk_ptp_rate:250000000
[    0.525110] set mac address 00:11:22:bd:36:5a:
[    0.525112] (using random mac adress)
[    0.526302] (NULL device *): xj3_get_hw_features, tx_fifo_size:16384
[    0.527120] (NULL device *): xj3_get_hw_features, rx_fifo_size:16384
[    0.527938] st_gmac a5014000.ethernet: TSO supported
[    0.528578] st_gmac a5014000.ethernet: TSO feature enabled
[    0.529303] st_gmac a5014000.ethernet: Enable Rx Mitigation via HW Watchdog Timer
[    0.650376] libphy: hobot-mac-mdio: probed
[    0.651931] st_gmac a5014000.ethernet: hobot_eth_probe: probe sucessfully
[    0.653130] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_0v8 not found, using dummy regulator
[    0.654387] dwc3-of-simple b2000000.usb: usb regulator 0v8 enable succeed
[    0.655265] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_3v3 not found, using dummy regulator
[    0.656466] dwc3-of-simple b2000000.usb: usb regulator 3v3 enable succeed
[    0.658009] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    0.659666] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    0.661103] usbcore: registered new interface driver cdc_acm
[    0.661854] cdc_acm: USB Abstract Control Model driver for USB modems and ISDN adapters
[    0.662913] usbcore: registered new interface driver uas
[    0.663631] usbcore: registered new interface driver usb-storage
[    0.664466] usbcore: registered new interface driver usbserial
[    0.665258] usbcore: registered new interface driver usbserial_generic
[    0.666119] usbserial: USB Serial support registered for generic
[    0.666914] usbcore: registered new interface driver usb_serial_simple
[    0.667770] usbserial: USB Serial support registered for carelink
[    0.668571] usbserial: USB Serial support registered for zio
[    0.669335] usbserial: USB Serial support registered for funsoft
[    0.670127] usbserial: USB Serial support registered for flashloader
[    0.670963] usbserial: USB Serial support registered for google
[    0.671742] usbserial: USB Serial support registered for libtransistor
[    0.672598] usbserial: USB Serial support registered for vivopay
[    0.673411] usbserial: USB Serial support registered for moto_modem
[    0.674234] usbserial: USB Serial support registered for motorola_tetra
[    0.675101] usbserial: USB Serial support registered for novatel_gps
[    0.675938] usbserial: USB Serial support registered for hp4x
[    0.676695] usbserial: USB Serial support registered for suunto
[    0.677494] usbserial: USB Serial support registered for siemens_mpi
[    0.678340] usbcore: registered new interface driver rio500
[    0.679174] mousedev: PS/2 mouse device common for all mice
[    0.690221] hobot-rtc a6002000.rtc: rtc core: registered hobot-rtc as rtc0
[    0.691217] i2c /dev entries driver
[    0.691823] hobot-i2c a5009000.i2c: hobot i2c probe start
[    0.692590] hobot-i2c a5009000.i2c: round_rate:96000000
[    0.693289] hobot-i2c a5009000.i2c: I2C bus speed is 400000
[    0.694007] hobot-i2c a5009000.i2c: clkdiv = 0x1d
[    0.694613] hobot-i2c a5009000.i2c: i2c0 diag register....
[    0.695706] hobot-i2c a5009000.i2c: hobot_i2c_0 probe done
[    0.696511] hobot-i2c a500a000.i2c: hobot i2c probe start
[    0.697295] hobot-i2c a500a000.i2c: round_rate:96000000
[    0.697972] hobot-i2c a500a000.i2c: I2C bus speed is 400000
[    0.698689] hobot-i2c a500a000.i2c: clkdiv = 0x1d
[    0.699295] hobot-i2c a500a000.i2c: i2c1 diag register....
[    0.700308] hobot-i2c a500a000.i2c: hobot_i2c_1 probe done
[    0.701294] lirc_dev: IR Remote Control driver registered, major 239
[    0.702111] IR LIRC bridge handler initialized
[    0.702867] sif_mclk clock frequence is 544000000
[    0.703503] mipi_rx0_ipi clock frequence is 544000000
[    0.704191] mipi_rx1_ipi clock frequence is 544000000
[    0.704890] mipi_rx2_ipi clock frequence is 544000000
[    0.705623] mipi_rx3_ipi clock frequence is 544000000
[    0.706344] mipi_tx_ipi clock frequence is 544000000
[    0.707064] mipi_cfg_host clock frequence is 102000000
[    0.707817] pym_mclk clock frequence is 1188000000
[    0.708539] mipi_dev_ref clock frequence is 24000000
[    0.709312] mipi_host_ref clock frequence is 24000000
[    0.710089] sensor0_mclk clock frequence is 37125000
[    0.710865] sensor1_mclk clock frequence is 37125000
[    0.711655] sensor2_mclk clock frequence is 37125000
[    0.712454] sensor3_mclk clock frequence is 37125000
[    0.713094] [FRT:D] x3_ips_probe(0)
[    0.714122] hobot swinfo sel reg ro=0x1 boot dump
[    0.715032] pvt a1009000.pvt: SCRATCH test: 1234abcd, pvt is alive.
[    0.715957] pvt a1009000.pvt: VM Calibrated data detected
[    0.717135] hobot_wdt a1002000.watchdog: watchdog setting [pet:6s bark:11s bite:15s]
[    0.718481] hobot_wdt a1002000.watchdog: Hobot Watchdog Timer at ffffff8009db3000 with timeout 15s
[    0.719832] device-mapper: uevent: version 1.0.3
[    0.720594] device-mapper: ioctl: 4.37.0-ioctl (2017-09-20) initialised: dm-devel@redhat.com
[    0.721802] device-mapper: verity-avb: AVB error handler initialized with vbmeta device:
[    0.724212] Synopsys Designware Multimedia Card Interface Driver
[    0.725253] dwmmc_hobot a5010000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.726080] dwmmc_hobot a5010000.dwmmc: card-detect-delay not found.
[    0.726899] dwmmc_hobot a5010000.dwmmc: data-addr not found.
[    0.727938] mmc_host mmc0: card is non-removable.
[    0.766369] dwmmc_hobot a5011000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.769215] dwmmc_hobot a5011000.dwmmc: card-detect-delay not found.
[    0.770043] dwmmc_hobot a5011000.dwmmc: data-addr not found.
[    0.774812] dwmmc_hobot a5011000.dwmmc: mmc set to fixed voltage 1800
[    0.775873] mmc_host mmc1: card is non-removable.
[    0.873359] dwmmc_hobot a5012000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.874202] dwmmc_hobot a5012000.dwmmc: card-detect-delay not found.
[    0.875045] dwmmc_hobot a5012000.dwmmc: data-addr not found.
[    0.876008] dwmmc_hobot a5012000.dwmmc: Got CD GPIO
[    0.986963] mmc1: queuing unknown CIS tuple 0x80 (2 bytes)
[    0.989160] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.991353] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.994726] mmc1: queuing unknown CIS tuple 0x80 (7 bytes)
[    0.998693] mmc1: queuing unknown CIS tuple 0x81 (9 bytes)
[    1.065498] ledtrig-cpu: registered to indicate activity on CPUs
[    1.066350] hidraw: raw HID events driver (C) Jiri Kosina
[    1.067226] usbcore: registered new interface driver usbhid
[    1.067950] usbhid: USB HID core driver
[    1.068534] logger: created 256K log 'log_main'
[    1.069207] logger: created 256K log 'log_events'
[    1.069886] logger: created 256K log 'log_radio'
[    1.070552] logger: created 256K log 'log_system'
[    1.071611] set dmc devfreq governor to performance
[    1.072260] hobot_dmcfreq_target: dmcfreq->rate:2666000000, target_rate:2666000000
[    1.073272] buf:, powersave_rate:2666000000, dmcfreq->pre_state:0
[    1.080146] usbcore: registered new interface driver snd-usb-audio
[    1.081350] Netfilter messages via NETLINK v0.30.
[    1.081992] ip_set: protocol 6
[    1.082489] ipip: IPv4 and MPLS over IPv4 tunneling driver
[    1.083514] ip_tables: (C) 2000-2006 Netfilter Core Team
[    1.088576] arp_tables: arp_tables: (C) 2002 David S. Miller
[    1.089425] Initializing XFRM netlink socket
[    1.090299] NET: Registered protocol family 10
[    1.091489] Segment Routing with IPv6
[    1.091999] sit: IPv6, IPv4 and MPLS over IPv4 tunneling driver
[    1.093095] NET: Registered protocol family 17
[    1.093763] Key type dns_resolver registered
[    1.095390] Loading compiled-in X.509 certificates
[    1.098901] Loaded X.509 cert 'Build time autogenerated kernel key: 81cb0ef77db2fac76e9588c2120c82422367d268'
[    1.100233] zswap: loaded using pool lzo/zbud
[    1.111479] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    1.113149] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    1.114152] console [netcon0] enabled
[    1.114626] netconsole: network logging started
[    1.115413] hobot-rtc a6002000.rtc: setting system clock to 1970-01-01 00:00:00 UTC (0)
[    1.116608] vps mipi_dphy: probe with x3vio done
[    1.117332] hobot_wdt_test: wdt_test_init: wdt test init
[    1.120037] VCC_CNN0: disabling
[    1.120446] VCC_CNN1: disabling
[    1.121410] vps mipi_host0: ver 140* port0(0:0)
[    1.122316] vps mipi_host1: ver 140* port1(1:0)
[    1.123200] vps mipi_host2: ver 140* port2(0:1)
[    1.123985] vps mipi_host3: ver 140* port3(1:1)
[    1.124815] ALSA device list:
[    1.125240]   No soundcards found.
[    1.125883] md: Skipping autodetection of RAID arrays. (raid=autodetect will force)
[    1.127003] VFS: Cannot open root device "mmcblk2p2" or unknown-block(0,0): error -6
[    1.127997] Please append a correct "root=" boot option; here are the available partitions:
[    1.129071] 0100          102400 ram0
[    1.129074]  (driver?)
[    1.129884] 0101          102400 ram1
[    1.129886]  (driver?)
[    1.130675] 0102          102400 ram2
[    1.130677]  (driver?)
[    1.131464] 0103          102400 ram3
[    1.131466]  (driver?)
[    1.132254] 0104          102400 ram4
[    1.132256]  (driver?)
[    1.133044] 0105          102400 ram5
[    1.133046]  (driver?)
[    1.133875] 0106          102400 ram6
[    1.133877]  (driver?)
[    1.134666] 0107          102400 ram7
[    1.134668]  (driver?)
[    1.135455] 0108          102400 ram8
[    1.135457]  (driver?)
[    1.136245] 0109          102400 ram9
[    1.136247]  (driver?)
[    1.137035] 010a          102400 ram10
[    1.137037]  (driver?)
[    1.137864] 010b          102400 ram11
[    1.137866]  (driver?)
[    1.138666] 010c          102400 ram12
[    1.138667]  (driver?)
[    1.139466] 010d          102400 ram13
[    1.139468]  (driver?)
[    1.140267] 010e          102400 ram14
[    1.140269]  (driver?)
[    1.141068] 010f          102400 ram15
[    1.141070]  (driver?)
[    1.141895] 1f00          131072 mtdblock0
[    1.141897]  (driver?)
[    1.142740] hobot_fusa: set_fusa_error_pin:75 set error pin to 1
[    1.143511] hobot_fusa: fusa errpin not ready
[    1.143515] Kernel panic - not syncing: VFS: Unable to mount root fs on unknown-block(0,0)
[    1.145133] Kernel Offset: disabled
[    1.145585] CPU features: 0x0002004
[    1.146034] Memory Limit: none
[    1.150553] Rebooting in 1 seconds..
[    1.221409] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.222132] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 1
[    1.223587] xhci-hcd xhci-hcd.0.auto: hcc params 0x0220fe6d hci version 0x110 quirks 0x0000000000010010
[    1.224823] xhci-hcd xhci-hcd.0.auto: irq 178, io mem 0xb2000000
[    1.225801] usb usb1: New USB device found, idVendor=1d6b, idProduct=0002, bcdDevice= 4.14
[    1.226865] usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.227793] usb usb1: Product: xHCI Host Controller
[    1.228422] usb usb1: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.229128] usb usb1: SerialNumber: xhci-hcd.0.auto
[    1.230080] hub 1-0:1.0: USB hub found
[    1.230378] mmc1: new HSSDIO card at address 0001
[    1.231188] hub 1-0:1.0: 1 port detected
[    1.231882] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.232596] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 2
[    1.233605] xhci-hcd xhci-hcd.0.auto: Host supports USB 3.0 SuperSpeed
[    1.234481] usb usb2: We don't know the algorithms for LPM for this host, disabling LPM.
[    1.235584] usb usb2: New USB device found, idVendor=1d6b, idProduct=0003, bcdDevice= 4.14
[    1.236647] usb usb2: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.237583] usb usb2: Product: xHCI Host Controller
[    1.238213] usb usb2: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.238919] usb usb2: SerialNumber: xhci-hcd.0.auto
[    1.239826] hub 2-0:1.0: USB hub found
[    1.240326] hub 2-0:1.0: 1 port detected
[    1.489168] usb 1-1: new high-speed USB device number 2 using xhci-hcd
[    1.641351] usb 1-1: New USB device found, idVendor=1a40, idProduct=0101, bcdDevice= 1.11
[    1.642404] usb 1-1: New USB device strings: Mfr=0, Product=1, SerialNumber=0
[    1.643321] usb 1-1: Product: USB 2.0 Hub
[    1.682649] hub 1-1:1.0: USB hub found
[    1.683166] hub 1-1:1.0: 4 ports detected
[    1.961167] mmc2: new UHS SDR104 SDHC card at address 0001
[    1.962187] mmcblk2: mmc2:0001 SD16G 29.8 GiB
[    1.963789]  mmcblk2: p1 p2
[    2.151065] SMP: stopping secondary CPUs
[    2.151573] psci: psci_sys_reset(reboot_mode=0)
NOTICE:  fast_boot:0

S
F
L
O
NOTICE:  efuse cpu_cfg = 0
W
NOTICE:  Booting Trusted Firmware
NOTICE:  BL1: v1.4(release):HR-ROM-Rel-v1.1-141-ga91d4dd-dirty
NOTICE:  BL1: Built : 11:24:44, Oct 23 2019
NOTICE:  boot src: 2
NOTICE:  GigaDev SPI NAND was found.
NOTICE:  Block size: 128 KiB, page size: 2048
NOTICE:  BL1: Booting BL2
Auth pass
NOTICE:  bl1_main exit
SPL normal reset flow
check_reset_state (2): wakeup address = 0x0, hw wakeup status = 0x3, wakeup src=0x100
patch for sys_pll 1200 with 100M eth
SFLOW_INIT
CHIP ID:PCB941/WAFER: W04/ X: X20/ Y: Y36
secondary_jump_to_spl: secure chip flow
X3 SPL : secondary core wake up and jump to spl done (cpu_core_cfg=0)
SFLOW_FIN_HW_A

U-Boot SPL 2018.09-g4ca851534c-dirty (May 11 2022 - 20:09:50 +0800)
SPACC Init - ID: (00000061)
SPL nand boot mode (from strap)
GigaDev SPI NAND was found.
Block size: 128 KiB, page size: 2048
ddr_type = 1 (LPDDR4)
hb_chip_package_type:3
load ddr header src_addr: 100000, load_addr: 802ca020, src_len: a00
find valid ddr image
ddr_hdr.ecc_gran: 0x0
ddr_hdr.ecc_map: 0x0
ddr_hdr.sbr_pattern0: 0x0
ddr_hdr.sbr_pattern1: 0x0
ddr_freq = 05
board id = 31540334
ddr datarate: 3200
### SAMSUNG DDR ###
no ddr pin set
detect part number: 108
detect ddr freq: c80
board id alternative:0x3
index is 12
index is 15
index is 19
hb_ddr_index: 19
ddr_type = 1, ddr_vendor=3, ddr_freq=3200
dram_pll_init
sscg disabled
control load ddrc src_addr: 15ae00, load_addr: 802caa20, src_len: 920
[DDR INFO]      ==ddr_release_info==
[DDR INFO]      VERSION:        develop
[DDR INFO]      BUILD:          2022-05-11-20:09
[DDR INFO]      GIT COMMIT:     4ca851534c1616ace920fdaa000c6fb717c1fb74
[DDR INFO]      GIT TIME:       Wed, 20 Apr 2022 18:28:49 +0800
[DDR INFO]      ==ddr_features==
[DDR INFO]      RDBI:           0
[DDR INFO]      WDBI:           1
[DDR INFO]      InlineECC:      0
[DDR INFO]      DM:             1
[DDR INFO]      DDC:            1
[DDR INFO]      SSCG:           0
[DDR INFO]      BOARD:          XS_ENABLE
[DDR INFO] ddr_controller_cfg done
load ddr phy src_addr: 15b800, load_addr: 802caa20, src_len: 420
ATxSlewRate     : 15f
ATxImpedance    : 7f
TxSlewRate      : 19f
TxOdtDrvStren   : 600
TxImpedanceCtrl : e3f
CalDrvStr0      : 11
VrefInGlobal    : 104
board_type = 4 (CUSTOMER_BOARD)
load dqmap src addr: 15d600, load_addr: 802caa20, src_len: 20
[DDR INFO] dwc_ddrphy_train start
magic = 544f4248
load imem1 src_addr: 11ce00, load_addr: 802caa20, src_len: 8000
load dmem1 src_addr: 15a000, load_addr: 802caa20, src_len: 684
executing 1D fw
load imem2 src_addr: 124e00, load_addr: 802caa20, src_len: 8000
load dmem2 src_addr: 15a800, load_addr: 802caa20, src_len: 564

*******************************************************
p_dmem_lpddr4_2d_16b->MR11_A0:54
p_dmem_lpddr4_2d_16b->MR14_A0:54
p_dmem_lpddr4_2d_16b->MR12_A0:51
p_dmem_lpddr4_2d_16b->MR22_A0:14

p_dmem_lpddr4_2d_16b->MR3_A0:b3
p_dmem_lpddr4_2d_16b->Reserved00:40
p_dmem_lpddr4_2d_16b->Reserved0E:4
p_dmem_lpddr4_2d_16b->Delay_Weight2D:20
p_dmem_lpddr4_2d_16b->Voltage_Weight2D:80
*******************************************************

executing 2D fw
load pie src_addr: 15be00, load_addr: 802caa20, src_len: 11f0
Set QoS.
get_ddr_mr_info:cs_num=1, mr5=0x1, mr8=0x10
no magic in efuse file,bypass efuse
total_sz = 4096
SPL_VERSION:7
uboot partition is uboot_A
load u-boot: src_addr=0x380000, dest_addr=0x4000000, len=2097152
load warm boot spl: addr=0x800, dest_addr=0x80000000, len=31232
load bl31: addr=0x300000, dest_addr=0x0, len=524288
SFLOW_AUTH_BL31
verify signature of header:  verify ok!
verify signature of image:  verify ok!
bypass bpu image
clear keybank!!!!
SFLOW_DBG_EN
Trying to boot from RAM
SPL: bl31 will jump to u-boot or other entry (0x4000000)
SFLOW_CLR_KEY
SFLOW_REG_LD
install_portal copy portal
install_portal call smc and jump to bl31 cold entry(0x0)
hb som type: 5
X3 PI reset VDD_SD done

U-Boot 2018.09-g40785bca (May 27 2022 - 16:30:48 +0800)

Model: Hobot XJ3 Soc Board
DRAM:  system DDR size: 0xffe00000
4 GiB
MMC:   dwmmc@A5010000: 0, dwmmc@A5011000: 1, dwmmc@A5012000: 2
Loading Environment from UBI... GigaDevice SPI NAND was found.
128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
*** Warning - bad CRC, using default environment

In:    serial@a5000000
Out:   serial@a5000000
Err:   serial@a5000000
Net:   x3 sdb reset eth phy done

Warning: ethernet@A5014000 (eth0) using random MAC address - 66:60:15:80:01:5c
eth0: ethernet@A5014000
Disable cnn cores ..
dtb_name:hobot-x3-pi.dtb
base board type: X3 SDB
bootmode: NAND
board_id = 31540334
damaged volume, update marker is setdamaged volume, update marker is setdamaged volume, update marker is sethb_boot_args_cmd_set custom_bootargs 0 ubuntu_boot 0
Hit any key to stop autoboot:  0
enable watchdog success !
switch to partitions #0, OK
mmc2 is current device
Scanning mmc 2:2...
Found U-Boot script /boot/boot.scr
664 bytes read in 1 ms (648.4 KiB/s)
## Executing script at 03c10000
Boot script loaded from devtype:mmc devnum:2 devplist:2
bootargs = console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
Loading fdt file: /boot/hobot/hobot-x3-pi.dtb
69633 bytes read in 8 ms (8.3 MiB/s)
Loading kernel: /boot/Image
19163144 bytes read in 845 ms (21.6 MiB/s)
## Flattened Device Tree blob at 03c00000
   Booting using the fdt blob at 0x3c00000
   Loading Device Tree to 0000000003c00000, end 0000000003c1ffff ... OK
chip_id: ab36300
The address of the fdt is 0x3c00000
Changed status Done
Can't get fdt_addr !!!Orign(MAX) bpu model Reserve Mem Size to 64M!!

Starting kernel ...

[    0.000000] OF: reserved mem: OVERLAP DETECTED!
[    0.000000] image_r5_mem (0x0000000080000000--0x0000000080010000) overlaps with msg_r5_mem (0x000000008000f000--0x0000000080010000)
[    0.000000] Reserved memory: created CMA memory pool at 0x0000000004000000, size 672 MiB
[    0.000000] OF: reserved mem: initialized node ion_cma, compatible id shared-dma-pool
[    0.000000] cma: Reserved 16 MiB at 0x000000007f000000
[    0.000000] On node 0 totalpages: 1047808
[    0.000000]   DMA zone: 8180 pages used for memmap
[    0.000000]   DMA zone: 0 pages reserved
[    0.000000]   DMA zone: 523520 pages, LIFO batch:31
[    0.000000]   Normal zone: 8192 pages used for memmap
[    0.000000]   Normal zone: 524288 pages, LIFO batch:31
[    0.000000] psci: probing for conduit method from DT.
[    0.000000] psci: PSCIv1.1 detected in firmware.
[    0.000000] psci: Using standard PSCI v0.2 function IDs
[    0.000000] psci: MIGRATE_INFO_TYPE not supported.
[    0.000000] psci: SMC Calling Convention v1.1
[    0.000000] percpu: Embedded 25 pages/cpu @ffffffc17ff2a000 s65176 r8192 d29032 u102400
[    0.000000] pcpu-alloc: s65176 r8192 d29032 u102400 alloc=25*4096
[    0.000000] pcpu-alloc: [0] 0 [0] 1 [0] 2 [0] 3
[    0.000000] Detected VIPT I-cache on CPU0
[    0.000000] CPU features: enabling workaround for ARM erratum 845719
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 1031436
[    0.000000] Kernel command line: earlycon loglevel=8 kgdboc=ttyS0 video=hobot:x3sdb-hdmi  console=ttyS0,921600 raid=noautodetect hobotboot.reson=PANIC_RESET rootfstype=ext4 root=/dev/mmcblk2p2
[    0.000000] PID hash table entries: 4096 (order: 3, 32768 bytes)
[    0.000000] Dentry cache hash table entries: 524288 (order: 10, 4194304 bytes)
[    0.000000] Inode-cache hash table entries: 262144 (order: 9, 2097152 bytes)
[    0.000000] software IO TLB [mem 0x7afff000-0x7efff000] (64MB) mapped at [ffffffc07afff000-ffffffc07effefff]
[    0.000000] Memory: 3319580K/4191232K available (10494K kernel code, 1306K rwdata, 5756K rodata, 1088K init, 9553K bss, 167140K reserved, 704512K cma-reserved)
[    0.000000] Virtual kernel memory layout:
[    0.000000]     modules : 0xffffff8000000000 - 0xffffff8008000000   (   128 MB)
[    0.000000]     vmalloc : 0xffffff8008000000 - 0xffffffbebfff0000   (   250 GB)
[    0.000000]       .text : 0xffffff8008000000 - 0xffffff8008a40000   ( 10496 KB)
[    0.000000]     .rodata : 0xffffff8008a40000 - 0xffffff8008ff0000   (  5824 KB)
[    0.000000]       .init : 0xffffff8008ff0000 - 0xffffff8009100000   (  1088 KB)
[    0.000000]       .data : 0xffffff8009100000 - 0xffffff8009246808   (  1307 KB)
[    0.000000]        .bss : 0xffffff8009246808 - 0xffffff8009b9aed8   (  9554 KB)
[    0.000000]     fixed   : 0xffffffbefe7fd000 - 0xffffffbefec00000   (  4108 KB)
[    0.000000]     PCI I/O : 0xffffffbefee00000 - 0xffffffbeffe00000   (    16 MB)
[    0.000000]     vmemmap : 0xffffffbf00000000 - 0xffffffc000000000   (     4 GB maximum)
[    0.000000]               0xffffffbf00008000 - 0xffffffbf06000000   (    95 MB actual)
[    0.000000]     memory  : 0xffffffc000200000 - 0xffffffc180000000   (  6142 MB)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=4, Nodes=1
[    0.000000] ftrace: allocating 36277 entries in 142 pages
[    0.000000] Preemptible hierarchical RCU implementation.
[    0.000000]  Tasks RCU enabled.
[    0.000000] NR_IRQS: 64, nr_irqs: 64, preallocated irqs: 0
[    0.000000] parent_rate: 0,  dclk->rate:2666000000, pre_ddr_rate:0, res.a0:139716712
[    0.000000] arch_timer: cp15 timer(s) running at 24.00MHz (virt).
[    0.000000] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0x588fe9dc0, max_idle_ns: 440795202592 ns
[    0.000004] sched_clock: 56 bits at 24MHz, resolution 41ns, wraps every 4398046511097ns
[    0.001194] clocksource: hobot_clocksource: mask: 0xffffffffffffffff max_cycles: 0x1d854df40, max_idle_ns: 3526361616960 ns
[    0.002970] Console: colour dummy device 80x25
[    0.003541] Calibrating delay loop (skipped), value calculated using timer frequency.. 48.00 BogoMIPS (lpj=96000)
[    0.004847] pid_max: default: 32768 minimum: 301
[    0.005501] Security Framework initialized
[    0.006019] AppArmor: AppArmor disabled by boot time parameter
[    0.006862] Mount-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.007730] Mountpoint-cache hash table entries: 8192 (order: 4, 65536 bytes)
[    0.023773] ASID allocator initialised with 65536 entries
[    0.031770] Hierarchical SRCU implementation.
[    0.063829] smp: Bringing up secondary CPUs ...
[    0.100037] Detected VIPT I-cache on CPU1
[    0.100072] CPU1: Booted secondary processor [410fd034]
[    0.136086] Detected VIPT I-cache on CPU2
[    0.136107] CPU2: Booted secondary processor [410fd034]
[    0.172145] Detected VIPT I-cache on CPU3
[    0.172165] CPU3: Booted secondary processor [410fd034]
[    0.172218] smp: Brought up 1 node, 4 CPUs
[    0.176280] SMP: Total of 4 processors activated.
[    0.176874] CPU features: detected feature: 32-bit EL0 Support
[    0.177693] CPU: All CPU(s) started at EL1
[    0.178221] alternatives: patching kernel code
[    0.179809] devtmpfs: initialized
[    0.188869] random: get_random_u32 called from bucket_table_alloc+0x108/0x270 with crng_init=0
[    0.190455] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 7645041785100000 ns
[    0.191702] futex hash table entries: 1024 (order: 5, 131072 bytes)
[    0.208209] xor: automatically using best checksumming function   32regs
[    0.209146] pinctrl core: initialized pinctrl subsystem
[    0.210380] NET: Registered protocol family 16
[    0.211701] vdso: 2 pages (1 code @ ffffff8008a46000, 1 data @ ffffff8009104000)
[    0.212646] hw-breakpoint: found 6 breakpoint and 4 watchpoint registers.
[    0.214237] DMA: preallocated 256 KiB pool for atomic allocations
[    0.219074] pstore: using zlib compression
[    0.219869] console [pstore-1] enabled
[    0.220468] pstore: Registered ramoops as persistent store backend
[    0.221253] ramoops: attached 0x40000@0x3fc0000, ecc: 0/0
[    0.226251] hobot_dma a1005000.dma: Hobot DMA Engine Driver Probed!!
[    0.239836] SCSI subsystem initialized
[    0.240496] media: Linux media interface: v0.10
[    0.241091] Linux video capture interface: v2.00
[    0.241737] pps_core: LinuxPPS API ver. 1 registered
[    0.242364] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.243540] PTP clock support registered
[    0.244851] ion_dummy: not reserve carveout memory, try to alloc from cma
[    0.381576] Advanced Linux Sound Architecture Driver Initialized.
[    0.382774] usbcore: registered new interface driver usbfs
[    0.383503] usbcore: registered new interface driver hub
[    0.384231] usbcore: registered new device driver usb
[    0.385200] clocksource: Switched to clocksource arch_sys_counter
[    0.432882] VFS: Disk quotas dquot_6.6.0
[    0.433443] VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
[    0.434381] FS-Cache: Loaded
[    0.434867] CacheFiles: Loaded
[    0.440187] NET: Registered protocol family 2
[    0.441106] TCP established hash table entries: 32768 (order: 6, 262144 bytes)
[    0.442253] TCP bind hash table entries: 32768 (order: 7, 524288 bytes)
[    0.443503] TCP: Hash tables configured (established 32768 bind 32768)
[    0.444416] UDP hash table entries: 2048 (order: 4, 65536 bytes)
[    0.445273] UDP-Lite hash table entries: 2048 (order: 4, 65536 bytes)
[    0.446274] NET: Registered protocol family 1
[    0.447092] RPC: Registered named UNIX socket transport module.
[    0.447843] RPC: Registered udp transport module.
[    0.448440] RPC: Registered tcp transport module.
[    0.449038] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.450606] hw perfevents: enabled with armv8_cortex_a53 PMU driver, 7 counters available
[    0.452831] audit: initializing netlink subsys (disabled)
[    0.453638] audit: type=2000 audit(0.452:1): state=initialized audit_enabled=0 res=1
[    0.453949] Initialise system trusted keyrings
[    0.454024] workingset: timestamp_bits=46 max_order=20 bucket_order=0
[    0.457690] zbud: loaded
[    0.459253] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.460112] exFAT: Version 1.2.9
[    0.460592] FS-Cache: Netfs 'nfs' registered for caching
[    0.461852] NFS: Registering the id_resolver key type
[    0.462505] Key type id_resolver registered
[    0.463032] Key type id_legacy registered
[    0.463547] nfs4filelayout_init: NFSv4 File Layout Driver Registering...
[    0.464401] Installing knfsd (copyright (C) 1996 okir@monad.swb.de).
[    0.468543] NET: Registered protocol family 38
[    0.469115] async_tx: api initialized (async)
[    0.469679] Key type asymmetric registered
[    0.470196] Asymmetric key parser 'x509' registered
[    0.470878] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 245)
[    0.471897] io scheduler noop registered
[    0.472557] io scheduler cfq registered (default)
[    0.473152] io scheduler mq-deadline registered
[    0.473737] io scheduler kyber registered
[    0.474934] pinctrl-single a6003170.pinctrl_voltag: 64 pins at pa ffffff8009c4d170 size 8
[    0.476279] pinctrl-single a6004000.pinctrl: 128 pins at pa ffffff8009c61000 size 512
[    0.477661] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: start probe
[    0.478556] pinctrl_cdev soc:pinctrl_cdev@0xA6004000: probe ok
[    0.479428] gpio-x3 a6003000.gpio: x3 gpio probe start!!!
[    0.480119] gpio-x3 a6003000.gpio: x3 gpio add gpiochip start!!!
[    0.481040] gpio-x3 a6003000.gpio: diable all gpio irq
[    0.483302] gpio-x3 a6003000.gpio: irqbase:57
[    0.483854] gpio-x3 a6003000.gpio: x3 irq add start!!!
[    0.484511] irq: Cannot allocate irq_descs @ IRQ57, assuming pre-allocated
[    0.485555] gpio-x3 a6003000.gpio: x3 irq add ok!!!
[    0.486209] gpio-x3 a6003000.gpio: x3 irqchip ops add ok!!!
[    0.486915] gpio-x3 a6003000.gpio: x3 gpio probe ok!!!
[    0.488011] hobot-pwm: hobot-pwmchip0 registered
[    0.488765] hobot-pwm: hobot-pwmchip1 registered
[    0.490268] diag dev [ver:1.1] init done
[    0.491171] hobot_ddr_monitor: LPDDR4 detected
[    0.491933] hobot_ddr_monitor: ddr monitor init finished.
[    0.492321] [vcam] init start
[    0.493396] vcam probe start
[    0.493867] vcam probe end successful
[    0.494328] [vcam] init end
[    0.495262] a5000000.serial: ttyS0 at MMIO 0xa5000000 (irq = 10, base_baud = 12000000) is a hobot-uart
[    0.496484] console [ttyS0] enabled
[    0.496484] console [ttyS0] enabled
[    0.497401] bootconsole [hobot0] disabled
[    0.497401] bootconsole [hobot0] disabled
[    0.498739] hobot-uart a5001000.serial: Failed to create debugfs root directory
[    0.499743] a5001000.serial: ttyS1 at MMIO 0xa5001000 (irq = 11, base_baud = 12000000) is a hobot-uart
[    0.501187] hobot-uart a5003000.serial: Failed to create debugfs root directory
[    0.502338] a5003000.serial: ttyS3 at MMIO 0xa5003000 (irq = 12, base_baud = 12000000) is a hobot-uart
[    0.503877] KGDB: Registered I/O driver kgdboc
[    0.504715] cacheinfo: Unable to detect cache hierarchy for CPU 0
[    0.510165] brd: module loaded
[    0.514707] loop: module loaded
[    0.516279] spi-nand hr_nand.0: GigaDevice SPI NAND was found.
[    0.517040] spi-nand hr_nand.0: 128 MiB, block size: 128 KiB, page size: 2048, OOB size: 64
[    0.519663] hobot_spi a5006000.spi: ver: HOBOT-spi_V20.200330 master
[    0.520706] libphy: Fixed MDIO Bus: probed
[    0.522007] st_gmac a5014000.ethernet: found phy-handle subnode
[    0.522842] st_gmac a5014000.ethernet: xj3_mtl_setup, plat->rx-queues-to-use:4, and tx:4
[    0.524028] st_gmac a5014000.ethernet: xj3_probe_config_dt, clk_ptp_rate:250000000
[    0.525030] set mac address 00:11:22:7c:3f:81:
[    0.525032] (using random mac adress)
[    0.526175] (NULL device *): xj3_get_hw_features, tx_fifo_size:16384
[    0.526992] (NULL device *): xj3_get_hw_features, rx_fifo_size:16384
[    0.527810] st_gmac a5014000.ethernet: TSO supported
[    0.528450] st_gmac a5014000.ethernet: TSO feature enabled
[    0.529156] st_gmac a5014000.ethernet: Enable Rx Mitigation via HW Watchdog Timer
[    0.650241] libphy: hobot-mac-mdio: probed
[    0.651827] st_gmac a5014000.ethernet: hobot_eth_probe: probe sucessfully
[    0.653024] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_0v8 not found, using dummy regulator
[    0.654266] dwc3-of-simple b2000000.usb: usb regulator 0v8 enable succeed
[    0.655143] dwc3-of-simple b2000000.usb: b2000000.usb supply usb_3v3 not found, using dummy regulator
[    0.656346] dwc3-of-simple b2000000.usb: usb regulator 3v3 enable succeed
[    0.657887] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    0.659543] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    0.660971] usbcore: registered new interface driver cdc_acm
[    0.661723] cdc_acm: USB Abstract Control Model driver for USB modems and ISDN adapters
[    0.662783] usbcore: registered new interface driver uas
[    0.663499] usbcore: registered new interface driver usb-storage
[    0.664326] usbcore: registered new interface driver usbserial
[    0.665101] usbcore: registered new interface driver usbserial_generic
[    0.665982] usbserial: USB Serial support registered for generic
[    0.666778] usbcore: registered new interface driver usb_serial_simple
[    0.667635] usbserial: USB Serial support registered for carelink
[    0.668436] usbserial: USB Serial support registered for zio
[    0.669181] usbserial: USB Serial support registered for funsoft
[    0.669991] usbserial: USB Serial support registered for flashloader
[    0.670827] usbserial: USB Serial support registered for google
[    0.671606] usbserial: USB Serial support registered for libtransistor
[    0.672462] usbserial: USB Serial support registered for vivopay
[    0.673268] usbserial: USB Serial support registered for moto_modem
[    0.674092] usbserial: USB Serial support registered for motorola_tetra
[    0.674959] usbserial: USB Serial support registered for novatel_gps
[    0.675796] usbserial: USB Serial support registered for hp4x
[    0.676555] usbserial: USB Serial support registered for suunto
[    0.677355] usbserial: USB Serial support registered for siemens_mpi
[    0.678202] usbcore: registered new interface driver rio500
[    0.679037] mousedev: PS/2 mouse device common for all mice
[    0.690091] hobot-rtc a6002000.rtc: rtc core: registered hobot-rtc as rtc0
[    0.691083] i2c /dev entries driver
[    0.691688] hobot-i2c a5009000.i2c: hobot i2c probe start
[    0.692455] hobot-i2c a5009000.i2c: round_rate:96000000
[    0.693133] hobot-i2c a5009000.i2c: I2C bus speed is 400000
[    0.693874] hobot-i2c a5009000.i2c: clkdiv = 0x1d
[    0.694482] hobot-i2c a5009000.i2c: i2c0 diag register....
[    0.695573] hobot-i2c a5009000.i2c: hobot_i2c_0 probe done
[    0.696374] hobot-i2c a500a000.i2c: hobot i2c probe start
[    0.697130] hobot-i2c a500a000.i2c: round_rate:96000000
[    0.697830] hobot-i2c a500a000.i2c: I2C bus speed is 400000
[    0.698548] hobot-i2c a500a000.i2c: clkdiv = 0x1d
[    0.699154] hobot-i2c a500a000.i2c: i2c1 diag register....
[    0.700169] hobot-i2c a500a000.i2c: hobot_i2c_1 probe done
[    0.701124] lirc_dev: IR Remote Control driver registered, major 239
[    0.701962] IR LIRC bridge handler initialized
[    0.702725] sif_mclk clock frequence is 544000000
[    0.703362] mipi_rx0_ipi clock frequence is 544000000
[    0.704050] mipi_rx1_ipi clock frequence is 544000000
[    0.704749] mipi_rx2_ipi clock frequence is 544000000
[    0.705479] mipi_rx3_ipi clock frequence is 544000000
[    0.706199] mipi_tx_ipi clock frequence is 544000000
[    0.706919] mipi_cfg_host clock frequence is 102000000
[    0.707672] pym_mclk clock frequence is 1188000000
[    0.708393] mipi_dev_ref clock frequence is 24000000
[    0.709147] mipi_host_ref clock frequence is 24000000
[    0.709941] sensor0_mclk clock frequence is 37125000
[    0.710718] sensor1_mclk clock frequence is 37125000
[    0.711507] sensor2_mclk clock frequence is 37125000
[    0.712308] sensor3_mclk clock frequence is 37125000
[    0.712948] [FRT:D] x3_ips_probe(0)
[    0.713974] hobot swinfo sel reg ro=0x1 boot dump
[    0.714884] pvt a1009000.pvt: SCRATCH test: 1234abcd, pvt is alive.
[    0.715805] pvt a1009000.pvt: VM Calibrated data detected
[    0.716986] hobot_wdt a1002000.watchdog: watchdog setting [pet:6s bark:11s bite:15s]
[    0.718328] hobot_wdt a1002000.watchdog: Hobot Watchdog Timer at ffffff8009db3000 with timeout 15s
[    0.719689] device-mapper: uevent: version 1.0.3
[    0.720452] device-mapper: ioctl: 4.37.0-ioctl (2017-09-20) initialised: dm-devel@redhat.com
[    0.721631] device-mapper: verity-avb: AVB error handler initialized with vbmeta device:
[    0.724053] Synopsys Designware Multimedia Card Interface Driver
[    0.725051] dwmmc_hobot a5010000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.725903] dwmmc_hobot a5010000.dwmmc: card-detect-delay not found.
[    0.726722] dwmmc_hobot a5010000.dwmmc: data-addr not found.
[    0.727761] mmc_host mmc0: card is non-removable.
[    0.770424] dwmmc_hobot a5011000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.773286] dwmmc_hobot a5011000.dwmmc: card-detect-delay not found.
[    0.775118] dwmmc_hobot a5011000.dwmmc: data-addr not found.
[    0.779892] dwmmc_hobot a5011000.dwmmc: mmc set to fixed voltage 1800
[    0.780957] mmc_host mmc1: card is non-removable.
[    0.877408] dwmmc_hobot a5012000.dwmmc: ver: HOBOT-mmc_V20.200402
[    0.878238] dwmmc_hobot a5012000.dwmmc: card-detect-delay not found.
[    0.879073] dwmmc_hobot a5012000.dwmmc: data-addr not found.
[    0.880042] dwmmc_hobot a5012000.dwmmc: Got CD GPIO
[    0.990955] mmc1: queuing unknown CIS tuple 0x80 (2 bytes)
[    0.993142] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.995337] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
[    0.998704] mmc1: queuing unknown CIS tuple 0x80 (7 bytes)
[    1.002657] mmc1: queuing unknown CIS tuple 0x81 (9 bytes)
[    1.069489] ledtrig-cpu: registered to indicate activity on CPUs
[    1.070342] hidraw: raw HID events driver (C) Jiri Kosina
[    1.071208] usbcore: registered new interface driver usbhid
[    1.071933] usbhid: USB HID core driver
[    1.072517] logger: created 256K log 'log_main'
[    1.073166] logger: created 256K log 'log_events'
[    1.073866] logger: created 256K log 'log_radio'
[    1.074523] logger: created 256K log 'log_system'
[    1.075565] set dmc devfreq governor to performance
[    1.076206] hobot_dmcfreq_target: dmcfreq->rate:2666000000, target_rate:2666000000
[    1.077185] buf:, powersave_rate:2666000000, dmcfreq->pre_state:0
[    1.084063] usbcore: registered new interface driver snd-usb-audio
[    1.085256] Netfilter messages via NETLINK v0.30.
[    1.085889] ip_set: protocol 6
[    1.086380] ipip: IPv4 and MPLS over IPv4 tunneling driver
[    1.087398] ip_tables: (C) 2000-2006 Netfilter Core Team
[    1.088404] arp_tables: arp_tables: (C) 2002 David S. Miller
[    1.089219] Initializing XFRM netlink socket
[    1.090083] NET: Registered protocol family 10
[    1.091301] Segment Routing with IPv6
[    1.091809] sit: IPv6, IPv4 and MPLS over IPv4 tunneling driver
[    1.092918] NET: Registered protocol family 17
[    1.093601] Key type dns_resolver registered
[    1.095212] Loading compiled-in X.509 certificates
[    1.098713] Loaded X.509 cert 'Build time autogenerated kernel key: 81cb0ef77db2fac76e9588c2120c82422367d268'
[    1.100043] zswap: loaded using pool lzo/zbud
[    1.111334] dwc3 b2000000.dwc3: Configuration mismatch. user dr_mode(otg) not equal with hardware default mode(peripheral). still use otg mode
[    1.112997] dwc3 b2000000.dwc3: found 6 IN and 3 OUT endpoints
[    1.114008] console [netcon0] enabled
[    1.114499] netconsole: network logging started
[    1.115279] hobot-rtc a6002000.rtc: setting system clock to 1970-01-01 00:00:00 UTC (0)
[    1.116466] vps mipi_dphy: probe with x3vio done
[    1.117166] hobot_wdt_test: wdt_test_init: wdt test init
[    1.119897] VCC_CNN0: disabling
[    1.120308] VCC_CNN1: disabling
[    1.121287] vps mipi_host0: ver 140* port0(0:0)
[    1.122213] vps mipi_host1: ver 140* port1(1:0)
[    1.123105] vps mipi_host2: ver 140* port2(0:1)
[    1.123892] vps mipi_host3: ver 140* port3(1:1)
[    1.124729] ALSA device list:
[    1.125114]   No soundcards found.
[    1.125785] md: Skipping autodetection of RAID arrays. (raid=autodetect will force)
[    1.126925] VFS: Cannot open root device "mmcblk2p2" or unknown-block(0,0): error -6
[    1.127919] Please append a correct "root=" boot option; here are the available partitions:
[    1.128993] 0100          102400 ram0
[    1.128995]  (driver?)
[    1.129805] 0101          102400 ram1
[    1.129807]  (driver?)
[    1.130596] 0102          102400 ram2
[    1.130598]  (driver?)
[    1.131386] 0103          102400 ram3
[    1.131387]  (driver?)
[    1.132176] 0104          102400 ram4
[    1.132177]  (driver?)
[    1.132965] 0105          102400 ram5
[    1.132967]  (driver?)
[    1.133819] 0106          102400 ram6
[    1.133821]  (driver?)
[    1.134610] 0107          102400 ram7
[    1.134612]  (driver?)
[    1.135400] 0108          102400 ram8
[    1.135402]  (driver?)
[    1.136190] 0109          102400 ram9
[    1.136191]  (driver?)
[    1.136979] 010a          102400 ram10
[    1.136981]  (driver?)
[    1.137829] 010b          102400 ram11
[    1.137831]  (driver?)
[    1.138631] 010c          102400 ram12
[    1.138633]  (driver?)
[    1.139432] 010d          102400 ram13
[    1.139434]  (driver?)
[    1.140233] 010e          102400 ram14
[    1.140235]  (driver?)
[    1.141034] 010f          102400 ram15
[    1.141036]  (driver?)
[    1.141857] 1f00          131072 mtdblock0
[    1.141859]  (driver?)
[    1.142703] hobot_fusa: set_fusa_error_pin:75 set error pin to 1
[    1.143473] hobot_fusa: fusa errpin not ready
[    1.143477] Kernel panic - not syncing: VFS: Unable to mount root fs on unknown-block(0,0)
[    1.145096] Kernel Offset: disabled
[    1.145547] CPU features: 0x0002004
[    1.145996] Memory Limit: none
[    1.150550] Rebooting in 1 seconds..
[    1.221448] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.222170] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 1
[    1.223625] xhci-hcd xhci-hcd.0.auto: hcc params 0x0220fe6d hci version 0x110 quirks 0x0000000000010010
[    1.224858] xhci-hcd xhci-hcd.0.auto: irq 178, io mem 0xb2000000
[    1.225831] usb usb1: New USB device found, idVendor=1d6b, idProduct=0002, bcdDevice= 4.14
[    1.226894] usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.227823] usb usb1: Product: xHCI Host Controller
[    1.228451] usb usb1: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.229158] usb usb1: SerialNumber: xhci-hcd.0.auto
[    1.230105] hub 1-0:1.0: USB hub found
[    1.230607] hub 1-0:1.0: 1 port detected
[    1.231298] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    1.232011] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 2
[    1.233000] xhci-hcd xhci-hcd.0.auto: Host supports USB 3.0 SuperSpeed
[    1.233886] usb usb2: We don't know the algorithms for LPM for this host, disabling LPM.
[    1.234992] usb usb2: New USB device found, idVendor=1d6b, idProduct=0003, bcdDevice= 4.14
[    1.236055] usb usb2: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.236983] usb usb2: Product: xHCI Host Controller
[    1.237621] usb usb2: Manufacturer: Linux 4.14.87 xhci-hcd
[    1.238328] usb usb2: SerialNumber: xhci-hcd.0.auto
[    1.239227] hub 2-0:1.0: USB hub found
[    1.239727] hub 2-0:1.0: 1 port detected
[    1.485209] usb 1-1: new high-speed USB device number 2 using xhci-hcd
[    1.633394] usb 1-1: New USB device found, idVendor=1a40, idProduct=0101, bcdDevice= 1.11
[    1.634446] usb 1-1: New USB device strings: Mfr=0, Product=1, SerialNumber=0
[    1.635363] usb 1-1: Product: USB 2.0 Hub
[    1.682054] hub 1-1:1.0: USB hub found
[    1.682571] hub 1-1:1.0: 4 ports detected
[    2.069213] mmc2: new UHS SDR104 SDHC card at address 0001
[    2.070232] mmcblk2: mmc2:0001 SD16G 29.8 GiB
[    2.071847]  mmcblk2: p1 p2
[    2.151061] SMP: stopping secondary CPUs
[    2.151569] psci: psci_sys_reset(reboot_mode=0)
NOTICE:  fast_boot:0

S
F
L
O
NOTICE:  efuse cpu_cfg = 0
W
NOTICE:  Booting Trusted Firmware
NOTICE:  BL1: v1.4(release):HR-ROM-Rel-v1.1-141-ga91d4dd-dirty
NOTICE:  BL1: Built : 11:24:44, Oct 23 2019
NOTICE:  boot src: 2
NOTICE:  GigaDev SPI NAND was found.
NOTICE:  Block size: 128 KiB, page size: 2048
NOTICE:  BL1: Booting BL2
Auth pass
NOTICE:  bl1_main exit
SPL normal reset flow
check_reset_state (2): wakeup address = 0x0, hw wakeup status = 0x3, wakeup src=0x100
patch for sys_pll 1200 with 100M eth
SFLOW_INIT
CHIP ID:PCB941/WAFER: W04/ X: X20/ Y: Y36
secondary_jump_to_spl: secure chip flow
X3 SPL : secondary core wake up and jump to spl done (cpu_core_cfg=0)
SFLOW_FIN_HW_A

U-Boot SPL 2018.09-g4ca851534c-dirty (May 11 2022 - 20:09:50 +0800)
SPACC Init - ID: (00000061)
SPL nand boot mode (from strap)
GigaDev SPI NAND was found.
Block size: 128 KiB, page size: 2048
ddr_type = 1 (LPDDR4)
hb_chip_package_type:3
load ddr header src_addr: 100000, load_addr: 802ca020, src_len: a00
find valid ddr image
ddr_hdr.ecc_gran: 0x0
ddr_hdr.ecc_map: 0x0
ddr_hdr.sbr_pattern0: 0x0
ddr_hdr.sbr_pattern1: 0x0
ddr_freq = 05
board id = 31540334
ddr datarate: 3200
### SAMSUNG DDR ###
no ddr pin set
detect part number: 108
detect ddr freq: c80
board id alternative:0x3
index is 12
index is 15
index is 19
hb_ddr_index: 19
ddr_type = 1, ddr_vendor=3, ddr_freq=3200
dram_pll_init
sscg disabled
control load ddrc src_addr: 15ae00, load_addr: 802caa20, src_len: 920
[DDR INFO]      ==ddr_release_info==
[DDR INFO]      VERSION:        develop
[DDR INFO]      BUILD:          2022-05-11-20:09
[DDR INFO]      GIT COMMIT:     4ca851534c1616ace920fdaa000c6fb717c1fb74
[DDR INFO]      GIT TIME:       Wed, 20 Apr 2022 18:28:49 +0800
[DDR INFO]      ==ddr_features==
[DDR INFO]      RDBI:           0
[DDR INFO]      WDBI:           1
[DDR INFO]      InlineECC:      0
[DDR INFO]      DM:             1
[DDR INFO]      DDC:            1
[DDR INFO]      SSCG:           0
[DDR INFO]      BOARD:          XS_ENABLE
[DDR INFO] ddr_controller_cfg done
load ddr phy src_addr: 15b800, load_addr: 802caa20, src_len: 420
ATxSlewRate     : 15f
ATxImpedance    : 7f
TxSlewRate      : 19f
TxOdtDrvStren   : 600
TxImpedanceCtrl : e3f
CalDrvStr0      : 11
VrefInGlobal    : 104
board_type = 4 (CUSTOMER_BOARD)
load dqmap src addr: 15d600, load_addr: 802caa20, src_len: 20
[DDR INFO] dwc_ddrphy_train start
magic = 544f4248
load imem1 src_addr: 11ce00, load_addr: 802caa20, src_len: 8000
load dmem1 src_addr: 15a000, load_addr: 802caa20, src_len: 684
executing 1D fw
load imem2 src_addr: 124e00, load_addr: 802caa20, src_len: 8000
load dmem2 src_addr: 15a800, load_addr: 802caa20, src_len: 564

*******************************************************
p_dmem_lpddr4_2d_16b->MR11_A0:54
p_dmem_lpddr4_2d_16b->MR14_A0:54
p_dmem_lpddr4_2d_16b->MR12_A0:51
p_dmem_lpddr4_2d_16b->MR22_A0:14

p_dmem_lpddr4_2d_16b->MR3_A0:b3
p_dmem_lpddr4_2d_16b->Reserved00:40
p_dmem_lpddr4_2d_16b->Reserved0E:4
p_dmem_lpddr4_2d_16b->Delay_Weight2D:20
p_dmem_lpddr4_2d_16b->Voltage_Weight2D:80
*******************************************************

executing 2D fw
load pie src_addr: 15be00, load_addr: 802caa20, src_len: 11f0
Set QoS.
get_ddr_mr_info:cs_num=1, mr5=0x1, mr8=0x10
no magic in efuse file,bypass efuse
total_sz = 4096
SPL_VERSION:7
uboot partition is uboot_A
load u-boot: src_addr=0x380000, dest_addr=0x4000000, len=2097152